**COMMITTEE DRAFT AMENDMENT****© ISO/IEC 2020 – All rights reserved****Text of ISO/IEC 23008-2:201x/CDAM 2** **63****Part 2: High efficiency video coding, AMENDMENT 2: Additional supplemental enhancement information****Information technology — High efficiency coding and media delivery in heterogeneous environments****Élément introductif — Élément central — Partie 2: Titre de la partie****Information technology — High efficiency coding and media delivery in heterogeneous environments — Part 2: High efficiency video coding, AMENDMENT 2: Additional supplemental enhancement information****E****2020-01-17****(30) Committee****ISO/IEC****ISO/IEC J****201x****2****Amendment****International Standard****201x****19121****ISO/IEC 23008‑****ISO/IEC 23008‑2****ISO/IEC 23008-2:201x/CDAM 2****JISC****Coding of audio, picture, multimedia and hypermedia information****Information technology****11****29****1** **2****見出し 2****見出し 1****0****2****STD Version 2.1c2****30** **4** **ISO/IEC JTC 1/SC 29 /WG 11 N 19121**

Date: **2020-01-17**

**Text of ISO/IEC 23008-2:201x/CDAM 2**

ISO/IEC JTC 1/SC 29/WG 11

Secretariat:  JISC

**Information technology — High efficiency coding and media delivery in heterogeneous environments — Part 2: High efficiency video coding, AMENDMENT 2: Additional supplemental enhancement information**

*Élément introductif — Élément central — Partie 2: Titre de la partie*

|  |
| --- |
| **Warning**  This document is not an ISO International Standard. It is distributed for review and comment. It is subject to change without notice and may not be referred to as an International Standard.  Recipients of this draft are invited to submit, with their comments, notification of any relevant patent rights of which they are aware and to provide supporting documentation |

**Copyright notice**

This ISO document is a working draft or committee draft and is copyright-protected by ISO. While the reproduction of working drafts or committee drafts in any form for use by participants in the ISO standards development process is permitted without prior permission from ISO, neither this document nor any extract from it may be reproduced, stored or transmitted in any form for any other purpose without prior written permission from ISO.

Requests for permission to reproduce this document for the purpose of selling it should be addressed as shown below or to ISO's member body in the country of the requester:

[Indicate the full address, telephone number, fax number, telex number, and electronic mail address, as appropriate, of the Copyright Manger of the ISO member body responsible for the secretariat of the TC or SC within the framework of which the working document has been prepared.]

Reproduction for sales purposes may be subject to royalty payments or a licensing agreement.

Violators may be prosecuted.

Foreword

ISO (the International Organization for Standardization) and IEC (the International Electrotechnical Commission) form the specialized system for worldwide standardization. National bodies that are members of ISO or IEC participate in the development of International Standards through technical committees established by the respective organization to deal with particular fields of technical activity. ISO and IEC technical committees collaborate in fields of mutual interest. Other international organizations, governmental and non-governmental, in liaison with ISO and IEC, also take part in the work. In the field of information technology, ISO and IEC have established a joint technical committee, ISO/IEC JTC 1. In some areas of information technology which fall within the purview of ISO and IEC, the necessary standards are prepared on a collaborative basis with ITU-T.

International Standards are drafted in accordance with the rules given in the ISO/IEC Directives, Part 2.

The main task of the joint technical committee is to prepare International Standards. Draft International Standards adopted by the joint technical committee are circulated to national bodies for voting. Publication as an International Standard requires approval by at least 75 % of the national bodies casting a vote.

Attention is drawn to the possibility that some of the elements of this document may be the subject of patent rights. ISO and IEC shall not be held responsible for identifying any or all such patent rights.

Amendment 2 to ISO/IEC 23008-2:201x was prepared by Joint Technical Committee ISO/IEC JTC 1, *Coding of audio, picture, multimedia and hypermedia information*, Subcommittee SC 29, *Coding of moving pictures and audio*, in a joint collaboration with ITU-T Study Group 16. Technically aligned twin text is developed as Recommendation ITU-T H.265.

Information technology — High efficiency coding and media delivery in heterogeneous environments — Part 2: High efficiency video coding, AMENDMENT 2: Additional supplemental enhancement information

*Clause 4*

*Add an abbreviation to clause 4, as follows:*

ATSC Advanced Television Systems Committee

*D.2.1*

*Replace the contents of D.2.1 with the following:*

**D.2.1 General SEI message syntax**

|  |  |
| --- | --- |
| sei\_payload( payloadType, payloadSize ) { | **Descriptor** |
| if( nal\_unit\_type = = PREFIX\_SEI\_NUT ) |  |
| if( payloadType = = 0 ) |  |
| buffering\_period( payloadSize ) |  |
| else if( payloadType = = 1 ) |  |
| pic\_timing( payloadSize ) |  |
| else if( payloadType = = 2 ) |  |
| pan\_scan\_rect( payloadSize ) |  |
| else if( payloadType = = 3 ) |  |
| filler\_payload( payloadSize ) |  |
| else if( payloadType = = 4 ) |  |
| user\_data\_registered\_itu\_t\_t35( payloadSize ) |  |
| else if( payloadType = = 5 ) |  |
| user\_data\_unregistered( payloadSize ) |  |
| else if( payloadType = = 6 ) |  |
| recovery\_point( payloadSize ) |  |
| else if( payloadType = = 9 ) |  |
| scene\_info( payloadSize ) |  |
| else if( payloadType = = 15 ) |  |
| picture\_snapshot( payloadSize ) |  |
| else if( payloadType = = 16 ) |  |
| progressive\_refinement\_segment\_start( payloadSize ) |  |
| else if( payloadType = = 17 ) |  |
| progressive\_refinement\_segment\_end( payloadSize ) |  |
| else if( payloadType = = 19 ) |  |
| film\_grain\_characteristics( payloadSize ) |  |
| else if( payloadType = = 22 ) |  |
| post\_filter\_hint( payloadSize ) |  |
| else if( payloadType = = 23 ) |  |
| tone\_mapping\_info( payloadSize ) |  |
| else if( payloadType = = 45 ) |  |
| frame\_packing\_arrangement( payloadSize ) |  |
| else if( payloadType = = 47 ) |  |
| display\_orientation( payloadSize ) |  |
| else if( payloadType = = 56 ) |  |
| green\_metadata( payloadsize ) /\* specified in ISO/IEC 23001-11 \*/ |  |
| else if( payloadType = = 128 ) |  |
| structure\_of\_pictures\_info( payloadSize ) |  |
| else if( payloadType = = 129 ) |  |
| active\_parameter\_sets( payloadSize ) |  |
| else if( payloadType = = 130 ) |  |
| decoding\_unit\_info( payloadSize ) |  |
| else if( payloadType = = 131 ) |  |
| temporal\_sub\_layer\_zero\_idx( payloadSize ) |  |
| else if( payloadType = = 133 ) |  |
| scalable\_nesting( payloadSize ) |  |
| else if( payloadType = = 134 ) |  |
| region\_refresh\_info( payloadSize ) |  |
| else if( payloadType = = 135 ) |  |
| no\_display( payloadSize ) |  |
| else if( payloadType = = 136 ) |  |
| time\_code( payloadSize ) |  |
| else if( payloadType = = 137 ) |  |
| mastering\_display\_colour\_volume( payloadSize ) |  |
| else if( payloadType = = 138 ) |  |
| segmented\_rect\_frame\_packing\_arrangement( payloadSize ) |  |
| else if( payloadType = = 139 ) |  |
| temporal\_motion\_constrained\_tile\_sets( payloadSize ) |  |
| else if( payloadType = = 140 ) |  |
| chroma\_resampling\_filter\_hint( payloadSize ) |  |
| else if( payloadType = = 141 ) |  |
| knee\_function\_info( payloadSize ) |  |
| else if( payloadType = = 142 ) |  |
| colour\_remapping\_info( payloadSize ) |  |
| else if( payloadType = = 143 ) |  |
| deinterlaced\_field\_identification( payloadSize ) |  |
| else if( payloadType = = 144 ) |  |
| content\_light\_level\_info( payloadSize ) |  |
| else if( payloadType = = 145 ) |  |
| dependent\_rap\_indication( payloadSize ) |  |
| else if( payloadType = = 146 ) |  |
| coded\_region\_completion( payloadSize ) |  |
| else if( payloadType = = 147 ) |  |
| alternative\_transfer\_characteristics( payloadSize ) |  |
| else if( payloadType = = 148 ) |  |
| ambient\_viewing\_environment( payloadSize ) |  |
| else if( payloadType  = =  149 ) |  |
| content\_colour\_volume( payloadSize ) |  |
| else if( payloadType  = =  150 ) |  |
| equirectangular\_projection( payloadSize ) |  |
| else if( payloadType  = =  151 ) |  |
| cubemap\_projection( payloadSize ) |  |
| else if( payloadType  = =  152 ) |  |
| fisheye\_video\_info( payloadSize ) |  |
| else if( payloadType  = =  154 ) |  |
| sphere\_rotation( payloadSize ) |  |
| else if( payloadType  = =  155 ) |  |
| regionwise\_packing( payloadSize ) |  |
| else if( payloadType  = =  156 ) |  |
| omni\_viewport( payloadSize ) |  |
| else if( payloadType  = =  157 ) |  |
| regional\_nesting( payloadSize ) |  |
| else if( payloadType  = =  158 ) |  |
| mcts\_extraction\_info\_sets( payloadSize ) |  |
| else if( payloadType  = =  159 ) |  |
| mcts\_extraction\_info\_nesting( payloadSize ) |  |
| else if( payloadType = = 160 ) |  |
| layers\_not\_present( payloadSize ) /\* specified in Annex F \*/ |  |
| else if( payloadType = = 161 ) |  |
| inter\_layer\_constrained\_tile\_sets( payloadSize ) /\* specified in Annex F \*/ |  |
| else if( payloadType = = 162 ) |  |
| bsp\_nesting( payloadSize ) /\* specified in Annex F \*/ |  |
| else if( payloadType = = 163 ) |  |
| bsp\_initial\_arrival\_time( payloadSize ) /\* specified in Annex F \*/ |  |
| else if( payloadType = = 164 ) |  |
| sub\_bitstream\_property( payloadSize ) /\* specified in Annex F \*/ |  |
| else if( payloadType = = 165 ) |  |
| alpha\_channel\_info( payloadSize ) /\* specified in Annex F \*/ |  |
| else if( payloadType = = 166 ) |  |
| overlay\_info( payloadSize ) /\* specified in Annex F \*/ |  |
| else if( payloadType = = 167 ) |  |
| temporal\_mv\_prediction\_constraints( payloadSize ) /\* specified in Annex F \*/ |  |
| else if( payloadType = = 168 ) |  |
| frame\_field\_info( payloadSize ) /\* specified in Annex F \*/ |  |
| else if( payloadType = = 176 ) |  |
| three\_dimensional\_reference\_displays\_info( payloadSize ) /\* specified in Annex G \*/ |  |
| else if( payloadType = = 177 ) |  |
| depth\_representation\_info( payloadSize ) /\* specified in Annex G \*/ |  |
| else if( payloadType = = 178 ) |  |
| multiview\_scene\_info( payloadSize ) /\* specified in Annex G \*/ |  |
| else if( payloadType = = 179 ) |  |
| multiview\_acquisition\_info( payloadSize ) /\* specified in Annex G \*/ |  |
| else if( payloadType = = 180 ) |  |
| multiview\_view\_position( payloadSize ) /\* specified in Annex G \*/ |  |
| else if( payloadType = = 181 ) |  |
| alternative\_depth\_info( payloadSize ) /\* specified in Annex I \*/ |  |
| else if( payloadType = = 200 ) |  |
| sei\_manifest( payloadSize ) |  |
| else if( payloadType = = 201 ) |  |
| sei\_prefix\_indication( payloadSize ) |  |
| else if( payloadType  = =  202 ) |  |
| annotated\_regions( payloadSize ) |  |
| else if( payloadType = = 203 ) |  |
| shutter\_interval\_info( payloadSize ) |  |
| else |  |
| reserved\_sei\_message( payloadSize ) |  |
| else /\* nal\_unit\_type = = SUFFIX\_SEI\_NUT \*/ |  |
| if( payloadType = = 3 ) |  |
| filler\_payload( payloadSize ) |  |
| else if( payloadType = = 4 ) |  |
| user\_data\_registered\_itu\_t\_t35( payloadSize ) |  |
| else if( payloadType = = 5 ) |  |
| user\_data\_unregistered( payloadSize ) |  |
| else if( payloadType = = 17 ) |  |
| progressive\_refinement\_segment\_end( payloadSize ) |  |
| else if( payloadType = = 22 ) |  |
| post\_filter\_hint( payloadSize ) |  |
| else if( payloadType = = 132 ) |  |
| decoded\_picture\_hash( payloadSize ) |  |
| else if( payloadType = = 146 ) |  |
| coded\_region\_completion( payloadSize ) |  |
| else |  |
| reserved\_sei\_message( payloadSize ) |  |
| if( more\_data\_in\_payload( ) ) { |  |
| if( payload\_extension\_present( ) ) |  |
| **reserved\_payload\_extension\_data** | u(v) |
| **payload\_bit\_equal\_to\_one** /\* equal to 1 \*/ | f(1) |
| while( !byte\_aligned( ) ) |  |
| **payload\_bit\_equal\_to\_zero** /\* equal to 0 \*/ | f(1) |
| } |  |
| } |  |

*D.2.48*

*Renumber subclause D.2.48 (Reserved SEI message syntax) as D.2.49.*

*D.2.48*

*Add a new subclause D.2.48, as follows:*

**D.2.48 Shutter interval information SEI message syntax**

|  |  |
| --- | --- |
| shutter\_interval\_info( payloadSize ) { | **Descriptor** |
| **sii\_time\_scale** | u(32) |
| **fixed\_shutter\_interval\_within\_clvs\_flag** | u(1) |
| if( fixed\_shutter\_interval\_within\_clvs\_flag ) |  |
| **sii\_num\_units\_in\_shutter\_interval** | u(32) |
| else { |  |
| **sii\_max\_sub\_layers\_minus1** | u(3) |
| for( i = 0; i <= sii\_max\_sub\_layers\_minus1; i++ ) |  |
| **sub\_layer\_num\_units\_in\_shutter\_interval**[ i ] | u(32) |
| } |  |
| } |  |

*D.3.1*

*In D.3.1, replace the following paragraphs:*

The list SingleLayerSeiList is set to consist of the payloadType values 3, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 129, 131, 132, 134 to 152, inclusive, 154 to 159, inclusive, and 200 to 202, inclusive.

The list VclAssociatedSeiList is set to consist of the payloadType values 2, 3, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 131, 132, 134 to 152, inclusive, 154 to 159, inclusive, and 200 to 202, inclusive.

The list PicUnitRepConSeiList is set to consist of the payloadType values 0, 1, 2, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 129, 131, 132, 133, 135 to 152, inclusive, 154 to 159, inclusive, and 200 to 202, inclusive.

*with the following:*

The list SingleLayerSeiList is set to consist of the payloadType values 3, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 129, 131, 132, 134 to 152, inclusive, 154 to 159, inclusive, and 200 to 203, inclusive.

The list VclAssociatedSeiList is set to consist of the payloadType values 2, 3, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 131, 132, 134 to 152, inclusive, 154 to 159, inclusive, and 200 to 203, inclusive.

The list PicUnitRepConSeiList is set to consist of the payloadType values 0, 1, 2, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 129, 131, 132, 133, 135 to 152, inclusive, 154 to 159, inclusive, and 200 to 203, inclusive.

*D.3.1*

*In subclause D.3.1, in Table D.1, append the following row to the end of the table:*

|  |  |
| --- | --- |
| Shutter interval information | The CLVS containing the SEI message |

*D.3.48*

*Add new subclause D.3.48, as follows:*

**D.3.48 Shutter interval information SEI message syntax**

The shutter interval information SEI message indicates the shutter interval for the associated video source pictures prior to encoding and display, e.g., for camera-captured content, the shutter interval is amount of time that an image sensor is exposed to produce each source picture.

When a shutter interval information SEI message is present for any picture of a CLVS of a particular layer, a shutter interval information SEI message shall be present for the first picture of the CLVS. The shutter interval information SEI message persists for the current layer in decoding order from the current picture until the end of the CLVS. All shutter interval information SEI messages that apply to the same CLVS shall have the same content.

**sii\_time\_scale** specifies the number of time units that pass in one second. The value of sii\_time\_scale shall be greater than 0. For example, a time coordinate system that measures time using a 27 MHz clock has an sii\_time\_scale of 27 000 000.

**fixed\_shutter\_interval\_within\_clvs\_flag** equal to 1 specifies that the indicated shutter interval is the same for all temporal sub-layers in the CLVS. fixed\_shutter\_interval\_within\_clvs\_flagequal to 0 specifies that the indicated shutter interval may not be the same for all temporal sub-layers in the CLVS. When the value of sps\_max\_sub\_layers\_minus1 is equal to 0, the value of fixed\_shutter\_interval\_within\_clvs\_flag shall be equal to 1.

**sii\_num\_units\_in\_shutter\_interval**, when fixed\_shutter\_interval\_within\_clvs\_flag is equal to 1, specifies the number of time units of a clock operating at the frequency sii\_time\_scale Hz that corresponds to the indicated shutter interval of each picture in the CLVS. The value 0 may be used to indicate that the associated video content contains screen capture content, computer generated content, or other non-camera-captured content.

The indicated shutter interval, denoted by the variable shutterInterval, in units of seconds, is equal to the quotient of sii\_num\_units\_in\_shutter\_interval divided by sii\_time\_scale. For example, to represent a shutter interval equal to 0.04 seconds, sii\_time\_scale may be equal to 27 000 000 and sii\_num\_units\_in\_shutter\_interval may be equal to 1 080 000.

**sii\_max\_sub\_layers\_minus1** plus 1 specifies the maximum number of temporal sub-layers that may be present in each CLVS referring to the SPS. The value of sii\_max\_sub\_layers\_minus1 shall be equal to the value of sps\_max\_sub\_layers\_minus1 in the SPS.

NOTE – For example, the information conveyed in this SEI message is intended to be adequate for purposes corresponding to the use of ATSC A/341:2019 Annex D when sii\_max\_sub\_layers\_minus1 is equal to 1 and fixed\_shutter\_interval\_within\_clvs\_flag is equal to 0.

**sub\_layer\_num\_units\_in\_shutter\_interval**[ i ], when present, specifies the number of time units of a clock operating at the frequency sii\_time\_scale Hz that corresponds to the shutter interval of each picture in the sub-layer representation with TemporalId equal to i in the CLVS. The sub-layer shutter interval for the sub-layer representation with TemporalId equal to i, denoted by the variable subLayerShutterInterval[ i ], in units of seconds, is equal to the quotient of sub\_layer\_num\_units\_in\_shutter\_interval[ i ] divided by sii\_time\_scale.

The variable subLayerShutterInterval[ i ], corresponding to the indicated shutter interval of each picture in the sub-layer representation with TemporalId equal to i in the CLVS, is thus derived as follows:

if( fixed\_shutter\_interval\_within\_clvs\_flag )  
 subLayerShutterInterval[ i ] = sii\_num\_units\_in\_shutter\_interval ÷ sii\_time\_scale (D.X)  
else  
 subLayerShutterInterval[ i ] = sub\_layer\_num\_units\_in\_shutter\_interval[ i ] ÷ sii\_time\_scale

*F.14.3.1*

*In F.14.3.1 (General SEI payload semantics), replace the following paragraphs:*

The list VclAssociatedSeiList is set to consist of the payloadType values 2, 3, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 131, 132, 134 to 152, inclusive, 154 to 159, inclusive, 161, 165, 167, 168, and 200 to 202, inclusive.

The list PicUnitRepConSeiList is set to consist of the payloadType values 0, 1, 2, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 129, 131, 132, 133, 135 to 152, inclusive, 154 to 168, inclusive, and 200 to 202, inclusive.

*with the following:*

The list VclAssociatedSeiList is set to consist of the payloadType values 2, 3, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 131, 132, 134 to 152, inclusive, 154 to 159, inclusive, 161, 165, 167, 168, and 200 to 203, inclusive.

The list PicUnitRepConSeiList is set to consist of the payloadType values 0, 1, 2, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 129, 131, 132, 133, 135 to 152, inclusive, 154 to 168, inclusive, and 200 to 203, inclusive.

*G.14.3.1*

*In G.14.3.1 (General SEI payload semantics), replace the following paragraphs:*

The list VclAssociatedSeiList is set to consist of payloadType values 2, 3, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 131, 132, 134 to 152, inclusive, 154 to 159, inclusive, 161, 165, 167, 168, 177, 178, 179, and 200 to 202, inclusive.

The list PicUnitRepConSeiList is set to consist of payloadType values 0, 1, 2, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 129, 131, 132, 133, 135 to 152, inclusive, 154 to 168, inclusive, 176 to 180, inclusive, and 200 to 202, inclusive.

*with the following:*

The list VclAssociatedSeiList is set to consist of payloadType values 2, 3, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 131, 132, 134 to 152, inclusive, 154 to 159, inclusive, 161, 165, 167, 168, 177, 178, 179, and 200 to 203, inclusive.

The list PicUnitRepConSeiList is set to consist of payloadType values 0, 1, 2, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 129, 131, 132, 133, 135 to 152, inclusive, 154 to 168, inclusive, 176 to 180, inclusive, and 200 to 203, inclusive.

*I.14.3.1*

*In I.14.3.1 (General SEI payload semantics), replace the following paragraphs:*

The list VclAssociatedSeiList is set to consist of payloadType values 2, 3, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 131, 132, 134 to 152, inclusive, 154 to 159, inclusive, 161, 165, 167, 168, 177, 178, 179, and 200 to 202, inclusive.

The list PicUnitRepConSeiList is set to consist of payloadType values 0, 1, 2, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 129, 131, 132, 133, 135 to 152, inclusive, 154 to 168, inclusive, 176 to 181, inclusive, and 200 to 202, inclusive.

*with the following:*

The list VclAssociatedSeiList is set to consist of payloadType values 2, 3, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 131, 132, 134 to 152, inclusive, 154 to 159, inclusive, 161, 165, 167, 168, 177, 178, 179, and 200 to 203, inclusive.

The list PicUnitRepConSeiList is set to consist of payloadType values 0, 1, 2, 6, 9, 15, 16, 17, 19, 22, 23, 45, 47, 56, 128, 129, 131, 132, 133, 135 to 152, inclusive, 154 to 168, inclusive, 176 to 181, inclusive, and 200 to 203, inclusive.

*Bibliography*

*Add the following additional entry to the Bibliography (replacing “xx” with the appropriate bibliography entry number):*

[xx]     ATSC A/341 (2019), *Video – HEVC*

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_