**ISO/IEC JTC 1/SC 29/WG 03 N0777**

**ISO/IEC JTC 1/SC 29/WG 03  
MPEG Systems   
Convenorship: KATS (Korea, Republic of)**

**Document type:** Output Document

**Title:** Technologies under Consideration for ISO/IEC 23090-6

**Status:** Approved

**Date of document:** 2023-01-23

**Source:** ISO/IEC JTC 1/SC 29/WG 03

**No. of pages:** 4 (with cover page)

**Email of Convenor:** young.L@samsung.com

**Committee URL:** <https://isotc.iso.org/livelink/livelink/open/jtc1sc29wg3>

**INTERNATIONAL ORGANIZATION FOR STANDARDIZATION**

**ORGANISATION INTERNATIONALE DE NORMALISATION**

**ISO/IEC JTC 1/SC 29/WG 03 MPEG SYSTEMS**

**ISO/IEC JTC 1/SC 29/WG 03 N0777**

**January 2023, Online**

|  |  |
| --- | --- |
| **Title** | **Technologies under Consideration for ISO/IEC 23090-6** |
| **Source** | **WG 03, MPEG Systems** |
| **Status** | **Approved** |
| **Serial Number** | **22301** |

# Introduction

This document includes technologies under consideration for 23090-6 (Metrics)

This includes the following:

1. Viewpoint mismatch duration metric (m56832)

# Viewpoint Mismatch Duration Metric

It is asserted that, V3C/OMAFv2 Content could be shown from a different viewpoint (viewer perspective) than its corresponding “content-viewpoint” (e.g. outside the indicated viewing space) even when no viewpoint switching occurs. A metric showing how long this situation persists would be useful as a perceived quality indicator.

A new metric is proposed (m56832) to show the duration that content is shown for a different viewpoint (viewer perspective) that that corresponding “content-viewpoint” (e.g. outside the indicated viewing space).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Key** | | | **Type** | **Description** |
| ViewpointMismatchDuration | | | List | List of Viewpoint mismatch durations. |
|  | *Entry* | | Object | An entry for a Viewpoint mismatch duration. |
|  |  | t | Real-Time | Specifies the measurement time of the viewpoint mismatch duration in wall-clock time. |
|  |  | DeltaViewpoint | ViewpointMismatchType | Delta of the viewpoint between the user position and the viewpoint used for content generation |
|  |  | duration | Integer | Specifies the duration in milliseconds for which the user shows content with a mismatch of the real viewpoint corresponding to the shown content and the viewpoint used for rendering. |

With

|  |  |  |  |
| --- | --- | --- | --- |
| **Key** | | **Type** | **Description** |
| ViewpointMismatchType | | Object | Viewpoint Mismatch. |
|  | vp\_diff\_x | Float | Indicates the difference in x coordinate of the position of the viewpoint in centimetres in the global reference coordinate system, as defined in clause 9.2.2.2 of ISO/IEC 23090-10 compared to the center viewpoint of the corresponding viewport\_id. The values shall be expressed in 32-bit binary floating-point format with the 4 bytes in big-endian order and with the parsing process as specified in IEEE 754. |
|  | vp\_diff\_y | Float | Indicates the difference in y coordinate of the position of the viewpoint in centimetres in the global reference coordinate system, as defined in clause 9.2.2.2 of ISO/IEC 23090-10 compared to the center viewpoint of the corresponding viewport\_id. The values shall be expressed in 32-bit binary floating-point format with the 4 bytes in big-endian order and with the parsing process as specified in IEEE 754. |
|  | vp\_diff\_z | Float | Indicates the difference in z coordinate of the position of the viewpoint in centimetres in the global reference coordinate system, as defined in clause 9.2.2.2 of ISO/IEC 23090-10 compared to the center viewpoint of the corresponding viewport\_id. The values shall be expressed in 32-bit binary floating-point format with the 4 bytes in big-endian order and with the parsing process as specified in IEEE 754. |

----