ISO/IEC JTC 1/SC 29 N

Date: 2024-01

DIS 14496-12:202x(E)

ISO/IEC JTC 1/SC 29/WG 11

Secretariat: JISC

Information technology — Coding of audio-visual objects — Part 12: ISO base media file format

*Technologies de l'information — Codage des objets audiovisuels — Partie 12: Format ISO de base pour les fichiers médias*

**Copyright notice**

This ISO document is a working draft or committee draft and is copyright-protected by ISO. While the reproduction of working drafts or committee drafts in any form for use by participants in the ISO standards development process is permitted without prior permission from ISO, neither this document nor any extract from it may be reproduced, stored or transmitted in any form for any other purpose without prior written permission from ISO.

Requests for permission to reproduce this document for the purpose of selling it should be addressed as shown below or to ISO's member body in the country of the requester:

[Indicate the full address, telephone number, fax number, telex number, and electronic mail address, as appropriate, of the Copyright Manger of the ISO member body responsible for the secretariat of the TC or SC within the framework of which the working document has been prepared.]

Reproduction for sales purposes may be subject to royalty payments or a licensing agreement.

Violators may be prosecuted.

Contents Page

1 Scope 1

2 Normative references 1

3 Terms, definitions and abbreviated terms 2

3.1 Terms and definitions 2

3.2 Abbreviated terms 9

4 Object-structured file organization 10

4.1 File structure 10

4.2 Object structure 10

4.3 File-type box 14

4.4 Extended type box 15

5 Void 16

6 ISO base media file organization 16

6.1 Files, segments, and streams 16

6.2 Presentation structure 16

6.2.1 Object structure of a presentation 16

6.2.2 Meta data and media data 17

6.2.3 Data offsets 17

6.3 Structure-data (objects) 18

6.3.1 Box 18

6.3.2 Data types and fields 18

6.3.3 URIs as type indicators 20

6.3.4 Box order 20

6.4 Time structure overview 25

6.5 Identifiers 26

6.6 Brand identification 26

6.7 Uniform resource locators (URLs) 26

7 Streaming support 26

8 Box structures 26

8.1 File structure and general boxes 26

8.1.1 Media data box 26

8.1.2 Free space box 27

8.1.3 Progressive download information box 27

8.1.4 Identified media data box 28

8.2 Movie structure 29

8.2.1 Movie box 29

8.2.2 Movie header box 29

8.3 Track structure 31

8.3.1 Track box 31

8.3.2 Track header box 31

8.3.3 Track reference box 35

8.3.4 Track group box 37

8.3.6 Track type box 45

8.4 Track media structure 45

8.4.1 Media box 45

8.4.2 Media header box 45

8.4.3 Handler box 46

8.4.4 Media information box 47

8.4.5 Media information header boxes 47

8.4.6 Extended language tag 48

8.5 Sample tables 49

8.5.1 Sample table box 49

8.5.2 Sample description box 50

8.5.3 Degradation priority box 52

8.5.4 Sample scale box 52

8.6 Track time structures 53

8.6.1 Time to sample boxes 53

8.6.2 Sync sample box 59

8.6.3 Shadow sync 59

8.6.4 Independent and disposable samples box 61

8.6.5 Edit box 63

8.6.6 Edit list box 63

8.7 Track data layout structures 66

8.7.1 Data information box 66

8.7.2 Data reference box 66

8.7.3 Sample size boxes 68

8.7.4 Sample to chunk box 70

8.7.5 Chunk offset box 71

8.7.6 Padding bits box 72

8.7.7 Sub-sample information box 72

8.7.8 Sample auxiliary information sizes box 74

8.7.9 Sample auxiliary information offsets box 75

8.8 Movie fragments 76

8.8.1 Movie extends box 76

8.8.2 Movie extends header box 78

8.8.3 Track extends box 78

8.8.4 Movie fragment box 79

8.8.5 Movie fragment header box 80

8.8.6 Track fragment box 80

8.8.7 Track fragment header box 81

8.8.8 Track fragment run box 83

8.8.9 Movie fragment random access box 85

8.8.10 Track fragment random access box 85

8.8.11 Movie fragment random access offset box 87

8.8.12 Track fragment decode time box 87

8.8.13 Level assignment box 89

8.8.14 Sample auxiliary information in movie fragments 91

8.8.15 Track Extension Properties box 91

8.8.16 Alternative startup sequence properties box 92

8.8.17 Metadata and user data in movie fragments 92

8.9 Sample group structures 93

8.9.1 Overview 93

8.9.2 Sample to group box 94

8.9.3 Sample group description box 96

8.9.4 Representation of group structures in movie fragments 99

8.9.5 Compact sample to group box 100

8.10 User data 102

8.10.1 User data box 102

8.10.2 Copyright box 103

8.10.3 Track selection box 103

8.10.4 Track kind 105

8.10.5 Label box 106

8.11 Metadata support 107

8.11.1 MetaBox 107

8.11.2 XML boxes 108

8.11.3 Item location box 109

8.11.4 Primary item box 113

8.11.5 Item protection box 113

8.11.6 Item information box 114

8.11.7 Additional metadata container box 117

8.11.8 Metabox Relation box 117

8.11.9 URL forms for MetaBoxes 117

8.11.10 Static metadata 118

8.11.11 Item data box 119

8.11.12 Item reference box 119

8.11.13 Auxiliary video metadata 120

8.11.14 Item properties box 121

8.11.15 Brand item property 123

8.12 Void 124

8.13 File delivery format support 124

8.13.1 Overview 124

8.13.2 FD item information box 124

8.13.3 File partition box 125

8.13.4 FEC reservoir box 127

8.13.5 FD session group box 128

8.13.6 Group ID to name box 129

8.13.7 File reservoir box 129

8.14 Sub tracks 130

8.14.1 Overview 130

8.14.2 Backward compatibility 130

8.14.3 Sub track box 131

8.14.4 Sub track information box 131

8.14.5 Sub track definition box 133

8.14.6 Sub track sample group box 133

8.15 Void 134

8.16 Segments 134

8.16.1 Overview 134

8.16.2 Segment type box 134

8.16.3 Segment index box 134

8.16.4 Subsegment index box 139

8.16.5 Producer reference time box 140

8.17 Void 142

8.18 Entity grouping 142

8.18.1 General 142

8.18.2 Groups list box 142

8.18.3 Entity to group box 143

8.18.4 Entity group definitions 144

8.19 Compressed boxes 146

8.19.1 Overview and processing 146

8.19.2 Processing model 146

8.19.3 General syntax 148

8.19.4 General semantics 148

8.19.5 Original file-type box 148

8.19.6 Compressed movie box 149

8.19.7 Compressed movie fragment box 149

8.19.8 Compressed segment index box 150

8.19.9 Compressed subsegment index box 150

9 Hint track formats 151

9.1 RTP and SRTP hint track format 151

9.1.1 Overview 151

9.1.2 Sample entry format 151

9.1.3 Sample format 153

9.1.4 SDP information 156

9.1.5 Statistical information 157

9.2 ALC/LCT and FLUTE hint track format 158

9.2.1 Overview 158

9.2.2 Design principles 159

9.2.3 Sample entry format 160

9.2.4 Sample format 161

9.3 MPEG-2 transport hint track format 165

9.3.1 Overview 165

9.3.2 Design principles 165

9.3.3 Sample entry format 167

9.3.4 Sample format 169

9.3.5 Protected MPEG 2 transport stream hint track 172

9.4 RTP, RTCP, SRTP and SRTCP reception hint tracks 173

9.4.1 RTP reception hint track 173

9.4.2 RTCP reception hint track 176

9.4.3 SRTP reception hint track 178

9.4.4 SRTCP reception hint tracks 180

9.4.5 Protected RTP reception hint track 181

9.4.6 Recording procedure 181

9.4.7 Parsing procedure 181

10 Sample groups 181

10.1 Random access recovery points 181

10.2 Rate share groups 182

10.2.1 Overview 182

10.2.2 Rate share sample group description entry 184

10.2.3 Relationship between tracks 185

10.2.4 Bitrate allocation 186

10.3 Alternative startup sequences 186

10.4 Random access point (RAP) sample group 191

10.5 Temporal level sample group 191

10.6 Stream access point sample group 192

10.7 Sample-to-item sample group 193

10.8 Dependent random access point (DRAP) sample group 194

10.9 Pixel Aspect Ratio Sample Grouping 195

10.10 Clean Aperture Sample Grouping 195

10.11 EDRAP sample group 196

10.11.1 Definition 196

10.11.2 Syntax 196

10.11.3 Semantics 196

10.12 Essential descriptions hierarchy sample grouping 197

10.12.1 Definition 197

10.12.2 Syntax 198

10.12.3 Semantics 199

11 Derived file formats 199

12 Media-specific definitions 199

12.1 Video media 199

12.1.1 Media handler 199

12.1.2 Video media header 200

12.1.3 Sample entry 200

12.1.4 Pixel aspect ratio and clean aperture 201

12.1.5 Colour information 203

12.1.6 Content light level 204

12.1.7 Mastering display colour volume 204

12.1.8 Content colour volume 205

12.1.9 Ambient viewing environment 206

12.2 Audio media 206

12.2.1 Media handler 206

12.2.2 Sound media header 206

12.2.3 Sample entry 207

12.2.4 Channel layout 209

12.2.5 Downmix instructions 212

12.2.6 DRC information 216

12.2.7 Audio stream loudness 217

12.2.8 Audio rendering indication box 220

12.2.9 Audio element box 221

12.2.10 Audio element description box 221

12.2.11 Audio element positioning interactivity polar box 222

12.2.12 Audio element prominence interactivity box 223

12.2.13 Audio element selection box 224

12.2.14 Audio element selection description box 224

12.3 Metadata media 224

12.3.1 Media handler 224

12.3.2 Media header 225

12.3.3 Sample entry 225

12.4 Hint media 227

12.4.1 Overview 227

12.4.2 Media handler 228

12.4.3 Hint media header 228

12.4.4 Sample entry 229

12.5 Text media 229

12.5.1 Media handler 229

12.5.2 Media header 229

12.5.3 Sample entry 229

12.6 Subtitle media 230

12.6.1 Media handler 230

12.6.2 Subtitle media header 230

12.6.3 Sample entry 230

12.7 Font media 231

12.7.1 Media handler 231

12.7.2 Media header 231

12.7.3 Sample entry 231

12.8 Void 232

12.9 Multiplexed timed metadata tracks 232

12.9.1 General 232

12.9.2 Overall design 232

12.9.3 Sample format 232

12.9.4 Sample entry format 232

12.9.5 Defined formats 236

12.10 Volumetric visual media 237

12.10.1 Media handler 237

12.10.2 Media header 237

12.10.3 Sample entry 238

12.10.4 Sample format 238

12.11 Haptic media 238

12.11.1 Media handler 238

12.11.2 Media header 238

12.11.3 Sample entry 238

12.11.4 Sample format 239

13 Transformed media tracks 239

13.1 General 239

13.2 Multiple transformations for a single transformed media track 239

13.3 Determining the untransformed sample entry type 239

13.3.2 Example for protected and restricted media (informative) 240

13.3.3 The 'codecs' MIME parameter for a transformed media track 240

13.4 Support for protected streams 240

13.4.1 Overview 240

13.4.2 Protection scheme information box 242

13.4.3 Original format box 243

13.4.4 IPMPInfoBox 243

13.4.5 IPMP control box 243

13.4.6 Scheme type box 243

13.4.7 Scheme information box 244

13.4.8 Scramble Scheme Information Box 244

13.5 Restricted media tracks 245

13.5.1 General 245

13.5.2 Restricted sample entry transformation 245

13.5.3 Restricted scheme information box 247

13.5.4 Scheme for stereoscopic video arrangements 247

13.5.5 Compatible scheme type box 250

13.5.6 Sample-packed tracks 250

13.6 Support for incomplete tracks 251

13.6.1 General 251

13.6.2 Transformation 252

13.6.3 Complete track information box 253

Annex A (informative) Overview and tutorial 254

A.1 Annex overview 254

A.2 Design considerations 254

A.2.1 Usage 254

A.3 Design principles 255

A.4 Core concepts 256

A.5 Physical structure of the media 256

A.6 Temporal structure of the media 257

A.7 Interleave 257

A.8 Composition 257

A.9 Random access 258

A.10 Fragmented movie files 258

A.11 Construction of fragmented movies 259

A.12 Transformed streaming over streaming protocols 260

A.12.1 Design considerations for streaming protocols 260

A.12.2 Design considerations for streaming protocols 261

Annex B (informative) Guidance on deriving from this document 264

B.1 General 264

B.2 General principles 264

B.2.1 General 264

B.2.2 Base layer operations 264

B.3 Boxes 265

B.4 Brand identifiers 266

B.4.1 Overview 266

B.4.2 Usage of the brand 266

B.4.3 Introduction of a new brand 266

B.4.4 Player guideline 267

B.4.5 Authoring guideline 267

B.4.6 Example 267

B.5 Storage of new media types 268

B.6 Tracks 269

B.6.1 Data location 269

B.6.2 Time 270

B.6.3 Media types 270

B.6.4 Coding types 270

B.6.5 Sub-sample information 270

B.6.6 Sample dependency 271

B.6.7 Sample groups 271

B.6.8 Track-level 271

B.6.9 Protection 271

B.7 Metadata 272

B.8 Sample groups, timed metadata tracks, and sample auxiliary information 272

Annex C (normative) Fragment identifiers for ISO base media resources 274

C.1 Overview 274

C.2 Syntax and semantics 274

Annex D (informative) Management of extension code-points 276

D.1 Code points 276

D.2 Procedure for the request of an extension code-point 277

Annex E (normative) File format brands 278

E.1 General 278

E.2 The 'isom' brand 279

E.3 The 'avc1' brand 280

E.4 The 'iso2' brand 280

E.5 The 'mp71' brand 281

E.6 The 'iso3' brand 282

E.7 The 'iso4' brand 282

E.8 The 'iso5' brand 283

E.9 The 'iso6' brand 284

E.10 The 'iso7' brand 284

E.11 The 'iso8' brand 285

E.12 The 'iso9' brand 285

E.13 The 'isoa' brand 285

E.14 The 'isob' brand 286

E.15 The 'relo' brand 286

E.15.1 Requirements for files 286

E.15.2 Requirements for readers 286

E.15.3 Use cases (informative) 287

E.16 The 'isoc' brand 289

E.17 The 'comp' brand 289

E.18 The 'unif' brand 289

E.18.1 General 289

E.18.2 Requirements for files 290

E.18.3 Requirements for readers 290

E.19 The 'isod' brand 290

Annex F (normative) MIME type registration of segments 292

F.1 Overview 292

F.2 Registration 292

Annex G (informative) URI-labelled metadata forms 293

G.1 UUID-labelled metadata 293

G.2 ISO OID-labelled metadata 293

G.3 SMPTE-labelled metadata 293

Annex H (informative) Processing of RTP streams and reception hint tracks 295

H.1 General 295

H.1.1 Overview 295

H.1.2 Structure 295

H.1.3 Specific definitions 295

H.2 Synchronization of RTP streams 295

H.3 Recording of RTP streams 296

H.3.1 Overview 296

H.3.2 Compensation for unequal starting for position of received RTP streams 299

H.3.3 Recording of SDP 300

H.3.4 Creation of a sample within an RTP reception hint track 300

H.3.5 Representation of RTP timestamps 301

H.3.6 Recording operations to facilitate inter-stream synchronization in playback 304

H.3.7 Representation of reception times 306

H.3.8 Creation of media samples 306

H.3.9 Creation of hint samples referring to media samples 307

H.4 Playing of recorded RTP streams 307

H.4.1 Overview 307

H.4.2 Preparation for the playback 308

H.4.3 Decoding of a sample within an RTP reception hint track 308

H.4.4 Lip synchronization 308

H.4.5 Random access 310

H.5 Re-sending recorded RTP streams 310

H.5.1 Overview 310

H.5.2 Re-sending RTP packets 311

H.5.3 RTCP processing 312

Annex I (normative) Stream access points 314

I.1 General 314

I.2 SAP properties 314

I.2.1 General 314

I.2.2 SAP properties for layers 315

I.3 SAP types 316

I.4 SAP definitions for the ISO base media file format 317

Annex J (informative) Segment index examples 318

J.1 General 318

J.2 Examples 318

J.2.1 Simple one-level indexing 318

J.2.2 Hierarchical 319

J.2.3 Daisy-chain 320

J.2.4 Combination hierarchical and daisy-chain 321

Annex K (normative) Use of IETF RFC 6381 for ISOBMFF files 324

K.1 General 324

K.2 Use of the 'codecs' parameter 324

K.2.1 General rules 324

K.2.2 Syntax 325

K.3 The 'codecs' parameter for transformed media tracks 325

K.4 Use of the 'profiles' parameter 326

K.5 Use of the 'itemtypes' parameter 327

K.6 Use of the 'essential' parameter 327

Foreword

ISO (the International Organization for Standardization) and IEC (the International Electrotechnical Commission) form the specialized system for worldwide standardization. National bodies that are members of ISO or IEC participate in the development of International Standards through technical committees established by the respective organization to deal with particular fields of technical activity. ISO and IEC technical committees collaborate in fields of mutual interest. Other international organizations, governmental and non-governmental, in liaison with ISO and IEC, also take part in the work.

The procedures used to develop this document and those intended for its further maintenance are described in the ISO/IEC Directives, Part 1. In particular, the different approval criteria needed for the different types of document should be noted. This document was drafted in accordance with the editorial rules of the ISO/IEC Directives, Part 2 (see [www.iso.org/directives](http://www.iso.org/directives) or [www.iec.ch/members\_experts/refdocs](http://www.iec.ch/members_experts/refdocs)).

Attention is drawn to the possibility that some of the elements of this document may be the subject of patent rights. ISO and IEC shall not be held responsible for identifying any or all such patent rights. Details of any patent rights identified during the development of the document will be in the Introduction and/or on the ISO list of patent declarations received (see [www.iso.org/patents](https://www.iso.org/iso-standards-and-patents.html)) or the IEC list of patent declarations received (see [patents.iec.ch](https://patents.iec.ch)).

Any trade name used in this document is information given for the convenience of users and does not constitute an endorsement.

For an explanation of the voluntary nature of standards, the meaning of ISO specific terms and expressions related to conformity assessment, as well as information about ISO's adherence to the World Trade Organization (WTO) principles in the Technical Barriers to Trade (TBT) see [www.iso.org/iso/foreword.html](http://www.iso.org/iso/foreword.html). In the IEC, see [www.iec.ch/understanding-standards](https://www.iec.ch/understanding-standards).

This document was prepared by Joint Technical Committee ISO/IEC JTC 1, *Information technology*, Subcommittee SC 29, *Coding of audio, picture, multimedia and hypermedia information*.

This eigth edition cancels and replaces the seventh edition (ISO/IEC 14496-12:2022), which has been technically revised.

The main changes compared to the previous edition are as follows:

— Specification of essential sample groups

— Addition of the essential descriptions hierarchy sample group

— Addition of the preselection entity group and related boxes

— Addition of the extended dependent random access point (EDRAP) sample group

— Specification of the sample-packed restricted video track

— Addition of the associated external stream track reference

— Relaxing the presence requirements of the HandlerBox within a MetaBox

— Addition of the handler property for items

A list of all parts in the ISO/IEC 14496 series can be found on the ISO and IEC websites.

Any feedback or questions on this document should be directed to the user’s national standards body. A complete listing of these bodies can be found at [www.iso.org/members.html](http://www.iso.org/members.html) and [www.iec.ch/national-committees](http://www.iec.ch/national-committees).

Introduction

The ISO base media file format is designed to contain timed media information for a presentation in a flexible, extensible format that facilitates interchange, management, editing, and presentation of the media. This presentation may be ‘local’ to the system containing the presentation, or may be via a network or other stream delivery mechanism.

The file structure is object-oriented; a file can be decomposed into constituent objects very simply, and the structure of the objects inferred directly from their type.

The file format is designed to be independent of any particular network protocol while enabling efficient support for them in general.

The ISO base media file format is a base format for media file formats.

The International Organization for Standardization (ISO) and International Electrotechnical Commission (IEC) draw attention to the fact that it is claimed that compliance with this document may involve the use of patents.

ISO and IEC take no position concerning the evidence, validity and scope of these patent rights

The holders of these patent rights have assured ISO and IEC that they are willing to negotiate licences under reasonable and non-discriminatory terms and conditions with applicants throughout the world. In this respect, the statements of the holders of these patent rights are registered with ISO and IEC. Information may be obtained from the patent database available at [www.iso.org/patents](http://www.iso.org/patents).

Attention is drawn to the possibility that some of the elements of this document may be the subject of patent rights other than those in the patent database. ISO and IEC shall not be held responsible for identifying any or all such patent rights.

Structure of this document

Clause 4 defines object-structured files; files that are built from boxes.

Clause 6 gives the core concepts and data-types for time-based presentations, called 'movies' in this document.

Clause 8 defines the boxes used by time-based presentations, and other formats.

Clause 9 defines the hint track formats used to support some streaming protocols.

Clause 10 builds on the concept of sample groups as defined in subclause 8.9 and defines some sample groups.

Clause 11 defines how to base a file format on this document.

Clause 12 builds on the general concepts of tracks as defined in Clause 8, and defines track formats for various general types of media (video, sound, etc.).

Annex A provides an informative introduction to time-based presentations, which may be of assistance to first-time readers and implementers.

Annex B provides guidance on writing derived specifications.

Annex C provides the syntax for uniform resource identifier (URI) fragments.

Annex D documents how identifier values defined externally to this document are managed.

Annex E defines brands that may be used to identify the conformance and reader requirements to the structures defined in this document for time-based presentations.

Annex F contains the formal IANA registration of segments.

Annex G defines some forms used for labelling metadata with uniform resource identifier (URI) labels.

Annex H provides an overview of the use of hint tracks for RTP streams and RTP stream reception.

Annex I contains the formal definitions of the types of stream access points in timed media streams.

Annex J contains examples of the use of the SegmentIndexBox defined in 8.16.3.

Annex K defines the MIME parameters that may be used to annotate MIME types for time-based presentations based on Clause 6.

Information technology — Coding of audio-visual objects —

Part 12:  
ISO base media file formatINTERNATIONAL STANDARD© ISO/IEC 2015 – All rights reservedISO/IEC 15444-12:2015(E) 63Part 12: ISO base media file formatInformation technology — JPEG 2000 image coding systemTechnologies de l'information — Codage des objets audiovisuels — Partie 12: Format ISO de base pour les fichiers médiasInformation technology — JPEG 2000 image coding system — Part 12: ISO base media file formatE2015-02-20(60) PublicationISO/IECISO/IEC J   International Standard 2015ISO/IEC 15444‑ISO/IEC 15444‑12ISO/IEC 15444-12  Coding of audio, picture, multimedia and hypermedia informationInformation technology 291 2見出し 2見出し 1    02 STD Version 2.1c260   4C:\Users\shinji\_w\AppData\Roaming\Microsoft\Templates\STD\w15177\_14496\_5th.-restyle-R1.doc

# Scope

This document specifies the ISO base media file format, which is a general format forming the basis for a number of other more specific file formats. This format contains the timing, structure, and media information for timed sequences of media data, such as audio-visual presentations.

# Normative references

The following documents are referred to in the text in such a way that some or all of their content constitutes requirements of this document. For dated references, only the edition cited applies. For undated references, the latest edition of the referenced document (including any amendments) applies.

ISO 639-2, *Codes for the representation of names of languages — Part 2: Alpha-3 code*

ITU-T X.667 | ISO/IEC 9834-8, *Information technology – Procedures for the operation of object identifier registration authorities – Part 8: Generation of universally unique identifiers (UUIDs) and their use in object identifiers*

ISO/IEC 10646 *Information technology – Universal coded character set (UCS)*

ISO/IEC 13818‑2:2013, *Information technology — Generic coding of moving pictures and associated audio information — Part 2: Video*

ISO/IEC 14496-1: *Information technology — Coding of audio-visual objects — Part 1: Systems*

ISO/IEC 14496-10:2014, *Information technology — Coding of audio-visual objects — Part 10: Advanced Video Coding*

ISO 15076‑1, *Image technology colour management — Architecture, profile format and data structure — Part 1: Based on ICC.1:2010*

ISO/IEC 15938-1, *Information technology — Multimedia content description interface — Part 1: Systems*

ISO/IEC 23001-1, *Information technology — MPEG systems technologies — Part 1: Binary MPEG format for XML*

ISO/IEC 23001-14, *Information technology — MPEG systems technologies — Part 14: Partial file format*

ISO/IEC 23002-3, *Information technology — MPEG video technologies — Part 3: Representation of auxiliary video and supplemental information*

ISO/IEC 23003‑4 *Information technology — MPEG audio technologies — Part 4: Dynamic range control*

ITU-T H.265 | ISO/IEC 23008-2, , *Information technology — High efficiency coding and media delivery in heterogeneous environments — Part 2:* High efficiency video coding

ISO/IEC 23091-2, Information technology —Coding-independent code points*— Part 2: Video*

ISO/IEC 23091-3, *Information technology —Coding-independent code points — Part 3: Audio*

IETF RFC 1951, *DEFLATE Compressed Data Format Specification version 1.3*

IETF RFC 2045, *Multipurpose Internet Mail Extensions (MIME) Part One: Format of Internet Message Bodies*

IETF RFC 2046, *Multipurpose Internet Mail Extensions (MIME) Part Two: Media Types*

IETF RFC 3629, *UTF-8, a transformation format of ISO 10646*

IETF RFC 3711:2004, *The Secure Real-time Transport Protocol (SRTP)*

IETF RFC 5052, *Forward Error Correction (FEC) Building Block*

IETF RFC 5905, *Network Time Protocol Version 4: Protocol and Algorithms Specification*

ITU-R TF.460-6:2002, *Standard-frequency and time-signal emissions*

ITU-R BS.1770-4, *Algorithms to measure audio programme loudness and true-peak audio level*

IETF  BCP 47, *Tags for Identifying Languages*

IETF RFC 4122, A Universally Unique IDentifier (UUID) URN Namespace

IETF RFC 3061, A URN Namespace of Object Identifiers

W3C Recommendation, *Extensible Markup Language (XML) 1.0 (Fifth Edition)*, 26 November 2008, <https://www.w3.org/TR/2008/REC-xml-20081126/>

# Terms, definitions and abbreviated terms

## Terms and definitions

For the purposes of this document, the following terms and definitions apply.

ISO and IEC maintain terminology databases for use in standardization at the following addresses:

— ISO Online browsing platform: available at [https://www.iso.org/obp](https://www.iso.org/obp/ui)

— IEC Electropedia: available at <https://www.electropedia.org/>

* + 1. access unit

media data pertaining to a particular composition time in a media stream, usually carried in one sample of a media track

* + 1. box

object-oriented building block defined by a unique type identifier and length

Note 1 to entry Called ‘atom’ in some specifications, including the first definition of MP4.

* + 1. chunk

contiguous set of samples for one track

* + 1. clean aperture

part of a decoded video image from which undesirable pixels introduced for coding purposes such as having integer number of coding blocks have been removed for presentation

* + 1. container box

box whose sole purpose is to contain and group a set of related boxes

Note 1 to entry Container boxes are normally not derived from FullBox

* + 1. dual-headed file

ISO base media file that is both an item file and a movie file

* + 1. EDRAP sample

sample for which all subsequent samples in both decoding and output order can be correctly decoded provided that the required preceding SAP or EDRAP samples are available for decoding the sample and the subsequent samples, where the required preceding SAP or EDRAP samples consist of one or more of the set of samples starting from the closest preceding SAP sample of type 1, 2, or 3 in decoding order closestSapSample, and including all EDRAP samples between closestSapSample and the sample in decoding order

* + 1. essential sample group

sample group that describes essential information for the associated samples and is associated with a sample group description for which the version field is equal to 3

* + 1. file level

byte position in an ISO base media file not contained in a Box structure

* + 1. full aperture

decoded video image as output by the decoder which may contain undesirable pixels for presentation

* + 1. hint track

special track which does not contain media data, but instead contains instructions for packaging one or more tracks into a streaming channel

* + 1. hinter

tool that is run on a file containing only media, to add one or more hint tracks to the file and so facilitate streaming

* + 1. index file

ISO base media file containing only SegmentIndexBox

* + 1. ISO base media file

file conforming to the file format described in this document (either a movie file, a item file, a segment file or an index file)

Note 1 to entry This document uses this term even when data delivered is not stored as a file but on the wire as payload of a protocol data unit (e.g. HTTP, RTP, MMT, …). In this case, it is assumed that the payload of the protocol data unit is first saved into a file and then the normative statements of this document that use the term “file” apply.

* + 1. item

data which does not require timed processing, as opposed to sample data

* + 1. item data

concatenation of the extents of an item as specified by the definition of ItemLocationBox

* + 1. item file

ISO base media file containing a top-level MetaBox

Note 1 to entry A movie file can also be an item file, and vice-versa. Such a file can be called a dual-headed file.

* + 1. leading sample

sample associated with a random access point (RAP) that precedes the RAP in composition order and immediately follows the RAP or another leading sample in decoding order, and which possibly cannot be correctly decoded when decoding starts from the RAP

* + 1. leaf subsegment

subsegment that does not contain any indexing information that enables its further division into subsegments

* + 1. mod

modulo operator: (x mod y) = x-y floor (x/y)

* + 1. media data box

box which can hold the actual media data for a presentation ('mdat')

* + 1. movie box

container box whose sub-boxes define the structure-data for a presentation ('moov')

* + 1. movie file

ISO base media file containing a MovieBox

* + 1. movie fragment

fragment of the information contained in a MovieBox, defined by a MovieFragmentBox and its contents

* + 1. structure-data

data that provides the location, size, timing, and characteristics of the media data (e.g. the coded frames of audio and video)

* + 1. movie-fragment relative addressing

signalling of offsets for media data in movie fragments that is relative to the start of those movie fragments, specifically setting the flags base-data-offset-present to 0 and default-base-is-moof to 1 in TrackFragmentHeaderBoxes

Note 1 to entry Setting the default-base-is-moof flag to 1 is only relevant for movie fragments that contain more than one track run (either in the same or several tracks).

* + 1. object-structured file

file that is formed as a series of boxes including a FileTypeBox and contains no data outside the series of boxes

* + 1. open random access point

sample after which all samples in composition order can be correctly decoded, but some samples following the random access point in decoding order and preceding the random access point in composition order need not be correctly decodable

EXAMPLE An intra picture starting a group of pictures can be followed in decoding order by (bi-)predicted pictures that however precede the intra picture in composition order; though they possibly cannot be correctly decoded if the decoding starts from the intra picture, they are not needed.

* + 1. pixel aspect ratio

scaling required to be applied to the output pixel of a decoder to produce a non-distorted image

Note 1 to entry The term "Sample Aspect Ratio" is sometimes used for this term, but "sample" in this standard has a specific meaning.

* + 1. preselection

set of one or more tracks representing one version of the media presentation for simultaneous decoding or presentation

* + 1. presentation

one or more motion sequences, possibly combined with audio

* + 1. presentation time

timeline of a track that aligns with the timelines of other tracks established by an explicit or implied edit list applied to the composition timestamps

* + 1. random access

decoding of a media stream starting from a particular sample without decoding of any sample in the media stream earlier in decoding order

Note 1 to entry Sync samples and SAPs provide random accessing capabilities.

* + 1. timeline

monotonic linear representation of times with respect to a zero origin point

* + 1. timescale

number of timestamp values that represent a duration of one second

* + 1. timestamp

integer coded value representing an instant of time on an associated timeline

* + 1. decoding timestamp

timestamp on the media timeline such that samples are decoded in decoding timestamp order

Note 1 to entry: The decoding timestamps primarily define the required decoding order; systems may decode at a time of their choosing; in the case of signed composition offsets, decoding timestamps do not necessarily precede composition timestamps

* + 1. composition timestamp

timestamp on the media timeline such that samples are presented in composition timestamp order and that establishes their relative composition timing

* + 1. sample duration

difference between the decoding timestamp of the following sample (when known) and the decoding timestamp of this sample

* + 1. random access point  
       RAP

sample in a track that starts at the ISAU of a SAP of type 1 or 2 or 3; informally, a sample, from which when decoding starts, the sample itself and all samples following in composition order can be correctly decoded

Note 1 to entry SAP types are defined in Annex I.

* + 1. random access recovery point

sample in a track with presentation time equal to the TSAP of a SAP of type 4

Note 1 to entry SAP types are defined in Annex I.

Note 2 to entry A random access recovery point relates to gradual decoding refresh and is the first sample that can be correctly decoded when the decoding started at the previous SAP of type 4 in decoding order.

* + 1. sample

all the data associated with a single time

Note 1 to entry No two samples within a track can share the same decoding timestamp; no two samples can share the same composition timestamp.

Note 2 to entry In non-hint tracks, a sample is, for example, an individual frame of video, a series of video frames in decoding order, or a compressed section of audio in decoding order; in hint tracks, a sample defines the formation of one or more streaming packets.

* + 1. sample entry

structure which defines and describes the format of some number of samples in a track

Note 1 to entry The term "sample description" has also been used, and has the same meaning.

* + 1. sample entry type

four-character code that is either a format value of a SampleEntry directly contained in SampleDescriptionBox or a data\_format value of OriginalFormatBox

* + 1. untransformed sample entry type

*sample entry type* that applied prior to transformations were performed to form a transformed media track

Note 1 to entry: This is the *sample entry type* that applied as the format value in a SampleEntry directly contained in the SampleDescriptionBox prior to transformations were performed to form a transformed media track.

* + 1. sample number

ordinal index number of a given sample where the first sample has sample number 1

* + 1. sample table

packed directory for the timing and physical layout of the samples in a track

* + 1. sync sample

sample in a track that starts at the ISAU of a SAP of type 1 or 2

Note 1 to entry SAP types are defined in Annex I.

Note 2 to entry Informally, a media sample that starts a new independent sequence of samples; if decoding starts at the sync sample, it and succeeding samples in decoding order can all be correctly decoded, and the resulting set of decoded samples forms the correct presentation of the media starting at the decoded sample that has the earliest composition time; a media format may provide a more precise definition of a sync sample for that format

* + 1. sync sample information

SyncSampleBox or sample\_is\_non\_sync\_sample equal to 0

* + 1. segment

portion of movie file, consisting of either (a) a MovieBox, with its associated media data (if any) and other associated boxes or (b) one or more MovieFragmentBoxes, with their associated media data, and other associated boxes

Note 1 to entry The associated media data can be found by following byte offsets, but the process of finding associated boxes is not given in this standard and may be derived by other specifications.

* + 1. segment file

ISO base media file containing one or more segment(s)

* + 1. subsegment

time interval of a segment formed from MovieFragmentBoxes, that is also a valid segment

* + 1. thumbnail image

smaller-resolution representation of an image

* + 1. top-level box

box contained at file level

* + 1. track

timed sequence of related samples (q.v.) in an ISO base media file

Note 1 to entry For media data, a track corresponds to a sequence of images or sampled audio; for hint tracks, a track corresponds to a streaming channel.

* + 1. transformed media track

media track that requires specific processing on top of the processing imposed by the untransformed sample entry type of the track

Note 1 to entry A transformed media track can be a protected, incomplete, or restricted media track, or any combination of them.

* + 1. haptic media

timed tactile signals to be presented as part of the media presentation

* + 1. volumetric visual media

timed visual media defining a visual coding in a three-dimensional space

Note 1 to entry: In contrast to video media, which defines a planar coding.

* + 1. container

<SAP information> file or segment compatible with the ISO base media file format

Note 1 to entry: This definition applies for the interpretation of SAP information for files and segments compatible with the ISO base media file format.

* + 1. media stream

<SAP information> samples of a track in their decoding order

Note 1 to entry: This definition applies for the interpretation of SAP information for files and segments compatible with the ISO base media file format.

* + 1. bitstream

<SAP information> file or segment compatible with the ISO base media file format

Note 1 to entry: This definition applies for the interpretation of SAP information for files and segments compatible with the ISO base media file format.

* + 1. SAP sample

sample associated with ISAU from which decoding of the media stream or the target layers can be started

## Abbreviated terms

|  |  |
| --- | --- |
| 4CC | four-character code |
| ALC | asynchronous layered coding | |
| AVC | advanced video coding | |
| EDRAP | extended dependent random access point |
| FD | file delivery | |
| FDT | file delivery table | |
| FEC | forward error correction | |
| FLUTE | file delivery over unidirectional transport | |
| IANA | internet assigned numbers authority | |
| IETF | internet engineering task force | |
| LCT | layered coding transport | |
| MBMS | multimedia broadcast/multicast service | |
| MIME | multipurpose internet mail extensions (as defined in IETF RFC 2045 and IETF RFC 2046) | |
| MVC | multiview video coding | |
| RAP | random access point |
| SAP | stream access point |
| SVC | scalable video coding | |
| UUID | universally unique identifier (as defined in IETF RFC 4122 and ISO/IEC 9834-8) | |

# Object-structured file organization

## File structure

Files are formed as a series of objects, called boxes in this document. All data is contained in boxes; there is no other data within the file. This includes any initial signature required by the specific file format.

All object-structured files conformant to Clause 4 (all object-structured files) shall contain a FileTypeBox.

In this document, top-level boxes (boxes not contained in other boxes) are indicated as being at ‘file’ level, with the notation “Container: File”.

## Object structure

* + 1. Object syntax conventions

The definitions of objects are given in the syntax description language (SDL) defined in ISO/IEC 14496-1.

NOTE Comments in the code fragments in this document are informative.

The fields in the objects are stored with the most significant byte first, commonly known as network byte order or big-endian format. When fields smaller than a byte are defined, or fields span a byte boundary, the bits are assigned from the most significant bits in each byte to the least significant. For example, a field of two bits followed by a field of six bits has the two bits in the high order bits of the byte.

In the SDL, the notation ‘=’ indicates that in this object, the field read from the bitstream (whose name and type are given in the left hand-side part) is expected to match the value given in the right hand-side part.

The following basic field types are defined. In these definitions, null-terminated means that the string is terminated by the first Unicode NUL, which shall be present, and hence an empty string is represented by a single Unicode NUL. Some fields using these types may restrict the characters permitted.

|  |  |
| --- | --- |
| **Name** | **Semantics** |
| utf8string | UTF-8 string as defined in IETF RFC 3629, null-terminated. |
| utfstring | null-terminated string encoded using either UTF-8 or UTF-16.  If UTF-16 is used, the sequence of bytes shall start with a byte order mark (BOM) and the null termination shall be 2 bytes set to 0. |
| utf8list | null-terminated list of space-separated UTF-8 strings |
| base64string | null-terminated base64 encoded data |
| signed int | same as int in ISO/IEC 14496-1, represented as two’s complement representation |

* + 1. Object definitions

An object in this terminology is a box.

Boxes start with a header which gives both size and type. The header permits compact or extended size (32 or 64 bits) and compact or extended types (32 bits or full universal unique identifiers, i.e. UUIDs). The standard boxes all use compact types (32-bit) and most boxes will use the compact (32-bit) size. Typically, only the MediaDataBox needs the 64-bit size.

To permit ease of identification, the 32-bit compact type can be expressed as four characters from the range 0020 to 007E, inclusive, of ISO/IEC 10646 (technically identical to the Unicode standard[27]) or ISO/IEC 8859-1[1]. Each character is hence expressible in a single byte. The four individual byte values of the field are placed in order in the file. Other fields may also use this 32-bit representation, referred to as a ‘four-character code’ (4CC). The maintenance of four-character codes used in the format is defined in Annex D.

The size is the entire size of the box, including the size and type header, fields, and all contained boxes. This facilitates general parsing of the file.

User extensions use an extended box type; in this case, the type field is set to 'uuid'.

aligned(8) class BoxHeader (  
 unsigned int(32) boxtype,  
 optional unsigned int(8) extended\_type[16])  
{  
 unsigned int(32) size;  
 unsigned int(32) type = boxtype;  
 if (size==1) {  
 unsigned int(64) largesize;  
 } else if (size==0) {  
 // box extends to end of file  
 }  
 if (boxtype=='uuid') {  
 unsigned int(8) usertype[16] = extended\_type;  
 }  
}

aligned(8) class Box (  
 unsigned int(32) boxtype,  
 optional unsigned int(8) extended\_type[16])  
{  
 BoxHeader(boxtype, extended\_type);  
 // the remaining bytes are the BoxPayload  
}

The semantics of these two fields are:

size is an integer that specifies the number of bytes in this box, including all its fields and contained boxes; if size is 1 then the actual size is in the field largesize; if size is 0, then this box shall be in a top-level box (i.e. not contained in another box), and be the last box in its 'file' , and its payload extends to the end of that enclosing 'file'. This is normally only used for a MediaDataBox.

type identifies the box type; user extensions use an extended type, and in this case, the type field is set to 'uuid'.

BoxPayload is defined as all the bytes in a Box, included by the size or largesize field (as appropriate), following the BoxHeader.

Boxes with an unrecognized type shall be ignored and skipped.

Many objects also contain a version number and flags field:

aligned(8) class FullBoxHeader(unsigned int(8) v, bit(24) f)  
{  
 unsigned int(8) version = v;  
 bit(24) flags = f;  
}

aligned(8) class FullBox(unsigned int(32) boxtype,  
 unsigned int(8) v, bit(24) f,  
 optional unsigned int(8) extended\_type[16])  
 extends Box(boxtype, extended\_type)  
{  
 FullBoxHeader(v, f);  
 // the remaining bytes are the FullBoxPayload  
}

The semantics of these two fields are:

version is an integer that specifies the version of this format of the box.

flags is a map of flags

When the syntax specifies version = 0, it means that this document only defines the syntax for version 0 of the FullBox. When “= 0” is not present, it means different values are possible and the syntax has actual differences depending on the actual version used. Derived specifications are not permitted to define a new version of a box defined in this document.

When the syntax specifies flags = 0 (or sometimes simply “0” for the flags), it means that this document does not define flag values for this FullBox. When “= 0” is not present, it means different flag values are defined. Unless specified otherwise, values of flags that are not specified in this document are reserved for future use by ISO/IEC. Additional flags may be defined and may be used to introduce backwards-compatible changes that parsers unaware of the change may safely omit. If parsers unaware of changed syntax of a box fail parsing the box (non-backwards-compatible), a new version will be used. Derived specifications should follow this practice. As a consequence, if a reader supports a version of a FullBox, it can and should keep parsing the box even if it does not recognize a flag value. Writers should not write flag values that they do not understand.

FullBoxPayload is defined as all the bytes in a FullBox, included by the size or largesize field (as appropriate), following the FullBoxHeader. Since BoxPayload is defined for any box extending from Box, FullBox has both BoxPayload and FullBoxPayload defined, the former including the latter (with BoxPayload of a FullBox including the FullBoxHeader).

The payload (contents) of a box are FullBoxPayload for a FullBox and BoxPayload for all boxes.

FullBoxes with an unrecognized version shall be ignored and skipped.

Boxes specified in this document may be extended but such extensions are reserved for future use by ISO/IEC. Syntax may be added at the end of a box derived from FullBox and an already specified version value may be kept, if it is not essential to parse such added syntax. When a parser has not reached the end of a box derived from FullBox as defined by the values of the size or largesize field (as appropriate) but does not recognize the remaining syntax elements, it shall ignore and skip the remaining of the box.

NOTE This document and derived specifications describe the different flags defined for a box extending from FullBox as hexadecimal values (e.g. 0x000001); these values correspond to 24-bit unsigned integers with the most significant byte first.

* + 1. Extensibility of object definitions

The normative objects defined in this document are identified by a 32-bit value, which is normally a four character compact code as defined in subclause 4.2.

To permit user extension of the format, to store new object types, and to permit the inter-operation of the files formatted to this documentwith certain distributed computing environments, there are a type mapping and a type extension mechanism that together form a pair.

Commonly used in distributed computing are UUIDs (universal unique identifiers), which are 16 bytes. Any normative type specified here can be mapped directly into the UUID space by composing the four byte type value with the twelve byte ISO reserved value, 0xXXXXXXXX-0011-0010-8000-00AA00389B71. The four character code replaces the XXXXXXXX in the preceding number. These types are reserved or specified in this document.

User objects use the escape type 'uuid'. They are documented above in subclause 6.3. After the size and type fields, there is a full 16-byte UUID.

Systems which wish to treat every object as having a UUID may employ the following algorithm:

size := read\_uint32();  
type := read\_uint32();  
if (type=='uuid')  
 then uuid := read\_uuid()  
 else uuid := form\_uuid(type, ISO\_12\_bytes);

Similarly when linearizing a set of objects into files formatted to this document, the following is applied:

write\_uint32( object\_size(object) );  
uuid := object\_uuid\_type(object);  
if (is\_ISO\_uuid(uuid) )  
 write\_uint32( ISO\_type\_of(uuid) )  
 else { write\_uint32('uuid'); write\_uuid(uuid); }

A file containing boxes from this document that have been written using the 'uuid' escape and the full UUID is not compliant; systems are not required to recognize standard boxes written using the 'uuid' and an ISO UUID.

## File-type box

* + 1. Definition

Box Type: 'ftyp'  
Container: File, or OriginalFileTypeBox  
Mandatory: Yes  
Quantity: Exactly one (but see below)

Files conformant to Clause 4 shall contain a FileTypeBox. For compatibility with an earlier edition of this document, files may be conformant to this document and not contain a FileTypeBox. Files with no FileTypeBox should be read as if they contained a FileTypeBox with Major\_brand='mp41', minor\_version=0, and the single compatible brand 'mp41'.

A media-file structured to this document may be compatible with more than one detailed specification, and it is therefore not always possible to speak of a single ‘type’ or ‘brand’ for the file. This means that the utility of the file name extension and multipurpose internet mail extension (MIME) type are somewhat reduced.

This box shall be placed as early as possible in the file (e.g. after any obligatory signature, but before any significant variable-size boxes such as a MovieBox, MediaDataBox, or FreeSpaceBox). It identifies which specification is the ‘best use’ of the file (the major\_brand), and a minor version of that specification; and also a set of other specifications to which the file complies (the compatible\_brands); the major\_brand should be repeated in the compatible\_brands list. Readers implementing this format should attempt to read files that are marked as compatible with any of the specifications that the reader implements. Any incompatible change in a specification should therefore register a new ‘brand’ identifier to identify files conformant to the new specification.

The minor version is informative only. It does not appear for compatible-brands, and is not used to determine the conformance of a file to a standard. It may allow more precise identification of the major specification, for inspection, debugging, or improved decoding.

Files are normally identified externally (e.g. with a file extension or MIME type) that identifies the ‘best use’ (major brand), or the brand that the author believes will provide the greatest compatibility.

This subclause does not define any brands. However, see subclause 6.6 for brands for files conformant to the whole document and not just this subclause. All file format brands defined in this document are included in Annex E with a summary of which features they require.

* + 1. Syntax

aligned(8) class GeneralTypeBox(code) extends Box(code)  
{  
 unsigned int(32) major\_brand;  
 unsigned int(32) minor\_version;  
 unsigned int(32) compatible\_brands[]; // to end of the box  
}

aligned(8) class FileTypeBox extends GeneralTypeBox ('ftyp')  
{  
}

* + 1. Semantics

This box identifies the specifications to which this file complies.

Each brand is a four character code, registered with ISO, that identifies a precise specification.

major\_brand – is a brand identifier

minor\_version – is an informative integer for the minor version of the major brand

compatible\_brands – is a list, to the end of the box, of brands

## Extended type box

* + 1. Definition

Box Type: 'etyp'  
Container: File, ItemPropertyContainerBox, or OriginalFileTypeBox  
Mandatory: No  
Quantity: Zero or more in file, zero or one per an item

Box Type: 'tyco'  
Container: ExtendedTypeBox  
Mandatory: Yes  
Quantity: One or more

The ExtendedTypeBox may be placed after the FileTypeBox, any SegmentTypeBox, or any TrackTypeBox, or used as an item property to indicate that a reader should only process the file, the segment, the track, or the item, respectively, if it supports the processing requirements of all the brands in at least one of the contained TypeCombinationBoxes, or at least one brand in the preceding FileTypeBox, SegmentTypeBox, or TrackTypeBox, or in the BrandProperty associated with the same item, respectively.

The TypeCombinationBox expresses that the associated file, segment, track, or item may contain any boxes or other code points required to be supported in any of the brands listed in the TypeCombinationBox and that the associated file, segment, track, or item complies with the intersection of the constraints of the brands listed in the TypeCombinationBox.

NOTE Effectively, if the compatible\_brands in the FileTypeBox are labeled C[1], C[2], etc., and the compatible\_brands in the first TypeCombinationBox D[1,1], D[1,2], and the second D[2,1], D[2,2], and so on, then a reader has to support:

C[1]   
or C[2]   
or …  
or ( D[1,1] and D[1,2] and …)  
or ( D[2,1] and D[2,2] and …)  
…

* + 1. Syntax

aligned(8) class TypeCombinationBox extends Box('tyco')  
{  
 unsigned int(32) compatible\_brands[]; // to end of the box  
}

aligned(8) class ExtendedTypeBox extends Box('etyp')  
{  
 TypeCombinationBox compatible\_combinations[]; // to end of the box  
}

* + 1. Semantics

compatible\_brands is a list of brands.

compatible\_combinations is a list of TypeCombinationBoxes.

# Void

# ISO base media file organization

## Files, segments, and streams

This document supports the exchange of presentations in three principle ways:

1. As a single file (e.g. on exchangeable media such as discs, or as a download).
2. As a series of segments, preceded by an initialization segment.
3. Transformed by supporting structures, called hint tracks, into a streaming protocol such as the IETF real-time protocol RTP specified in IETF RFC 3550 or an MPEG-2 transports stream specified in ISO/IEC 13818-1.

A movie file logically includes all its segments.

The file format supports transformation of media data into a streaming protocol as well as local playback. The process of sending protocol data units is time-based, just like the display of time-based data, and is therefore suitably described by a time-based format. A file or ‘movie’ that supports streaming includes information about the data units to stream. This information is included in additional tracks of the file called “hint” tracks. Hint tracks may also be used to record a stream; these are called Reception Hint Tracks, to differentiate them from plain (or server, or transmission) hint tracks.

## Presentation structure

### Object structure of a presentation

An ISO base media file is an object-structured file as defined in Clause 4 (and hence contains a FileTypeBox); some of these objects may contain other objects.

ISO base media files contain data that structures, orders, times, and describes the media data that is passed to decoders. This non-media data is called structure-data here.

The sequence of objects in a movie file shall contain exactly one MovieBox. It is usually close to the beginning or end of the file, to permit its easy location. The other objects found at this level include a FileTypeBox, FreeSpaceBox(es), MovieFragmentBox(es), a MetaBox, or MediaDataBox(es).

### Meta data and media data

The structure-data is contained within a structure-data wrapper (the MovieBox or MovieFragmentBox); the media data is contained either in the same file, within MediaDataBox(es), or in other files. The media data is composed, for example, of images or audio data; the media data containers, or media data files, may contain other un-referenced information.

The file containing the presentation structure-data may also contain all the media data, whereupon the presentation is self-contained. If the media data is externally referenced in other files, they are not required to be formatted to this document; they are used to contain media data, and may also contain unused media data, or other information. This document concerns the structure of the ISO base media file only. The format of the media-data files is constrained by this document only in that the media-data in the media files needs to be capable of description by the structure-data defined here.

NOTE Media-data files can comply with any format. It is possible to store only the media data itself in a media-data file, or media-data files can contain unused media data or other information that is not referenced by the ISO base media file. All timing and framing (position and size) information is in the ISO base media file.

### Data offsets

Each sample or item is mapped to a data reference entry that is present in the DataReferenceBox contained in the MediaInformationBox of the track or the MetaBox where the item is defined, respectively. The data reference entry specifies the container for the sample or item data among the following:

* the same file where this data reference entry is present;
* a resource identified by a given URL or URN;
* the IdentifiedMediaDataBox that contains a given identifier value;
* the IdentifiedMediaDataBox that contains the identifier value that is equal to sequence\_number of the MovieFragmentHeaderBox of the movie fragment containing the sample.

The location of samples and item data within its container is indicated through data offsets, which may be provided or inferred, for example based on the ChunkOffsetBox, TrackFragmentHeaderBox, or ItemLocationBox. Table 1 summarizes the different types of data offsets.

Table 1 – Data offset types

|  |  |  |  |
| --- | --- | --- | --- |
| **Type of data offset addressing** | **Signalling** | **The origin that the data offset is relative to** | **Usage examples** |
| Movie-fragment-relative | The base-data-offset-present and default-base-is-moof flags of the TrackFragmentHeaderBox (see subclause 8.8.7.1) | The first byte of the MovieFragmentBox defining the sample (if this is the first TrackFragmentHeaderBox of this track within the movie fragment), or  the end of the data defined by the preceding track fragment of the same track (otherwise) | Delivery of segments that contain one or more movie fragments |
| File-relative | Data reference entry of type 'url ' or 'urn ', and either no movie-fragment relative offsets indicated or construction\_method equal to 0 in ItemLocationBox | The first byte of the file identified by the data reference entry | Files that do not contain movie fragments.  NOTE It is theoretically possible to store media data in a movie-fragmented file and use file-relative data offsets. However, movie-fragment-relative data offsets are used in practice as it has the benefit of enabling delivery on movie fragment basis. |
| IdentifiedMedia‌DataBox-relative | Data reference entry of type 'imdt' or 'snim' | The first byte of the payload of the referenced IdentifiedMediaDataBox | File editing (see subclause E.15.3.1), partial image file reception (see subclause E.15.3.2), delivery of the MovieFragmentBox in a separate resource from the media data it references. |
| ItemDataBox-relative | construction\_method equal to 1 in ItemLocationBox | The first byte of the payload of the referenced ItemDataBox | Items that are small in size stored in the same MetaBox that defines them. |
| Item-relative | construction\_method equal to 2 in ItemLocationBox | The first byte of the concatenated data (of all the extents) of a given item | An item is made of the concatenation of one or more parts of existing items. |

## Structure-data (objects)

### Box

Type fields not defined here are reserved. Private extensions shall be achieved through the 'uuid' type. In addition, the following types either are not used in this document and will not be used, or are used only in their existing sense specified in this document and will not be used in any other sense, to avoid conflict with existing content using earlier pre-standard versions of this format:

clip, crgn, matt, kmat, pnot, ctab, load, imap;  
these track reference types (as found in the reference\_type of a TrackReferenceBox): tmcd, chap, sync, scpt, ssrc.

A number of boxes contain index values into sequences in other boxes. These indexes start with the value 1 (1 is the first entry in the sequence).

### Data types and fields

In a number of boxes in this document, there are two variant forms: version 0 using 32-bit fields, and version 1 using 64-bit sizes for those same fields. In general, if a version 0 box (32-bit field sizes) can be used, it should be; version 1 boxes should be used only when the 64-bit field sizes they permit, are required. Values for counters, offsets, times, durations etc. in this format do not ‘wrap’ to 0 when the maximum value that can be stored in their field is reached; appropriately large fields must be used for all values.

For convenience during content creation there are creation and modification times stored in the file. These can be 32-bit or 64-bit numbers, counting seconds since midnight, Jan. 1, 1904, which is a convenient date for leap-year calculations. 32 bits are sufficient until approximately year 2040. These times shall be expressed in Universal Time Coordinated (UTC) as defined in ITU-R TF.460-6:2002, Annex I, and therefore may need adjustment to local time if displayed.

Fixed-point numbers are signed or unsigned values resulting from dividing an integer by an appropriate power of 2. For example, a 30.2 fixed-point number is formed by dividing a 32-bit integer by 4.

Fields shown as “template” in the syntax are interpreted as follows:

* The value given after the equals sign in the syntax is a value defined in the context of this document and to be interpreted specifically by readers and writers, as indicated below.
* Derived specifications are permitted to define additional possible values for the field, but they shall indicate when these should be used, and they shall not modify the remaining syntax of the box to depend on the value of this field.
* Writers should write the value after the equal sign if they intend to write files compliant to this specification. If they intend to write files conformantto a derived specification, they may write another value, as permitted by that derived specification.
* Readers should expect any value and should keep parsing the box even if they do not recognize the value.

Fields whose name is “pre\_defined” are interpreted as follows:

* They had specific semantics in an earlier edition of this document, but their semantics are no longer in use. They are considered legacy fields.
* The value given after the equals sign in the syntax is the only permitted value.
* Derived specifications are not permitted to change this value.
* Writers shall always write this value to create conformant files.
* Readers should expect any value, and should keep parsing the box even if they do not recognize a value. Derived specifications may require stricter behaviour from readers (e.g. requiring reading to stop and emit an error when reading a different value).

Fields whose name is “reserved” are interpreted as follows:

* They may have a value defined in this document (typically 0) or they may not.
* Additional values are reserved for future use by ISO/IEC.
* Derived specifications are not permitted to define other values for this field.

[Editor’s note: The stvi box in this specification has a field reserved with template qualifier. This would need to be studied how to solve this contradiction.]

* A given syntax structure may contain multiple fields named “reserved”.
* This document guarantees the following:
  + When used in a FullBox, if a new value is introduced that requires changes to the syntax of the FullBox in a non-compatible way, this change will be done together with a change of version.
  + When used in other structures, new values may be defined but these will not affect the syntax of the structure.
* Writers shall always write the default value, if specified, or shall write a value of 0, if not specified.
* Readers should expect any value, and should keep parsing the box even if they do not recognize the value.

Matrix values which occur in the headers specify a transformation of video images for presentation. Not all derived specifications use matrices; if they are not used, they shall be set to the identity matrix. If a matrix is used, the point (p,q) is transformed into (p', q') using the matrix as follows:

(p q 1) \* | a b u | = (m n z)  
 | c d v |  
 | x y w |  
  
m = ap + cq + x; n = bp + dq + y; z = up + vq + w;  
  
p' = m/z; q' = n/z

The coordinates {p,q} are on the decompressed frame, and {p’, q’} are at the rendering output. Therefore, for example, the matrix {2,0,0, 0,2,0, 0,0,1} exactly doubles the pixel dimension of an image. The coordinates transformed by the matrix are not normalized in any way, and represent actual sample locations. Therefore {x,y} can, for example, be considered a translation vector for the image.

The coordinate origin is located at the upper left corner, and X values increase to the right, and Y values increase downwards. {p,q} and {p’,q’} are to be taken as absolute pixel locations relative to the upper left hand corner of the original image (after scaling to the size determined by the track header's width and height) and the transformed (rendering) surface, respectively.

Each track is composed using its matrix as specified into an overall image; this is then transformed and composed according to the matrix at the movie level in the MovieHeaderBox. It is application-dependent whether the resulting image is ‘clipped’ to eliminate pixels, which have no display, to a vertical rectangular region within a window, for example. So for example, if only one video track is displayed and it has a translation to {20,30}, and a unity matrix is in the MovieHeaderBox, an application may choose not to display the empty “L” shaped region between the image and the origin.

All the values in a matrix are stored as 16.16 fixed-point values, except for u, v and w, which are stored as 2.30 fixed-point values.

The values in the matrix are stored in the order {a,b,u, c,d,v, x,y,w}.

### URIs as type indicators

When URIs are used as a type indicator (e.g. in a sample entry or for un-timed metadata), the URI shall be absolute, not relative and the format and meaning of the data must be defined by the URI in question. This identification may be hierarchical, in that an initial sub-string of the URI identifies the overall nature or family of the data (e.g. urn:oid: identifies that the metadata is labelled by an ISO-standard object identifier).

The URI should be, but is not required to be, de-referencable. It may be string compared by readers with the set of URI types it knows and recognizes. URIs provide a large non-colliding non-registered space for type identifiers.

If the URI contains a domain name (e.g. it is a URL), then it should also contain a month-date in the form mmyyyy. That date shall be near the time of the definition of the extension, and it must be true that the URI was defined in a way authorized by the owner of the domain name at that date. (This avoids problems when domain names change ownership).

### Box order

An overall view of the normal encapsulation structure is provided in the following informative Table 2. In the event of a conflict between this table and the prose, the prose prevails. The order of boxes within its container is not necessarily indicated in Table 2.

The table shows those boxes that may occur at the top-level in the left-most column; indentation is used to show possible containment. Thus, for example, a TrackHeaderBox ('tkhd') is found in a TrackBox ('trak'), which is found in a MovieBox ('moov'). Not all boxes need to be used in all files; the mandatory boxes are marked with an asterisk (\*). See the description of the individual boxes for a discussion of what must be assumed if the optional boxes are not present.

Objects using an extended type may be placed in a wide variety of containers, not just the top level.

In order to improve interoperability and utility of the files, the following rules and guidelines shall be followed for the order of boxes:

1. The FileTypeBox shall occur before any variable-length box (e.g. movie, free space, media data). Only a fixed-size box such as a file signature, if required, may precede it.
2. It is strongly recommended that all header boxes be placed first in their container: these boxes are the MovieHeaderBox, TrackHeaderBox, MediaHeaderBox, and the specific media headers inside the MediaInformationBox (e.g. the VideoMediaHeaderBox).
3. Any movie fragment boxes should be in sequence order (see subclause 8.8.5).
4. It is recommended that the boxes within the SampleTableBox be in the following order: SampleDescriptionBox, TimeToSampleBox, SampleToChunkBox, SampleSizeBox, ChunkOffsetBox.
5. It is strongly recommended that the TrackReferenceBox and EditBox (if any) should precede the MediaBox, and the HandlerBox should precede the MediaInformationBox, and the DataInformationBox should precede the SampleTableBox.
6. It is recommended that UserDataBoxes be placed last in their container.
7. It is recommended that the MovieFragmentRandomAccessBox, if present, be last in the file.
8. It is recommended that the ProgressiveDownloadInfoBox be placed as early as possible in files, for maximum utility.

Table 2 — Box types, structure and cross-reference

| **Box types, structure, and cross-reference** | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ftyp |  |  |  |  |  |  | \* | 4.2.3 | *file type and compatibility* |
| otyp |  |  |  |  |  |  |  | 8.19.5 | *original file-type* |
| pdin |  |  |  |  |  |  |  | 8.1.3 | *progressive download information* |
| moov |  |  |  |  |  |  | \* | 8.2.1 | *container for all the structure-data* |
|  | mvhd |  |  |  |  |  | \* | 8.2.2 | *movie header, overall declarations* |
|  | meta |  |  |  |  |  |  | 8.11.1 | *metadata* |
|  |  | grpl |  |  |  |  |  | 8.18.2 | *entities groups list* |
|  |  |  | prsl |  |  |  |  | 8.18.4.1 | *preselection group* |
|  |  |  |  | elng |  |  |  | 8.4.6 | *extended language tag* |
|  |  |  |  | udta |  |  |  | 8.10.1 | *user-data* |
|  |  |  |  | kind |  |  |  | 8.10.4 | *track kind* |
|  |  |  |  | labl |  |  |  | 8.10.5 | *label* |
|  |  |  |  | chnl |  |  |  | 12.2.4 | *channel layout* |
|  |  |  |  | ardi |  |  |  | 12.2.8 | *audio rendering indication* |
|  |  |  |  | aelm |  |  |  | 12.2.9 | *audio element* |
|  |  |  |  |  | elng |  |  | 8.4.6 | *extended language tag* |
|  |  |  |  |  | kind |  |  | 8.10.4 | *track kind* |
|  |  |  |  |  | labl |  |  | 8.10.5 | *label* |
|  |  |  |  |  | chnl |  |  | 12.2.4 | *channel layout* |
|  |  |  |  |  | aedb |  |  | 12.2.10 | *audio element description* |
|  |  |  |  |  |  | aepp |  | 12.2.11 | *audio element positioning interactivity polar* |
|  |  |  |  |  |  | aepr |  | 12.2.12 | *audio element prominence interactivity* |
|  |  |  |  | aesb |  |  |  | 12.2.13 | *audio element selection* |
|  |  |  |  |  | labl |  |  | 8.10.5 | *label* |
|  |  |  |  |  | aelm |  |  | 12.2.9 | *audio element* |
|  |  |  |  |  |  | elng |  | 8.4.6 | *extended language tag* |
|  |  |  |  |  |  | kind |  | 8.10.4 | *track kind* |
|  |  |  |  |  |  | labl |  | 8.10.5 | *label* |
|  |  |  |  |  |  | chnl |  | 12.2.4 | *channel layout* |
|  |  |  |  |  |  | aedb |  | 12.2.10 | *audio element description*  *[Ed.Note] 'aepp' and 'aepr' child boxes are not described in the table due to lack of table columns* |
|  |  |  |  |  | aepp |  |  | 12.2.11 | *audio element positioning interactivity polar* |
|  |  |  |  |  | aepr |  |  | 12.2.12 | *audio element prominence interactivity* |
|  |  |  |  |  | aesd |  |  | 12.2.14 | *audio element selection description* |
|  | trak |  |  |  |  |  | \* | 8.3.1 | *container for an individual track or stream* |
|  |  | ttyp |  |  |  |  |  | 8.3.6 | *track type* |
|  |  | tkhd |  |  |  |  | \* | 8.3.2 | *track header, overall information about the track* |
|  |  | tref |  |  |  |  |  | 8.3.3 | *track reference container* |
|  |  | trgr |  |  |  |  |  | 8.3.4 | *track grouping indication* |
|  |  |  | msrc |  |  |  |  | 8.3.4.4.1 | *multi-source presentation track group type box* |
|  |  |  | ster |  |  |  |  | 8.3.4.4.2 | *stereoscopic pair track group type box* |
|  |  |  | ~~pres~~ |  |  |  |  | ~~8.3.4.4.3~~ | *~~preselection track group type box~~* |
|  |  |  |  | ~~prsp~~ |  |  |  | ~~8.3.4.4.3.4~~ | *~~preselection processing~~* |
|  |  | edts |  |  |  |  |  | 8.6.5 | *edit list container* |
|  |  |  | elst |  |  |  |  | 8.6.6 | *an edit list* |
|  |  | meta |  |  |  |  |  | 8.11.1 | *metadata* |
|  |  | mdia |  |  |  |  | \* | 8.4 | *container for the media information in a track* |
|  |  |  | mdhd |  |  |  | \* | 8.4.2 | *media header, overall information about the media* |
|  |  |  | hdlr |  |  |  | \* | 8.4.3 | *handler, declares the media (handler) type* |
|  |  |  | elng |  |  |  |  | 8.4.6 | *extended language tag* |
|  |  |  | minf |  |  |  | \* | 8.4.4 | *media information container* |
|  |  |  |  | vmhd |  |  |  | 12.1.2 | *video media header, overall information (video track only)* |
|  |  |  |  | smhd |  |  |  | 12.2.2 | *sound media header, overall information (sound track only)* |
|  |  |  |  | hmhd |  |  |  | 12.4.3 | *hint media header, overall information (hint track only)* |
|  |  |  |  | sthd |  |  |  | 12.6.2 | *subtitle media header, overall information (subtitle track only)* |
|  |  |  |  | nmhd |  |  |  | 8.4.5.2 | *Null media header, overall information (some tracks only)* |
|  |  |  |  | dinf |  |  | \* | 8.7.1 | *data information box, container* |
|  |  |  |  |  | dref |  | \* | 8.7.2 | *data reference box, declares source(s) of media data in track* |
|  |  |  |  | stbl |  |  | \* | 8.5.1 | *sample table box, container for the time/space map* |
|  |  |  |  |  | stsd |  | \* | 8.5.2 | *sample description box (codec types, initialization etc.)* |
|  |  |  |  |  | stts |  | \* | 8.6.1.2 | *(decoding) time-to-sample* |
|  |  |  |  |  | ctts |  |  | 8.6.1.3 | *(composition) time to sample* |
|  |  |  |  |  | cslg |  |  | 8.6.1.4 | *composition to decode timeline mapping* |
|  |  |  |  |  | stsc |  | \* | 8.7.4 | *sample-to-chunk, partial data-offset information* |
|  |  |  |  |  | stsz |  |  | 8.7.3.2 | *sample sizes (framing)* |
|  |  |  |  |  | stz2 |  |  | 8.7.3.3 | *compact sample sizes (framing)* |
|  |  |  |  |  | stco |  | \* | 8.7.5 | *chunk offset, partial data-offset information* |
|  |  |  |  |  | co64 |  |  | 8.7.5 | *64-bit chunk offset* |
|  |  |  |  |  | stss |  |  | 8.6.2 | *sync sample table* |
|  |  |  |  |  | stsh |  |  | 8.6.3 | *shadow sync sample table* |
|  |  |  |  |  | padb |  |  | 8.7.6 | *sample padding bits* |
|  |  |  |  |  | stdp |  |  | 8.7.6 | *sample degradation priority* |
|  |  |  |  |  | sdtp |  |  | 8.6.4 | *independent and disposable samples* |
|  |  |  |  |  | sbgp |  |  | 8.9.2 | *sample-to-group* |
|  |  |  |  |  | sgpd |  |  | 8.9.3 | *sample group description* |
|  |  |  |  |  | subs |  |  | 8.7.7 | *sub-sample information* |
|  |  |  |  |  | saiz |  |  | 8.7.8 | *sample auxiliary information sizes* |
|  |  |  |  |  | saio |  |  | 8.7.9 | *sample auxiliary information offsets* |
|  |  | udta |  |  |  |  |  | 8.10.1 | *user-data* |
|  |  |  | cprt |  |  |  |  | 8.10.2 | *copyright etc.* |
|  |  |  | tsel |  |  |  |  | 8.10.3 | *track selection box* |
|  |  |  | kind |  |  |  |  | 8.10.4 | *track kind box* |
|  |  |  | strk |  |  |  |  | 8.14.3 | *sub track box* |
|  |  |  |  | stri |  |  |  | 8.14.4 | *sub track information box* |
|  |  |  |  | strd |  |  |  | 8.14.5 | *sub track definition box* |
|  |  |  | ludt |  |  |  |  | 12.2.7 | *audio stream loudness* |
|  | tkgd |  |  |  |  |  |  | 8.3.5 | *track group description box* |
|  |  | prse |  |  |  |  |  | 8.3.5.4.1 | *preselection track group entry* |
|  |  |  | elng |  |  |  |  | 8.4.6 | *extended language tag* |
|  |  |  | udta |  |  |  |  | 8.10.1 | *user-data* |
|  |  |  | kind |  |  |  |  | 8.10.4 | *track kind* |
|  |  |  | labl |  |  |  |  | 8.10.5 | *label* |
|  |  |  | chnl |  |  |  |  | 12.2.4 | *channel layout* |
|  |  |  | ardi |  |  |  |  | 12.2.8 | *audio rendering indication* |
|  |  |  | aelm |  |  |  |  | 12.2.9 | *audio element* |
|  |  |  |  | elng |  |  |  | 8.4.6 | *extended language tag* |
|  |  |  |  | kind |  |  |  | 8.10.4 | *track kind* |
|  |  |  |  | labl |  |  |  | 8.10.5 | *label* |
|  |  |  |  | chnl |  |  |  | 12.2.4 | *channel layout* |
|  |  |  |  | aedb |  |  |  | 12.2.10 | *audio element description* |
|  |  |  |  |  | aepp |  |  | 12.2.11 | *audio element positioning interactivity polar* |
|  |  |  |  |  | aepr |  |  | 12.2.12 | *audio element prominence interactivity* |
|  |  |  | aesb |  |  |  |  | 12.2.13 | *audio element selection* |
|  |  |  |  | labl |  |  |  | 8.10.5 | *label* |
|  |  |  |  | aelm |  |  |  | 12.2.9 | *audio element* |
|  |  |  |  |  | elng |  |  | 8.4.6 | *extended language tag* |
|  |  |  |  |  | kind |  |  | 8.10.4 | *track kind* |
|  |  |  |  |  | labl |  |  | 8.10.5 | *label* |
|  |  |  |  |  | chnl |  |  | 12.2.4 | *channel layout* |
|  |  |  |  |  | aedb |  |  | 12.2.10 | *audio element description*  *[Ed.Note] 'aepp' and 'aepr' child boxes are not described in the table due to lack of table columns* |
|  |  |  |  | aepp |  |  |  | 12.2.11 | *audio element positioning interactivity polar* |
|  |  |  |  | aepr |  |  |  | 12.2.12 | *audio element prominence interactivity* |
|  |  |  |  | aesd |  |  |  | 12.2.14 | *audio element selection description* |
|  | mvex |  |  |  |  |  |  | 8.8.1 | *movie extends box* |
|  |  | mehd |  |  |  |  |  | 8.8.2 | *movie extends header box* |
|  |  | trex |  |  |  |  | \* | 8.8.3 | *track extends defaults* |
|  |  | leva |  |  |  |  |  | 8.8.13 | *level assignment* |
|  | udta |  |  |  |  |  |  | 8.10.1 | *user-data* |
|  |  | cprt |  |  |  |  |  | 8.10.2 | *copyright etc.* |
| moof |  |  |  |  |  |  |  | 8.8.4 | *movie fragment* |
|  | mfhd |  |  |  |  |  | \* | 8.8.5 | *movie fragment header* |
|  | meta |  |  |  |  |  |  | 8.11.1 | *metadata* |
|  | traf |  |  |  |  |  |  | 8.8.6 | *track fragment* |
|  |  | tfhd |  |  |  |  | \* | 8.8.7 | *track fragment header* |
|  |  | trun |  |  |  |  |  | 8.8.8 | *track fragment run* |
|  |  | sbgp |  |  |  |  |  | 8.9.2 | *sample-to-group* |
|  |  | sgpd |  |  |  |  |  | 8.9.3 | *sample group description* |
|  |  | subs |  |  |  |  |  | 8.7.7 | *sub-sample information* |
|  |  | saiz |  |  |  |  |  | 8.7.8 | *sample auxiliary information sizes* |
|  |  | saio |  |  |  |  |  | 8.7.9 | *sample auxiliary information offsets* |
|  |  | tfdt |  |  |  |  |  | 8.8.12 | *track fragment decode time* |
|  |  | meta |  |  |  |  |  | 8.11.1 | *metadata* |
|  |  | udta |  |  |  |  |  | 8.10.1 | *user-data* |
|  | udta |  |  |  |  |  |  | 8.10.1 | *user-data* |
| mfra |  |  |  |  |  |  |  | 8.8.9 | *movie fragment random access* |
|  | tfra |  |  |  |  |  |  | 8.8.10 | *track fragment random access* |
|  | mfro |  |  |  |  |  | \* | 8.8.11 | *movie fragment random access offset* |
| mdat |  |  |  |  |  |  |  | 8.2.2 | *media data container* |
| free |  |  |  |  |  |  |  | 8.1.2 | *free space* |
| skip |  |  |  |  |  |  |  | 8.1.2 | *free space* |
| imda |  |  |  |  |  |  |  | 8.1.4 | *media data container that contains an identifier to be used with data references* |
| meta |  |  |  |  |  |  |  | 8.11.1 | *metadata* |
|  | hdlr |  |  |  |  |  | \* | 8.4.3 | *handler, declares the metadata (handler) type* |
|  | dinf |  |  |  |  |  |  | 8.7.1 | *data information box, container* |
|  |  | dref |  |  |  |  |  | 8.7.2 | *data reference box, declares source(s) of metadata items* |
|  | iloc |  |  |  |  |  |  | 8.11.2.3 | *item location* |
|  | ipro |  |  |  |  |  |  | 8.11.5 | *item protection* |
|  |  | sinf |  |  |  |  |  | 13.4.2 | *protection scheme information box* |
|  |  |  | frma |  |  |  |  | 13.4.3 | *original format box* |
|  |  |  | schm |  |  |  |  | 13.4.6 | *scheme type box* |
|  |  |  | schi |  |  |  |  | 13.4.7 | *scheme information box* |
|  | iinf |  |  |  |  |  |  | 8.11.6 | *item information* |
|  | xml |  |  |  |  |  |  | 8.11.2 | *XML container* |
|  | bxml |  |  |  |  |  |  | 8.11.2 | *binary XML container* |
|  | pitm |  |  |  |  |  |  | 8.11.4 | *primary item reference* |
|  | fiin |  |  |  |  |  |  | 8.13.2 | *file delivery item information* |
|  |  | paen |  |  |  |  |  | 8.13.2 | *partition entry* |
|  |  |  | fire |  |  |  |  | 8.13.7 | *file reservoir* |
|  |  |  | fpar |  |  |  |  | 8.13.3 | *file partition* |
|  |  |  | fecr |  |  |  |  | 8.13.4 | *FEC reservoir* |
|  |  | segr |  |  |  |  |  | 8.13.5 | *file delivery session group* |
|  |  | gitn |  |  |  |  |  | 8.13.6 | *group id to name* |
|  | idat |  |  |  |  |  |  | 8.11.11 | *item data* |
|  | iref |  |  |  |  |  |  | 8.11.12 | *item reference* |
|  | grpl |  |  |  |  |  |  | 8.18.2 | *entities groups list* |
| styp |  |  |  |  |  |  |  | 8.16.2 | *segment type* |
| sidx |  |  |  |  |  |  |  | 8.16.3 | *segment index* |
| ssix |  |  |  |  |  |  |  | 8.16.4 | *subsegment index* |
| prft |  |  |  |  |  |  |  | 8.16.5 | *producer reference time* |
| !mov |  |  |  |  |  |  |  | 8.19.6 | *compressed movie box* |
| !mof |  |  |  |  |  |  |  | 8.19.7 | *compressed movie fragment box* |
| !six |  |  |  |  |  |  |  | 8.19.8 | *compressed segment index box* |
| !ssx |  |  |  |  |  |  |  | 8.19.9 | *compressed subsegment index box* |

## Time structure overview

Tracks identify, in *decoding order*, of a sequence of *samples.* Each sample has a *decoding timestamp* that is computed by adding to the previous sample's decoding timestamp, the previous sample's duration (as given by the values in the TimeToSampleBox or the equivalent field in movie fragments). The decoding timestamp of the first sample is defined as being at time zero. This forms the decoding timeline of a track.

In some coding systems (notably video) samples are coded in a different order from their presentation order. In this case, each sample is assigned a *composition time* (as given by the values in the CompositionOffsetBox or the equivalent field in movie fragments), which is computed by adding a *composition offset* to the decoding timestamp. This forms the composition timeline, and re-orders the samples into *composition order*.

The *presentation timeline* for each track is formed by the concatenation of sections of the composition timeline by means of explicit or implicit *edit lists*.

The presentation timelines of all the tracks are aligned at their zero point. This forms the presentation timeline for the presentation as a whole. This aligned zero point is the nominal time at which presentation starts and from which movie and track durations are measured.

Composition offsets can be signed or unsigned. When they are unsigned, the composition timeline and the decoding timeline are related, and the decoding and compositions times can be considered as enabling a hypothetical system, that is capable of instant decoding, to manage buffering. When they are signed, the composition timeline and the decoding timeline are disconnected. They can be reconnected using the CompositionToDecodeBox, if needed, though many systems do not use decoding timestamps, merely decoding in decoding order.

## Identifiers

The track identifiers used in a movie file are unique within that file; no two tracks shall use the same identifier. Under unified identifier handling (see E.18) this uniqueness requirement is extended to other identifiers.

The next track identifier value stored in next\_track\_ID in the MovieHeaderBox generally contains a value one greater than the largest identifier value, of the set required to be unique, found in the file. This enables easy generation of a unique identifier under most circumstances. However, if this value is equal to ones (32-bit unsigned maxint), then a search for an unused unique identifier is needed for all additions.

## Brand identification

The definitions of the brands that apply to timed presentations are specified in Annex E.

## Uniform resource locators (URLs)

When a file conformant to this document is identified by URL, a URL fragment (if present) shall follow the syntax(es) documented in Annex C.

When files are identified by a MIME type, the syntax specified in IETF RFC 6381[25] and Annex K shall be used for any parameters.

# Streaming support

Segmented streaming is supported by segments as defined in 3.1.50 and 8.16.

Transformed streaming into streaming protocols is supported by hint tracks as defined in 12.4, with specific formats for some protocols in Clause 9; there is a general overview in A.12.

# Box structures

## File structure and general boxes

### Media data box

* + - 1. Definition

Box Type: 'mdat'  
Container: File  
Mandatory: No  
Quantity: Zero or more

This box contains the media data. For example, this box contains video frames for video tracks. A presentation may contain zero or more MediaDataBoxes. The actual media data follows the type field; its structure is described by the structure-data (see particularly the SampleTableBox, subclause 8.5, and the ItemLocationBox, subclause 8.11.2.3).

In large presentations, it may be desirable to have more data in this box than a 32-bit size permits. In this case, the large variant of the size field, above in subclause 4.2, is used.

There may be any number of these boxes in the file (including zero, if all the media data is in other files). The structure-data refers to media data by its absolute offset within the file (see subclause 8.7.5, the ChunkOffsetBox); so MediaDataBox headers and free space may easily be skipped, and files without any box structure may also be referenced and used.

* + - 1. Syntax

aligned(8) class MediaDataBox extends Box('mdat')  
{  
 bit(8) data[];  
}

* + - 1. Semantics

data is the contained media data

### Free space box

* + - 1. Definition

Box Types: 'free', 'skip'  
Container: File or other box  
Mandatory: No  
Quantity: Zero or more

The contents of a FreeSpaceBox are irrelevant and may be ignored, or the box deleted, without affecting the presentation. (Care should be exercised when deleting the box, as this may invalidate offsets used to refer to other data, unless this box is after all the media data).

* + - 1. Syntax

aligned(8) class FreeSpaceBox extends Box(free\_type)  
{  
 unsigned int(8) data[];  
}

* + - 1. Semantics

free\_type shall be 'free' or 'skip'.

### Progressive download information box

* + - 1. Definition

Box Types: 'pdin'  
Container: File  
Mandatory: No  
Quantity: Zero or One

The ProgressiveDownloadInfoBox aids the progressive download of an ISO base media file. The box contains pairs of numbers (to the end of the box) specifying combinations of effective file download bitrate in units of bytes/sec and a suggested initial playback delay in units of milliseconds.

A receiving party can estimate the download rate it is experiencing, and from that obtain an upper estimate for a suitable initial delay by linear interpolation between pairs, or by extrapolation from the first or last entry.

It is recommended that the ProgressiveDownloadInfoBox be placed as early as possible in files, for maximum utility.

* + - 1. Syntax

aligned(8) class ProgressiveDownloadInfoBox  
 extends FullBox('pdin', version = 0, 0)  
{  
 for (i=0; ; i++) { // to end of box  
 unsigned int(32) rate;  
 unsigned int(32) initial\_delay;  
 }  
}

* + - 1. Semantics

rate is a download rate expressed in bytes/second

initial\_delay is the suggested delay to use when playing the file, such that if download continues at the given rate, all data within the file will arrive in time for its use and playback should not need to stall.

### Identified media data box

* + - 1. Definition

Box Type: 'imda'  
Container: File  
Mandatory: No  
Quantity: Zero or more

This box contains the media data. Its semantics are the same as those for MediaDataBox but it additionally contains an identifier that is used in setting up data references to the contained media data.

* + - 1. Syntax

aligned(8) class IdentifiedMediaDataBox extends Box('imda')  
{  
 unsigned int(32) imda\_identifier;  
 bit(8) data[]; // until the end of the box  
}

* + - 1. Semantics

imda\_identifier shall differ from the imda\_identifier values of the other IdentifiedMediaDataBoxes of the file.

## Movie structure

### Movie box

* + - 1. Definition

Box Type: 'moov'  
Container: File  
Mandatory: Yes  
Quantity: Exactly one

The structure-data for a presentation is stored in the single MovieBox which occurs at the top-level of a file. Normally this box is close to the beginning or end of the file, though this is not required.

* + - 1. Syntax

aligned(8) class MovieBox extends Box('moov')  
{  
}

### Movie header box

* + - 1. Definition

Box Type: 'mvhd'  
Container: MovieBox  
Mandatory: Yes  
Quantity: Exactly one

This box defines overall information which is media-independent, and relevant to the entire presentation considered as a whole.

The duration of a movie is usually the duration of the longest track (as documented by the duration field of the TrackHeaderBox); if any track has an indefinite duration, the movie should also have an indefinite duration. If there are tracks longer than the movie duration, it is recommended that playback terminate at the movie duration (i.e. that the longer tracks be implicitly trimmed to the movie duration); this can happen when two media have frame durations that are not exactly divisible, for example.

* + - 1. Syntax

aligned(8) class MovieHeaderBox extends FullBox('mvhd', version, 0)  
{  
 if (version==1) {  
 unsigned int(64) creation\_time;  
 unsigned int(64) modification\_time;  
 unsigned int(32) timescale;  
 unsigned int(64) duration;  
 } else { // version==0  
 unsigned int(32) creation\_time;  
 unsigned int(32) modification\_time;  
 unsigned int(32) timescale;  
 unsigned int(32) duration;  
 }  
 template int(32) rate = 0x00010000; // typically 1.0  
 template int(16) volume = 0x0100; // typically, full volume  
 const bit(16) reserved = 0;  
 const unsigned int(32) reserved[2] = 0;  
 template int(32) matrix[9] =  
 { 0x00010000,0,0,0,0x00010000,0,0,0,0x40000000 };  
 // Unity matrix  
 bit(32) pre\_defined[6] = 0;  
 unsigned int(32) next\_track\_ID;  
}

* + - 1. Semantics

version is an integer that specifies the version of this box (0 or 1 in this document)

creation\_time is an integer that declares the creation time of the presentation (in seconds since midnight, Jan. 1, 1904, in UTC time)

modification\_time is an integer that declares the most recent time the presentation was modified (in seconds since midnight, Jan. 1, 1904, in UTC time)

timescale is an integer that specifies the time-scale for the entire presentation; this is the number of time units that pass in one second. For example, a time coordinate system that measures time in sixtieths of a second has a time scale of 60.

duration is an integer that declares length of the presentation (in the indicated timescale). This property is derived from the presentation’s tracks: the value of this field corresponds to the duration of the longest track in the presentation. If the duration cannot be determined then duration is set to all 1s.

rate is a fixed point 16.16 number that indicates the preferred rate to play the presentation; 1.0 (0x00010000) is normal forward playback

volume is a fixed point 8.8 number that indicates the preferred playback volume. 1.0 (0x0100) is full volume.

matrix provides a transformation matrix for the video; (u,v,w) are restricted here to (0,0,1), hex values (0,0,0x40000000).

next\_track\_ID is a non-zero integer that indicates a value to use for the track\_ID of the next track to be added to this presentation. Zero is not a valid track\_ID value. The value of next\_track\_ID shall be larger than the largest track\_ID in use. If this value is equal to all 1s (32-bit maxint), and a new media track is to be added, then a search must be made in the file for an unused value of track\_ID.

## Track structure

### Track box

* + - 1. Definition

Box Type: 'trak'  
Container: MovieBox  
Mandatory: Yes  
Quantity: One or more

This is a container box for a single track of a presentation. A presentation consists of one or more tracks. Each track carries its own temporal and spatial information. Each track will contain its associated MediaBox.

Tracks are used for a number of purposes, including: (a) to contain media data (media tracks) and (b) to contain packetization information for streaming protocols (hint tracks).

There shall be at least one media track within a MovieBox, and all the media tracks that contributed to the hint tracks shall remain in the file, even if the media data within them is not referenced by the hint tracks; after deleting all hint tracks, the entire un-hinted presentation shall remain.

* + - 1. Syntax

aligned(8) class TrackBox extends Box('trak')  
{  
}

### Track header box

* + - 1. Definition

Box Type: 'tkhd'  
Container: TrackBox  
Mandatory: Yes  
Quantity: Exactly one

This box specifies the characteristics of a single track. Exactly one TrackHeaderBox is contained in a track.

In the absence of an edit list, the presentation of a track starts at the beginning of the overall presentation. An ‘empty’ edit is used to offset the start time of a track (see 8.6.6).

The tracks marked with the track\_in\_movie flag set to 1 are those that are intended by the file writer for direct presentation. Thus a track that is used as input to another track — either before or after decoding — but that is not presented by itself — should have the track\_in\_movie flag set to 0. Tracks having the track\_in\_movie flag set are candidates for playback, regardless of whether they are media tracks or reception hint tracks. A track may be used as input and also have the track\_in\_movie flag set to 1.

If a track is a member of a group that presents alternatives for presentation, either by using the alternate\_group field in the track header, or by using the TrackGroupBox with a group type that defines alternatives, then either only the preferred or default choice track should have the track\_in\_movie flag set to 1, or all tracks should have the track\_in\_movie flag set to 1 (if no default is to be indicated).

If an 'altr' entity group contains entities for playing, track\_in\_movie should be equal to 1 in all the tracks of the entity group.

If in a presentation no tracks have track\_in\_movie set, and therefore it appears that there is nothing to present, then a player may enable a track from each group for presentation; derived specifications can give further guidance and/or restrictions.

Tracks that are marked as not enabled (track\_enabled set to 0) shall be ignored and treated as if not present. Application environments may offer a way to enable/disable tracks at run-time and dynamically alter the state of this flag.

The processing of the pixel data from the output of the decoder to its rendering on the screen is not a conformance point of ISOBMFF. However, several structures enable signaling of such rendering features. They are based on the following assumptions:

1. Under the 'iso3' brand or brands that share its requirements, the TrackHeaderBox width and height assume that the rendered pixels are square (i.e. that the pixel aspect ratio is 1:1). For other brands, the use of the associated structure for rendering is undetermined.
2. The VisualSampleEntry documents the expected size of the pixel buffer needed to receive the codec output, possibly cropped by in-stream structures.

EXAMPLE: If a video codec works only with multiples of 16 pixels per line or column, and if the width and height of the video fed to the encoder is 1000x500, the encoder will typically, internally use 64x32 blocs of pixels, but it is expected to use codec-specific cropping structures, that are not exposed at the ISOBMFF level to output a 1000x500 video. The width and height of the VisualSampleEntry fields in this case will be 1000x500.

1. The PixelAspectRatioBox documents the aspect ratio that should be applied to the pixels output by the decoder but does not imply the adjustment. The associated adjustment should be taken care of by setting scaled values in the TrackHeaderBox.

EXAMPLE If prior to the encoder, the pixels are scaled horizontally by a factor of 1/2, at the output of the decoder, the inverse scaling should be applied to present non distorted videos. This is done by setting the TrackHeaderBox height equal to the VisualSampleEntry height and the TrackHeaderBox width equal to the double of the VisualSampleEntry width. Additionally, a PixelAspectRatioBox with a hSpacing twice bigger than its vSpacing field may be used, if in-stream structures do not carry that information.

1. Additionally, a CleanApertureBox may be provided to further crop the video.

The processing of the decoded pixel is assumed to be as follows:

1. Any cropping documented by a CleanApertureBox is applied on the pixels output by the decoder,
2. Then, if a CleanApertureBox is present, the cropped image is then scaled horizontally by the factor TrackHeaderBox.width/CleanAperture.width and vertically by TrackHeaderBox.height/CleanAperture.height
3. Otherwise, if a CleanApertureBox is not present, the decoded image is then scaled horizontally by the factor TrackHeaderBox.width/SampleEntry.width and vertically by TrackHeaderBox.height/SampleEntry.height.

NOTE 1 This operation is called in previous editions "normalization to track dimensions".

1. The matrix of the TrackHeaderBox is then applied
2. All visual tracks are superposed in increasing order of the TrackHeaderBox.layer value
3. The matrix of the MovieHeaderBox is then applied to the composition.

NOTE 2 This is a theoretical processing model and concrete implementations following it should avoid resampling the image, in particular when the combination of the above operations results in the identity transformation.

The duration field here does not include the duration of following movie fragments, if any, but only of the media in the enclosing MovieBox. The MovieExtendsHeaderBox may be used to document the duration including movie fragments, when desired and possible.

* + - 1. Syntax

aligned(8) class TrackHeaderBox extends FullBox('tkhd', version, flags)  
{  
 if (version==1) {  
 unsigned int(64) creation\_time;  
 unsigned int(64) modification\_time;  
 unsigned int(32) track\_ID;  
 const unsigned int(32) reserved = 0;  
 unsigned int(64) duration;  
 } else { // version==0  
 unsigned int(32) creation\_time;  
 unsigned int(32) modification\_time;  
 unsigned int(32) track\_ID;  
 const unsigned int(32) reserved = 0;  
 unsigned int(32) duration;  
 }  
 const unsigned int(32) reserved[2] = 0;  
 template int(16) layer = 0;  
 template int(16) alternate\_group = 0;  
 template int(16) volume = {if track\_is\_audio 0x0100 else 0};  
 const unsigned int(16) reserved = 0;  
 template int(32) matrix[9]=  
 { 0x00010000,0,0,0,0x00010000,0,0,0,0x40000000 };  
 // unity matrix  
 unsigned int(32) width;  
 unsigned int(32) height;  
}

* + - 1. Semantics

version is an integer that specifies the version of this box (0 or 1 in this document)

flags is a 24-bit integer with flags; the following values are defined:

track\_enabled: Flag mask is 0x000001. The value 1 indicates that the track is enabled. A disabled track (when the value of this flag is zero) is treated as if it were not present.

track\_in\_movie: Flag mask is 0x000002. The value 1 indicates that the track, or one of its alternatives (if any) forms a direct part of the presentation. The value 0 indicates that the track does not represent a direct part of the presentation.

NOTE When playing only this track results in an incomplete experience, the track\_in\_movie flag is suggested to be set to ‘0’ to prevent players from playing only the track. An example for setting the track\_in\_movie flag of a track to ‘0’ in the context of a preselection is when the track contains only the narrative speaker of an audio description service (also known as Visual Description Service).

track\_in\_preview: Flag mask is 0x000004. This flag currently has no assigned meaning, and the value should be ignored by readers. In the absence of further guidance (e.g. from derived specifications), the same value as for track\_in\_movie should be written.

track\_size\_is\_aspect\_ratio: Flag value is 0x000008. The value 1 indicates that the width and height fields are not expressed in pixel units. The values have the same units but these units are not specified. The values are only an indication of the desired aspect ratio. If the aspect ratios of this track and other related tracks are not identical, then the respective positioning of the tracks is undefined, possibly defined by external contexts.

creation\_time is an integer that declares the creation time of this track (in seconds since midnight, Jan. 1, 1904, in UTC time).

modification\_time is an integer that declares the most recent time the track was modified (in seconds since midnight, Jan. 1, 1904, in UTC time).

track\_ID is an integer that uniquely identifies this track over the entire life-time of this presentation; track\_IDs are never re-used and cannot be zero.

duration is an integer that indicates the duration of this track (in the timescale indicated in the MovieHeaderBox) This duration field may be indefinite (all 1s) when either there is no edit list and the MediaHeaderBox duration is indefinite (i.e. all 1s), or when an indefinitely repeated edit list is desired (see subclause 8.6.6 for repeated edits).. If there is no edit list and the duration is not indefinite, then the duration shall be equal to the media duration given in the MediaHeaderBox, converted into the timescale in the MovieHeaderBox. Otherwise the value of this field is equal to the sum of the durations of all of the track’s edits (possibly including repetitions).

layer specifies the front-to-back ordering of video tracks; tracks with lower numbers are closer to the viewer. 0 is the normal value, and -1 is in front of track 0, and so on.

alternate\_group is an integer that specifies a group or collection of tracks. If this field is 0 there is no information on possible relations to other tracks. If this field is not 0, it should be the same for tracks that contain alternate data for one another and different for tracks belonging to different such groups. Only one track within an alternate group should be played or streamed at any one time, and shall be distinguishable from other tracks in the group via attributes such as bitrate, codec, language, packet size etc. A group may have only one member.

volume is a fixed 8.8 value specifying the track's relative audio volume. Full volume is 1.0 (0x0100) and is the normal value. Its value is irrelevant for a purely visual track. Tracks may be composed by combining them according to their volume, and then using the overall MovieHeaderBox volume setting; or more complex audio composition (e.g. MPEG-4 BIFS) may be used.

matrix provides a transformation matrix for the video; (u,v,w) are restricted here to (0,0,1), hex (0,0,0x40000000).

width and height fixed-point 16.16 values are track-dependent as follows:

For text and subtitle tracks, they may, depending on the coding format, describe the suggested size of the rendering area. For such tracks, the value 0x0 may also be used to indicate that the data may be rendered at any size, that no preferred size has been indicated and that the actual size may be determined by the external context or by reusing the width and height of another track. For those tracks, the flag track\_size\_is\_aspect\_ratio may also be used.

For non-visual tracks (e.g. audio), they should be set to zero.

For all other tracks, they specify the track's visual presentation size. These need not be the same as the pixel dimensions of the images, which is documented in the sample entries; all images in the sequence are scaled to this size, before any overall transformation of the track represented by the matrix.Unless scaling is desired or needed, writers should set width and height to the dimensions of the images.

### Track reference box

* + - 1. Definition

Box Type: 'tref'  
Container: TrackBox  
Mandatory: No  
Quantity: Zero or one

This box includes a set of TrackReferenceTypeBoxes, each of which indicates, by its type, that the enclosing track has one of more references of that type. Each reference type shall occur at most once. Within each TrackReferenceTypeBox there is an array of track\_IDs; within a given array, a given value shall occur at most once. Other structures in the file formats index through these arrays; index values start at 1.

Exactly one TrackReferenceBox can be contained within the TrackBox.

If this box is not present, the track is not referencing any other track in any way. The reference array is sized to fill the reference type box.

* + - 1. Syntax

aligned(8) class TrackReferenceBox extends Box('tref')  
{  
 TrackReferenceTypeBox [];  
}

aligned(8) class TrackReferenceTypeBox (unsigned int(32) reference\_type) extends Box(reference\_type)  
{  
 unsigned int(32) track\_IDs[];  
}

* + - 1. Semantics

The TrackReferenceBox contains TrackReferenceTypeBoxes. There shall be at most one TrackReferenceTypeBox of a given type in a TrackReferenceBox.

track\_IDsis an array of integers providing the track identifiers of the referenced tracks or track\_group\_id values of the referenced track groups. Each value track\_IDs[i], where i is a valid index to the track\_IDs[] array,is an integer that provides a reference from the containing track to the track with track\_ID equal to track\_IDs[i] or to the track group with both track\_group\_id equal to track\_IDs[i] and (flags & 1) of TrackGroupTypeBox equal to 1. When a track\_group\_id value is referenced, the track reference applies to each track of the referenced track group individually unless stated otherwise in the semantics of particular track reference types. The value 0 shall not be present. In the array there shall be no duplicated value; however, a track\_ID may appear in the array and also be a member of one or more track groups for which the track\_group\_ids appear in the array. This means that in forming the list of tracks, after replacing track\_group\_ids by the track\_IDs of the tracks in those groups, there might be duplicate track\_IDs. A track\_group\_id shall not be used when the semantics of the reference requires that the reference be to a single track.

The reference\_type shall be set to one of the following values, or a value registered or from a derived specification or registration:

* 'hint' the referenced track(s) contain the original media for this hint track.
* 'cdsc' links a descriptive or metadata track to the content which it describes
* 'font' this track uses fonts carried/defined in the referenced track.
* 'hind' indicates that the referenced track(s) may contain media data required for decoding of the track containing the track reference, i.e., it should only be used if the referenced hint track is used. The referenced tracks shall be hint tracks. The 'hind' dependency can, for example, be used for indicating the dependencies between hint tracks documenting layered IP multicast over RTP.
* 'vdep' this track contains auxiliary depth video information for the referenced video track.
* 'vplx' this track contains auxiliary parallax video information for the referenced video track.
* 'subt' this track contains subtitle, timed text or still images of symbols or icons for the referenced track or any track in the alternate group to which the track belongs, if any.
* 'thmb' this track contains thumbnail images for the referenced track. A thumbnail track shall not be linked to another thumbnail track with the 'thmb' track reference.
* 'auxl' this track contains auxiliary media for the indicated track (e.g. depth map or alpha plane for video).
* 'cdtg' describes the referenced media tracks and track groups collectively; the 'cdtg' track reference shall only be present in timed metadata tracks.
* 'shsc' links a shadow sync track to a main track; see subclause 8.6.3
* 'aest' associated external stream track; see subclause 8.3.3.4.1.

NOTE 1 A track with reference type 'auxl' can have a coding dependency; its use is clarified by specifications that use it.

NOTE 2 When multiple track references describe an auxiliary video track, derived specifications can constrain or recommend which track references are used. For example, derived specifications can constrain or recommend whether to use 'vdep' or 'auxl' or both for auxiliary depth video track.

NOTE 3 Other structures index through the array of track references and hence position and order of them can be significant.

NOTE 4 A timed metadata track containing 'cdsc' track reference to a track\_group\_id value describes each track in the track group individually.

* + - 1. Track reference definitions
         1. Associated external stream track reference

A track reference of type 'aest' (meaning "associated external stream track") may be included in a media track. When present, the TrackReferenceTypeBox with reference\_type equal to 'aest' shall contain only a track identifier and shall not contain any track group identifier.

When a media track has a track reference of type 'aest', the following applies:

* The media track should have at least one sample identified as an EDRAP sample by being associated with an EDRAP sample group.
* The referenced track shall comply to the following constraints:
  + Each sample in the referenced track shall be identified as a sync sample.
  + The referenced track shall have both header flags track\_in\_movie and track\_in\_preview equal to 0.
  + The referenced track shall use a restricted scheme as follows:
    - The scheme\_type field in the SchemeTypeBox, which is in the RestrictedSchemeInfoBox, is equal to 'spkt' and the value of the mode field in the SamplePackingInformationBox is equal to 1.
    - Bit 0 of the flags field of the SchemeTypeBox is equal to 0, such that the value of (flags & 0x000001) is equal to 0.
* For each EDRAP sample sampleA in the media track, there shall be one and only one sample sampleB in the referenced track that has the same decoding time as sampleA, and sampleB shall contain all media data of the closest SAP sample of type 1, 2, or 3 that precedes sampleA in decoding order and the required preceding SAP or EDRAP samples of sampleA.

### Track group box

* + - 1. Definition

Box Type: 'trgr'  
Container: TrackBox  
Mandatory: No  
Quantity: Zero or one

This box enables indication of groups of tracks, where all tracks in a group share a particular characteristic or the tracks within a group have a particular relationship. The box contains zero or more boxes, and the particular characteristic or the relationship is indicated by the box type of the contained boxes. The contained boxes include an identifier, which can be used to conclude the tracks belonging to the same track group. The tracks that contain the same type of a contained box within the TrackGroupBox and have the same identifier value within these contained boxes belong to the same track group.

Track groups shall not be used to indicate dependency relationships between tracks. Instead, the TrackReferenceBox is used for such purposes.

Boxes derived from TrackGroupTypeBox shall have version equal to 0 unless defined otherwise for the value of track\_group\_type.

(flags & 1) equal to 1 in a TrackGroupTypeBox of a particular track\_group\_type indicates that track\_group\_id in that TrackGroupTypeBox is not equal to any track\_ID value and is not equal to track\_group\_id of any other TrackGroupTypeBox with a different track\_group\_type. When (flags & 1) is equal to 1 in a TrackGroupTypeBox with particular values of track\_group\_type and track\_group\_id, (flags & 1) shall be equal to 1 in all TrackGroupTypeBoxes of the same values of track\_group\_type and track\_group\_id, respectively.

Any values of flags such that (flags & 0x000FFE) is not equal to 0 are reserved. The values of flags shall be such that (flags & 0xFFF000) is equal to 0 unless defined otherwise for the value of track\_group\_type.

* + - 1. Syntax

aligned(8) class TrackGroupBox extends Box('trgr')  
{  
 Box boxes[];  
}

aligned(8) class TrackGroupTypeBox(unsigned int(32) track\_group\_type)   
 extends FullBox(track\_group\_type, version, flags)  
{  
 unsigned int(32) track\_group\_id;  
 // the remaining data may be specified   
 // for a particular track\_group\_type  
}

* + - 1. Semantics

boxes is an array of boxes that shall derive from TrackGroupTypeBox or FreeSpaceBox.

track\_group\_type indicates the track grouping type and shall be set to one of the following values, or a value registered, or a value from a derived specification or registration:

'msrc' indicates that this track belongs to a multi-source presentation. Specified in 8.3.4.4.1.

'ster' indicates that this track is either the left or right view of a stereo pair suitable for playback on a stereoscopic display. Specified in 8.3.4.4.2.

~~'pres' indicates that this track contributes to a preselection. Specified in 8.3.4.4.3.~~

The pair of track\_group\_id and track\_group\_type identifies a track group. The tracks that contain a particular TrackGroupTypeBox having the same value of track\_group\_id and track\_group\_type belong to the same track group.

* + - 1. Track group definitions
         1. Multi-source presentation

track\_group\_type equal to 'msrc' indicates that this track belongs to a multi-source presentation. The tracks that have the same value of track\_group\_id within a TrackGroupTypeBox of track\_group\_type 'msrc' are mapped as being originated from the same source. For example, a recording of a video telephony call may have both audio and video for both participants, and the value of track\_group\_id associated with the audio track and the video track of one participant differs from value of track\_group\_id associated with the tracks of the other participant.

* + - * 1. Stereoscopic pair

Definition

TrackGroupTypeBox with track\_group\_type equal to 'ster' indicates that this track is either the left or right view of a stereo pair suitable for playback on a stereoscopic display.

The tracks that have the same value of track\_group\_id within StereoVideoGroupBox form a stereo pair, and there shall be no more than two of such tracks for the same value of track\_group\_id.

NOTE Usually there are two tracks indicated to be a stereo pair with the StereoVideoGroupBox having the same value of track\_group\_id. However, only one track can be associated with a stereo pair in specific cases. For example, the file can be edited in a manner that one of the tracks forming a stereo pair gets removed. In another example, only one of the tracks of a stereo pair is selected for transmission, e.g. using DASH.

Syntax

aligned(8) class StereoVideoGroupBox extends TrackGroupTypeBox('ster')   
{  
 unsigned int(1) left\_view\_flag;  
 bit(31) reserved;  
}

Semantics

left\_view\_flag equal to 0 indicates the right view of a stereo pair, and left\_view\_flag equal to 1 indicates the left view of a stereo pair. When there are two tracks with the same value of track\_group\_id, the value of left\_view\_flag shall differ.

[Ed.Note] Unless major issues are found by NB comments in the EntityToGroup solution, the preselection group box is at risk of being removed. Comments are welcome.

* + - * 1. Preselection group box

Definition

The presence of a TrackGroupTypeBox with track\_group\_type equal to 'pres', which is also referred to as a PreselectionGroupBox, in a track indicates that this track contributes to a preselection.

All the tracks that have a track group with track\_group\_type equal to 'pres' and a particular value of track\_group\_id are part of the same preselection. The particular value of track\_group\_id is also referred to as the ID of the preselection.

NOTE 1 This means that a preselection is uniquely identified by the track\_group\_id of the track group.

When multiple tracks contribute to a preselection, the optionally present PreselectionProcessingBox provides information on how to process the track containing this box in the context of the preselection and relative to other tracks. Consequently, the content of the PreselectionProcessingBox may differ for each track within a preselection.

NOTE 2 Preselections consisting of only one track do not require any track-related processing. In this case, the PreselectionProcessingBox is typically not present in the PreselectionGroupBox.

Syntax

aligned(8) class PreselectionGroupBox extends TrackGroupTypeBox('pres')  
{  
 PreselectionProcessingBox preselection\_processing; // optional  
}

Semantics

preselection\_processing is an instance of the PreselectionProcessingBox, providing information needed for processing the containing track in the context of the preselection and relative to other tracks.

[Ed.Note] Unless major issues are found by NB comments in the EntityToGroup solution, the preselection processing box is at risk of being removed. Comments are welcome.

Preselection processing box

Definition

Box Type: 'prsp'  
Container: PreselectionGroupBox  
Mandatory: No  
Quantity: Zero or one

This box contains information about how the tracks contributing to the preselection can be processed. Media type specific boxes may be used to describe further processing.

Syntax

aligned(8) class PreselectionProcessingBox   
 extends FullBox('prsp', version = 0, flags )  
{  
 unsigned int(8) track\_order;  
 unsigned int(1) sample\_merge\_flag;  
 unsigned int(7) reserved;  
 // further attributes and Boxes defining additional processing of  
 // the track contributing to the preselection  
}

Semantics

track\_order defines the order of this track relative to other tracks in the preselection as described below.

sample\_merge\_flag equal to 1 indicates that this track is enabled to be merged with another track as described below.

Sample entry specific specifications might require the tracks for a preselection to be provided to the respective decoder instances in a specific order. Since other means, such as the track\_id, are not reliable for this purpose, the track\_order is used to order tracks in a preselection relative to each other. A lower value of track\_order indicates that at a given decoding time the sample of the containing track is provided to the decoder before the sample with the same given decoding time of other tracks with higher number. If two tracks in a preselection have their track\_order set to the same value or if the preselection processing box is absent for at least one of the tracks, the order of these tracks is not relevant for the preselection, and the samples with a particular decoding time for these two tracks can be provided to the decoder in any order.

A merge group is defined as a group of tracks, sorted according to track\_order, where one track with the sample\_merge\_flag set to 0 is followed by a group of consecutive tracks with the sample\_merge\_flag set to 1. All tracks of a merge group shall be of the same media type and shall have all samples decoding-time-aligned.

If the sample entry type is associated with a codec-specific process to merge samples of a preselection, this process shall be used.

NOTE 1 If the tracks in the merge group are all of sample entry type of “mhm2” (MPEG-H 3D Audio), the merging process is defined in ISO/IEC 23008-3:2019, subclause 14.6.

NOTE 2 Tracks in a merge group may have different sample entry types.

If the sample entry type is not associated with a codec-specific process to merge samples of a preselection, the following process shall be used:

Merging within the merge group shall proceed by forming tuples of track samples with the same decoding time across contributing tracks. The ordering of samples within the tuple shall be determined by track\_order. These tuples shall be formed by byte-wise concatenation of the samples resulting in a single sample with having the respective decoding time assigned. If generation of new tracks is targeted, each merge group shall result in a separate output track conformant to a media type derived from the media types of the merged tracks.

For tracks not part of a merge group, a merging process is not specified by this document.

[Ed.Note] Unless major issues are found by NB comments in the EntityToGroup solution, the feature track group description box (including the preselection track group entry box) is at risk of being removed. Comments are welcome.

#### Track group description box

##### Definitions

Box Type: 'tkgd'  
Container: MovieBox  
Mandatory: No  
Quantity: Zero or One

The TrackGroupDescriptionBox provides an array of TrackGroupEntryBoxes, where each TrackGroupEntryBox provides detailed characteristics of a particular track group.

The syntax of the TrackGroupEntryBox is determined by track\_group\_entry\_type. TrackGroupEntryBox is mapped to the track group by a unique track\_group\_entry\_type that is associated with a track\_group\_type defined in subclause 8.3.4.3. More than one TrackGroupEntryBox with the same track\_group\_entry\_type may be present in TrackGroupDescriptionBox, in that case TrackGroupEntryBoxes shall have different track\_group\_id.

Boxes derived from TrackGroupEntryBox shall have version equal to 0 unless defined otherwise for the value of track\_group\_entry\_type.

Any values of flags such that flags & 0x000FFF is not equal to 0 are reserved. The values of flags shall be such that flags & 0xFFF000 is equal to 0 unless defined otherwise for the value of track\_group\_entry\_type.

##### Syntax

aligned(8) class TrackGroupDescriptionBox extends Box('tkgd')  
{  
 Box boxes[];  
}

aligned(8) abstract class TrackGroupEntryBox (   
 unsigned int(32) track\_group\_entry\_type,   
 unsigned int(8) version,   
 unsigned int(24) flags)   
 extends FullBox(track\_group\_entry\_type, version, flags)   
{   
 unsigned int(32) track\_group\_id;  
 // the remaining data may be specified   
 // for a particular track\_group\_entry\_type   
}

##### Semantics

boxes is an array of boxes that shall derive from TrackGroupEntryBox or FreeSpaceBox.

track\_group\_entry\_type indicates a 4CC that is associated with a track\_group\_type.

The pair of track\_group\_id and track\_group\_entry\_type identifies the track group that the TrackGroupEntryBox describes.

##### Track group entry definitions

* + - * 1. Preselection track group entry box

Definition

Box Type: 'prse'  
Container: TrackGroupDescriptionBox  
Mandatory: No  
Quantity: Zero or more

Preselections can be characterized, for example, by language, kind or media specific attributes like audio rendering indications, audio interactivity or channel layouts. Attributes signalled in a PreselectionTrackGroupEntryBox take precedence over attributes signalled in contributing tracks.

PreselectionTrackGroupEntryBox shall describe only track groups identified by track\_group\_type equal to 'prse'.

For any preselection, if at least one contributing track in this file has the track\_in\_movie flag equal to 1, the PreselectionTrackGroupEntryBox shall be present in this file for the preselection; otherwise, the presence of the PreselectionTrackGroupEntryBox for the preselection in this file is optional.

All attributes uniquely characterizing a preselection should be present in the PreselectionTrackGroupEntryBox for the preselection.

Syntax

aligned(8) class PreselectionTrackGroupEntryBox  
 extends TrackGroupEntryBox('prse', version=0, flags)  
{  
 unsigned int(8) num\_tracks;  
 if (flags & preselection\_tag\_present)  
 utf8string preselection\_tag;  
 if (flags & selection\_priority\_present)  
 unsigned int(8) selection\_priority;  
 // Boxes describing the preselection  
}

Semantics

This box contains information on what experience is available when this preselection is selected.

Boxes suitable to describe a preselection include but are not limited to the following list of boxes defined in this document:

* AudioElementBox (subclause 12.2.9)
* AudioElementSelectionBox (subclause 12.2.13)
* ExtendedLanguageBox (subclause 8.4.6)
* UserDataBox (subclause 8.10.1)
* KindBox (subclause 8.10.4)
* LabelBox (subclause 8.10.5)
* AudioRenderingIndicationBox (subclause 12.2.8)
* ChannelLayout (subclause 12.2.4)

When contained in a PreselectionTrackGroupEntryBox, a UserDataBox shall not carry any of the above boxes.

flags the following values are defined:

preselection\_tag\_present: Flag mask is 0x001000. The value 1 indicates the presence of the preselection\_tag element

selection\_priority\_present: Flag mask is 0x002000. The value 1 indicates the presence of the selection\_priority element

num\_tracks specifies the number of non-alternative tracks grouped by this preselection track group.

A track grouped by this preselection track group is a track that has the 'pres' track group with track\_group\_id equal to the ID of this preselection.  
The number of non-alternative tracks grouped by this preselection track group is the sum of the following:

* the number of tracks that have alternate\_group equal to 0 and are grouped by this preselection track group,
* the number of unique non-zero alternate\_group values in all tracks that are grouped by this preselection track group.

The value of num\_tracks shall be greater than or equal to the number of non-alternative tracks grouped by this preselection track group in this file.  
A value equal to 0 indicates that the number of tracks grouped by this track group is unknown or not essential for processing the track group.  
NOTE 1 The value of num\_tracks can be greater than the number of non-alternative tracks containing a PreselectionGroupBox with the same track\_group\_id in this file when the preselection is split into multiple files.  
NOTE 2 When a player has access to fewer non-alternative tracks grouped by this preselection track group than indicated by num\_tracks, the player might need to omit the tracks grouped by this preselection track group.

preselection\_tag is a codec specific value that a playback system can provide to a decoder to uniquely identify one out of several preselections in the media.

selection\_priority is an integer that declares the priority of the preselection in cases where no other differentiation such as through the media language is possible. A lower value of selection\_priority indicates a higher priority.

NOTE 3 Not all tracks contributing to the playout of a preselection may be delivered in the same file.

NOTE 4 The kind box might utilize the Role scheme defined in ISO/IEC 23009-1:2022, subclause 5.8.5.5 as it provides a commonly used scheme to describe characteristics of preselections.

NOTE 5 Optional boxes contained within this box can carry information about the initial experience of the preselection in the referenced tracks. The preselection experience can change during the playback of these tracks (e.g. audio language can change during playback). These changes are not subject to the information presented in this box.

Further media type specific boxes may be used to describe properties of the preselection. Readers may ignore and skip boxes that are not recognized.

### Track type box

##### Definition

Box Type: 'ttyp'  
Container: TrackBox  
Mandatory: No  
Quantity: Zero or one

The payload of TrackTypeBox has the same syntax as the payload of FileTypeBox. The content of an instance of TrackTypeBox shall be such that it applies as the content of FileTypeBox, when all other tracks of the file are removed and only the track containing this box, and the tracks it references by means of track references, remain in the file.

NOTE TrackTypeBox can be used in specifying media profiles or track-specific brands.

##### Syntax

aligned(8) class TrackTypeBox extends GeneralTypeBox ('ttyp')  
{  
}

## Track media structure

### Media box

* + - 1. Definition

Box Type: 'mdia'  
Container: TrackBox  
Mandatory: Yes  
Quantity: Exactly one

The media declaration container contains all the objects that declare information about the media data within a track.

* + - 1. Syntax

aligned(8) class MediaBox extends Box('mdia')  
{  
}

### Media header box

* + - 1. Definition

Box Type: 'mdhd'  
Container: MediaBox  
Mandatory: Yes  
Quantity: Exactly one

The media header declares overall information that is media-independent, and relevant to characteristics of the media in a track.

* + - 1. Syntax

aligned(8) class MediaHeaderBox extends FullBox('mdhd', version, 0)  
{  
 if (version==1) {  
 unsigned int(64) creation\_time;  
 unsigned int(64) modification\_time;  
 unsigned int(32) timescale;  
 unsigned int(64) duration;  
 } else { // version==0  
 unsigned int(32) creation\_time;  
 unsigned int(32) modification\_time;  
 unsigned int(32) timescale;  
 unsigned int(32) duration;  
 }  
 bit(1) reserved = 0;  
 unsigned int(5) language[3]; // ISO-639-2/T language code  
 unsigned int(16) pre\_defined = 0;  
}

* + - 1. Semantics

version is an integer that specifies the version of this box (0 or 1)

creation\_time is an integer that declares the creation time of the media in this track (in seconds since midnight, Jan. 1, 1904, in UTC time).

modification\_time is an integer that declares the most recent time the media in this track was modified (in seconds since midnight, Jan. 1, 1904, in UTC time).

timescale is an integer that specifies the number of time units that pass in one second for this media. For example, a time coordinate system that measures time in sixtieths of a second has a time scale of 60.

duration is an integer that declares the duration of this media (in the scale of the timescale) and should be the largest composition timestamp plus the duration of that sample. If the duration cannot be determined then duration is set to all 1s.

NOTE The duration of an audio track may be smaller than the duration of the audio samples output by the decoder. This depends on the decoding process. The decoding of the last ISOBMFF sample of a track may produce additional audio samples that are not meant to be rendered.

language declares the language code for this media, as a packed three-character code defined in ISO 639-2. Each character is packed as the difference between its ASCII value and 0x60. Since the code is confined to being three lower-case letters, these values are strictly positive.

### Handler box

* + - 1. Definition

Box Type: 'hdlr'  
Container: MediaBox or MetaBox  
Mandatory: Yes  
Quantity: Exactly one in MediaBox  
 Zero or one in MetaBox, as constrained in subclause 8.11.1.1

This box within a MediaBox declares media type of the track, and thus the process by which the media-data in the track is presented. For example, a format for which the decoder delivers video is stored in a video track, identified by being handled by a video handler. The documentation of the storage of a media format identifies the media type which that format uses.

This box when present within a MetaBox, declares the structure or format of the MetaBox contents.

There is a general handler for metadata streams of any type; the specific format is identified by the sample entry, as for video or audio, for example.

* + - 1. Syntax

aligned(8) class HandlerBox extends FullBox('hdlr', version = 0, 0)  
{  
 unsigned int(32) pre\_defined = 0;  
 unsigned int(32) handler\_type;  
 const unsigned int(32) reserved[3] = 0;  
 utf8string name;  
}

* + - 1. Semantics

version is an integer that specifies the version of this box

handler\_type

– when present in a MediaBox, contains a value as defined in Clause 12, or a value from a derived specification, or registration.

– when present in a MetaBox, contains an appropriate value to indicate the format of the MetaBox contents. The value 'null' can be used in the primary MetaBox to indicate that it is merely being used to hold resources.

name gives a human-readable name for the track type (for debugging and inspection purposes).

### Media information box

* + - 1. Definition

Box Type: 'minf'  
Container: MediaBox  
Mandatory: Yes  
Quantity: Exactly one

This box contains all the objects that declare characteristic information of the media in the track.

* + - 1. Syntax

aligned(8) class MediaInformationBox extends Box('minf')  
{  
}

### Media information header boxes

* + - 1. Definition

There is a different media information header for each track type (corresponding to the media handler-type); the matching header shall be present, which may be one of those defined in Clause 12, or one defined in a derived specification.

The type of media header is used is determined by the definition of the media type and shall match the media handler.

#### Null media header box

* + - * 1. Definition

Box Types: 'nmhd'  
Container: MediaInformationBox  
Mandatory: Yes  
Quantity: Exactly one specific media header shall be present

Streams for which no specific media header is identified use a NullMediaHeaderBox, as defined here.

* + - * 1. Syntax

aligned(8) class NullMediaHeaderBox  
 extends FullBox('nmhd', version = 0, flags)  
{  
}

* + - * 1. Semantics

version - is an integer that specifies the version of this box.

flags - is a 24-bit integer with flags (currently all zero).

### Extended language tag

* + - 1. Definition

Box Type: 'elng'  
Container: MediaBox, PreselectionGroupBox, AudioElementBox  
Mandatory: No  
Quantity: Zero or one

The ExtendedLanguageBox represents media language information, and shall contain a code in conformance with IETF  BCP 47. It is an optional peer of the MediaHeaderBox, and shall occur after the MediaHeaderBox.

The extended language tag can provide better language information than the language field in the MediaHeaderBox, including information such as region, script, variation, and so on, as parts (or subtags).

The ExtendedLanguageBox is optional, and if it is absent the media language should be used. The extended language tag overrides the media language if they are not consistent.

For best compatibility with earlier players, if an extended language tag is specified, the most compatible language code should be specified in the language field of the MediaHeaderBox (for example, "eng" if the extended language tag is "en-UK"). If there is no reasonably compatible tag, the packed form of 'und' can be used.

#### Syntax

aligned(8) class ExtendedLanguageBox extends FullBox('elng', 0, 0)  
{  
 utf8string extended\_language;  
}

#### Semantics

extended\_language contains a IETF  BCP 47 compliant language tag string, such as "en-US", "fr-FR", or "zh-CN".

## Sample tables

### Sample table box

* + - 1. Definition

Box Type: 'stbl'  
Container: MediaInformationBox  
Mandatory: Yes  
Quantity: Exactly one

The sample table contains all the time and data indexing of the media samples in a track. Using the tables here, it is possible to locate samples in time, determine their type (e.g. I-frame or not), and determine their size, container, and offset into that container.

If the track that contains the SampleTableBox references no data, then the SampleTableBox does not need to contain any sub-boxes (this is not a very useful media track).

If the track that the SampleTableBox is contained in does reference data, then the following sub-boxes are required: SampleDescriptionBox, SampleSizeBox (or CompactSampleSizeBox), SampleToChunkBox, and ChunkOffsetBox (or ChunkLargeOffsetBox). Further, the SampleDescriptionBox shall contain at least one entry. A SampleDescriptionBox is required because it contains the data reference index field which indicates which DataEntry to use to retrieve the media samples. Without the SampleDescriptionBox, it is not possible to determine where the media samples are stored. The SyncSampleBox is optional.

The SyncSampleBox should be present in the SampleTableBox if some samples in the track, includingany track fragments, are non sync samples, but the flag sample\_is\_non\_sync\_sample of samples in track fragments is valid and describes the samples, evenif the SyncSampleBox is not present. If the track is not fragmented and the SyncSampleBox is not present, all samples in the track are sync samples.

A.9 provides a narrative description of random access using the structures defined in the SampleTableBox.

* + - 1. Syntax

aligned(8) class SampleTableBox extends Box('stbl')  
{  
}

### Sample description box

* + - 1. Definition

Box Types: 'stsd'  
Container: SampleTableBox  
Mandatory: Yes  
Quantity: Exactly one

The sample description table gives detailed information about the coding type used, and any initialization information needed for that coding. The syntax of the sample entry used is determined by both the format field and the media handler type.

The information stored in the SampleDescriptionBox after the entry-count is both track-type specific as documented here, and can also have variants within a track type (e.g. different codings may use different specific information after some common fields, even within a video track).

Which type of sample entry form is used is determined by the media handler, using a suitable form, such as one defined in Clause 12, or defined in a derived specification, or registration.

Multiple descriptions may be used within a track.

NOTE 1 Though the count is 32 bits, the number of items is usually much fewer, and is restricted by the fact that the reference index in the sample table is only 16 bits

If the ‘format’ field of a SampleEntry is unrecognized, neither the sample entry itself, nor the associated media samples, shall be decoded.

NOTE 2 The format field of a SampleEntry is restricted in this document not to contain the character '.' (dot). Derived specifications are encouraged to avoid using it as well as any character that requires encoding of the "codecs" parameter; see Annex K.

Derived specifications deriving Sample Entry classes listed in the table of 13.4.1 should be extremely careful. Derivation by adding boxes at the end of the class should be preferred as it preserves Sample Entry parsing and does not require a new 'encX' value. Adding a new field to a class will not allow for the use of the associated 'encX' scheme for parsing reasons. A new 'encX' scheme will have to be defined for signaling encrypted stream based on that derived class.

The definition of sample entries specifies boxes in a particular order, and this is usually also followed in derived specifications. For maximum compatibility, writers should construct files respecting the order both within specifications and as implied by the inheritance, whereas readers should be prepared to accept any box order.

All SampleEntry boxes may contain “extra boxes” not explicitly defined in the box syntax of this or derived specifications. When present, such boxes shall follow all defined fields and should follow any defined contained boxes. Decoders shall presume a sample entry box can contain extra boxes and shall continue parsing as though they are present until the containing box length is exhausted.

An optional BitRateBox may be present in any SampleEntry to signal the bit rate information of a stream. This can be used for buffer configuration.

All string fields shall be of type utf8string and null-terminated, even if unused. “Optional” means there is at least one null byte.

Entries that identify the format by MIME type, such as a TextSubtitleSampleEntry, TextMetaDataSampleEntry, or SimpleTextSampleEntry, all of which contain a MIME type, may be used to identify the format of streams for which a MIME type applies. A MIME type applies if the contents of the string in the optional configuration box (without its null termination), followed by the contents of a set of samples, starting with a sync sample and ending at the sample immediately preceding a sync sample, are concatenated in their entirety, and the result meets the decoding requirements for documents of that MIME type. Non-sync samples should be used only if that format specifies the behaviour of ‘progressive decoding’, and then the sample times indicate when the results of such progressive decoding should be presented (according to the media type).

NOTE 3 The samples in a track that is all sync samples are therefore each a valid document for that MIME type.

In some classes derived from SampleEntry, namespace and schema\_location are used both to identify the XML document content and to declare “brand” or profile compatibility. Multiple namespace identifiers indicate that the track conforms to the specification represented by each of the identifiers, some of which may identify supersets of the features present. A decoder should be able to decode all the namespaces in order to be able to decode and present correctly the media associated with this sample entry.

NOTE 4 Additionally, namespace identifiers might represent performance constraints, such as limits on document size, font size, drawing rate, etc., as well as syntax constraints, such as features that are not permitted or ignored.

* + - 1. Syntax

aligned(8) abstract class SampleEntry (unsigned int(32) format)  
 extends Box(format)  
{  
 const unsigned int(8) reserved[6] = 0;  
 unsigned int(16) data\_reference\_index;  
}

class BitRateBox extends Box('btrt')  
{  
 unsigned int(32) bufferSizeDB;  
 unsigned int(32) maxBitrate;  
 unsigned int(32) avgBitrate;  
}

aligned(8) class SampleDescriptionBox()  
 extends FullBox('stsd', version, 0)  
{  
 int i;  
 unsigned int(32) entry\_count;  
 for (i = 1 ; i <= entry\_count ; i++){  
 SampleEntry(); // an instance of a class derived from SampleEntry  
 }  
}

* + - 1. Semantics

version is set to zero. A version number of 1 shall be treated as a version of 0.

entry\_count is an integer that gives the number of entries in the following table.

SampleEntry is the appropriate sample entry.

data\_reference\_index is an integer that contains the index of the DataEntry to use to retrieve data associated with samples that use this sample entry. Data entries are stored in DataReferenceBoxes. The index ranges from 1 to the number of data entries.

bufferSizeDB gives the size of the decoding buffer for the media stream in bytes.

maxBitrate gives the maximum rate in bits/second over any window of one second; this is a measured value for stored content, or a value that a stream is configured not to exceed; the stream shall not exceed this bitrate.

avgBitrate gives the average rate in bits/second of the stream; this is a measured value (cumulative over the entire presentation) for stored content, or the configured target average bitrate for a stream.

### Degradation priority box

* + - 1. Definition

Box Type: 'stdp'  
Container: SampleTableBox  
Mandatory: No.  
Quantity: Zero or one.

This box contains the degradation priority of each sample. The values are stored in the table, one for each sample. The size of the table, sample\_count is taken from the sample\_count in the SampleSizeBox. Specifications derived from this define the exact meaning and acceptable range of the priority field.

* + - 1. Syntax

aligned(8) class DegradationPriorityBox  
 extends FullBox('stdp', version = 0, 0)  
{  
 int i;  
 for (i=0; i < sample\_count; i++) {  
 unsigned int(16) priority;  
 }  
}

* + - 1. Semantics

version - is an integer that specifies the version of this box.

priority - is integer specifying the degradation priority for each sample.

### Sample scale box

This box has been deprecated and is no longer defined in this document.

## Track time structures

### Time to sample boxes

* + - 1. Definition

The composition timestamps (CT) and decoding timestamps (DT) of samples are derived from the time to sample boxes, of which there are two types. The decoding timestamp is defined by the TimeToSampleBox, which documents the sample duration, that is, the difference between the decoding timestamp of the following sample and the sample at hand. The composition timestamps are defined in the CompositionOffsetBox as time offsets from decoding timestamps. If the composition and decoding timestamps are identical for every sample in the track, then only the TimeToSampleBox is required; the CompositionOffsetBox shall not be present and all composition offsets are defined to be zero.

The TimeToSampleBox shall give non-zero durations for all samples with the possible exception of the last one. Durations in the TimeToSampleBox are strictly positive (non-zero), except for the very last entry, which may be zero. This rule derives from the rule that there shall not be two samples in a stream with the same decoding timestamp. Great care must be taken when adding samples to a stream, that the sample that was previously last may need to have a non-zero duration established, in order to observe this rule. One approach in the case where the the duration of the last sample is indeterminate is to use an arbitrary small value and a ‘dwell’ edit.

Some coding systems may allow samples that are used only for reference and not output (e.g. a non-displayed reference frame in video). When any such non-output sample is present in a track, the following applies:

1. A non-output sample shall be given a composition timestamp which is outside the time-range of the samples that are output.
2. An edit list shall be used to exclude the composition times of the non-output samples.
3. When the track includes a CompositionOffsetBox,
4. version 1 of the CompositionOffsetBox shall be used,
5. the value of sample\_offset shall be set equal to the most negative number possible (for 32-bit values, -231) for each non-output sample,
6. the CompositionToDecodeBox should be contained in the SampleTableBox of the track, and
7. when the CompositionToDecodeBox is present for the track, the value of leastDecodeToDisplayDelta field in the box shall be equal to the smallest composition offset in the CompositionOffsetBox excluding the sample\_offset values for non-output samples.

NOTE Thus, leastDecodeToDisplayDelta is greater than -231.

In the example in Table 3 and Table 4, there is a sequence of I, P, and B frames, each with a sample duration of 10. The samples are stored as follows, with the indicated values for their sample durations and composition time offsets (the actual composition timestamp, CT, and decoding timestamp, DT, are given for reference). The re-ordering occurs because the predicted P frames must be decoded before the bi-directionally predicted B frames. The value of DT for a sample is always the sum of the durations of the preceding samples. Thus, in the absence of composition offsets, the total of the sample durations is the duration of the media in this track.

Table 3 — Closed GOP example

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GOP | /-- | --- | --- | --- | --- | --- | --\ | /-- | --- | --- | --- | --- | --- | --\ |
|  | I1 | P4 | B2 | B3 | P7 | B5 | B6 | I8 | P11 | B9 | B10 | P14 | B12 | B13 |
| DT | 0 | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 110 | 120 | 130 |
| CT | 10 | 40 | 20 | 30 | 70 | 50 | 60 | 80 | 110 | 90 | 100 | 140 | 120 | 130 |
| Duration | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 |
| Composition offset | 10 | 30 | 0 | 0 | 30 | 0 | 0 | 10 | 30 | 0 | 0 | 30 | 0 | 0 |

Table 4 — Open GOP example

|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GOP | /-- | -- | -- | -- | -- | --\ | /- | -- | -- | -- | --- | --\ |
|  | I3 | B1 | B2 | P6 | B4 | B5 | I9 | B7 | B8 | P12 | B10 | B11 |
| DT | 0 | 10 | 20 | 30 | 40 | 50 | 60 | 70 | 80 | 90 | 100 | 110 |
| CT | 30 | 10 | 20 | 60 | 40 | 50 | 90 | 70 | 80 | 120 | 100 | 110 |
| Duration | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 | 10 |
| Composition offset | 30 | 0 | 0 | 30 | 0 | 0 | 30 | 0 | 0 | 30 | 0 | 0 |

#### Decoding time to sample box

* + - * 1. Definition

Box Type: 'stts'  
Container: SampleTableBox  
Mandatory: Yes  
Quantity: Exactly one

This box contains a compact version of a table that allows indexing from decoding timestamp to sample number. Other tables give sample sizes and pointers, from the sample number. Each entry in the table gives the number of consecutive samples with the same sample duration, and that sample duration. By adding the sample durations a complete time-to-sample map may be built.

The TimeToSampleBox contains sample durations, the differences in decoding timestamps (DT):

DT[n+1] = DT[n] + sample\_delta[n]

The sample entries are ordered by decoding timestamps; therefore all the values of sample\_delta shall be non-negative.

The DT axis has a zero origin; DT[i] = SUM[for j=0 to i-1 of sample\_delta[j]], and in the absence of composition offsets, the sum of all sample durations gives the duration of the media in the track (not mapped to the overall timescale, and not considering any edit list).

* + - * 1. Syntax

aligned(8) class TimeToSampleBox extends FullBox('stts', version = 0, 0)  
{  
 unsigned int(32) entry\_count;  
 int i;  
 for (i=0; i < entry\_count; i++) {  
 unsigned int(32) sample\_count;  
 unsigned int(32) sample\_delta;  
 }  
}

For example with Table 3, the values of the syntax elements are:

entry\_count = 1  
  
sample\_count = 14   
sample\_delta = 10

* + - * 1. Semantics

version - is an integer that specifies the version of this box.

entry\_count - is an integer that gives the number of entries in the following table.

sample\_count - is an integer that counts the number of consecutive samples that have the given duration.

sample\_delta - is an integer that gives the difference between the decoding timestamp of the next sample and this one, in the time-scale of the media.

#### Composition time to sample box

* + - * 1. Definition

Box Type: 'ctts'  
Container: SampleTableBox  
Mandatory: No  
Quantity: Zero or one

This box provides the offset between decoding timestamp and composition timestamp. In version 0 of this box the decoding timestamp must be less than the composition timestamp, and the offsets are expressed as unsigned numbers such that if CT is the composition timestamp, CT[n] = DT[n] + sample\_offset[n].

In version 1 of this box, the composition timestamp is still derived from the decoding timestamp, but the offsets are signed. It is recommended that for the computed composition timestamps, there is exactly one sample with the value 0 (zero), and that no sample have a composition timestamp less than zero.

NOTE the presentation of samples with a composition timestamp less than 0 is undefined, as time 0 is the start time of the presentation across all tracks; nor can edit lists refer to samples with such composition timestamps.

Composition cannot happen before actual decoding. If negative offsets are used such that the composition timestamp of a sample becomes smaller than its decoding timestamp: either the decoding timestamp is ignored (for systems that only need decoding order, for example) or if decoding timestamps are needed, the decoding timeline must be offset to ensure that decoding happens in time. The CompositionToDecodeBox can be used to give advice on what offset may be needed.

For either version of the box, each sample shall have a unique composition timestamp, that is, the composition timestamp for two samples in the same track shall never be the same.

It may be true that there is no frame to compose at time 0; the handling of this is unspecified (systems might display the first frame for longer, or a suitable fill colour).

When version 1 of this box is used, the CompositionToDecodeBox may also be present in the sample table to relate the composition and decoding timelines. When backwards-compatibility or compatibility with an unknown set of readers is desired, version 0 of this box should be used when possible. In either version of this box, but particularly under version 0, if it is desired that the media start at track time 0, and the first media sample does not have a composition timestamp of 0, an edit list may be used to ‘shift’ the media to time 0.

The composition time to sample table is optional and shall only be present if DT and CT differ for any samples.

For example with Table 3, the values of the syntax elements are:

entry\_count = 10  
  
sample\_count = 1  
sample\_offset = 10  
  
sample\_count = 1  
sample\_offset = 30  
  
sample\_count = 2  
sample\_offset = 0  
  
sample\_count = 1   
sample\_offset = 30  
  
sample\_count = 2   
sample\_offset = 0  
  
sample\_count = 1   
sample\_offset = 10  
  
sample\_count = 1   
sample\_offset = 30  
  
sample\_count = 2  
sample\_offset = 0  
  
sample\_count = 1   
sample\_offset = 30  
  
sample\_count = 2  
sample\_offset = 0

* + - * 1. Syntax

aligned(8) class CompositionOffsetBox extends FullBox('ctts', version, 0)  
{  
 unsigned int(32) entry\_count;  
 int i;  
 if (version==0) {  
 for (i=0; i < entry\_count; i++) {  
 unsigned int(32) sample\_count;  
 unsigned int(32) sample\_offset;  
 }  
 }  
 else if (version == 1) {  
 for (i=0; i < entry\_count; i++) {  
 unsigned int(32) sample\_count;  
 signed int(32) sample\_offset;  
 }  
 }  
}

* + - * 1. Semantics

version - is an integer that specifies the version of this box.

entry\_count is an integer that gives the number of entries in the following table.

sample\_count is an integer that counts the number of consecutive samples that have the given offset.

sample\_offset is an integer that gives the offset between CT and DT, such that CT[n] = DT[n]+ sample\_offset[n].

#### Composition to decode box

##### Definition

Box Type: 'cslg'  
Container: SampleTableBox or TrackExtensionPropertiesBox  
Mandatory: No  
Quantity: Zero or one

When signed composition offsets are used, this box may be used to relate the composition and decoding timelines, and deal with some of the ambiguities that signed composition offsets introduce. This box is only advisory; it documents values that can be calculated by inspecting the track. There is no normative processing associated with this box. Readers that want to assure that, for example, all decoding timestamps precede composition timestamps might subtract a value equal to or larger than compositionToDTSShift from the decoding timestamps in the stream (note that this may yield negative decoding timestamps).

All these fields apply to the entire media (not just that selected by any edits). It is recommended that any edits, explicit or implied, not select any portion of the composition timeline that does not map to a sample. For example, if the smallest composition timestamp is 1000, then the default edit from 0 to the media duration leaves the period from 0 to 1000 associated with no media sample. Player behaviour, and what is composed in this interval, is undefined under these circumstances. It is recommended that the smallest computed CTS be zero, or match the beginning of the first edit.

The composition duration of the last sample in a track might be (often is) ambiguous or unclear; the field for composition end time can be used to clarify this ambiguity and, with the composition start time, establish a clear composition duration for the track.

When the CompositionToDecodeBox is included in the SampleTableBox, it documents the composition and decoding time relationships of the samples in the MovieBox only, not including any subsequent movie fragments. When the CompositionToDecodeBox is included in the TrackExtensionPropertiesBox, it documents the composition and decoding time relationships of the samples in all movie fragments following the MovieBox.

Version 1 of this box supports 64-bit times and should only be used if needed (at least one value does not fit into 32 bits).

NOTE in the absence of this box when signed composition offsets are used, correct decoding timestamps cannot in general be re-computed, even with complete inspection of all the samples. Hence, in order to enable converting ISOBMFF content to formats that do not support negative composition offsets, the CompositionToDecodeBox may be necessary.

##### Syntax

class CompositionToDecodeBox extends FullBox('cslg', version, 0)   
{  
 if (version==0) {  
 signed int(32) compositionToDTSShift;  
 signed int(32) leastDecodeToDisplayDelta;  
 signed int(32) greatestDecodeToDisplayDelta;  
 signed int(32) compositionStartTime;  
 signed int(32) compositionEndTime;  
 } else {  
 signed int(64) compositionToDTSShift;  
 signed int(64) leastDecodeToDisplayDelta;  
 signed int(64) greatestDecodeToDisplayDelta;  
 signed int(64) compositionStartTime;  
 signed int(64) compositionEndTime;  
 }  
}

##### Semantics

compositionToDTSShift: if this value is added to the composition timestamps (as calculated by the CTS offsets from the DTS), then for all samples, their CTS is guaranteed to be greater than or equal to their DTS, and the buffer model implied by the indicated profile/level will be honoured; if leastDecodeToDisplayDelta is positive or zero, this field can be 0; otherwise it should be at least (- leastDecodeToDisplayDelta)

leastDecodeToDisplayDelta: the smallest composition offset in the CompositionOffsetBox in this track

greatestDecodeToDisplayDelta: the largest composition offset in the CompositionOffsetBox in this track

compositionStartTime: the smallest computed composition timestamp (CTS) for any sample in the media of this track

compositionEndTime: the composition timestamp plus the composition duration, of the sample with the largest computed composition timestamp (CTS) in the media of this track; if this field takes the value 0, the composition end time is unknown.

### Sync sample box

* + - 1. Definition

Box Type: 'stss'  
Container: SampleTableBox  
Mandatory: No  
Quantity: Zero or one

This box provides a compact marking of sync samples within the stream. The table is arranged in strictly increasing order of sample number.

If the SyncSampleBox is not present, every sample is a sync sample.

NOTE it is not required that every sync sample be marked by this table (or the equivalent flag in Movie Fragments), only that samples so marked actually be sync samples.

* + - 1. Syntax

aligned(8) class SyncSampleBox extends FullBox('stss', version = 0, 0)   
{  
 unsigned int(32) entry\_count;  
 int i;  
 for (i=0; i < entry\_count; i++) {  
 unsigned int(32) sample\_number;  
 }  
}

* + - 1. Semantics

version - is an integer that specifies the version of this box.

entry\_count is an integer that gives the number of entries in the following table. If entry\_count is zero, there are no sync samples within the stream and the following table is empty.

sample\_number gives, for each sync sample in the stream, its sample number.

### Shadow sync

* + - 1. Shadow sync support

There are two forms of support for shadow sync; the sample table box in this subclause, and the use of the shadow sync track reference type in 8.3.3.

A track containing an 'shsc' track reference is called a shadow sync sample track, and the tracks pointed to by the 'shsc' track reference are called main tracks.

The shadow sync sample track provides an optional set of sync samples that can be used when seeking to a position or for similar operations performed to any of the associated main tracks.

When an 'shsc' track reference is present, the following constraints shall be obeyed:

– All samples of the shadow sync sample track shall be sync samples.

– Each main track shall have a sample that is aligned in decoding time with each sample of the shadow sync sample track.

– A concatenation of the following samples in the following order shall conform to the sample entry of the main track:

o Any selected sample of the shadow sync sample track, with the sample duration of the sample of the main track that is aligned in decoding time with the selected sample of the shadow sync sample track.

o Samples of the main track following the sample of the main track that is aligned in decoding time with the selected sample of the shadow sync sample track.

An 'shsc' track reference indicates that the decoded samples resulting from the concatenation specified above have acceptable quality for playback.

NOTE The samples in the main track that are aligned in decoding time with the samples in the shadow sync sample track are "switchable" samples that are constrained so that no samples preceding a "switchable" sample in decoding order are used as a prediction reference for any sample following the "switchable" sample in decoding order.

* + - 1. Shadow sync sample box

##### Definition

Box Type: 'stsh'  
Container: SampleTableBox  
Mandatory: No  
Quantity: Zero or one

The shadow sync table provides an optional set of sync samples that can be used when seeking or for similar purposes. In normal forward play they are ignored.

Each entry in the ShadowSyncSampleBox consists of a pair of sample numbers. The first entry (shadowed-sample-number) indicates the number of the sample that a shadow sync will be defined for. This should always be a non-sync sample (e.g. a frame difference). The second sample number (sync-sample-number) indicates the sample number of the sync sample (i.e. key frame) that can be used when there is a need for a sync sample at, or before, the shadowed-sample-number.

The entries in the ShadowSyncSampleBox shall be sorted based on the shadowed-sample-number field.

The shadow sync samples are normally placed in an area of the track that is not presented during normal play (edited out by means of an edit list), though this is not a requirement. The shadow sync table can be ignored and the track will play (and seek) correctly if it is ignored (though perhaps not optimally).

The ShadowSyncSample replaces, not augments, the sample that it shadows (i.e. the next sample sent is shadowed-sample-number+1). The shadow sync sample is treated as if it occurred at the time of the sample it shadows, having the duration of the sample it shadows.

Hinting and transmission might become more complex if a shadow sample is used also as part of normal playback, or is used more than once as a shadow. In this case the hint track might need separate shadow syncs, all of which can get their media data from the one shadow sync in the media track, to allow for the different timestamps etc. needed in their headers.

##### Syntax

aligned(8) class ShadowSyncSampleBox  
 extends FullBox('stsh', version = 0, 0)   
{  
 unsigned int(32) entry\_count;  
 int i;  
 for (i=0; i < entry\_count; i++) {  
 unsigned int(32) shadowed\_sample\_number;  
 unsigned int(32) sync\_sample\_number;  
 }  
}

##### Semantics

version - is an integer that specifies the version of this box.

entry\_count - is an integer that gives the number of entries in the following table.

shadowed\_sample\_number - gives the number of a sample for which there is an alternative sync sample.

sync\_sample\_number - gives the number of the alternative sync sample.

### Independent and disposable samples box

* + - 1. Definition

Box Types: 'sdtp'  
Container: SampleTableBox  
Mandatory: No  
Quantity: Zero or one

This optional table answers three questions about sample dependency:

* + - 1. does this sample depend on others (e.g. is it an I-picture)?
      2. do no other samples depend on this one?
      3. does this sample contain multiple (redundant) encodings of the data at this time-instant (possibly with different dependencies)?

In the absence of this table:

* + - 1. the sync sample information (partly) answers the first question; in most video codecs, I-pictures are also sync points,
      2. the dependency of other samples on this one is unknown.
      3. the existence of redundant coding is unknown.

When performing ‘trick’ modes, such as fast-forward, it is possible to use the first piece of information to locate independently decodable samples. Similarly, when performing random access, it may be necessary to locate the previous sync sample or random access recovery point, and roll-forward from the sync sample or the pre-roll starting point of the random access recovery point to the desired point. While rolling forward, samples on which no others depend need not be retrieved or decoded.

The value of sample\_is\_depended\_on is independent of the existence of redundant codings. However, a redundant coding may have different dependencies from the primary coding; if redundant codings are available, the value of sample\_depends\_on documents only the primary coding.

A leading sample (usually a picture in video) is defined relative to a reference sample, which is the immediately prior sample that is marked as sample\_depends\_on having no dependency (an I picture). A leading sample has both a composition timestamp before the reference sample, and possibly also a decoding dependency on a sample before the reference sample. Therefore if, for example, playback and decoding were to start at the reference sample, those samples marked as leading are not be needed and are possibly not decodable. A leading sample itself shall therefore not be marked as having no dependency.

For tracks with a handler\_type that is not 'vide', 'soun', 'hint' or 'auxv', if another sample with sample\_depends\_on=2 or another sample tagged as a “Sync Sample” has already been processed and unless specified otherwise, a sample tagged with sample\_depends\_on=2, and sample\_has\_redundancy=1 can be discarded, and its duration added to the duration of the preceding one, to maintain the timing of subsequent samples.

The size of the table, sample\_count, is taken from the sample\_count in the SampleSizeBox or CompactSampleSizeBox.

* + - 1. Syntax

aligned(8) class SampleDependencyTypeBox  
 extends FullBox('sdtp', version = 0, 0)   
{  
 for (i=0; i < sample\_count; i++){  
 unsigned int(2) is\_leading;  
 unsigned int(2) sample\_depends\_on;  
 unsigned int(2) sample\_is\_depended\_on;  
 unsigned int(2) sample\_has\_redundancy;  
 }  
}

* + - 1. Semantics

is\_leading takes one of the following four values:

0: the leading nature of this sample is unknown;

1: this sample is a leading sample that has a dependency before the referenced I-picture (and is therefore not decodable);

2: this sample is not a leading sample;

3: this sample is a leading sample that has no dependency before the referenced I-picture (and is therefore decodable);

sample\_depends\_on takes one of the following four values:

0: the dependency of this sample is unknown;

1: this sample does depend on others (not an I picture);

2: this sample does not depend on others (I picture);

3: reserved

sample\_is\_depended\_on takes one of the following four values:

0: the dependency of other samples on this sample is unknown;

1: other samples may depend on this one (not disposable);

2: no other sample depends on this one (disposable);

3: reserved

sample\_has\_redundancy takes one of the following four values:

0: it is unknown whether there is redundant coding in this sample;

1: there is redundant coding in this sample;

2: there is no redundant coding in this sample;

3: reserved

### Edit box

* + - 1. Definition

Box Type: 'edts'  
Container: TrackBox  
Mandatory: No  
Quantity: Zero or one

An EditBox maps the presentation timeline to the media timeline as it is stored in the file. The EditBox is a container for the edit lists.

The EditBox is optional. In the absence of this box, there is an implicit one-to-one mapping of these timelines, and the presentation of a track starts at the beginning of the presentation. An empty edit is used to offset the start time of a track.

* + - 1. Syntax

aligned(8) class EditBox extends Box('edts')   
{  
}

### Edit list box

* + - 1. Definition

Box Type: 'elst'  
Container: EditBox  
Mandatory: No  
Quantity: Zero or one

This box contains an explicit timeline map. Each entry defines part of the track timeline: by mapping part of the composition timeline, or by indicating ‘empty’ time (portions of the presentation timeline that map to no media, an ‘empty’ edit), or by defining a ‘dwell’, where a single time-point in the media is held for a period.

NOTE 1 Edits are not restricted to fall on sample times. This means that when entering an edit, it can be necessary to (a) back up to a sync point, and pre-roll from there and then (b) be careful about the duration of the first sample — it might have been truncated if the edit enters it during its normal duration. If this is audio, that frame might need to be decoded, and then the final slicing done. Likewise, the duration of the last sample in an edit might need slicing. The length of the whole track in an EditListBox might be the overall duration of the whole movie excluding fragments of a fragment movie. Since edit lists cannot occur in movie fragments, there is an implied edit at the end of the current explicit or implied edit list, that inserts the new media material and the presentation of fragments starts after the presentation of the movie in the MovieBox.

Starting offsets for tracks (streams) are represented by an initial ‘empty’ edit.

A non-‘empty’ edit may insert a portion of the media timeline that is not present in the initial movie, and is present only in subsequent movie fragments.

Edit lists may be repeated; this is indicated with the RepeatEdits flag. When this flag is equal to 0 the edit list is not repeated, while the value 1 specifies that the edit list is repeated. When an EditListBox indicates the playback of zero samples or one sample, RepeatEdits shall be equal to 0. When the TrackHeaderBox duration is not indefinite (all 1s), then the edit list is repeated R times such that the total duration of the edit list multiplied by R equals the TrackHeaderBox duration (R is not necessarily an integer). If the TrackHeaderBox duration is indefinite, then the edit list is repeated indefinitely.

NOTE 2 When the edit list is repeated, media at time 0 resulting from the edit list follows immediately the media having the largest time resulting from the edit list. In other words, the edit list is repeated seamlessly.

When a movie is fragmented, and does not contain any MovieExtendsHeaderBox, the last entry in a track edit list may be a non-empty entry with a media duration field set to 0; in this case, readers shall interpret this media duration as being the accumulated duration of all samples defined in the initial movie and any further movie-fragments. If there is a MovieExtendsHeaderBox, the last entry in the edit list should be adjusted such that the total duration of all edits corresponds to the duration in the MovieExtendsHeaderBox.

It is recommended that such an edit be used to establish a presentation time of 0 for the first presented sample, when composition offsets are used.

In the case of a fragmented movie, starting offsets for tracks (streams) are also represented by an initial ‘empty’ edit, followed by a non-‘empty’ edit.

NOTE 3 The field edit\_duration used to be called segment\_duration in previous editions of this document.

* + - 1. Syntax

aligned(8) class EditListBox extends FullBox('elst', version, flags)   
{  
 unsigned int(32) entry\_count;  
 for (i=1; i <= entry\_count; i++) {  
 if (version==1) {  
 unsigned int(64) edit\_duration;  
 int(64) media\_time;  
 } else { // version==0  
 unsigned int(32) edit\_duration;  
 int(32) media\_time;  
 }  
 int(16) media\_rate\_integer;  
 int(16) media\_rate\_fraction;  
 }  
}

* + - 1. Semantics

version is an integer that specifies the version of this box (0 or 1)

flags the following values are defined. The values of flags greater than 1 are reserved.

RepeatEdits 1

entry\_count is an integer that gives the number of entries in the following table

edit\_duration is an integer that specifies the duration of this edit in units of the timescale in the MovieHeaderBox

media\_time is an integer containing the starting time within the media of this edit entry (in media time scale units, in composition time). If this field is set to –1, it is an empty edit. The last edit in a track shall never be an empty edit. Any difference between the duration in the MovieHeaderBox, and the track’s duration is expressed as an implicit empty edit at the end.

media\_rate specifies the relative rate at which to play the media corresponding to this edit entry. If this value is 0, then the edit is specifying a ‘dwell’: the media at media-time is presented for the edit\_duration. This is expressed as a 16.16 fixed-point integer (16 bits each for the integer and fractional part). The normal value, indicating normal-speed forward play, is 1.0 (integer part equal to 1, fraction part equal to 0).

* + - 1. Edit list examples

To play a track from its start for 30 seconds, but at 10 seconds into the presentation, we have the following edit list:

entry\_count = 2  
  
edit\_duration = 10 seconds  
media\_time = -1  
media\_rate = 1  
  
edit\_duration = 30 seconds (is possibly the length of the whole track)  
media\_time = 0 seconds  
media\_rate = 1

As an example of correcting for a non-zero initial composition timestamp, if the composition timestamp of the first composed frame is 20, then the edit that maps the media time from 20 onwards to movie time 0 onwards, reads:

entry\_count = 1  
  
edit\_duration = 0  
media\_time = 20  
media\_rate = 1

As an example of an initial offset, to play a track from its start for 0 seconds, but at 2 seconds into the presentation, we have the following edit list:

entry\_count = 2  
  
edit\_duration = 2 seconds  
media\_time = -1  
media\_rate = 1  
  
edit\_duration = 0 seconds  
media\_time = 0 seconds  
media\_rate = 1

## Track data layout structures

### Data information box

* + - 1. Definition

Box Type: 'dinf'  
Container: MediaInformationBox or MetaBox  
Mandatory: Yes (required within MediaInformationBox) and No (optional within MetaBox)  
Quantity: Exactly one

The DataInformationBox contains objects that declare the location of the media information in a track.

* + - 1. Syntax

aligned(8) class DataInformationBox extends Box('dinf')   
{  
}

### Data reference box

* + - 1. Definition

Box Type: 'dref'  
Container: DataInformationBox  
Mandatory: Yes  
Quantity: Exactly one

Box Types: 'url ', 'urn '  
Container: DataReferenceBox  
Mandatory: Yes (at least one of 'url ' or 'urn ' shall be present)  
Quantity: One or more

Box Type: 'imdt'  
Container: DataReferenceBox  
Mandatory: No.  
Quantity: Zero or more.

Box Type: 'snim'  
Container: DataReferenceBox  
Mandatory: No.  
Quantity: Zero or more.

The data reference object contains a table of data references (normally URLs) that declare the location(s) of the media data used within the presentation. The data reference index in the sample entry ties entries in this table to the samples in the track. A track may be split over several sources in this way.

If the flag is set indicating that the data is in the same file as this box, then no string (not even an empty one) shall be supplied in the entry field.

The entry\_count in the DataReferenceBox shall be 1 or greater.

NOTE Though the count is 32 bits, the number of items is usually much fewer, and is restricted by the fact that the reference index in the sample table is only 16 bits

When a file that has data entries with the flag set indicating that the media data is in the same file, is split into segments for transport, the value of this flag does not change, as the file is (logically) reassembled after the transport operation.

The DataEntryImdaBox identifies the IdentifiedMediaDataBox containing the media data accessed through the data\_reference\_index corresponding to this DataEntryImdaBox. The DataEntryImdaBox contains the value of imda\_identifier of the referred IdentifiedMediaDataBox. The media data offsets are relative to the first byte of the payload of the referred IdentifiedMediaDataBox. In other words, media data offset 0 points to the first byte of the payload of the referred IdentifiedMediaDataBox.

The DataEntrySeqNumImdaBox identifies the IdentifiedMediaDataBox containing the media data accessed through the data\_reference\_index corresponding to this DataEntrySeqNumImdaBox. When a data\_reference\_index included in a sample entry refers to DataEntrySeqNumImdaBox, each sample referring to the sample entry shall be contained in a movie fragment, and media data offset 0 points to the first byte of the payload of the IdentifiedMediaDataBox that has imda\_identifier equal to sequence\_number of the MovieFragmentHeaderBox of the movie fragment containing the sample.

* + - 1. Syntax

aligned(8) class DataEntryBaseBox(entry\_type, bit(24) flags)  
 extends FullBox(entry\_type, version = 0, flags)   
{  
}

aligned(8) class DataEntryUrlBox (bit(24) flags)  
 extends DataEntryBaseBox('url ', flags)   
{  
 utf8string location;  
}

aligned(8) class DataEntryUrnBox (bit(24) flags)  
 extends DataEntryBaseBox('urn ', flags)   
{  
 utf8string name;  
 utf8string location;  
}

aligned(8) class DataEntryImdaBox (bit(24) flags)  
 extends DataEntryBaseBox('imdt', flags)   
{  
 unsigned int(32) imda\_ref\_identifier;  
}

aligned(8) class DataEntrySeqNumImdaBox (bit(24) flags)  
 extends DataEntryBaseBox ('snim', flags)   
{  
}

aligned(8) class DataReferenceBox extends FullBox('dref', version = 0, 0)  
{  
 unsigned int(32) entry\_count;  
 for (i=1; i <= entry\_count; i++) {  
 DataEntryBaseBox data\_entry(entry\_type, entry\_flags);  
 }  
}

* + - 1. Semantics

version is an integer that specifies the version of this box

entry\_count is an integer that counts the actual entries

entry\_flags is a 24-bit integer with flags; one flag is defined (x000001) which means that the media data is in the same file as the Box containing this data reference. If this flag is set, the DataEntryUrlBox shall be used and no string is present; the box terminates with the entry-flags field.

data\_entry is an instance of a class derived from DataEntryBaseBox.

name is a URN, and is required in a URN entry

location is a URL, and is required in a URL entry and optional in a URN entry, where it gives a location to find the resource with the given name. The URL type should be of a service that delivers a file (e.g. URLs of type file, http, ftp etc.), and which services ideally also permit random access. Relative URLs are permissible and are relative to the file that contains this data reference.

imda\_ref\_identifier identifies the IdentifiedMediaDataBox containing the media data accessed through the data\_reference\_index corresponding to this DataEntryImdaBox. The referred IdentifiedMediaDataBox contains imda\_identifier that is equal to imda\_ref\_identifier.

### Sample size boxes

* + - 1. Definition

Box Type: 'stsz', 'stz2'  
Container: SampleTableBox  
Mandatory: Yes  
Quantity: Exactly one variant shall be present

This box contains the sample count and a table giving the size in bytes of each sample. This allows the media data itself to be unframed. The total number of samples in the media is always indicated in the sample count.

There are two variants of the sample size box. The first variant has a fixed size 32-bit field for representing the sample sizes; it permits defining a constant size for all samples in a track. The second variant permits smaller size fields, to save space when the sizes are varying but small. One of these boxes shall be present; the first version is preferred for maximum compatibility.

NOTE A sample size of zero is not prohibited in general, but it must be valid and defined for the coding system, as defined by the sample entry, that the sample belongs to.

#### Sample size box

* + - * 1. Syntax

aligned(8) class SampleSizeBox extends FullBox('stsz', version = 0, 0)   
{  
 unsigned int(32) sample\_size;  
 unsigned int(32) sample\_count;  
 if (sample\_size==0) {  
 for (i=1; i <= sample\_count; i++) {  
 unsigned int(32) entry\_size;  
 }  
 }  
}

* + - * 1. Semantics

version is an integer that specifies the version of this box

sample\_size is integer specifying the default sample size. If all the samples are the same size, this field contains that size value. If this field is set to 0, then the samples have different sizes, and those sizes are stored in the sample size table. If this field is not 0, it specifies the constant sample size, and no array follows.

sample\_count is an integer that gives the number of samples in the track; if sample\_size is 0, then it is also the number of entries in the following table.

entry\_size is an integer specifying the size of a sample, indexed by its number.

#### Compact sample size box

* + - * 1. Syntax

aligned(8) class CompactSampleSizeBox   
 extends FullBox('stz2', version = 0, 0)   
{  
 unsigned int(24) reserved = 0;  
 unsigned int(8) field\_size;  
 unsigned int(32) sample\_count;  
 for (i=1; i <= sample\_count; i++) {  
 unsigned int(field\_size) entry\_size;  
 }  
}

* + - * 1. Semantics

version is an integer that specifies the version of this box

field\_size is an integer specifying the size in bits of the entries in the following table; it shall take the value 4, 8 or 16. If the value 4 is used, then each byte contains two values:  
entry[i]<<4 + entry[i+1]; if the sizes do not fill an integral number of bytes, the last byte is padded with zeros.

sample\_count is an integer that gives the number of entries in the following table

entry\_size is an integer specifying the size of a sample, indexed by its number.

### Sample to chunk box

* + - 1. Definition

Box Type: 'stsc'  
Container: SampleTableBox  
Mandatory: Yes  
Quantity: Exactly one

Samples within the media data are grouped into chunks. Chunks can be of different sizes, and the samples within a chunk can have different sizes. This table can be used to find the chunk that contains a sample, its position, and the associated sample entry.

The table is compactly coded. Each entry gives the index of the first chunk of a run of chunks with the same characteristics. By subtracting one entry here from the previous one, it is possible to compute how many chunks are in this run. This can be converted to a sample count by multiplying by the appropriate samples-per-chunk.

* + - 1. Syntax

aligned(8) class SampleToChunkBox extends FullBox('stsc', version = 0, 0)  
{  
 unsigned int(32) entry\_count;  
 for (i=1; i <= entry\_count; i++) {  
 unsigned int(32) first\_chunk;  
 unsigned int(32) samples\_per\_chunk;  
 unsigned int(32) sample\_description\_index;  
 }  
}

* + - 1. Semantics

version is an integer that specifies the version of this box

entry\_count is an integer that gives the number of entries in the following table

first\_chunk is an integer that gives the index of the first chunk in this run of chunks that share the same samples-per-chunk and sample-description-index; the index of the first chunk in a track has the value 1 (the first\_chunk field in the first record of this box has the value 1, identifying that the first sample maps to the first chunk).

samples\_per\_chunk is an integer that gives the number of samples in each of these chunks

sample\_description\_index is an integer that gives the index of the sample entry that describes the samples in this chunk. The index ranges from 1 to the number of sample entries in the SampleDescriptionBox

### Chunk offset box

* + - 1. Definition

Box Type: 'stco', 'co64'  
Container: SampleTableBox  
Mandatory: Yes  
Quantity: Exactly one variant shall be present

The chunk offset table gives the index of each chunk into the containing file. There are two variants, permitting the use of 32-bit or 64-bit offsets. The latter is useful when managing very large presentations. At most one of these variants will occur in any single instance of a sample table.

When the referenced data reference entry is not DataEntryImdaBox or DataEntrySeqNumImdaBox, offsets are file offsets, not the offset into any box within the file (e.g. MediaDataBox). This permits referring to media data in files without any box structure. It does also mean that care must be taken when constructing a self-contained movie file with its structure-data (MovieBox) at the front, as the size of the MovieBox will affect the chunk offsets to the media data.

When the referenced data reference entry is DataEntryImdaBox or DataEntrySeqNumImdaBox, offsets are relative to the first byte of the payload of the IdentifiedMediaDataBox corresponding to the data reference entry. This permits reordering file-level boxes and receiving a subset of file-level boxes but possibly requires traversing the file-level boxes until the referenced IdentifiedMediaDataBox is found.

* + - 1. Syntax

aligned(8) class ChunkOffsetBox extends FullBox('stco', version = 0, 0)   
{  
 unsigned int(32) entry\_count;  
 for (i=1; i <= entry\_count; i++) {  
 unsigned int(32) chunk\_offset;  
 }  
}

aligned(8) class ChunkLargeOffsetBox  
 extends FullBox('co64', version = 0, 0)   
{  
 unsigned int(32) entry\_count;  
 for (i=1; i <= entry\_count; i++) {  
 unsigned int(64) chunk\_offset;  
 }  
}

* + - 1. Semantics

version is an integer that specifies the version of this box

entry\_count is an integer that gives the number of entries in the following table

chunk\_offset is a 32 or 64 bit integer that gives the offset of the start of a chunk. If the referenced data reference entry is DataEntryImdaBox or DataEntrySeqNumImdaBox, the value of chunk\_offset is relative to the first byte of the payload of the IdentifiedMediaDataBox corresponding to the data reference entry. Otherwise, the value of chunk\_offset is relative to the start of the containing media file.

### Padding bits box

* + - 1. Definition

Box Type: 'padb'  
Container: SampleTableBox  
Mandatory: No  
Quantity: Zero or one

In some streams the media samples do not occupy all bits of the bytes given by the sample size, and are padded at the end to a byte boundary. In some cases, it is necessary to record externally the number of padding bits used. This table supplies that information.

* + - 1. Syntax

aligned(8) class PaddingBitsBox extends FullBox('padb', version = 0, 0)   
{  
 unsigned int(32) sample\_count;  
 int i;  
 for (i=0; i < floor((sample\_count + 1)/2); i++) {  
 bit(1) reserved = 0;  
 bit(3) pad1;  
 bit(1) reserved = 0;  
 bit(3) pad2;  
 }  
}

* + - 1. Semantics

sample\_count – counts the number of samples in the track; it should match the count in other tables

pad1 – is a value from 0 to 7, indicating the number of padding bits at the end of sample (i\*2)+1.

pad2 – is a value from 0 to 7, indicating the number of padding bits at the end of sample (i\*2)+2

### Sub-sample information box

* + - 1. Definition

Box Type: 'subs'  
Container: SampleTableBox or TrackFragmentBox  
Mandatory: No  
Quantity: Zero or more

This box is designed to contain sub-sample information.

A sub-sample is a contiguous range of bytes of a sample. The specific definition of a sub-sample shall be supplied for a given coding system (e.g. for ISO/IEC 14496-10:2014, Advanced Video Coding). In the absence of such a specific definition, this box shall not be applied to samples using that coding system.

If subsample\_count is 0 for any entry, then those samples have no subsample information and no array follows. The table is sparsely coded; the table identifies which samples have sub-sample structure by recording the difference in sample-number between each entry. The first entry in the table records the sample number of the first sample having sub-sample information.

NOTE It is possible to combine subsample\_priority and discardable such that when subsample\_priority is smaller than a certain value, discardable is set to 1. However, since different systems may use different scales of priority values, separating them is safer, to have a clean solution for discardable sub-samples.

When more than one SubSampleInformationBox is present in the same container box, the value of flags shall differ in each of these SubSampleInformationBoxes. The semantics of flags, if any, shall be supplied for a given coding system. If flags have no semantics for a given coding system, the flags shall be 0.

* + - 1. Syntax

aligned(8) class SubSampleInformationBox  
 extends FullBox('subs', version, flags)   
{  
 unsigned int(32) entry\_count;  
 int i,j;  
 for (i=0; i < entry\_count; i++) {  
 unsigned int(32) sample\_delta;  
 unsigned int(16) subsample\_count;  
 if (subsample\_count > 0) {  
 for (j=0; j < subsample\_count; j++) {  
 if(version == 1) {  
 unsigned int(32) subsample\_size;  
 }  
 else {  
 unsigned int(16) subsample\_size;  
 }  
 unsigned int(8) subsample\_priority;  
 unsigned int(8) discardable;  
 unsigned int(32) codec\_specific\_parameters;  
 }  
 }  
 }  
}

* + - 1. Semantics

version is an integer that specifies the version of this box (0 or 1 in this document)

entry\_count is an integer that gives the number of entries in the following table.

sample\_delta is an integer that indicates the sample having sub‐sample structure. It is coded as the difference, in decoding order, between the desired sample number, and the sample number indicated in the previous entry. If the current entry is the first entry in the track, the value indicates the sample number of the first sample having sub-sample information, that is, the value is the difference between the sample number and zero (0). If the current entry is the first entry in a track fragment with preceding non-empty track fragments, the value indicates the difference between the sample number of the first sample having sub-sample information and the sample number of the last sample in the previous track fragment. If the current entry is the first entry in a track fragment without any preceding track fragments, the value indicates the sample number of the first sample having sub-sample information, that is, the value is the difference between the sample number and zero (0). This implies that the sample\_delta for the first entry describing the first sample in the track or in the track fragment is always 1.

subsample\_count is an integer that specifies the number of sub-sample for the current sample. If there is no sub-sample structure, then this field takes the value 0.

subsample\_size is an integer that specifies the size, in bytes, of the current sub-sample.

subsample\_priority is an integer specifying the degradation priority for each sub-sample. Higher values of subsample\_priority, indicate sub-samples which are important to, and have a greater impact on, the decoded quality.

discardable equal to 0 means that the sub-sample is required to decode the current sample, while equal to 1 means the sub-sample is not required to decode the current sample but may be used for enhancements, e.g. the sub-sample consists of supplemental enhancement information (SEI) messages.

codec\_specific\_parameters is defined by the codec in use. If no such definition is available, this field shall be set to 0.

### Sample auxiliary information sizes box

#### Definition

Box Type: 'saiz'  
Container: SampleTableBox or TrackFragmentBox  
Mandatory: No  
Quantity: Zero or more

Per-sample sample auxiliary information may be stored anywhere in the same file as the sample data itself; for self-contained ISO base media files, this is typically in a MediaDataBox or a box from a derived specification. It is stored either (a) in multiple chunks, with the number of samples per chunk, as well as the number of chunks, matching the chunking of the primary sample data or (b) in a single chunk for all the samples in a movie sample table (or a movie fragment). The sample auxiliary information for all samples contained within a single chunk (or track run) is stored contiguously (similarly to sample data).

Sample auxiliary information, when present, is always stored in the same file as the samples to which it relates as they share the same data reference ('dref') structure. However, this data may be located anywhere within this file, using auxiliary information offsets ('saio') to indicate the location of the data.

Whether sample auxiliary information is permitted or required may be specified by the brands or the coding format in use. The format of the sample auxiliary information is determined by aux\_info\_type. If aux\_info\_type and aux\_info\_type\_parameter are omitted then the implied value of aux\_info\_type is either (a) in the case of transformed content, such as protected content, the scheme\_type included in the ProtectionSchemeInfoBox or ScrambleSchemeInfoBox, or otherwise (b) the sample entry type. In the case of tracks containing multiple transformations, aux\_info\_type and aux\_info\_type\_parameter shall not be omitted. The default value of the aux\_info\_type\_parameter is 0. Some values of aux\_info\_type may be restricted to be used only with particular track types. A track may have multiple streams of sample auxiliary information of different types. The types are managed according to Annex D.

While aux\_info\_type determines the format of the sample auxiliary information, several streams of sample auxiliary information having the same format may be used when their value of aux\_info\_type\_parameter differs. The semantics of aux\_info\_type\_parameter for a particular aux\_info\_type value shall be specified along with specifying the semantics of the particular aux\_info\_type value and the implied sample auxiliary information format.

This box provides the size of the sample auxiliary information for each sample. For each instance of this box, there shall be a matching SampleAuxiliaryInformationOffsetsBox with the same values of aux\_info\_type and aux\_info\_type\_parameter, providing the offset information for this sample auxiliary information.

NOTE For discussions on the use of sample auxiliary information versus other mechanisms, see Annex B.8.

#### Syntax

aligned(8) class SampleAuxiliaryInformationSizesBox  
 extends FullBox('saiz', version = 0, flags)  
{  
 if (flags & 1) {  
 unsigned int(32) aux\_info\_type;  
 unsigned int(32) aux\_info\_type\_parameter;  
 }  
 unsigned int(8) default\_sample\_info\_size;  
 unsigned int(32) sample\_count;  
 if (default\_sample\_info\_size == 0) {  
 unsigned int(8) sample\_info\_size[ sample\_count ];  
 }  
}

#### Semantics

aux\_info\_type is an integer that identifies the type of the sample auxiliary information. At most one occurrence of this box with the same values for aux\_info\_type and aux\_info\_type\_parameter shall exist in the containing box.

aux\_info\_type\_parameter identifies the “stream” of sample auxiliary information having the same value of aux\_info\_type and associated to the same track. The semantics of aux\_info\_type\_parameter are determined by the value of aux\_info\_type.

default\_sample\_info\_size is an integer specifying the sample auxiliary information size for the case where all the indicated samples have the same sample auxiliary information size. If the size varies then this field shall be zero.

sample\_count is an integer that gives the number of samples for which a size is defined. For a SampleAuxiliaryInformationSizesBox appearing in the SampleTableBox this shall be the same as, or less than, the sample\_count within the SampleSizeBox or CompactSampleSizeBox. For a SampleAuxiliaryInformationSizesBox appearing in a TrackFragmentBox this shall be the same as, or less than, the sum of the sample\_count entries within the TrackRunBoxes of the track fragment. If this is less than the number of samples, then auxiliary information is supplied for the initial samples, and the remaining samples have no associated auxiliary information.

sample\_info\_size gives the size of the sample auxiliary information in bytes. This may be zero to indicate samples with no associated auxiliary information.

### Sample auxiliary information offsets box

#### Definition

Box Type: 'saio'  
Container: SampleTableBox or TrackFragmentBox  
Mandatory: No  
Quantity: Zero or more

For an introduction to sample auxiliary information, see the definition of the SampleAuxiliaryInformationSizesBox.

This box provides the position information for the sample auxiliary information, in a way similar to the chunk offsets for sample data.

#### Syntax

aligned(8) class SampleAuxiliaryInformationOffsetsBox  
 extends FullBox('saio', version, flags)  
{  
 if (flags & 1) {  
 unsigned int(32) aux\_info\_type;  
 unsigned int(32) aux\_info\_type\_parameter;  
 }  
 unsigned int(32) entry\_count;  
 if ( version == 0 ) {  
 unsigned int(32) offset[ entry\_count ];  
 }  
 else {  
 unsigned int(64) offset[ entry\_count ];  
 }  
}

#### Semantics

aux\_info\_type and aux\_info\_type\_parameter are defined as in the SampleAuxiliaryInformationSizesBox

entry\_count gives the number of entries in the following table. For a SampleAuxiliaryInformationOffsetsBox appearing in a Sample Table Box this shall be equal to one or to the value of the entry\_count field in the ChunkOffsetBox or ChunkLargeOffsetBox. For a SampleAuxiliaryInformationOffsetsBox appearing in a TrackFragmentBox, this shall be equal to one or to the number of TrackRunBoxes in the TrackFragmentBox.

offset gives the position in the file of the sample auxiliary information for each chunk or track fragment run. If entry\_count is one, then the sample auxiliary information for all chunks or track fragment runs is contiguous in the file in chunk or run order. When in the SampleTableBox, the offsets are relative to the same base offset as derived for the respective samples through the data\_reference\_index of the sample entry referenced by the samples. In a TrackFragmentBox, this value is relative to the base offset established by the TrackFragmentHeaderBox in the same track fragment (see 8.8.14).

## Movie fragments

### Movie extends box

* + - 1. Definition

Box Type: 'mvex'  
Container: MovieBox  
Mandatory: No  
Quantity: Zero or one

This box warns readers that there might be MovieFragmentBoxes in this file. To know of all samples in the tracks, these MovieFragmentBoxes must be found and scanned in order, and their information logically added to that found in the MovieBox.

There is a narrative introduction to movie fragments in Annex A.

There are functional equivalences between structures and fields in fragmented and non-fragmented movies, as documented by Table 5.

Table 5 — Equivalences between fragmented and non-fragmented movies

|  |  |
| --- | --- |
| ***Movie Fragment*** | ***Non-Fragmented Movie*** |
| MovieExtendsHeaderBox:fragment\_duration | TrackHeaderBox:duration |
| TrackExtendsBox:default\_sample\_flags  TrackFragmentHeaderBox:default\_sample\_flags  TrackRunBox:(first\_sample\_flags, sample\_flags) |  |
| :is\_leading | SampleDependencyTypeBox:is\_leading |
| :sample\_depends\_on | SampleDependencyTypeBox:sample\_depends\_on |
| :sample\_is\_depended\_on | SampleDependencyTypeBox:sample\_is\_depended\_on |
| :sample\_has\_redundancy | SampleDependencyTypeBox:sample\_has\_redundancy |
| :sample\_padding\_value | PaddingBitsBox:(pad1, pad2) |
| :sample\_is\_non\_sync\_sample | ¬ present(SyncSampleBox:sample\_number) |
| :sample\_degradation\_priority | DegradationPriorityBox:priority |
| TrackExtendsBox:default\_sample\_description\_index  TrackFragmentHeaderBox:sample\_description\_index | SampleToChunkBox:sample\_description\_index |
| TrackExtendsBox:default\_sample\_duration  TrackFragmentHeaderBox:default\_sample\_duration  TrackRunBox:sample\_duration | TimeToSampleBox:sample\_delta |
| TrackExtendsBox:default\_sample\_size  TrackFragmentHeaderBox:default\_sample\_size  TrackRunBox:sample\_size | SampleSizeBox:(sample\_size , entry\_size)  CompactSampleSizeBox:entry\_size |
| TrackRunBox:sample\_composition\_time\_offset | CompositionOffsetBox:sample\_offset |

* + - 1. Syntax

aligned(8) class MovieExtendsBox extends Box('mvex'){  
}

### Movie extends header box

* + - 1. Definition

Box Type: 'mehd'  
Container: MovieExtendsBox  
Mandatory: No  
Quantity: Zero or one

The movie extends header is optional, and provides the overall duration, including fragments, of a fragmented movie. If this box is not present, the overall duration must be computed by examining each fragment.

If the duration fields in all tracks are 0, and movie fragments are present, the duration in MovieHeaderBox should be set to indefinite or 0. If movie fragments are present but there is no MediaExtendsHeaderBox and the movie duration is 0, the movie duration should be interpreted as indefinite duration.

* + - 1. Syntax

aligned(8) class MovieExtendsHeaderBox  
 extends FullBox('mehd', version, 0)  
{  
 if (version==1) {  
 unsigned int(64) fragment\_duration;  
 } else { // version==0  
 unsigned int(32) fragment\_duration;  
 }  
}

* + - 1. Semantics

fragment\_duration is an integer that declares length of the presentation of the whole movie including fragments (in the timescale indicated in the MovieHeaderBox). The value of this field corresponds to the duration of the longest track, including movie fragments. If an MP4 file is created in real-time, such as used in live streaming, it is not likely that the fragment\_duration is known in advance and this box may be omitted.

### Track extends box

* + - 1. Definition

Box Type: 'trex'  
Container: MovieExtendsBox  
Mandatory: Yes  
Quantity: Exactly one for each track in the MovieBox

This sets up default values used by the movie fragments. By setting defaults in this way, space and complexity can be saved in each TrackFragmentBox.

The sample flags field in sample fragments (default\_sample\_flags here and in a TrackFragmentHeaderBox, and sample\_flags and first\_sample\_flags in a TrackRunBox) is coded as a 32-bit value. It has the following structure:

bit(4) reserved=0;  
unsigned int(2) is\_leading;  
unsigned int(2) sample\_depends\_on;  
unsigned int(2) sample\_is\_depended\_on;  
unsigned int(2) sample\_has\_redundancy;  
bit(3) sample\_padding\_value;  
bit(1) sample\_is\_non\_sync\_sample;  
unsigned int(16) sample\_degradation\_priority;

The is\_leading, sample\_depends\_on, sample\_is\_depended\_on and sample\_has\_redundancy values are defined as documented in the SampleDependencyTypeBox.

The flag sample\_is\_non\_sync\_sample provides the same information as the SyncSampleBox. When this value is set to 0 for a sample, it is the same as if the sample were not in a movie fragment and marked with an entry in the SyncSampleBox (or, if all samples are sync samples, the SyncSampleBox were absent).

The sample\_padding\_value is defined as for the PaddingBitsBox. The sample\_degradation\_priority is defined as for the DegradationPriorityBox.

* + - 1. Syntax

aligned(8) class TrackExtendsBox extends FullBox('trex', 0, 0){  
 unsigned int(32) track\_ID;  
 unsigned int(32) default\_sample\_description\_index;  
 unsigned int(32) default\_sample\_duration;  
 unsigned int(32) default\_sample\_size;  
 unsigned int(32) default\_sample\_flags;  
}

* + - 1. Semantics

track\_ID identifies the track; this shall be the track\_ID of a track in the MovieBox

default\_sample\_description\_index: indicates the index of the sample entry that describes, by default, the samples in the track fragments

default\_sample\_duration: indicates the default duration of the samples in the track fragments

default\_sample\_size: indicates the default size of the samples in the track fragments

default\_sample\_flags: indicate the default flags values for the samples in the track fragments. (See 8.8.7 for the possible values)

### Movie fragment box

* + - 1. Definition

Box Type: 'moof'  
Container: File  
Mandatory: No  
Quantity: Zero or more

The movie fragments extend the presentation in time. They provide the information that, when fragments are not used, is present in the MovieBox. The actual samples are in MediaDataBoxes, as usual, if they are in the same file. The data reference index is in the sample entry, so it is possible to build incremental presentations where the media data is in files other than the file containing the MovieBox.

The MovieFragmentBox is a top-level box, (i.e. a peer to the MovieBox and MediaDataBoxes). It contains a MovieFragmentHeaderBox, and then one or more TrackFragmentBoxes.

NOTE There is no requirement that any particular movie fragment extend all tracks present in the movie header, and there is no restriction on the location of the media data referred to by the movie fragments. However, derived specifications may make such restrictions.

* + - 1. Syntax

aligned(8) class MovieFragmentBox extends Box('moof')  
{  
}

### Movie fragment header box

* + - 1. Definition

Box Type: 'mfhd'  
Container: MovieFragmentBox  
Mandatory: Yes  
Quantity: Exactly one

The movie fragment header contains a sequence number, as a safety check. The sequence number usually starts at 1 and increases for each movie fragment in the file, in the order in which they occur. This allows readers to verify integrity of the sequence in environments where undesired re-ordering might occur.

* + - 1. Syntax

aligned(8) class MovieFragmentHeaderBox extends FullBox('mfhd', 0, 0)  
{  
 unsigned int(32) sequence\_number;  
}

* + - 1. Semantics

sequence\_number a number associated with this fragment

### Track fragment box

* + - 1. Definition

Box Type: 'traf'  
Container: MovieFragmentBox  
Mandatory: No  
Quantity: Zero or more

Within the movie fragment there is a set of track fragments, zero or more per track. The track fragments in turn contain zero or more track runs, each of which documents a contiguous run of samples for that track. Within these structures, many fields are optional and can be defaulted.

It is possible to add 'empty time' to a track using these structures, as well as adding samples. Empty inserts can be used in audio tracks doing silence suppression, for example. These are referred to in this document as ‘empty’ edits (portions of the presentation timeline that map to no media).

* + - 1. Syntax

aligned(8) class TrackFragmentBox extends Box('traf')  
{  
}

### Track fragment header box

* + - 1. Definition

Box Type: 'tfhd'  
Container: TrackFragmentBox  
Mandatory: Yes  
Quantity: Exactly one

Each movie fragment can add zero or more fragments to each track; and a track fragment can add zero or more contiguous runs of samples. The track fragment header sets up information and defaults used for those runs of samples.

The data origin that base\_data\_offset is relative to and the value of base\_data\_offset, when not present, are inferred as specified inTable 6.

Table 6 - Derivation of the value and data origin of base\_data\_offset

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Conditions**  A: base-data-offset-present flag  B: default-base-is-moof flag  C: the referenced data reference entry is DataEntryImdaBox or DataEntrySeqNumImdaBox  D: this TrackFragmentBox is the first TrackFragmentBox in the containing MovieFragmentBox | | | |  |  |
| **A** | **B** | **C** | **D** | **base\_data\_offset value** | **Data origin of base\_data\_offset** |
| 0 | 1 | true or false | true or false | base\_data\_offset is inferred to be equal to 0 | base\_data\_offset is relative to the first byte of the MovieFragmentBox containing this box |
| 0 | 0 | true or false | false | base\_data\_offset is inferred to be equal to 1 | base\_data\_offset is relative to the end of the data defined by the preceding track fragment |
| 0 | 0 | true | true | base\_data\_offset is inferred to be equal to 0 | base\_data\_offset is relative to the first byte of the payload of the IdentifiedMediaDataBox corresponding to the data reference entry |
| 0 | 0 | false | true | base\_data\_offset is inferred to be equal to 0 | base\_data\_offset is relative to the first byte of the MovieFragmentBox containing this box |
| 1 | 0 or 1 | true | true or false | base\_data\_offset is present | base\_data\_offset is relative to the first byte of the payload of the IdentifiedMediaDataBox corresponding to the data reference entry |
| 1 | 0 or 1 | false | true or false | base\_data\_offset is present | base\_data\_offset is relative to the file identified by the referenced data reference entry |

NOTE 1 base-data-offset-present flag is advised to be set equal to 1 only if the file identified by the referenced data reference entry is not meant to be delivered with movie fragments in separate segments or the referenced data reference entry is DataEntryImdaBox or DataEntrySeqNumImdaBox.

When base-data-offset-present flag is equal to 1 and the referenced data reference entry is of type 'url ' with (entry\_flags & 1) equal to 1 (indicating that the media data is in the same file as the DataReferenceBox containing the referenced data reference entry), this TrackFragmentHeaderBox shall be present in the same file as the MovieBox.

The following flags are defined in the tf\_flags:

0x000001 base-data-offset-present: indicates the presence of the base-data-offset field. This provides an explicit anchor for the data offsets in each track run (see below).

0x000002 sample-description-index-present: indicates the presence of this field, which over-rides, in this fragment, the default set up in the TrackExtendsBox.

0x000008 default-sample-duration-present

0x000010 default-sample-size-present

0x000020 default-sample-flags-present

0x010000 duration-is-empty: this indicates that the duration provided in either default-sample-duration, or by the default-sample-duration in the TrackExtendsBox, is empty, i.e. that there are no samples for this time interval. It is an error to make a presentation that has both edit lists in the MovieBox, and empty-duration fragments.

0x020000 default-base-is-moof: if base-data-offset-present is 1, this flag is ignored. Support for the default-base-is-moof flag is required under the 'iso5' brand, and it shall not be used in brands or compatible brands earlier than 'iso5'.

NOTE 2 The default-base-is-moof flag cannot be set when 'isom', 'avc1', 'iso2', 'iso3', or 'iso4' brand is included in the FileTypeBox.

When both the base-data-offset-present flag and the default-base-is-moof flag are equal to 0, the value of data\_reference\_index shall be equal in this TrackFragmentHeaderBox and in the previous TrackFragmentHeaderBox of the same track.

* + - 1. Syntax

aligned(8) class TrackFragmentHeaderBox  
 extends FullBox('tfhd', 0, tf\_flags)  
{  
 unsigned int(32) track\_ID;  
 // all the following are optional fields  
 // their presence is indicated by bits in the tf\_flags  
 unsigned int(64) base\_data\_offset;  
 unsigned int(32) sample\_description\_index;  
 unsigned int(32) default\_sample\_duration;  
 unsigned int(32) default\_sample\_size;  
 unsigned int(32) default\_sample\_flags;  
}

* + - 1. Semantics

base\_data\_offset the base offset to use when calculating data offsets

sample\_description\_index, default\_sample\_duration, default\_sample\_size, default\_sample\_flags: see 8.8.3.3

### Track fragment run box

* + - 1. Definition

Box Type: 'trun'  
Container: TrackFragmentBox  
Mandatory: No  
Quantity: Zero or more

Within the TrackFragmentBox, there are zero or more TrackRunBoxes. If the duration-is-empty flag is set in the tf\_flags, there are no track runs. A track run documents a contiguous set of samples for a track.

The number of optional fields is determined from the number of bits set in the lower byte of the flags, and the size of a record from the bits set in the second byte of the flags. This procedure shall be followed, to allow for new fields to be defined.

When data\_offset is not present, the data for this run starts immediately after the data of the previous run, or at base\_data\_offset defined by the track fragment header if this is the first run in a track fragment.

When data\_offset is present, it is relative to base\_data\_offset established in the track fragment header.

The following flags are allowed to be set in the tr\_flags:

0x000001 data-offset-present.

0x000004 first-sample-flags-present; this overrides the default flags for the first sample only, defined in 8.8.3.1. This makes it possible to record a group of frames where the first is a key and the rest are difference frames, without supplying explicit flags for every sample. If this flag and field are used, sample-flags-present shall not be set.

0x000100 sample-duration-present: indicates that each sample has its own duration, otherwise the default is used.

0x000200 sample-size-present: each sample has its own size, otherwise the default is used.

0x000400 sample-flags-present; each sample has its own flags, otherwise the default is used.

0x000800 sample-composition-time-offsets-present; each sample has a composition time offset.

The composition offset values in the CompositionOffsetBox and in the TrackRunBox may be signed or unsigned. The recommendations given in the CompositionOffsetBox concerning the use of signed composition offsets also apply here.

* + - 1. Syntax

aligned(8) class TrackRunBox extends FullBox('trun', version, tr\_flags)  
{  
 unsigned int(32) sample\_count;  
 // the following are optional fields  
 signed int(32) data\_offset;  
 unsigned int(32) first\_sample\_flags;  
 // all fields in the following array are optional  
 // as indicated by bits set in the tr\_flags  
 {  
 unsigned int(32) sample\_duration;  
 unsigned int(32) sample\_size;  
 unsigned int(32) sample\_flags  
 if (version == 0)  
 { unsigned int(32) sample\_composition\_time\_offset; }  
 else  
 { signed int(32) sample\_composition\_time\_offset; }  
 }[ sample\_count ]  
}

* + - 1. Semantics

sample\_count the number of samples being added in this run; also the number of rows in the following table (the rows can be empty)

data\_offset is added to the implicit or explicit base\_data\_offset established in the track fragment header.

first\_sample\_flags provides a set of flags for the first sample only of this run.

### Movie fragment random access box

* + - 1. Definition

Box Type: 'mfra'  
Container: File  
Mandatory: No  
Quantity: Zero or one

The MovieFragmentRandomAccessBox provides a table which may assist readers in finding sync samples in a file using movie fragments. It contains a TrackFragmentRandomAccessBox for each track for which information is provided (which may not be all tracks). It is usually placed at or near the end of the file; the last box within the MovieFragmentRandomAccessBox provides a copy of the length field from the MovieFragmentRandomAccessBox. Readers may attempt to find this box by examining the last 32 bits of the file, or scanning backwards from the end of the file for a MovieFragmentRandomAccessOffsetBox and using the size information in it, to see if that locates the beginning of a MovieFragmentRandomAccessBox.

This box provides only a hint as to where sync samples are; the movie fragments themselves are definitive. It is recommended that readers take care in both locating and using this box as modifications to the file after it was created may render either the pointers, or the declaration of sync samples, incorrect.

* + - 1. Syntax

aligned(8) class MovieFragmentRandomAccessBox extends Box('mfra')  
{  
}

### Track fragment random access box

* + - 1. Definition

Box Type: 'tfra'  
Container: MovieFragmentRandomAccessBox  
Mandatory: No  
Quantity: Zero or one per track

Each entry contains the location and the presentation time of the sync sample. Not every sync sample in the track needs to be listed in the table.

The absence of this box does not mean that all the samples are sync samples. Random access information in the 'trun', 'traf' and 'trex' shall be set appropriately regardless of the presence of this box.

* + - 1. Syntax

aligned(8) class TrackFragmentRandomAccessBox  
 extends FullBox('tfra', version, 0)   
{  
 unsigned int(32) track\_ID;  
 const unsigned int(26) reserved = 0;  
 unsigned int(2) length\_size\_of\_traf\_num;  
 unsigned int(2) length\_size\_of\_trun\_num;  
 unsigned int(2) length\_size\_of\_sample\_num;  
 unsigned int(32) number\_of\_entry;  
 for (i=1; i <= number\_of\_entry; i++){  
 if(version==1){  
 unsigned int(64) time;  
 unsigned int(64) moof\_offset;  
 }else{  
 unsigned int(32) time;  
 unsigned int(32) moof\_offset;  
 }  
 unsigned int((length\_size\_of\_traf\_num+1) \* 8) traf\_number;  
 unsigned int((length\_size\_of\_trun\_num+1) \* 8) trun\_number;  
 unsigned int((length\_size\_of\_sample\_num+1) \* 8) sample\_delta;  
 }  
}

* + - 1. Semantics

track\_ID is an integer providing the track identifier for which random access information is provided

length\_size\_of\_traf\_num indicates the length in bytes of the traf\_number field minus one.

length\_size\_of\_trun\_num indicates the length in bytes of the trun\_number field minus one.

length\_size\_of\_sample\_num indicates the length in bytes of the sample\_number field minus one.

number\_of\_entry is an integer that gives the number of the entries for this track. If this value is zero, it indicates that every sample is a sync sample and no table entry follows.

time is a 32 or 64 bit integer that indicates the presentation time of the sync sample in units defined in the MediaHeaderBox of the associated track.

NOTE Presentation times are usually expressed in movie timescale, except for the specific case of TrackFragmentRandomAccessBox where it is expressed in media timescale.

moof\_offset is a 32 or 64 bits integer that gives the offset of the 'moof' used in this entry. Offset is the byte-offset between the beginning of the file and the beginning of the 'moof'.

traf\_number indicates the 'traf' number that contains the sync sample. The number ranges from 1 (the first 'traf' is numbered 1) in each 'moof'.

trun\_number indicates the 'trun' number that contains the sync sample. The number ranges from 1 in each 'traf'.

sample\_delta indicates the sample number of the sync sample. It is coded as one plus the desired sample number minus the sample number of the first sample in the TrackRunBox.

### Movie fragment random access offset box

* + - 1. Definition

Box Type: 'mfro'  
Container: MovieFragmentRandomAccessBox  
Mandatory: Yes  
Quantity: Exactly one

The MovieFragmentRandomAccessOffsetBox provides a copy of the size field from the enclosing MovieFragmentRandomAccessBox. It is placed last within that box, so that the size field is also last in the enclosing MovieFragmentRandomAccessBox. When the MovieFragmentRandomAccessBox is also last in the file this permits its easy location. The size field here shall be correct. However, neither the presence of the MovieFragmentRandomAccessBox, nor its placement last in the file, are assured.

* + - 1. Syntax

aligned(8) class MovieFragmentRandomAccessOffsetBox  
 extends FullBox('mfro', version, 0)   
{  
 unsigned int(32) parent\_size;  
}

* + - 1. Semantics

parent\_size is an integer that gives the number of bytes of the enclosing MovieFragmentRandomAccessBox box. This field is placed last in the enclosing box to assist readers scanning from the end of the file in finding the MovieFragmentRandomAccessBox.

### Track fragment decode time box

#### Definition

Box Type: 'tfdt'  
Container: TrackFragmentBox  
Mandatory: No  
Quantity: Zero or one

The TrackFragmentBaseMediaDecodeTimeBox provides the absolute decoding timestamp, measured on the decoding timeline, of the first sample in decoding order in the track fragment. This can be useful, for example, when performing random access in a file; it is not necessary to sum the sample durations of all preceding samples in previous fragments to find this value.

The TrackFragmentBaseMediaDecodeTimeBox, if present, shall be positioned after the TrackFragmentHeaderBox and before the first TrackRunBox.

NOTE 1 The decoding timeline is a media timeline, established before any explicit or implied mapping of composition time to presentation time, for example by an edit list or similar structure. See subclause 6.4.

If the time expressed in the TrackFragmentBaseMediaDecodeTimeBox exceeds the sum of the sample durations of the samples in the preceding movie and movie fragments, then the duration of the last sample preceding this track fragment is extended such that the sum now equals the time given in this box. In this way, it is possible to generate a fragment containing a sample when the time of the next sample is not yet known, by assigning it a small or even zero sample duration, that is then overriden by the time expressed in this box in the following fragment. The time expressed in the TrackFragmentBaseMediaDecodeTimeBox shall not be less than the sum of the sample durations of the samples in the preceding movie and movie fragments.

If no samples were present in the preceding movie and movie fragments for this track, the time expressed in the TrackFragmentBaseMediaDecodeTimeBox defines the decoding timestamp of the first sample in this track.

Players may choose to skip over an initial empty media range in tracks where the first decoding timestamp is defined by a TrackFragmentBaseMediaDecodeTimeBox with non-zero time.

In particular, an empty track fragment (with no samples, but with a track fragment decode time box) may be used to establish the duration of the last sample.

NOTE 2 If fragments are delivered out-of-order, file readers might need additional information to determine if the duration of the last sample of the last fragment needs to be extended using the track decode time of the next fragment to come, or if it should wait until all fragments have been received (also indicated by out-of-band means) to do that operation. Derived specifications are permitted to require specific handling of the sequence\_number of the MovieFragmentHeaderBox, for example (e.g. that sequence numbers start at and increment by 1).

#### Syntax

aligned(8) class TrackFragmentBaseMediaDecodeTimeBox  
 extends FullBox('tfdt', version, 0)   
{  
 if (version==1) {  
 unsigned int(64) baseMediaDecodeTime;  
 } else { // version==0  
 unsigned int(32) baseMediaDecodeTime;  
 }  
}

#### Semantics

version is an integer that specifies the version of this box (0 or 1 in this document).

baseMediaDecodeTime is an integer equal to the sum of the decode durations of all earlier samples in the media, expressed in the media's timescale. It does not include the samples added in the enclosing track fragment.

### Level assignment box

#### Definition

Box Type: 'leva'  
Container: MovieExtendsBox  
Mandatory: No  
Quantity: Zero or one

Levels specify subsets of the file. Samples mapped to level n may depend on any samples of levels m, where m <= n, and shall not depend on any samples of levels p, where p > n. For example, levels can be specified according to temporal level (e.g. temporal\_id of SVC or MVC).

Levels cannot be specified for the initial movie. When the LevelAssignmentBox is present, it applies to all movie fragments subsequent to the initial movie.

For the context of the LevelAssignmentBox, a fraction is defined to consist of one or more MovieFragmentBoxes and the associated MediaDataBoxes, possibly including only an initial part of the last MediaDataBox. Within a fraction, data for each level shall appear contiguously. Data for levels within a fraction shall appear in increasing order of level value. All data in a fraction shall be assigned to levels.

NOTE In the context of DASH (ISO/IEC 23009-1), each subsegment indexed within a SubsegmentIndexBox is a fraction.

The LevelAssignmentBox provides a mapping from features, such as scalability layers, to levels. A feature can be specified through a track, a sub-track within a track, or a sample grouping of a track.

When padding\_flag is equal to 1 this indicates that a conforming fraction can be formed by concatenating any positive integer number of levels within a fraction and padding the last MediaDataBox by zero bytes up to the full size that is indicated in the header of the last MediaDataBox. The use of padding\_flag is deprecated.

#### Syntax

aligned(8) class LevelAssignmentBox extends FullBox('leva', 0, 0)  
{  
 unsigned int(8) level\_count;  
 for (j=1; j <= level\_count; j++) {  
 unsigned int(32) track\_ID;  
 unsigned int(1) padding\_flag;  
 unsigned int(7) assignment\_type;  
 if (assignment\_type == 0) {  
 unsigned int(32) grouping\_type;  
 }  
 else if (assignment\_type == 1) {  
 unsigned int(32) grouping\_type;  
 unsigned int(32) grouping\_type\_parameter;  
 }  
 else if (assignment\_type == 2) {}  
 // no further syntax elements needed  
 else if (assignment\_type == 3) {}  
 // no further syntax elements needed  
 else if (assignment\_type == 4) {  
 unsigned int(32) sub\_track\_ID;  
 }  
 // other assignment\_type values are reserved  
 }  
}

#### Semantics

level\_count specifies the number of levels each fraction is grouped into. level\_count shall be greater than or equal to 2.

track\_ID for loop entry j specifies the track identifier of the track assigned to level j.

padding\_flag equal to 1 indicates that a conforming fraction can be formed by concatenating any positive integer number of levels within a fraction and padding the last MediaDataBox by zero bytes up to the full size that is indicated in the header of the last MediaDataBox. When padding\_flag is equal to 0 this is not assured.

assignment\_type indicates the mechanism used to specify the assignment to a level. assignment\_type values greater than 4 are reserved, while the semantics for the other values are specified as follows. The sequence of assignment\_types is restricted to be a set of zero or more of type 2 or 3, followed by zero or more of exactly one type.

* 0: sample groups are used to specify levels, i.e., samples mapped to different sample group description indexes of a particular sample grouping lie in different levels within the identified track; other tracks are not affected and shall have all their data in precisely one level;
* 1: as for assignment\_type 0 except assignment is by a parameterized sample group;
* 2, 3: level assignment is by track (see the SubsegmentIndexBox for the difference in processing of these levels)
* 4: the respective level contains the samples for a sub-track. The sub-tracks are specified through the SubTrackBox; other tracks are not affected and shall have all their data in precisely one level;

grouping\_type and grouping\_type\_parameter, if present, specify the sample grouping used  
to map sample group description entries in the SampleGroupDescriptionBox to levels. Level n contains the samples that are mapped to the SampleGroupDescriptionEntry having index n in the SampleGroupDescriptionBox having the same values of grouping\_type and grouping\_type\_parameter, if present, as those provided in this box.

sub\_track\_ID specifies that the sub-track identified by sub\_track\_ID within loop entry j is mapped to level j.

### Sample auxiliary information in movie fragments

When sample auxiliary information (8.7.8 and 8.7.9) is present in the MovieFragmentBox, the offsets in the SampleAuxiliaryInformationOffsetsBox are treated the same as the data\_offset in the TrackRunBox, that is, they are relative to any base\_data\_offset value established for that track fragment.

If only one offset is provided, then the Sample Auxiliary Information for all the track runs in the fragment is stored contiguously, otherwise exactly one offset shall be provided for each track run.

If the field default\_sample\_info\_size is non-zero in one of these boxes, then the size of the auxiliary information is constant for the identified samples.

In addition, if:

* this box is present in the MovieBox,
* and default\_sample\_info\_size is non-zero in the box in the MovieBox,
* and the SampleAuxiliaryInformationSizesBox is absent in a movie fragment,

then the auxiliary information has this same constant size for every sample in the movie fragment also; it is then not necessary to repeat the box in the movie fragment.

### Track Extension Properties box

#### Definition

Box Type: 'trep'  
Container: MovieExtendsBox  
Mandatory: No  
Quantity: Zero or more. (Zero or one per track)

This box can be used to document or summarize characteristics of the track in the subsequent movie fragments. It may contain any number of child boxes.

#### Syntax

class TrackExtensionPropertiesBox extends FullBox('trep', 0, 0)   
{  
 unsigned int(32) track\_ID;  
 // Any number of boxes may follow  
}

#### Semantics

track\_ID indicates the track for which the track extension properties are provided in this box.

### Alternative startup sequence properties box

#### Definition

Box Type: 'assp'  
Container: TrackExtensionPropertiesBox  
Mandatory: No  
Quantity: Zero or one

This box indicates the properties of alternative startup sequence sample groups in the subsequent track fragments of the track indicated in the containing TrackExtensionPropertiesBox.

Version 0 of the AlternativeStartupSequencePropertiesBox shall be used if version 0 of the SampleToGroupBox is used for the alternative startup sequence sample grouping. Version 1 of the AlternativeStartupSequencePropertiesBox shall be used if version 1 of the SampleToGroupBox is used for the alternative startup sequence sample grouping.

#### Syntax

class AlternativeStartupSequencePropertiesBox   
 extends FullBox('assp', version, 0)   
{  
 if (version == 0) {  
 signed int(32) min\_initial\_alt\_startup\_offset;  
 }  
 else if (version == 1) {  
 unsigned int(32) num\_entries;  
 for (j=1; j <= num\_entries; j++) {  
 unsigned int(32) grouping\_type\_parameter;  
 signed int(32) min\_initial\_alt\_startup\_offset;  
 }  
 }  
}

#### Semantics

min\_initial\_alt\_startup\_offset: No value of sample\_offset[ 1 ] of the referred sample group description entries of the alternative startup sequence sample grouping shall be smaller than min\_initial\_alt\_startup\_offset. In version 0 of this box, the alternative startup sequence sample grouping using version 0 of the Sample to Group box is referred to. In version 1 of this box, the alternative startup sequence sample grouping using version 1 of the SampleToGroupBox is referred to as further constrained by grouping\_type\_parameter.

num\_entries indicates the number of alternative startup sequence sample groupings documented in this box.

grouping\_type\_parameter indicates which one of the alternative sample groupings this loop entry applies to.

### Metadata and user data in movie fragments

When MetaBoxes occur in MovieFragmentBoxes or TrackFragmentBoxes, the following applies. The file shall have been fragmented such that any metadata needed in the movie or track fragment is formed from the union of the metadata in the MovieBox and the fragment, not considering or using metadata in any other fragment. Metadata in a movie or track fragment is logically ‘arriving late’ but is valid for the entire track. When a file is de-fragmented, the metadata in the movie or track fragments must be merged into the movie or track boxes, respectively. This process allows for ‘just in time’ delivery of support resources, and bandwidth management, while preserving the essentially atemporal nature of untimed metadata. If metadata truly changes over time, a timed metadata track may be needed.

If, during this merge, there are either (a) metadata items with the same item\_ID or (b) user-data items with the same type, then the following applies:

1. all occurrences of the data (user-data box or metadata item) must be ‘true’ for the entire movie including all fragments;
2. the occurrences in higher-numbered movie fragments (‘later’ occurrences) may be more accurate or ‘preferred’;
3. in particular, data in an empty initial MovieBox may be only estimates or ‘not to exceed’ values, and data in a final otherwise empty movie fragment may be the ‘final’ or most accurate values.

Consequently, for MetaBox, the redefinition of an item with the same item\_ID in a subsequent MetaBox is equivalent to an item replacement, the new item applying for the entire track or file. For UserDataBox, there may be multiple occurrences of a user data of a given type (for example CopyrightBox with different languages), and these occurrences may be delivered in different movie fragments or in the initial movie. Readers should be careful when attempting at removing duplicates of such boxes in a defragmentation process, since checking the type of the user data for removal might not be sufficient; the language or other fields specific to the type of user-data may need inspection.

## Sample group structures

### Overview

This clause specifies a generic mechanism for representing a partition of the samples in a track. A *sample grouping* is an assignment of each sample in a track to be a member of one *sample group,* based on a grouping criterion. A sample group in a sample grouping is not limited to being contiguous samples and may contain non-adjacent samples. As there may be more than one sample grouping for the samples in a track, each sample grouping has a type field to indicate the type of grouping. For example, a file might contain two sample groupings for the same track: one based on an assignment of sample to layers and another to sub-sequences.

Sample groupings are represented by two linked data structures: (1) a SampleToGroupBox represents the assignment of samples to sample groups; (2) a SampleGroupDescriptionBox contains a *sample group description entry* for each sample group describing the properties of the group. There may be multiple instances of the SampleToGroupBox and SampleGroupDescriptionBoxes based on different grouping criteria. These are distinguished by a type field used to indicate the type of grouping.

A grouping of a particular grouping\_type may use a parameter in the sample to group mapping; if so, the meaning of the parameter must be documented with the group. An example of this might be documented the sync points in a multiplex of several video streams; the group definition might be ‘Is an I frame’, and the group parameter might be the identifier of each stream. Since the SampleToGroupBox occurs once for each stream, it is now both compact, and informs the reader about each stream separately.

One example of using these tables is to represent the assignments of samples to *layers.* In this case each sample group represents one layer, with an instance of the SampleToGroupBox describing which layer a sample belongs to.

In general, it is not required that a sample to group mapping marks every sample for which the associated sample group description applies. It is only required that the mapping is correct for mapped samples. However, this general principle may be overridden by the definition of specific sample groups.

NOTE There might not be a SampleToGroupBox of a given grouping\_type corresponding to a SampleGroupDescriptionBox with the same grouping\_type because references to the SampleGroupDescriptionBox (in particular to its entries) might be provided by specific constructs in derived specifications.

### Sample to group box

* + - 1. Definition

Box Type: 'sbgp'  
Container: SampleTableBox or TrackFragmentBox  
Mandatory: No  
Quantity: Zero or more.

This table can be used to find the group that a sample belongs to and the associated description of that sample group. The table is compactly coded with each entry giving the index of the first sample of a run of samples with the same sample group descriptor. The sample group description ID is an index that refers to a SampleGroupDescriptionBox, which contains entries describing the characteristics of each sample group.

There may be multiple instances of this box if there is more than one sample grouping for the samples in a track or track fragment. Each instance of the SampleToGroup box has a type that distinguishes different sample groupings. Within a track, whether declared in the SampleTableBox or in TrackFragmentBox, there shall be at most one instance of this box with a particular grouping\_type, and, if present, a grouping\_type\_parameter. The associated SampleGroupDescriptionBox shall indicate the same value for the grouping\_type. When there are multiple SampleToGroupBoxes with a particular value of grouping\_type in a container box, the version of all the SampleToGroupBoxes shall be 1. When the version of a SampleToGroupBox is 0, there shall be only one occurrence of SampleToGroupBox with this grouping\_type in a container box.

Version 1 of this box should only be used if a grouping\_type\_parameter is needed. When the grouping\_type\_parameter is not explicitly defined in this standard, its semantics may be overridden by derived specifications.

For a SampleGroupDescriptionBox with a given grouping\_type, there may be more than one SampleToGroupBox with the same grouping\_type if and only if each SampleToGroupBox has a different value of grouping\_type\_parameter; there may also be no SampleToGroupBox with the given grouping\_type if no samples are mapped to a description of that grouping\_type, or if all samples are mapped to the default entry identified by the SampleGroupDescriptionBox.

* + - 1. Syntax

aligned(8) class SampleToGroupBox extends FullBox('sbgp', version, 0)  
{  
 unsigned int(32) grouping\_type;  
 if (version == 1) {  
 unsigned int(32) grouping\_type\_parameter;  
 }  
 unsigned int(32) entry\_count;  
 for (i=1; i <= entry\_count; i++)  
 {  
 unsigned int(32) sample\_count;  
 unsigned int(32) group\_description\_index;  
 }  
}

* + - 1. Semantics

version is an integer that specifies the version of this box, either 0 or 1.

grouping\_type is an integer that identifies the type (i.e. criterion used to form the sample groups) of the sample grouping and links it to its sample group description table with the same value for grouping\_type. At most one occurrence of this box with the same value for grouping\_type (and, if used, grouping\_type\_parameter) shall exist for a track.

grouping\_type\_parameter is an indication of the sub-type of the grouping

entry\_count is an integer that gives the number of entries in the following table.

sample\_count is an integer that gives the number of consecutive samples with the same sample group descriptor. The total sample count is defined to be equal to the sample\_count documented in SampleSizeBox or CompactSampleSizeBox when this box is contained in SampleTableBox, and equal to the total number of samples in all the track fragment runs of the track fragment when this box is contained in TrackFragmentBox. It is an error for the total of all of the sample\_count in this box to be greater than the total sample count, and consequently the reader behaviour is undefined. If the sum of the sample count in this box with grouping\_type value is less than the total sample count, or there is no SampleToGroupBox for a value of grouping\_type that applies to some samples (e.g. it is absent from a track fragment), then those samples are associated with the group identified by the default\_group\_description\_index in the SampleGroupDescriptionBox with the same value of grouping\_type, if any, or else with no group.

group\_description\_index is an integer that gives the index of the sample group description entry which describes the samples in this group. The index ranges from 1 to the number of sample group description entries in the SampleGroupDescriptionBox, or takes the value 0 to indicate that this sample is a member of no group of this type.

NOTE When a movie is fragmented, group\_description\_index can refer to a sample group description entry of the SampleGroupDescriptionBox with same grouping\_type either in the MovieBox or in the TrackFragmentBox as specified in 8.9.4.

### Sample group description box

* + - 1. Definition

Box Type: 'sgpd'  
Container: SampleTableBox or TrackFragmentBox  
Mandatory: No  
Quantity: Zero or more, with exactly one for each grouping\_type in a SampleToGroupBox.

This description table gives information about the characteristics of sample groups. The descriptive information is any other information needed to define or characterize the sample group. The syntax of the sample group description entry used is determined by both the grouping\_type and the media handler type.

There may be multiple instances of this box if there is more than one sample grouping for the samples in a track. Each instance of the SampleGroupDescriptionBox has a type that distinguishes different sample groupings. There shall be at most one instance of this box with a particular grouping\_type in a track (i.e. defined in a SampleTableBox or TrackFragmentBox).

The flags field of the SampleGroupDescriptionBox shall be zero when the box is in a TrackFragmentBox. When the box is in a SampleTableBox, either or both of the two lowest bits may be set:

* static\_group\_description: Flag mask is 0x000001. When set to 1, this flag indicates that there are no SampleGroupDescriptionBoxes of this grouping\_type in any TrackFragmentBox of this track.
* static\_mapping: Flag mask is 0x000002. When set to 1, this flag indicates that there are no SampleToGroupBoxes of this grouping\_type in this track (in neither the SampleTableBox nor any TrackFragmentBox of this track); all samples therefore map to the default.

NOTE 1 When static\_mapping is set to 1 and default\_group\_description\_index is equal to zero or is unspecified, this means that none of the entries of the SampleGroupDescriptionBox actually map to samples per default, but this default can be changed for a given fragment by defining a SampleGroupDescriptionBox with version >= 2, same grouping\_type and default\_group\_description\_index > 0 in this fragment.

These flags may be used in combination with the version of the SampleGroupDescriptionBox to signal various possibilities.

* static\_group\_description without static\_mapping:

the SampleGroupDescriptionBox shall only be in the MovieBox for the given grouping\_type, but samples of the track, including in movie fragments, can map to any entry in this SampleGroupDescriptionBox..

* static\_mapping without static\_group\_description:

everything in a fragment maps to at most one group; there may be new SampleGroupDescriptionBoxes of this type in fragments; depending on their version, the SampleGroupDescriptionBoxes can identify a default sample group, or that samples are unmapped.

* both static\_group\_description and static\_mapping:

every sample maps to the default indicated in the SampleGroupDescriptionBox in the MovieBox; that SampleGroupDescriptionBox can indicate a default sample group or indicate that all samples are unmapped, depending on its version.

The information is stored in the SampleGroupDescriptionBox after the entry-count. An abstract entry type is defined and sample groupings shall define derived types to represent the description of each sample group.

NOTE 2 In version 0 of the entries the base classes for sample group description entries are neither boxes nor have a size that is signalled. For this reason, use of version 0 entries is deprecated. When defining derived classes, ensure either that they have a fixed size, or that the size is explicitly indicated with a length field. An implied size (e.g. achieved by parsing the data) is not recommended as this makes scanning the array difficult.

An essential sample group description is a sample group description for which the version field is equal to 3, and the associated sample group is also referred to as an essential sample group. An essential sample group description describes essential information for the associated samples, and parsers shall not attempt to process any track for which unrecognized sample group descriptions marked as essential are present.

The grouping\_type in any SampleGroupDescriptionBox with version equal to 3 shall not be equal to any scheme\_type present in the same track.

* + - 1. Syntax

// Sequence Entry  
abstract class SampleGroupDescriptionEntry (unsigned int(32) grouping\_type)  
{  
}

abstract class VisualSampleGroupEntry (unsigned int(32) grouping\_type) extends SampleGroupDescriptionEntry (grouping\_type)  
{  
}

abstract class AudioSampleGroupEntry (unsigned int(32) grouping\_type) extends SampleGroupDescriptionEntry (grouping\_type)  
{  
}

abstract class HintSampleGroupEntry (unsigned int(32) grouping\_type) extends SampleGroupDescriptionEntry (grouping\_type)  
{  
}

abstract class SubtitleSampleGroupEntry (unsigned int(32) grouping\_type) extends SampleGroupDescriptionEntry (grouping\_type)  
{  
}

abstract class TextSampleGroupEntry (unsigned int(32) grouping\_type) extends SampleGroupDescriptionEntry (grouping\_type)  
{  
}

abstract class MetadataSampleGroupEntry (unsigned int(32) grouping\_type) extends SampleGroupDescriptionEntry (grouping\_type)  
{  
}

abstract class HapticSampleGroupEntry (unsigned int(32) grouping\_type) extends SampleGroupDescriptionEntry (grouping\_type)  
{  
}

abstract class VolumetricVisualSampleGroupEntry (unsigned int(32) grouping\_type) extends SampleGroupDescriptionEntry (grouping\_type)  
{  
}

aligned(8) class SampleGroupDescriptionBox ()  
 extends FullBox('sgpd', version, flags)  
{  
 unsigned int(32) grouping\_type;  
 if (version>=1) { unsigned int(32) default\_length; }  
 if (version>=2) {  
 unsigned int(32) default\_group\_description\_index;  
 }  
 unsigned int(32) entry\_count;  
 int i;  
 for (i = 1 ; i <= entry\_count ; i++){  
 if (version>=1) {  
 if (default\_length==0) {  
 unsigned int(32) description\_length;  
 }  
 }  
 SampleGroupDescriptionEntry (grouping\_type);  
 // an instance of a class derived from SampleGroupDescriptionEntry  
 // that is appropriate and permitted for the media type  
 }  
}

* + - 1. Semantics

version is an integer that specifies the version of this box.

grouping\_type is an integer that identifies the SampleToGroupBox that is associated with this sample group description.

default\_group\_description\_index: specifies the index of the sample group description entry which applies to all samples in the track for which no sample to group mapping is provided through a SampleToGroupBox with the same value of grouping\_type. For version strictly less than 2, this field is not coded and *file readers shall behave as if the field had been coded with a value of zero*. A value of zero indicates that no default mapping for samples to a group description entry for this grouping\_type is provided.

NOTE 1 When a movie is fragmented, default\_group\_description\_index can refer to a sample group description entry of the SampleGroupDescriptionBox with same grouping\_type either in the MovieBox or in the TrackFragmentBox as specified in 8.9.4.

entry\_count is an integer that gives the number of entries in the following table.

default\_length indicates the length of every group entry (if the length is constant), or zero (0) if it is variable

description\_length indicates the length of an individual group entry, in the case it varies from entry to entry and default\_length is therefore 0

NOTE 2 The field default\_group\_description\_index used to be called default\_sample\_description\_index in previous editions of this document.

### Representation of group structures in movie fragments

Support for sample group structures within movie fragments is provided by the use of the SampleToGroupBox with the container for this box being the TrackFragmentBox. The definition, syntax and semantics of this Box is as specified in subclause 8.9.2.

The SampleToGroupBox can be used to find the group that a sample in a track fragment belongs to and the associated description of that sample group. The table is compactly coded with each entry giving the index of the first sample of a run of samples with the same sample group descriptor. The sample group description ID is an index that refers to a SampleGroupDescriptionBox, which contains entries describing the characteristics of each sample group and present in the SampleTableBox.

There may be multiple instances of the SampleToGroupBox if there is more the one sample grouping for the samples in a track fragment. Each instance of the SampleToGroupBox has a grouping\_type, and possibly grouping\_type\_parameter, that distinguishes different sample groupings. The associated SampleGroupDescriptionBox shall indicate the same value for the grouping\_type.

The total number of samples represented in any SampleToGroupBox in the track fragment shall match the total number of samples in all the track fragment runs. Each SampleToGroupBox documents a different grouping of the same samples.

Zero or more SampleGroupDescriptionBoxes may also be present in a TrackFragmentBox. These definitions are additional to the definitions provided in the SampleTableBox of the track. Group definitions within a movie fragment can only be referenced and used from within that same movie fragment.

Within the SampleToGroupBox in that movie fragment, the group description indexes for groups defined within the same fragment start at 0x10001, i.e. the index value 1, with the value 1 in the top 16 bits. This means there must be fewer than 65536 group definitions for this track and grouping\_type in the SampleTableBox of the track.

When changing the size of movie fragments, or removing them, these fragment-local group definitions will need to be merged into the definitions in the MovieBox, or into the new movie fragments, and the index numbers in the SampleToGroupBox(es) adjusted accordingly. It is recommended that, in this process, identical (and hence duplicate) definitions not be made in any SampleGroupDescriptionBox, but that duplicates be merged and the indexes adjusted accordingly.

When a SampleGroupDescriptionBox “A”, declaring a default\_group\_description\_index, is present in a TrackFragmentBox, that default\_group\_description\_index shall indicate either:

* 0 or 0x10000, if no default sample group description is defined for that track fragment
* the index of a sample group description entry in a SampleGroupDescriptionBox of the same grouping\_type declared in the SampleTableBox of the track
* the index incremented by 0x10000 of the entry of that SampleGroupDescriptionBox “A”.

The index value for the first entry in a SampleGroupDescriptionBox is 1.

For any track fragment, the default sample group description entry for a given grouping\_type is the one indicated by the default\_group\_description\_index of the SampleGroupDescriptionBox of the same grouping\_type declared in that track fragment, if any; otherwise by default\_group\_description\_index of the SampleGroupDescriptionBox of the same grouping\_type declared in the SampleTableBox of the track, if any; otherwise, no default entry is used for that grouping\_type.

The default sample group identified in a SampleGroupDescriptionBox in the SampleTableBox shall identify a group within that box, i.e. the index value of the default is less than 0x10000.

### Compact sample to group box

#### 8.9.5.1 Definition

Box Type: 'csgp'  
Container: SampleTableBox or TrackFragmentBox  
Mandatory: No  
Quantity: Zero or more.

The compact sample to group box provides a more compact way to represent the mapping from sample to group, especially in the cases where there are repeating patterns, and when there are few sample groups of a particular type.

The design uses a vector of concatenated *patterns* each of which is used once by a mapping array, which associates runs of samples with repeats of that pattern. This is illustrated by the following example. In the following, each letter represents a different sample group description index value (possibly 0).

If a track has the following associations, starting from the first sample:

a b c b a b c b a b c x x a b c b a b d b

those associations might be represented by the following:

1. pattern\_length=4; sample\_count=11;  
 2. pattern\_length=1; sample\_count=2;  
 3. pattern\_length=4; sample\_count=6;  
 4. pattern\_length=2; sample\_count=2;  
  
 pattern=[  
 a b c b // pattern 1 of length 4  
 x // pattern 2 of length 1  
 a b c b // pattern 3 of length 4  
 d b // pattern 4 of length 2  
 ] // the pattern\_length is thus 4+1+4+2=11

When sample\_count[i] is equal to pattern\_length[i], the pattern is not repeated.

When sample\_count[i] is greater than pattern\_length[i], the sample\_group\_description\_index values of the i-th pattern are used repeatedly to map the sample\_count[i] values. It is not necessarily the case that sample\_count[i] is a multiple of pattern\_length[i]; the cycling may terminate in the middle of the pattern.

When the total of the sample\_count[i] values for all values of i in the range of 1 to pattern\_count, inclusive, is less than the total sample count, the reader should associate the samples that have no explicit group association with the default group defined in the SampleGroupDescriptionBox, if any, or else with no group.

It is an error for the total of the sample\_count[i] values to be greater than the total count of actual samples described by the encompassing TrackBox or TrackFragmentBox, and consequently the reader behaviour is undefined.

The 24-bit flag field is defined as follows:

unsigned int(16) reserved = 0;  
 unsigned int(1) index\_msb\_indicates\_fragment\_local\_description;  
 unsigned int(1) grouping\_type\_parameter\_present;  
 unsigned int(2) pattern\_size\_code;  
 unsigned int(2) count\_size\_code;  
 unsigned int(2) index\_size\_code;

#### 8.9.5.2 Syntax

unsigned int(8) function f(unsigned int(2) index) {  
 switch(index) {  
 case 0: return 4;  
 case 1: return 8;  
 case 2: return 16;  
 case 3: return 32;  
}

aligned(8) class CompactSampleToGroupBox  
 extends FullBox('csgp', version, flags)  
{  
 unsigned int(32) grouping\_type;  
 if (grouping\_type\_parameter\_present == 1) {  
 unsigned int(32) grouping\_type\_parameter;  
 }  
 unsigned int(32) pattern\_count;  
 totalPatternLength = 0;  
 for (i=1; i <= pattern\_count; i++) {  
 unsigned int(f(pattern\_size\_code)) pattern\_length[[i]];  
 unsigned int(f(count\_size\_code)) sample\_count[[i]];  
 }  
 for (j=1; j <= pattern\_count; j++) {  
 for (k=1; k <= pattern\_length[j]; k++) {  
 unsigned int(f(index\_size\_code))  
 sample\_group\_description\_index[[j]][[k]];  
 // whose msb might indicate fragment\_local or global  
 }  
 }  
}

#### 8.9.5.3 Semantics

version is an integer that specifies the version of this box, currently 0.

grouping\_type is an integer that identifies the type (i.e. criterion used to form the sample groups) of the sample grouping and links it to its sample group description table with the same value for grouping type. At most one occurrence of either the 'csgp' or 'sbgp' with the same value for grouping\_type (and, if used, grouping\_type\_parameter) shall exist for a track.

grouping\_type\_parameter is an indication of the sub-type of the grouping.

index\_msb\_indicates\_fragment\_local\_description is a flag that shall be zero when this box appears inside a TrackBox but may be 0 or 1 when this box appears inside a TrackFragmentBox. When it is 1, it indicates that the most significant bit (MSB) of every sample\_group\_description\_index does not form part of the index number but instead indicates which SampleGroupDescriptionBox the group description is to be found in: if the MSB is 0, the index identifies a group description from the TrackBox's SampleGroupDescriptionBox; if the MSB is 1, the index identifies a group description from the TrackFragmentBox's SampleGroupDescriptionBox.

field\_size\_code, pattern\_size\_code, index\_size\_code are integers specifying the size in bits of the entries in the array of the pattern\_length, sample\_count and sample\_group\_description\_index values respectively; the matching code values map to the sizes: code 0 indicates a 4-bit size, code 1 an 8-bit size, code 2 a 16-bit size, and code 3 a 32-bit size. If the field size 4 is used for the pattern\_size, then it shall also be used for the count\_size (to maintain byte alignment), though this is probably rarely useful; if it is used for sample\_group\_description\_index, then each byte contains two values: entry[i]<<4 + entry[i+1]; if the sizes do not fill an integral number of bytes, the last byte is padded with zeros.

pattern\_count indicates the length of the associated pattern in the pattern array that follows it. The sum of the included sample\_count values indicates the number of mapped samples.

pattern\_length[i] corresponds to a pattern within the second array of sample\_group\_description\_index[j] values. Each instance of pattern\_length[i] shall be greater than 0.

sample\_count[i] specifies the number of samples that use the i-th pattern. sample\_count[i] shall be greater than zero, and sample\_count[i] shall be greater than or equal to pattern\_length[i].

sample\_group\_description\_index[j][k] is an integer that gives the index of the sample group description entry which describes the samples in this group. The index ranges from 1 to the number of sample group description entries in the SampleGroupDescriptionBox, inclusive, or takes the value 0 to indicate that this sample is a member of no group of this type.

## User data

### User data box

* + - 1. Definition

Box Type: 'udta'  
Container: MovieBox, TrackBox, MovieFragmentBox, TrackFragmentBox or PreselectionGroupBox  
Mandatory: No  
Quantity: Zero or one

This box contains objects that declare user information about the containing box and its data (presentation or track).

The UserDataBox is a container box for informative user-data. This user data is formatted as a set of boxes with more specific box types, which declare more precisely their content. The contained boxes are normal boxes, using a defined, registered, or UUID extension box type.

The handling of user-data in movie fragments is described in 8.8.17.

* + - 1. Syntax

aligned(8) class UserDataBox extends Box('udta')   
{  
}

### Copyright box

* + - 1. Definition

Box Type: 'cprt'  
Container: UserDataBox  
Mandatory: No  
Quantity: Zero or more

The CopyrightBox contains a copyright declaration which applies to the entire presentation, when contained within the MovieBox, or, when contained in a track, to that entire track. There may be multiple copyright boxes using different language codes.

* + - 1. Syntax

aligned(8) class CopyrightBox extends FullBox('cprt', version = 0, 0)   
{  
 const bit(1) pad = 0;  
 unsigned int(5) language[3]; // ISO-639-2/T language code  
 utfstring notice;  
}

* + - 1. Semantics

language declares the language code for the following text, in the form of a packed three-character code from ISO 639-2. Each character is packed as the difference between its ASCII value and 0x60. The code is confined to being three lower-case letters, so these values are strictly positive.

notice gives a copyright notice.

### Track selection box

#### Overview

A typical presentation stored in a file contains one alternate group per media type: one for video, one for audio, etc. Such a file may include several video tracks, although, at any point in time, only one of them should be played or streamed. This is achieved by assigning all video tracks to the same alternate group. (See subclause 8.3.2 for the definition of alternate groups.)

All tracks in an alternate group are candidates for media selection, but it may not make sense to switch between some of those tracks during a session. One may for instance allow switching between video tracks at different bitrates and keep frame size but not allow switching between tracks of different frame size. In the same manner it may be desirable to enable selection – but not switching – between tracks of different video codecs or different audio languages.

The distinction between tracks for *selection* and *switching* is addressed by assigning tracks to switch groups in addition to alternate groups. One alternate group may contain one or more switch groups. All tracks in an alternate group are candidates for media selection, while tracks in a switch group are also available for switching during a session. Different switch groups represent different operation points, such as different frame size, high/low quality, etc.

For the case of non-scalable bitstreams, several tracks may be included in a switch group. The same also applies to non-layered scalable bitstreams, such as traditional AVC streams.

By labelling tracks with attributes it is possible to characterize them. Each track can be labelled with a list of attributes which can be used to describe tracks in a particular switch group or differentiate tracks that belong to different switch groups.

* + - 1. Definition

Box Type: 'tsel'  
Container: UserDataBox of the corresponding TrackBox  
Mandatory: No  
Quantity: Zero or One

The track selection box is contained in the user data box of the track it modifies.

* + - 1. Syntax

aligned(8) class TrackSelectionBox  
 extends FullBox('tsel', version = 0, 0)   
{  
 template int(32) switch\_group = 0;  
 unsigned int(32) attribute\_list[]; // to end of the box  
}

* + - 1. Semantics

switch\_group is an integer that specifies a group or collection of tracks. If this field is 0 (default value) or if the TrackSelectionBox is absent there is no information on whether the track can be used for switching during playing or streaming. If this integer is not 0 it shall be the same for tracks that can be used for switching between each other. Tracks that belong to the same switch group shall belong to the same alternate group. A switch group may have only one member.

attribute\_list is a list, to the end of the box, of attributes. The attributes in this list should be used as descriptions of tracks or differentiation criteria for tracks in the same alternate or switch group. Each differentiating attribute is associated with a pointer to the field or information that distinguishes the track.

* + - 1. Attributes

The following attributes are descriptive:

|  |  |  |
| --- | --- | --- |
| *Name* | *Attribute* | *Description* |
| Temporal scalability | 'tesc' | The track can be temporally scaled. |
| Fine-grain SNR scalability | 'fgsc' | The track can be scaled in terms of quality. |
| Coarse-grain SNR scalability | 'cgsc' | The track can be scaled in terms of quality. |
| Spatial scalability | 'spsc' | The track can be spatially scaled. |
| Region-of-interest scalability | 'resc' | The track can be region-of-interest scaled. |
| View scalability | 'vwsc' | The track can be scaled in terms of number of views. |

The following attributes are differentiating:

|  |  |  |
| --- | --- | --- |
| *Name* | *Attribute* | *Pointer* |
| Codec | 'cdec' | Sample Entry (in SampleDescriptionBox of media track) |
| Screen size | 'scsz' | Width and height fields of VisualSampleEntry. |
| Max packet size | 'mpsz' | Maxpacketsize field in RtpHintSampleEntry |
| Media type | 'mtyp' | Handlertype in HandlerBox (of media track) |
| Media language | 'mela' | Language field in MediaHeaderBox |
| Bitrate | 'bitr' | Total size of the samples in the track divided by the duration in the TrackHeaderBox |
| Frame rate | 'frar' | Number of samples in the track divided by duration in the TrackHeaderBox |
| Number of views | 'nvws' | Number of views in the track |

Descriptive attributes characterize the tracks they modify, whereas differentiating attributes differentiate between tracks that belong to the same alternate or switch groups. The pointer of a differentiating attribute indicates the location of the information that differentiates the track from other tracks with the same attribute.

### Track kind

#### Definition

Box Type: 'kind'  
Container: AudioElementBox, PreselectionGroupBox, or   
 UserDataBox of the corresponding TrackBox  
Mandatory: No  
Quantity: Zero or more

The KindBox labels a track with its role or kind.

It contains a URI, possibly followed by a value. If only a URI occurs, then the kind is defined by that URI; if a value follows, then the naming scheme for the value is identified by the URI.

More than one of these may occur in a track, with different contents but with appropriate semantics (e.g. two schemes that both define a kind that indicates sub-titles).

#### Syntax

aligned(8) class KindBox extends FullBox('kind', version = 0, 0)   
{  
 utf8string schemeURI;  
 utf8string value;  
}

#### Semantics

schemeURI declares either the identifier of the kind, if no value follows, or the identifier of the naming scheme for the following value.

value is a name from the declared scheme

### Label box

#### Definition

Box Type: 'labl'  
Container: UserDataBox of a TrackBox, AudioElementBox,   
 AudioElementSelectionBox, or PreselectionroupBox   
Mandatory: No  
Quantity: Zero or more

Labels provide the ability to annotate data structures in an ISOBMFF file to provide a description of the context of the entity to which the label is assigned. Such labels may for example be used by playback clients to provide a selection choice to the user. The label may also be used for simple annotation in another context.

Multiple labels can be used to provide the textual description. To annotate the entity to a multilingual audience, the annotation can be provided in multiple languages.

When is\_group\_label is equal to 1 this indicates that the label text in this box specifies a summary or title of all labels with the same label\_id. This may be used as the title on a selection menu containing a collection of labels.

#### Syntax

aligned(8) class LabelBox extends FullBox('labl', version=0, 0 )  
{  
 unsigned int(1) is\_group\_label;  
 bit(7) reserved = 0;  
 unsigned int(16) label\_id;  
 utf8string language;  
 utf8string label;  
}

#### Semantics

is\_group\_label specifies if the label contains a summary label for a group of labels.

label\_id is an integer that contains an identifier for the label. Labels with the same value belong to a label group. The value of zero indicates that the label does not belong to any label group.

language contains an IETF BCP 47 compliant language tag string, such as "en-US", "fr-FR", or "zh-CN", the language being the language the label is targeted at.

label contains the textual description.

## Metadata support

### MetaBox

* + - 1. Definition

Box Type: 'meta'  
Container: File, Segment, MovieBox, TrackBox, MovieFragmentBox or TrackFragmentBox  
Mandatory: No  
Quantity: Zero or one (in File, MovieBox, and TrackBox),  
 Zero or one (in Segment, MovieFragmentBox or TrackFragmentBox)

A common base structure is used to contain general untimed metadata. This structure is called the MetaBox as it was originally designed to carry metadata, i.e. data that is annotating other data. However, it is now used for a variety of purposes including the carriage of data that is not annotating other data, especially when present at ‘file level’. The handling of metadata in movie fragments is described in 8.8.17.

NOTE In previous editions of this document, the presence of the HandlerBox was mandatory. The 'isod' brand and any brands derived thereof allow omission of the HandlerBox unless specified otherwise below.

When a HandlerBox is present, it applies to all items without a HandlerProperty and may provide additional requirements on items with a HandlerProperty with different handler\_type than the one in the HandlerBox.

When the MetaBox contains a PrimaryItemBox and a HandlerBox, and the item indicated by the PrimaryItemBox has a HandlerProperty, the HandlerBox and the HandlerProperty of the primary item shall identify the same handler type.

When the MetaBox contains a GroupsListBox, any handler\_type may be used including 'null'. This rule may be overridden by grouping\_type specific definitions.

When the MetaBox contains neither a PrimaryItemBox nor a GroupsListBox, the MetaBox is required to contain a HandlerBox indicating the structure or format of the MetaBox contents.

When item indicated by PrimaryItemBox does not have a HandlerProperty, but has an ItemInfoEntry with an item\_type, the handler type in HandlerBox may be the same as the item\_type.

The other boxes defined here may be defined as optional or mandatory for a given format. If they are used, then they shall take the form specified here. These optional boxes include a DataInformationBox, which documents other files in which metadata values (e.g. pictures) are placed, and an ItemLocationBox, which documents where in those files each item is located (e.g. in the common case of multiple pictures stored in the same file).

At most one MetaBox may occur at each of the file level, segment, movie level, or track level.

If an ItemProtectionBox occurs, then some or all of the metadata, including possibly the primary resource, may have been protected and be un-readable unless the protection system is taken into account.

NOTE The MetaBox is unusual in that it is a container box yet extends FullBox, not Box.

Metadata items are identified by item\_ID. Within a given MetaBox, a given item\_ID shall uniquely refer to a single item. When an item is updated in movie fragments, the item\_ID refers to the latest received version.

Derived specifications may further restrict the criteria for uniqueness: unique among the item\_IDs in both file and movie-level boxes, or unique within that set extended with the track\_ID of the tracks in a movie box. The item\_ID value of 0 should not be used, and shall not be used when the set is extended to include track\_IDs.

There are three scopes for item\_IDs: file and segments; MovieBox and MovieFragmentBox; and TrackBox and TrackFragmentBox. In other words, there shall be only one item with a given item\_ID within a given scope (e.g. in the TrackBox and all TrackFragmentBox with the same track\_ID).

* + - 1. Syntax

aligned(8) class MetaBox (handler\_type)  
 extends FullBox('meta', version = 0, 0)   
{  
 HandlerBox(handler\_type) theHandler; // optional  
 PrimaryItemBox primary\_resource; // optional  
 DataInformationBox file\_locations; // optional  
 ItemLocationBox item\_locations; // optional  
 ItemProtectionBox protections; // optional  
 ItemInfoBox item\_infos; // optional  
 IPMPControlBox IPMP\_control; // optional  
 ItemReferenceBox item\_refs; // optional  
 ItemPropertiesBox item\_properties; // optional  
 ItemDataBox item\_data; // optional  
 GroupsListBox entity\_groups; // optional  
 Box other\_boxes[]; // optional  
}

### XML boxes

* + - 1. Definition

Box Type: 'xml ' or 'bxml'  
Container: MetaBox  
Mandatory: No  
Quantity: Zero or one

When the primary data is in XML format as defined by the W3C Recommendation, *Extensible Markup Language (XML)* and it is desired that the XML be stored directly in the MetaBox, one of these forms may be used. The BinaryXMLBox may only be used when there is a single well-defined binarization of the XML for that defined format as identified by the handler.

The use of the XMLBox in new specifications is deprecated. The preferred technique is to use an item, identify it as a primary item, and identify its precise XML format in the ItemInfoBox.

Previous edition of this standard did not mandate the XML data to be null-terminated, while this edition does. Writers conformant to this edition shall use a null termination character. Readers should tolerate boxes missing this null termination character.

* + - 1. Syntax

aligned(8) class XMLBox extends FullBox('xml ', version = 0, 0)   
{  
 utfstring xml;  
}

aligned(8) class BinaryXMLBox extends FullBox('bxml', version = 0, 0)   
{  
 unsigned int(8) data[]; // to end of box  
}

* + - 1. Semantics

xml is a zero-terminated string containing the XML data.

data contains the encoded XML data.

### Item location box

* + - 1. Definition

Box Type: 'iloc'  
Container: MetaBox  
Mandatory: No  
Quantity: Zero or one

The ItemLocationBox provides a directory of resources in this or other files, by locating their container, their offset within that container, and their length. Using byte offsets and lengths enables common handling of this data, even by systems which do not understand the particular metadata system (handler) used. For example, a system might integrate all the externally referenced metadata resources into one place, re-adjusting offsets and references accordingly.

The box starts with three or four values, specifying the size in bytes of the offset field, length field, base\_offset field, and, in versions 1 and 2 of this box, the item\_reference\_index fields, respectively. These values shall be from the set {0, 4, 8}.

The construction\_method field indicates the ‘construction method’ for the item:

1. file\_offset: by absolute byte offsets into the file or the payload of IdentifiedMediaDataBox referenced by data\_reference\_index;  (construction\_method == 0)
2. idat\_offset: by byte offsets into the ItemDataBox in the same MetaBox; neither the data\_reference\_index nor item\_reference\_index fields are used; (construction\_method == 1)
3. item\_offset: by byte offset into the items indicated by the item\_reference\_index field, which is only used (currently) by this construction method. (construction\_method == 2).

The item\_reference\_index is only used for the method item\_offset; it indicates the 1-based index of the item reference with referenceType 'iloc' linked from this item. If index\_size is 0, then the value 1 is implied; the value 0 is reserved.

The data\_reference\_index may take the value 0, indicating a reference into the same file as this MetaBox, or an index into the data references in the DataInformationBox in the containing MetaBox, with value 1 indicating the first entry in the data reference list.

NOTE 1 A reference to the ‘same file’ can also be coded by setting data\_reference\_index to a non-zero value pointing to a data reference entry of type 'urn ' with the flag 0x000001 set. However, using data\_reference\_index 0 is recommended.

Items may be stored fragmented into extents, e.g. to enable interleaving. An extent is a contiguous subset of the bytes of the resource identified by an offset and a length; the resource is formed by concatenating the extents in the order specified in this box. The size of the item is the sum of the extent lengths.

NOTE 2 Extents can be interleaved with the chunks defined by the sample tables of tracks.

The offsets are relative to a data origin. That origin is determined as follows:

1. when construction\_method = 0 (file offset):
2. when the data reference points to the ‘same file’ and when the MetaBox is in a Movie Fragment, the data origin is the first byte of the enclosing MovieFragmentBox (as for the default-base-is-moof flag in the TrackFragmentHeaderBox
3. when the data reference indicates DataEntryImdaBox or DataEntrySeqNumImdaBox, the data origin is the first byte of the payload of the corresponding IdentifiedMediaDataBox;
4. in all other cases, the data origin is the beginning of the file identified by the data reference;
5. when the construction\_method==1 (offsets into the ItemDataBox), the data origin is the beginning of data[] in the ItemDataBox;

NOTE 3 There are offset calculations in other parts of this document based on the beginning of a box header; in contrast, item data offsets are calculated relative to the box payload.

1. when construction\_method==2 (offsets into another item), the data origin is the first byte of the concatenated data (of all the extents) of that item;

A value of 0 for extent\_length is interpreted as follows:

1. when construction\_method = 0 (file offset):
2. when the data reference points to the ‘same file’, the length of the extent is assumed to be the length of the data between the offset (if specified) or the origin (if not specified), and the end of the file.
3. when the data reference indicates a DataEntryImdaBox or DataEntrySeqNumImdaBox, the extent\_length is assumed to be the length of the data between the offset (if specified) or the origin (if not specified), and the end of the payload of the corresponding IdentifiedMediaDataBox.
4. in all other cases, the extent\_length is assumed to be the length of the referenced file between the offset (if specified) or the origin (if not specified) and the end of the file.
5. when the construction\_method==1 (offsets into the ItemDataBox), the length of the extent is assumed to be the length of the data between the offset (if specified) or the origin (if not specified) and the end of the payload of the ItemDataBox;
6. when construction\_method==2 (offsets into another item), the length of the extent is assumed to be the size of the item minus the offset (if specified)

If only one extent is used (extent\_count = 1) then either or both of the offset and length may be implied, i.e. by setting offset\_size or length\_size to 0.

References into the same file as this structure-data, or items divided into more than one extent, should have an explicit offset and length, or use a MIME type requiring a different interpretation of the file, to avoid infinite recursion.

Some referenced data may itself use offset/length techniques to address resources within it (e.g. an MP4 file might be ‘included’ in this way). Normally such offsets in the item itself are relative to the beginning of the containing file. The field ‘base offset’ provides an additional offset for offset calculations within that contained data. For example, if an MP4 file is included within a file formatted to this document, then normally data-offsets within that MP4 section are relative to the beginning of file; the base offset adds to those offsets.

If an item is constructed from other items, and those source items are protected, the offset and length information apply to the source items after they have been de-protected. That is, the target item data is formed from unprotected source data.

For maximum compatibility, version 0 of this box should be used in preference to version 1 with construction\_method==0, or version 2 when possible. Similarly, version 2 of this box should only be used when support for large item\_ID values (exceeding 65535) is required or expected to be required.

NOTE 4 When construction\_method 2 is used and one item needs to have an offset of 0 into another item, the base\_offset field is set to 0.

* + - 1. Syntax

aligned(8) class ItemLocationBox extends FullBox('iloc', version, 0)   
{  
 unsigned int(4) offset\_size;  
 unsigned int(4) length\_size;  
 unsigned int(4) base\_offset\_size;  
 if ((version == 1) || (version == 2)) {  
 unsigned int(4) index\_size;  
 } else {  
 unsigned int(4) reserved;  
 }  
 if (version < 2) {  
 unsigned int(16) item\_count;  
 } else if (version == 2) {  
 unsigned int(32) item\_count;  
 }  
 for (i=0; i<item\_count; i++) {  
 if (version < 2) {  
 unsigned int(16) item\_ID;  
 } else if (version == 2) {  
 unsigned int(32) item\_ID;  
 }  
 if ((version == 1) || (version == 2)) {  
 unsigned int(12) reserved = 0;  
 unsigned int(4) construction\_method;  
 }  
 unsigned int(16) data\_reference\_index;  
 unsigned int(base\_offset\_size\*8) base\_offset;  
 unsigned int(16) extent\_count;  
 for (j=0; j<extent\_count; j++) {  
 if (((version == 1) || (version == 2)) && (index\_size > 0)) {  
 unsigned int(index\_size\*8) item\_reference\_index;  
 }  
 unsigned int(offset\_size\*8) extent\_offset;  
 unsigned int(length\_size\*8) extent\_length;  
 }  
 }  
}

* + - 1. Semantics

offset\_size is taken from the set {0, 4, 8} and indicates the length in bytes of the offset field.

length\_size is taken from the set {0, 4, 8} and indicates the length in bytes of the length field.

base\_offset\_size is taken from the set {0, 4, 8} and indicates the length in bytes of the base\_offset field.

index\_size is taken from the set {0, 4, 8} and indicates the length in bytes of the item\_reference\_index field.

item\_count counts the number of resources in the following array.

item\_ID is an arbitrary integer ‘name’ for this resource which can be used to refer to it (e.g. in a URL).

construction\_method is taken from the set 0 (file), 1 (idat) or 2 (item)

data\_reference\_index is either zero ('this file') or an index, with value 1 indicating the first entry, into the data references in the DataInformationBox.

base\_offset provides a base value for offset calculations within the referenced data. If base\_offset\_size is 0, base\_offset takes the value 0, i.e. it is unused.

extent\_count provides the count of the number of extents into which the resource is fragmented; it shall have the value 1 or greater

item\_reference\_index provides an index as defined for the construction method

extent\_offset provides the absolute offset, in bytes from the data origin of the container, of this extent data. If offset\_size is 0, extent\_offset takes the value 0

extent\_length provides the absolute length in bytes of this metadata item extent. If length\_size is 0, extent\_length takes the value 0.

### Primary item box

* + - 1. Definition

Box Type: 'pitm'  
Container: MetaBox  
Mandatory: No  
Quantity: Zero or one

The item data for the primary item may be one of the referenced items when it is desired that it be stored elsewhere, or divided into extents; or the primary metadata may be contained in the MetaBox (e.g. in an XMLBox). Either this box shall occur, or there shall be a box within the MetaBox (e.g. an XMLBox) containing the primary information in the format required by the identified handler.

* + - 1. Syntax

aligned(8) class PrimaryItemBox extends FullBox('pitm', version, 0)   
{  
 if (version == 0) {  
 unsigned int(16) item\_ID;  
 } else {  
 unsigned int(32) item\_ID;  
 }  
}

* + - 1. Semantics

item\_ID is the identifier of the primary item, which shall be the identifier of an item in the MetaBox containing the PrimaryItemBox. Version 1 should only be used when large item\_ID values (exceeding 65535) are required or expected to be required.

### Item protection box

* + - 1. Definition

Box Type: 'ipro'  
Container: MetaBox  
Mandatory: No  
Quantity: Zero or one

The ItemProtectionBox provides an array of item protection information, for use by the ItemInfoBox.

The ProtectionSchemeInfoBoxes shall not contain an OriginalFormatBox when present in an ItemProtectionBox.

* + - 1. Syntax

aligned(8) class ItemProtectionBox  
 extends FullBox('ipro', version = 0, 0)   
{  
 unsigned int(16) protection\_count;  
 for (i=1; i<=protection\_count; i++) {  
 ProtectionSchemeInfoBox protection\_information;  
 }  
}

### Item information box

* + - 1. Definition

Box Type: 'iinf'  
Container: MetaBox  
Mandatory: No  
Quantity: Zero or one

The ItemInfoBox provides extra information about selected items, including symbolic ('file') names. It may optionally occur, but if it does, it shall be interpreted, as item protection or content encoding may have changed the format of the data in the item. If both content encoding and protection are indicated for an item, a reader should first un-protect the item, and then decode the item’s content encoding. If more control is needed, an IPMP sequence code may be used.

This box contains an array of entries, and each entry is formatted as a box. This array is sorted by increasing item\_ID in the entry records. The item\_name shall be a valid URL (e.g. a simple name, or path name) and shall not be an absolute URL.

Four versions of the item info entry are defined. Version 1 includes additional information to version 0 as specified by an extension type. For instance, it shall be used with extension type 'fdel' for items that are referenced by the FilePartitionBox, which is defined for source file partitionings and applies to file delivery transmissions. Versions 2 and 3 provide an alternative structure in which metadata item types are indicated by a 32-bit registered or defined code (typically a four character code); two of these codes are defined to indicate a MIME type or metadata typed by a URI. Version 2 supports 16-bit item\_ID values, whereas version 3 supports 32-bit item\_ID values.

If no extension is desired, the box may terminate without the extension\_type field and the extension; if, in addition, content\_encoding is not desired, that field also may be absent and the box terminate before it. If an extension is desired without an explicit content\_encoding, a single null byte, signifying the empty string, shall be supplied for the content\_encoding, before the indication of extension\_type.

If file delivery item information is needed and a version 2 or 3 ItemInfoEntry is used, then the file delivery information is stored as a separate item of type 'fdel' that is also linked by an item reference from the item, to the file delivery information, of type 'fdel'. There shall be exactly one such reference if file delivery information is needed.

It is possible that there are valid URI forms for MPEG-7 metadata as defined in ISO/IEC 15938-1 (e.g. a schema URI with a fragment identifying a particular element), and it may be possible that these structures can be used for MPEG-7. However, there is explicit support for MPEG-7 in ISO base media files, and this explicit support is preferred as it allows, among other things:

a) incremental update of the metadata (logically, I/P coding, in video terms) whereas this draft is ‘I-frame only’;

b) binarization and thus compaction;

c) the use of multiple schemas.

Therefore, the use of these structures for MPEG-7 is deprecated (and undocumented).

Information on URI forms for some metadata systems can be found in Annex G.

Version 1 of ItemInfoBox should only be used when support for a large number of itemInfoEntries (exceeding 65535) is required or expected to be required.

The flags field of ItemInfoEntry with version greater than or equal to 2 is specified as follows:

* (flags & 1) equal to 1 indicates that the item is not intended to be a part of the presentation. .
* (flags & 1) equal to 0 indicates that the item is intended to be a part of the presentation.
  + - 1. Syntax

aligned(8) class ItemInfoExtension(unsigned int(32) extension\_type)  
{  
}

aligned(8) class FDItemInfoExtension() extends ItemInfoExtension ('fdel') {  
 utf8string content\_location;  
 utf8string content\_MD5;  
 unsigned int(64) content\_length;  
 unsigned int(64) transfer\_length;  
 unsigned int(8) entry\_count;  
 for (i=1; i <= entry\_count; i++)  
 unsigned int(32) group\_id;  
}

aligned(8) class ItemInfoEntry extends FullBox('infe', version, flags)   
{  
 if ((version == 0) || (version == 1)) {  
 unsigned int(16) item\_ID;  
 unsigned int(16) item\_protection\_index;  
 utf8string item\_name;  
 utf8string content\_type;  
 utf8string content\_encoding; //optional  
 }  
 if (version == 1) {  
 unsigned int(32) extension\_type; //optional  
 ItemInfoExtension(extension\_type); //optional  
 }  
 if (version >= 2) {  
 if (version == 2) {  
 unsigned int(16) item\_ID;  
 } else if (version == 3) {  
 unsigned int(32) item\_ID;  
 }  
 unsigned int(16) item\_protection\_index;  
 unsigned int(32) item\_type;  
 utf8string item\_name;  
 if (item\_type=='mime') {  
 utf8string content\_type;  
 utf8string content\_encoding; //optional  
 } else if (item\_type == 'uri ') {  
 utf8string item\_uri\_type;  
 }  
 }  
}

aligned(8) class ItemInfoBox extends FullBox('iinf', version, 0)   
{  
 if (version == 0) {  
 unsigned int(16) entry\_count;  
 } else {  
 unsigned int(32) entry\_count;  
 }  
 ItemInfoEntry item\_infos[ entry\_count ];  
}

* + - 1. Semantics

item\_ID contains either 0 for the primary resource (e.g. the XML contained in an XMLBox) or the ID of the item for which the following information is defined.

item\_protection\_index contains either 0 for an unprotected item, or the index, with value 1 indicating the first entry, into the ItemProtectionBox defining the protection applied to this item (the first box in the ItemProtectionBox has the index 1).

item\_name is the symbolic name of the item (source file for file delivery transmissions).

item\_type is a 32-bit value, typically 4 printable characters, that is a defined valid item type indicator, such as 'mime'

content\_type is the MIME type of the item. If the item is content encoded (see below), then the content type refers to the item after content decoding.

item\_uri\_type is an absolute URI, that is used as a type indicator.

content\_encoding optionally indicates that the binary file is encoded and needs to be decoded before interpreted. The values are as defined for Content-Encoding for HTTP/1.1. Some possible values are “gzip”, “compress” and “deflate”. An empty string indicates no content encoding. Note that the item is stored after the content encoding has been applied.

extension\_type is a four character code that identifies the extension fields of version 1 with respect to version 0 of the Item information entry.

content\_location contains the URI of the file as defined in HTTP/1.1 (IETF RFC 2616[13]).

content\_MD5 contains an MD5 digest of the file. See HTTP/1.1 (IETF RFC 2616[13]) and IETF RFC 1864[12].

content\_length gives the total length (in bytes) of the (un-encoded) file.

transfer\_length gives the total length (in bytes) of the (encoded) file. Transfer length is equal to content length if no content encoding is applied (see above).

entry\_count provides a count of the number of entries in the following array.

group\_ID indicates a file group to which the file item (source file) belongs. See 3GPP TS 26.346[29] for more details on file groups.

### Additional metadata container box

This box has been deprecated and is no longer defined in this document.

### Metabox Relation box

This box has been deprecated and is no longer defined in this document.

### URL forms for MetaBoxes

When a MetaBox is used, then URLs may be used to refer to items in the MetaBox, either using an absolute URL, or using a relative URL.

When interpreting data that is in the context of a MetaBox, the items in the MetaBox are treated as *shadowing* files in the same location as that from which file containing the MetaBox (the 'container file') came, i.e. the contents of the item is the same as the file located at the URL obtained by resolving an absolute URL from the absolute container file URL used as base URL and from the item\_name (if not empty) used as relative URL. This shadowing means that a reference to another *file* in the same location as the container file may be resolved to an *item* within the container file itself.

Items can be addressed within the container file by appending a fragment to the URL for the container file itself as specified in Annex C.

Consider the following example:

<http://a.com/d/v.qrv#item\_name=tree.html\*branch1>.

We assume that v.qrv is a file with a MetaBox at the file level. First, the client strips the fragment and fetches v.qrv from a.com using HTTP. It then inspects the top-level MetaBox and adds the items in it, logically, to its cache of the directory “d” on a.com. It then re-forms the URL as <http://a.com/d/tree.html#branch1>. See that the fragment has been elevated to a full file name, and the first “\*” has been transformed back into a “#”. The client then either finds an item named tree.html in the MetaBox, or fetches tree.html from a.com, and it then finds the anchor “branch1” within tree.html. If within that html, a file was referenced using a relative URL, e.g. “flower.gif”, then the client converts this to an absolute URL using the normal rules: <http://a.com/d/flower.gif> and again it checks to see if flower.gif is a named item (and hence shadowing a separate file of this name), and then if it is not, fetches flower.gif from a.com.

### Static metadata

#### General

This subclause defines the storage of static (un-timed) metadata in ISO base media files.

Reader support for metadata in general is optional, and therefore it is also optional for the formats defined here or elsewhere, unless made mandatory by a derived specification.

#### Simple textual

There is existing support for simple textual tags in the form of the user-data boxes; currently only one is defined – the copyright notice. Other metadata is permitted using this simple form if:

1. it uses a registered box-type or it uses the UUID escape (the latter is permitted today);
2. it uses a registered tag, the equivalent MPEG-7 construct must be documented as part of the registration.

#### Other forms

When other forms of metadata are desired, then a MetaBox as defined above may be included at the appropriate level of the document. If the document is intended to be primarily a metadata document per se, then the MetaBox is at file level. If the metadata annotates an entire presentation, then the MetaBox is at the movie level; an entire stream, at the track level.

#### MPEG-7 metadata

When MPEG-7 metadata as defined in ISO/IEC 15938-1 is stored in MetaBoxes the requirements of this clause apply.

* 1. When the handler-type is 'mp7t' the metadata shall be in textual form, shall conform to ISO/IEC 15938-1, and shall use the encoding defined in ISO/IEC 10646 (technically identical to the Unicode standard[27]).
  2. When the handler-type is 'mp7b' the metadata shall be in binary form compressed in the BIM format as specified in ISO/IEC 23001-1. In this case, the BinaryXMLBox contains the configuration information immediately followed by the binarized XML.
  3. When the format is textual, there shall be either another box in the MetaBox, called 'xml ', which contains the textual MPEG-7 document, or there shall be a PrimaryItemBox identifying the item containing the MPEG-7 XML.
  4. When the format is binary, there shall be either another box in the MetaBox, called 'bxml', which contains the binary MPEG-7 document, or a PrimaryItemBox identifying the item containing the MPEG-7 binarized XML.
  5. If an MPEG-7 box is used at the file level, then the brand 'mp71' should be a member of the compatible-brands list in the FileTypeBox.

### Item data box

#### Definition

Box Type: 'idat'  
Container: MetaBox  
Mandatory: No  
Quantity: Zero or one

This box contains the data of metadata items that use the construction method indicating that an item’s data extents are stored within this box.

#### Syntax

aligned(8) class ItemDataBox extends Box('idat')   
{  
 bit(8) data[];  
}

#### Semantics

data is the contained metadata

### Item reference box

#### Definition

Box Type: 'iref'  
Container: MetaBox  
Mandatory: No  
Quantity: Zero or one

The ItemReferenceBox allows the linking of one item to others via typed references. All the references for one item of a specific type are collected into a SingleItemTypeReferenceBox, whose type is the reference type, and which has a from\_item\_ID field indicating which item is linked. The items linked to are then represented by an array of to\_item\_IDs; within a given array, a given value shall occur at most once. Other structures in the file formats index through these arrays; index values start at 1.

All these single item type reference boxes are then collected into the ItemReferenceBox. The reference types defined for the track reference box defined in 8.3.3 may be used here if appropriate, or other registered reference types. Version 1 of ItemReferenceBox with SingleItemReferenceBoxLarge should only be used when large from\_item\_ID or to\_item\_ID values (exceeding 65535) are required or expected to be required.

NOTE 1 This design makes it fairly easy to find all the references of a specific type, or from a specific item.

An item reference of type 'font' may be used to indicate that an item uses fonts carried/defined in the referenced item.

NOTE 2 Other structures index through the array of item references and hence position and order of them can be significant.

#### Syntax

aligned(8) class SingleItemTypeReferenceBox(referenceType)   
 extends Box(referenceType)   
{  
 unsigned int(16) from\_item\_ID;  
 unsigned int(16) reference\_count;  
 for (j=0; j<reference\_count; j++) {  
 unsigned int(16) to\_item\_ID;  
 }  
}

aligned(8) class SingleItemTypeReferenceBoxLarge(referenceType)   
 extends Box(referenceType)   
{  
 unsigned int(32) from\_item\_ID;  
 unsigned int(16) reference\_count;  
 for (j=0; j<reference\_count; j++) {  
 unsigned int(32) to\_item\_ID;  
 }  
}

aligned(8) class ItemReferenceBox extends FullBox('iref', version, 0)   
{  
 if (version==0) {  
 SingleItemTypeReferenceBox references[];  
 } else if (version==1) {  
 SingleItemTypeReferenceBoxLarge references[];  
 }  
}

#### Semantics

referenceType contains an indication of the type of the reference

from\_item\_ID contains the item\_ID of the item that refers to other items

reference\_count is the number of references

to\_item\_ID contains the item\_ID of the item referred to

### Auxiliary video metadata

An auxiliary video track used for depth or parallax information may carry a metadata item of type 'auvd' (auxiliary video descriptor); the data of that item shall be exactly one si\_rbsp() as specified in ISO/IEC 23001-14, *Information technology — MPEG systems technologies — Part 14: Partial file format*

ISO/IEC 23002-3. (Note that si\_rbsp() is externally framed, and the length is supplied by the item location information in the file format). There may be more than one of these metadata items (e.g. one for parallax info and one for depth, in the case that the same stream serves).

### Item properties box

#### Definition

Box Type: 'iprp'  
Container: MetaBox  
Mandatory: No  
Quantity: Zero or one

The ItemPropertiesBox enables the association of any item with an ordered set of item properties. Item properties are small data records.

The ItemPropertiesBox consists of two parts: ItemPropertyContainerBox that contains an implicitly indexed list of item properties, and one or more ItemPropertyAssociationBox(es) that associate items with item properties.

Each item property is a Box or FullBox. The boxtype of the item property specifies the property type. The FreeSpaceBox may occur in the ItemPropertyContainerBox; it has no meaning, and should not be associated with any item.

NOTE Item Properties are based on the box format documented in 4.2 which means that boxes with an extended\_type and the type field set to 'uuid' are permissible as item properties.

Each property association may be marked as either essential or non-essential. A reader shall not process an item that is associated with a property that is not recognized or not supported by the reader and that is marked as essential to the item. A reader may ignore an associated item property that is marked non-essential to the item.

Specifications deriving from this document may specify property types and the respective item property box definitions as well as constraints and requirements for the property associations.

When defining item properties, it is recommended that they be small. When large data records need to be associated with an item, a separate item and item reference are more suitable.

Each ItemPropertyAssociationBox shall be ordered by increasing item\_ID, and there shall be at most one occurrence of a given item\_ID, in the set of ItemPropertyAssociationBox boxes. The version 0 should be used unless 32-bit item\_ID values are needed; similarly, flags should be equal to 0 unless there are more than 127 properties in the ItemPropertyContainerBox. There shall be at most one ItemPropertyAssociationBox with a given pair of values of version and flags.

#### Syntax

aligned(8) class ItemProperty(property\_type) extends Box(property\_type)  
{  
}

aligned(8) class ItemFullProperty(property\_type, version, flags)  
 extends FullBox(property\_type, version, flags)  
{  
}

aligned(8) class ItemPropertyContainerBox extends Box('ipco')  
{  
 Box properties[]; // boxes derived from  
 // ItemProperty or ItemFullProperty, or FreeSpaceBox(es)  
 // to fill the box  
}

aligned(8) class ItemPropertyAssociationBox  
 extends FullBox('ipma', version, flags)  
{  
 unsigned int(32) entry\_count;  
 for (i = 0; i < entry\_count; i++) {  
 if (version < 1)  
 unsigned int(16) item\_ID;  
 else  
 unsigned int(32) item\_ID;  
 unsigned int(8) association\_count;  
 for (j=0; j<association\_count; j++) {  
 bit(1) essential;  
 if (flags & 1)  
 unsigned int(15) property\_index;  
 else  
 unsigned int(7) property\_index;  
 }  
 }  
}

aligned(8) class ItemPropertiesBox extends Box('iprp')   
{  
 ItemPropertyContainerBox property\_container;  
 ItemPropertyAssociationBox association[];  
}

#### Semantics

item\_ID identifies the item with which properties are associated

essential when set to 1 indicates that the associated property is essential to the item, otherwise it is non-essential

property\_index is either 0 indicating that no property is associated (the essential indicator shall also be 0), or is the 1-based index (counting all boxes, including FreeSpace boxes) of the associated property box in the ItemPropertyContainerBox contained in the same ItemPropertiesBox. property\_index shall not be greater than the number of boxes contained in the associated ItemPropertyContainerBox.

### Brand item property

#### Definition

Box Type: 'brnd'  
Property Type: Descriptive item property  
Container: ItemPropertyContainerBox  
Mandatory (per an item): No  
Quantity (per an item): Zero or one

The payload of BrandProperty has the syntax of the GeneralTypeBox.

The content of an instance of BrandProperty shall be such that it applies as the content of FileTypeBox, when the following modifications are made to the file:

* All tracks of the file are removed.
* All items except the following are removed:
  + The item associated with this BrandProperty, referred to as currItem.
  + The items, referred to as referencedItemsList, that currItem directly or indirectly references to, as indicated in the ItemReferenceBox.
* When the current primary item is not a member of the set including currItem and referencedItems, currItem is set to be the primary item in the PrimaryItemBox.

#### Syntax

aligned(8) class BrandProperty extends GeneralTypeBox ('brnd')   
{  
}

**8.11.16 Handler property**

**8.11.16.1 Definition**

Box Type: 'hdlp'  
Property Type: Descriptive item property  
Container: ItemPropertyContainerBox  
Mandatory: No  
Quantity: zero or more

HandlerProperty provides a mapping of a media handler with an item in a MetaBox. Items that are alternatives of each other shall have the same handler property, or none.

NOTE Items that are alternatives of each other are included in the same 'altr' entity group. One example of two items being alternatives of each other is two coded image items, as defined in ISO/IEC 23008-12, that represent the same original image but are coded with different codecs or have different spatial resolution. When the HandlerBox of the MetaBox containing these two coded image items has a handler type different from 'pict' defined in ISO/IEC 23008-12, both of these coded image items can be associated with the same HandlerProperty having handler\_type equal to 'pict'.

**8.11.16.2 Syntax**

aligned(8) class HandlerProperty   
 extends ItemFullProperty('hdlp', version = 0, flags = 0)   
{  
 unsigned int(32) handler\_type;  
}

**8.11.16.3 Semantics**

handler\_type is a four-character-code which corresponds to a media handler type. When the HandlerProperty is associated with the primary item, handler\_type of the HandlerProperty shall be equal to the handler\_type of the MetaBox. When no specific handler type needs to be signalled for an item, the HandlerProperty for the item may be absent or the handler\_type may be 'null'.

## Void

## File delivery format support

### Overview

Files intended for transmission over ALC/LCT or FLUTE are stored as items in a top-level MetaBox. The ItemLocationBox specifies the actual storage location of each item within the container file as well as the file size of each item. File name, content type (MIME type), etc., of each item are provided by version 1 of the ItemInfoBox.

Pre-computed FEC reservoirs are stored as additional items in the MetaBox. If a source file is split into several source blocks, FEC reservoirs for each source block are stored as separate items. The relationship between FEC reservoirs and original source items is recorded in the PartitionEntry located in the FDItemInformationBox.

Pre-composed File reservoirs are stored as additional items in the container file. If a source file is split into several source blocks, each source block is stored as a separate item called a file reservoir. The relationship between File reservoirs and original source items is recorded in the PartitionEntry located in the FDItemInformationBox.

See subclause 9.2 for more details on the usage of the file delivery format.

### FD item information box

* + - 1. Definition

Box Type: 'fiin'  
Container: MetaBox  
Mandatory: No  
Quantity: Zero or one

The FDItemInformationBox is optional, although it is mandatory for files using FD hint tracks. It provides information on the partitioning of source files and how FD hint tracks are combined into FD sessions. Each partition entry provides details on a particular file partitioning, FEC encoding and associated File and FEC reservoirs. It is possible to provide multiple entries for one source file (identified by its item\_ID) if alternative FEC encoding schemes or partitionings are used in the file. All partition entries are implicitly numbered and the first entry has number 1.

* + - 1. Syntax

aligned(8) class PartitionEntry() extends Box('paen')   
{  
 FilePartitionBox blocks\_and\_symbols;  
 FECReservoirBox FEC\_symbol\_locations; //optional  
 FileReservoirBox File\_symbol\_locations; //optional  
}

aligned(8) class FDItemInformationBox  
 extends FullBox('fiin', version = 0, 0)   
{  
 unsigned int(16) entry\_count;  
 PartitionEntry partition\_entries[ entry\_count ];  
 FDSessionGroupBox session\_info; //optional  
 GroupIdToNameBox group\_id\_to\_name; //optional  
}

* + - 1. Semantics

entry\_count provides a count of the number of entries in the following array.

The semantics of the boxes are described where the boxes are documented.

### File partition box

* + - 1. Definition

Box Type: 'fpar'  
Container: PartitionEntry  
Mandatory: Yes  
Quantity: Exactly one

The FilePartitionBox identifies the source file and provides a partitioning of that file into source blocks and symbols. Further information about the source file, e.g. filename, content location and group IDs, is contained in the ItemInfoBox, where the ItemInfoEntry corresponding to the item\_ID of the source file is of version 1 and includes a FDItemInfoExtension. Version 1 of FilePartitionBox should only be used when support for large item\_ID or entry\_count values (exceeding 65535) is required or expected to be required.

* + - 1. Syntax

aligned(8) class FilePartitionBox extends FullBox('fpar', version, 0)   
{  
 if (version == 0) {  
 unsigned int(16) item\_ID;  
 } else {  
 unsigned int(32) item\_ID;  
 }  
 unsigned int(16) packet\_payload\_size;  
 unsigned int(8) reserved = 0;  
 unsigned int(8) FEC\_encoding\_ID;  
 unsigned int(16) FEC\_instance\_ID;  
 unsigned int(16) max\_source\_block\_length;  
 unsigned int(16) encoding\_symbol\_length;  
 unsigned int(16) max\_number\_of\_encoding\_symbols;  
 base64string scheme\_specific\_info;  
 if (version == 0) {  
 unsigned int(16) entry\_count;  
 } else {  
 unsigned int(32) entry\_count;  
 }  
 for (i=1; i <= entry\_count; i++) {  
 unsigned int(16) block\_count;  
 unsigned int(32) block\_size;  
 }  
}

* + - 1. Semantics

item\_ID references the item in the ItemLocationBox that the file partitioning applies to.

packet\_payload\_size gives the target ALC/LCT or FLUTE packet payload size of the partitioning algorithm. Note that UDP packet payloads are larger, as they also contain ALC/LCT or FLUTE headers.

FEC\_encoding\_ID shall identify the FEC encoding scheme using a "Reliable Multicast Transport (RMT) FEC Encoding ID" declared at IANA, as defined in IETF RFC 5052. Note that i) value zero corresponds to the "Compact No-Code FEC scheme" also known as "Null-FEC" (IETF RFC 3695[17]); ii) value one corresponds to the “MBMS FEC” (3GPP TS 26.346[29]); iii) for values in the range of 0 to 127, inclusive, the FEC scheme is Fully-Specified, whereas for values in the range of 128 to 255, inclusive, the FEC scheme is Under-Specified.

FEC\_instance\_ID shall provide a more specific identification of the FEC encoder being used for an Under-Specified FEC scheme. This value should be set to zero for Fully-Specified FEC schemes and shall be ignored when parsing a file with FEC\_encoding\_ID in the range of 0 to 127, inclusive. FEC\_instance\_ID is scoped by the FEC\_encoding\_ID. See IETF RFC 5052 for further details.

max\_source\_block\_length gives the maximum number of source symbols per source block.

encoding\_symbol\_length gives the size (in bytes) of one encoding symbol. All encoding symbols of one item have the same length, except the last symbol which may be shorter.

max\_number\_of\_encoding\_symbols gives the maximum number of encoding symbols that can be generated for a source block for those FEC schemes in which the maximum number of encoding symbols is relevant, such as FEC encoding ID 129 defined in IETF RFC 5052. For those FEC schemes in which the maximum number of encoding symbols is not relevant, the semantics of this field is unspecified.

scheme\_specific\_info is the scheme-specific object transfer information (FEC-OTI-Scheme-Specific-Info). The definition of the information depends on the FEC encoding ID.

entry\_count gives the number of entries in the list of (block\_count, block\_size) pairs that provides a partitioning of the source file. Starting from the beginning of the file, each entry indicates how the next segment of the file is divided into source blocks and source symbols.

block\_count indicates the number of consecutive source blocks of size block\_size.

block\_size indicates the size of a block (in bytes). A block\_size that is not a multiple of the encoding\_symbol\_length symbol size indicates with Compact No-Code FEC that the last source symbols includes padding that is not stored in the item. With MBMS FEC (3GPP TS 26.346[29]) the padding may extend across multiple symbols but the size of padding should never be more than encoding\_symbol\_length.

### FEC reservoir box

* + - 1. Definition

Box Type: 'fecr'  
Container: PartitionEntry  
Mandatory: No  
Quantity: Zero or One

The FECReservoirBox associates the source file identified in the FilePartitionBox with FEC reservoirs stored as additional items. It contains a list that starts with the first FEC reservoir associated with the first source block of the source file and continues sequentially through the source blocks of the source file. Version 1 of FECReservoirBox should only be used when support for large item\_ID values and entry\_count (exceeding 65535) is required or expected to be required.

* + - 1. Syntax

aligned(8) class FECReservoirBox extends FullBox('fecr', version, 0)   
{  
 if (version == 0) {  
 unsigned int(16) entry\_count;  
 } else {  
 unsigned int(32) entry\_count;  
 }  
 for (i=1; i <= entry\_count; i++) {  
 if (version == 0) {  
 unsigned int(16) item\_ID;  
 } else {  
 unsigned int(32) item\_ID;  
 }  
 unsigned int(32) symbol\_count;  
 }  
}

* + - 1. Semantics

entry\_count gives the number of entries in the following list. An entry count here should match the total number of blocks in the corresponding FilePartitionBox.

item\_ID indicates the location of the FEC reservoir associated with a source block.

symbol\_count indicates the number of repair symbols contained in the FEC reservoir.

### FD session group box

* + - 1. Definition

Box Type: 'segr'  
Container: FDItemInformationBox  
Mandatory: No  
Quantity: Zero or One

The FDSessionGroupBox is optional, although it is mandatory for files containing more than one FD hint track. It contains a list of sessions as well as all file groups and hint tracks that belong to each session. An FD session sends simultaneously over all FD hint tracks (channels) that are listed in the FD session group box for a particular FD session.

Only one session group should be processed at any time. The first listed hint track in a session group specifies the base channel. If the server has no preference between the session groups, the default choice should be the first session group. The group IDs of all file groups containing the files referenced by the hint tracks shall be included in the list of file groups. The file group IDs can in turn be translated into file group names (using the group ID to name box) that can be included by the server in FDTs.

* + - 1. Syntax

aligned(8) class FDSessionGroupBox extends Box('segr')   
{  
 unsigned int(16) num\_session\_groups;  
 for (i=0; i < num\_session\_groups; i++) {  
 unsigned int(8) entry\_count;  
 for (j=0; j < entry\_count; j++) {  
 unsigned int(32) group\_ID;  
 }  
 unsigned int(16) num\_channels\_in\_session\_group;  
 for (k=0; k < num\_channels\_in\_session\_group; k++) {  
 unsigned int(32) hint\_track\_ID;  
 }  
 }  
}

* + - 1. Semantics

num\_session\_groups specifies the number of session groups.

entry\_count gives the number of entries in the following list comprising all file groups that the session group complies with. The session group contains all files included in the listed file groups as specified by the item information entry of each source file. The FDT for the session group should only contain those groups that are listed in this structure.

group\_ID indicates a file group that the session group complies with.

num\_channels\_in\_session\_groups specifies the number of channels in the session group. The value of num\_channels\_in\_session\_groups shall be a positive integer.

hint\_track\_ID specifies the track identifier of the FD hint track belonging to a particular session group. Note that one FD hint track corresponds to one LCT channel.

### Group ID to name box

* + - 1. Definition

Box Type: 'gitn'  
Container: FDItemInformationBox  
Mandatory: No  
Quantity: Zero or One

The GroupIdToNameBox associates file group names to file group IDs used in the version 1 item information entries in the ItemInfoBox.

* + - 1. Syntax

aligned(8) class GroupIdToNameBox extends FullBox('gitn', version = 0, 0)  
{  
 unsigned int(16) entry\_count;  
 for (i=1; i <= entry\_count; i++) {  
 unsigned int(32) group\_ID;  
 utf8string group\_name;  
 }  
}

* + - 1. Semantics

entry\_count gives the number of entries in the following list.

group\_ID indicates a file group.

group\_name is the file group name.

### File reservoir box

#### Definition

Box Type: 'fire'  
Container: PartitionEntry  
Mandatory: No  
Quantity: Zero or One

The FileReservoirBox associates the source file identified in the FilePartitionBox with File reservoirs stored as additional items. It contains a list that starts with the first File reservoir associated with the first source block of the source file and continues sequentially through the source blocks of the source file. Version 1 of FileReservoirBox should only be used when support for large item\_ID or entry\_count values (exceeding 65535) is required or expected to be required.

#### Syntax

aligned(8) class FileReservoirBox extends FullBox('fire', version, 0)   
{  
 if (version == 0) {  
 unsigned int(16) entry\_count;  
 } else {  
 unsigned int(32) entry\_count;  
 }  
 for (i=1; i <= entry\_count; i++) {  
 if (version == 0) {  
 unsigned int(16) item\_ID;  
 } else {  
 unsigned int(32) item\_ID;  
 }  
 unsigned int(32) symbol\_count;  
 }  
}

#### Semantics

entry\_count gives the number of entries in the following list. An entry count here should match the total number or blocks in the corresponding FilePartitionBox.

item\_ID indicates the location of the File reservoir associated with a source block.

symbol\_count indicates the number of source symbols contained in the file reservoir.

## Sub tracks

### Overview

Sub tracks are used to assign parts of tracks to alternate and switch groups in the same way as (entire) tracks can be assigned to alternate and switch groups to indicate whether those tracks are alternatives to each other and whether it makes sense to switch between them during a session. Sub tracks are suitable for layered media (e.g. SVC and MVC), where media alternatives often are incommensurate with track structures. By defining alternate and switch groups at sub-track level it is possible to use existing rules for media selection and switching for such layered codecs. The over-all syntax is generic for all kinds of media and backward compatible with track-level definitions. Sub-track level alternate and switch groups use the same numbering as track level groups. The numberings are global over all tracks such that groups can be defined across track and sub-track boundaries.

In order to define sub tracks, media-specific definitions are required. Definitions for SVC and MVC are specified in the AVC file format (ISO/IEC 14496-15[3]). Another way is to define sample groups and map them to sub tracks using the SubTrackSampleGroupBox defined here. The syntax can also be extended to include other media-specific definitions.

For each sub track that shall be defined a SubTrackBox shall be included in the UserDataBox of the corresponding track. The SubTrackBox contains objects that define and provide information about a sub track in the same track. The TrackSelectionBox for this same track is already located here.

### Backward compatibility

The default is to assign alternate and switch groups to 0 (zero) for (entire) tracks, which means that there is no information on alternate and/or switch groups for those (entire) tracks. However, file readers that are aware of sub-track definitions will be able to find sub-track information on alternate and switch groups even if the track indication is set to 0. This way it is possible to indicate that a file can be used by legacy readers by including the appropriate brand in the FileTypeBox. A file creator that requires a reader to be aware of sub-track information should not include legacy brands.

The same method of assigning sub track information can also be applied if all parts of a track except a sub track belong to the same alternate or switch group. Then the overall definitions can be made on track level as usual and specific assignments can be made at sub-track level. For sub tracks without specific assignments, track level assignments apply by default. As before, if a file creator requires a reader to be aware of sub-track information it should not include legacy brands (that do not require sub track support and hence indicate that sub track information can be skipped).

### Sub track box

#### Definition

Box Type: 'strk'  
Container: UserDataBox of the corresponding TrackBox  
Mandatory: No  
Quantity: Zero or more

This box contains objects that define and provide information about a sub track in the present track.

#### Syntax

aligned(8) class SubTrackBox extends Box('strk')   
{  
}

### Sub track information box

#### Definition

Box Type: 'stri'  
Container: SubTrackBox  
Mandatory: Yes  
Quantity: One

#### Syntax

aligned(8) class SubTrackInformationBox  
 extends FullBox('stri', version = 0, 0)  
{  
 template int(16) switch\_group = 0;  
 template int(16) alternate\_group = 0;  
 template unsigned int(32) sub\_track\_ID = 0;  
 unsigned int(32) attribute\_list[]; // to the end of the box  
}

#### Semantics

switch\_group is an integer that specifies a group or collection of tracks and/or sub tracks. If this field is 0 (default value), then there is no information on whether the sub track can be used for switching during playing or streaming. If this integer is not 0 it shall be the same for tracks and/or sub tracks that can be used for switching between each other. Tracks that belong to the same switch group shall belong to the same alternate group. A switch group may have only one member.

alternate\_group is an integer that specifies a group or collection of tracks and/or sub tracks. If this field is 0 (default value), then there is no information on possible relations to other tracks/sub-tracks. If this field is not 0, it should be the same for tracks/sub-tracks that contain alternate data for one another and different for tracks/sub-tracks belonging to different such groups. Only one track/sub-track within an alternate group should be played or streamed at any one time.

sub\_track\_ID is an integer. A non-zero value uniquely identifies the sub track locally within the track. A zero value (default) means that sub\_track\_ID is not assigned.

attribute\_list is a list, to the end of the box, of attributes. The attributes in this list should be used as descriptions of sub tracks or differentiating criteria for tracks and sub tracks in the same alternate or switch group.

The following attributes are descriptive:

|  |  |  |
| --- | --- | --- |
| *Name* | *Attribute* | *Description* |
| Temporal scalability | 'tesc' | The sub-track can be temporally scaled. |
| Fine-grain SNR scalability | 'fgsc' | The sub-track can be scaled in terms of quality. |
| Coarse-grain SNR scalability | 'cgsc' | The sub-track can be scaled in terms of quality. |
| Spatial scalability | 'spsc' | The sub-track can be spatially scaled. |
| Region-of-interest scalability | 'resc' | The sub-track can be region-of-interest scaled. |
| View scalability | 'vwsc' | The sub-track can be scaled in terms of number of views. |

The following attributes are differentiating:

|  |  |  |
| --- | --- | --- |
| *Name* | *Attribute* | *Pointer* |
| Bitrate | 'bitr' | Total size of the samples in the sub track divided by the duration in the TrackHeaderBox |
| Frame rate | 'frar' | Number of samples in the sub track divided by duration in the TrackHeaderBox |
| Number of views | 'nvws' | Number of views in the sub track |

### Sub track definition box

#### Definition

Box Type: 'strd'  
Container: SubTrackBox  
Mandatory: Yes  
Quantity: One

This box contains objects that provide a definition of the sub track.

#### Syntax

aligned(8) class SubTrackDefinitionBox extends Box('strd')   
{  
}

### Sub track sample group box

#### Definition

Box Type: 'stsg'  
Container: SubTrackDefinitionBox  
Mandatory: No  
Quantity: Zero or more

This box defines a sub track as one or more sample groups by referring to the corresponding sample group descriptions describing the samples of each group.

#### Syntax

aligned(8) class SubTrackSampleGroupBox extends FullBox('stsg', 0, 0)  
{  
 unsigned int(32) grouping\_type;  
 unsigned int(16) item\_count;  
 for (i = 0; i< item\_count; i++) {  
 unsigned int(32) group\_description\_index;  
 }  
}

#### Semantics

grouping\_type is an integer that identifies the sample grouping. The value shall be the same as in the corresponding SampleToGroupBox and SampleGroupDescriptionBox.

item\_count counts the number of sample groups listed in this box.

group\_description\_index is an integer that gives the index of the sample group description entry which describes the samples in the group.

## Void

## Segments

### Overview

Media presentations may be divided into segments for delivery. For example, it is possible (e.g. in HTTP streaming) to form files that contain a segment – or concatenated segments – which do not necessarily form ISO base media file format compliant files (e.g. they do not contain a movie box).

When the MIME form registered in Annex F is used, it shall refer to a segment as defined here.

### Segment type box

#### Definition

Box Type: 'styp'  
Container: File  
Mandatory: No  
Quantity: Zero or more

If segments are stored in separate files (e.g. on a standard HTTP server) it is recommended that these ‘segment files’ contain a segment-type box, which shall be first if present, to enable identification of those files, and declaration of the specifications with which they are compliant.

A SegmentTypeBox has the same format as a FileTypeBox (see subclause 4.2.3), except that it takes the box type 'styp'. The brands within it may include the same brands that were included in the FileTypeBox that preceded the MovieBox, and may also include additional brands to indicate the compatibility of this segment with various specification(s).

Valid segment type boxes shall be the first box in a segment. Segment type boxes may be removed if segments are concatenated (e.g. to form a full file), but this is not required. Segment type boxes that are not first in their files may be ignored.

#### Syntax

aligned(8) class SegmentTypeBox extends GeneralTypeBox ('styp')  
{  
}

### Segment index box

#### Definition

Box Type: 'sidx'  
Container: File  
Mandatory: No  
Quantity: Zero or more

The SegmentIndexBox provides a compact index of one media stream within the media segment to which it applies. It is designed so that it can be used not only with media formats based on this document (i.e. segments containing sample tables or movie fragments), but also other media formats (for example, MPEG-2 transport streams in ISO/IEC 13818-1[1]). For this reason, the formal description of the box given here is deliberately generic (e.g. it uses the term “access unit”), and then at the end of this subclause the specific definitions for segments using movie fragments are given.

Each SegmentIndexBox documents how a (sub)segment is divided into one or more subsegments (which may themselves be further subdivided using SegmentIndexBoxes).

A subsegment is defined as a time interval of the containing (sub)segment, and corresponds to a single range of bytes of the containing (sub)segment. The durations of all the subsegments sum to the duration of the containing (sub)segment.

Each entry in the SegmentIndexBox contains a reference type that indicates whether the reference points directly to the media bytes of a referenced leaf subsegment, or to a SegmentIndexBox that describes how the referenced subsegment is further subdivided; as a result, the segment may be indexed in a ‘hierarchical’ or ‘daisy-chain’ or other form by documenting time and byte offset information for other SegmentIndexBoxes applying to portions of the same (sub)segment.

Each SegmentIndexBox provides information about a single media stream of the Segment, referred to as the reference stream. If provided, the first SegmentIndexBox in a segment, for a given media stream, shall document the entirety of that media stream in the segment, and shall precede any other SegmentIndexBox in the segment for the same media stream.

If a segment index is present for at least one media stream but not all media streams in the segment, then normally a media stream in which not every access unit is independently coded, such as video, is selected to be indexed. For any media stream for which no segment index is present, referred to as non-indexed stream, the media stream associated with the first SegmentIndexBox in the segment serves as a reference stream in a sense that it also describes the subsegments for any non-indexed media stream.

NOTE 1 Further restrictions can be specified in derived specifications.

SegmentIndexBoxes may be inline in the same file as the indexed media or, in some cases, in a separate file containing only indexing information.

A SegmentIndexBox contains a sequence of references to subsegments of the (sub)segment documented by the box. The referenced subsegments are contiguous in presentation time. Similarly, the bytes referred to by a SegmentIndexBox are always contiguous in both the media file, and the separate index segment, or in the single file if indexes are placed within the media file. The referenced size gives the count of the number of bytes in the material referenced.

NOTE 2 A media segment can be indexed by more than one “top-level” SegmentIndexBox that are independent of each other, each of which indexes one media stream within the media segment. In segments containing multiple media streams the referenced bytes can contain media from multiple streams, even though the SegmentIndexBox provides timing information for only one media stream.

In the file containing the SegmentIndexBox, the anchor point for a SegmentIndexBox is the first byte after that box. If there are two files, the anchor point in the media file is the beginning of the top-level segment (i.e. the beginning of the segment file if each segment is stored in a separate file). The material in the file containing media (which may also be the file that contains the SegmentIndexBoxes) starts at the indicated offset from the anchor point. If there are two files, the material in the index file starts at the anchor point, i.e. immediately following the SegmentIndexBox.

Within the two constraints (a) that, in time, the subsegments are contiguous, that is, each entry in the loop is consecutive from the immediately preceding one and (b) within a given file (integrated file, media file, or separate file containing only index information) the referenced bytes are contiguous, there are a number of possibilities, including:

1. a reference to a SegmentIndexBox may include, in its byte count, immediately following SegmentIndexBoxes that document subsegments;
2. in an integrated file, using the first\_offset field, it is possible to separate SegmentIndexBoxes from the media that they refer to;
3. in an integrated file, it is possible to locate SegmentIndexBoxes for subsegments close to the media they index;
4. when a separate file containing SegmentIndexBoxes is used, it is possible for the loop entries to have different reference\_type values, some to SegmentIndexBoxes in the index segment, some to media subsegments in the media file.

NOTE 3 Profiles can be used to restrict the placement of segment indexes, or the overall complexity of the indexing.

The SegmentIndexBox documents the presence of stream access points (SAPs), as specified in Annex I, in the referenced subsegments. The annex specifies characteristics of SAPs, such as ISAU, ISAP and TSAP, as well as SAP types, which are all used in the semantics below. A subsegment starts with a SAP when the subsegment contains a SAP, and for the first SAP, ISAU is the index of the first access unit that follows ISAP, and ISAP is contained in the subsegment.

For segments based on this document (i.e. based on movie sample tables or movie fragments):

* an access unit is a sample;
* a subsegment is a self-contained set of one or more consecutive movie fragments; a self-contained set contains one or more MovieFragmentBoxes with the corresponding MediaDataBox(es), and a MediaDataBox containing data referenced by a MovieFragmentBox shall follow that MovieFragmentBox and precede the next MovieFragmentBox containing information about the same track;
* Segment index boxes shall be placed before subsegment material they document, that is, before any MovieFragmentBox of the documented material of the subsegment;
* streams are tracks in the file format, and stream IDs are track\_IDs;
* a subsegment contains a stream access point if a track fragment within the subsegment for the track with track\_ID equal to reference\_ID contains a stream access point;
* initialisation data for SAPs consists of the movie box;
* presentation times are in the presentation timeline, that is they are composition times after the application of any edit list for the track;
* the ISAP is a position exactly pointing to the start of a top-level box, such as a movie fragment box 'moof';
* a SAP of type 1 or type 2 is indicated as a sync sample, or by sample\_is\_non\_sync\_sample equal to 0 in the movie fragment;
* a SAP of type 3 is marked as a member of a sample group of type 'rap ';
* a SAP of type 4 is marked as a member of a sample group of type 'roll' where the value of the roll\_distance field is greater than 0.

NOTE 4 For SAPs of type 5 and 6, no specific signalling in the ISO base media file format is supported.

Examples of the use of segment indexes can be found in Annex J.

#### Syntax

aligned(8) class SegmentIndexBox extends FullBox('sidx', version, 0)   
{  
 unsigned int(32) reference\_ID;  
 unsigned int(32) timescale;  
 if (version==0) {  
 unsigned int(32) earliest\_presentation\_time;  
 unsigned int(32) first\_offset;  
 }  
 else {  
 unsigned int(64) earliest\_presentation\_time;  
 unsigned int(64) first\_offset;  
 }  
 unsigned int(16) reserved = 0;  
 unsigned int(16) reference\_count;  
 for (i=1; i <= reference\_count; i++)  
 {  
 bit (1) reference\_type;  
 unsigned int(31) referenced\_size;  
 unsigned int(32) subsegment\_duration;  
 bit(1) starts\_with\_SAP;  
 unsigned int(3) SAP\_type;  
 unsigned int(28) SAP\_delta\_time;  
 }  
}

#### Semantics

reference\_ID provides the stream ID for the reference stream; if this SegmentIndexBox is referenced from a “parent” SegmentIndexBox, the value of reference\_ID shall be the same as the value of reference\_ID of the “parent” SegmentIndexBox;

timescale provides the timescale, in ticks per second, for the time and duration fields within this box; it is recommended that this match the timescale of the reference stream or track; for files based on this document, that is the timescale field of the media header box of the track;

earliest\_presentation\_time is the earliest presentation time of any content in the reference stream in the first subsegment, in the timescale indicated in the timescale field; the earliest presentation time is derived from media in access units, or parts of access units, that are not omitted by an edit list (if any);

first\_offset is the distance in bytes, in the file containing media, from the anchor point, to the first byte of the indexed material;

reference\_count provides the number of referenced items;

reference\_type: when set to 1 indicates that the reference is to a SegmentIndexBox; otherwise the reference is to media content (e.g. in the case of files based on this document, to a MovieFragmentBox); if a separate index segment is used, then entries with reference type 1 are in the index segment, and entries with reference type 0 are in the media file;

referenced\_size: the distance in bytes from the first byte of the referenced item to the first byte of the next referenced item, or in the case of the last entry, the end of the referenced material;

subsegment\_duration: when the reference is to SegmentIndexBox, this field carries the sum of the subsegment\_duration fields in that box; when the reference is to a subsegment, this field carries the difference between the earliest presentation time of any access unit of the reference stream in the next subsegment (or the first subsegment of the next segment, if this is the last subsegment of the segment, or the end presentation time of the reference stream if this is the last subsegment of the stream) and the earliest presentation time of any access unit of the reference stream in the referenced subsegment; the duration is in the same units as earliest\_presentation\_time;

starts\_with\_SAP indicates whether the referenced subsegments start with a SAP. For the detailed semantics of this field in combination with other fields, see Table 7.

SAP\_type indicates a SAP type as specified in Annex I, or the value 0. Other type values are reserved. For the detailed semantics of this field in combination with other fields, see the table below.

SAP\_delta\_time: indicates TSAP of the first SAP, in decoding order, in the referenced subsegment for the reference stream. If the referenced subsegments do not contain a SAP, SAP\_delta\_time is reserved with the value 0; otherwise SAP\_delta\_time is the difference between the earliest presentation time of the subsegment, and the TSAP (this difference may be zero, in the case that the subsegment starts with a SAP).

Table 7 — Semantics of SAP and reference type combinations

|  |  |  |  |
| --- | --- | --- | --- |
| starts\_with\_SAP | SAP\_type | reference\_type | Meaning |
| 0 | 0 | 0 or 1 | No information of SAPs is provided. |
| 0 | 1 to 6, inclusive | 0 (media) | The subsegment contains (but may not start with) a SAP of the given SAP\_type and the first SAP of the given SAP\_type corresponds to SAP\_delta\_time. |
| 0 | 1 to 6, inclusive | 1 (index) | All the referenced subsegments contain a SAP of at most the given SAP\_type and none of these SAPs is of an unknown type. |
| 1 | 0 | 0 (media) | The subsegment starts with a SAP of an unknown type. |
| 1 | 0 | 1 (index) | All the referenced subsegments start with a SAP which may be of an unknown type |
| 1 | 1 to 6, inclusive | 0 (media) | The referenced subsegment starts with a SAP of the given SAP\_type. |
| 1 | 1 to 6, inclusive | 1 (index) | All the referenced subsegments start with a SAP of at most the given SAP\_type and none of these SAPs is of an unknown type. |

### Subsegment index box

#### Definition

Box Type: 'ssix'  
Container: File  
Mandatory: No  
Quantity: Zero or more

The SubsegmentIndexBox provides a mapping from levels (as specified by the LevelAssignmentBox) to byte ranges of the indexed subsegment. In other words, this box provides a compact index for how the data in a subsegment is ordered according to levels into partial subsegments. It enables a client to easily access data for partial subsegments by downloading ranges of data in the subsegment.

Each byte in the subsegment shall be explicitly assigned to a level, and hence the range count shall be 2 or greater. If the range is not associated with any information in the level assignment, then any level that is not included in the level assignment may be used.

There shall be 0 or 1 SubsegmentIndexBoxes per each SegmentIndexBox that indexes only leaf subsegments, i.e. that only indexes subsegments but no segment indexes. A SubsegmentIndexBox, if any, shall be the next box after the associated SegmentIndexBox. A SubsegmentIndexBox documents the subsegments that are indicated in the immediately preceding SegmentIndexBox.

In general, the media data constructed from the byte ranges is incomplete, i.e. it does not conform to the media format of the entire subsegment.

For leaf subsegments based on this document (i.e. based on movie sample tables and movie fragments):

* Each level shall be assigned to exactly one partial subsegment, i.e. byte ranges for one level shall be contiguous.
* Levels of partial subsegments shall be assigned by increasing numbers within a subsegment, i.e., samples of a partial subsegment may depend on any samples of preceding partial subsegments in the same subsegment, but not the other way around. For example, each partial subsegment contains samples having an identical temporal level and partial subsegments appear in increasing temporal level order within the subsegment.
* When a partial subsegment is accessed in this way, for any assignment\_type other than 3, the final MediaDataBox may be incomplete, that is, less data is accessed than the length indication of the MediaDataBox indicates is present. The length of the MediaDataBox may need adjusting, or padding used. The padding\_flag in the LevelAssignmentBox indicates whether this missing data can be replaced by zeros. If not, the sample data for samples assigned to levels that are not accessed is not present, and care should be taken not to attempt to process such samples.
* The data ranges corresponding to partial subsegments include both MovieFragmentBoxes and MediaDataBoxes. The first partial subsegment, i.e. the lowest level, will correspond to a MovieFragmentBox as well as (parts of) MediaDataBox(es), whereas subsequent partial subsegments (higher levels) may correspond to (parts of) MediaDataBox(es) only.

NOTE assignment\_type equal to 0 (specified in the LevelAssignmentBox) can be used, for example, together with the temporal level sample grouping ('tele') when frames of a video bitstream are temporally ordered within subsegments; assignment\_type equal to 2 can be used, for example, when each view of a multiview video bitstream is contained in a separate track and the track fragments for all the views are contained in a single movie fragment. assignment\_type equal to 3 can be used, for example, when audio and video movie fragments (including the respective MediaDataBoxes) are interleaved. The first level can be specified to contain the audio movie fragments (including the respective MediaDataBoxes), whereas the second level can be specified to contain both audio and video movie fragments (including all MediaDataBoxes).

#### Syntax

aligned(8) class SubsegmentIndexBox extends FullBox('ssix', 0, 0)   
{  
 unsigned int(32) subsegment\_count;  
 for (i=1; i <= subsegment\_count; i++)  
 {  
 unsigned int(32) range\_count;  
 for (j=1; j <= range\_count; j++) {  
 unsigned int(8) level;  
 unsigned int(24) range\_size;  
 }  
 }  
}

#### Semantics

subsegment\_count is a positive integer specifying the number of subsegments for which partial subsegment information is specified in this box. subsegment\_count shall be equal to reference\_count (i.e., the number of movie fragment references) in the immediately preceding SegmentIndexBox.

range\_count specifies the number of partial subsegment levels into which the media data is grouped. This value shall be greater than or equal to 2.

range\_size indicates the size of the partial subsegment; the value 0 may be used in the last entry to indicate the remaining bytes of the segment, to the end of the segment.

level specifies the level to which this partial subsegment is assigned.

### Producer reference time box

#### Definition

Box Type: 'prft'  
Container: File  
Mandatory: No  
Quantity: Zero or more

The ProducerReferenceTimeBox supplies times corresponding to the production of associated movie fragments. When they are both produced and consumed in real time, this can provide clients with information to enable consumption and production to proceed at equivalent rates, thus avoiding possible buffer overflow or underflow.

This box is related to the next MovieFragmentBox that follows it in bitstream order. It shall follow any SegmentTypeBox or SegmentIndexBox (if any) in the segment, and occur before the following MovieFragmentBox (to which it refers).

The box contains a time value, expressed using the NTP format, and measured on a clock which increments at the same rate as a UTC-synchronized NTP clock as defined in IETF RFC 5905. This time is associated with a media time in the range of media times for one of the tracks in the movie fragment. Note that the media time does not need to match the actual decode or composition timestamp of a sample of that track.

Given a succession of ProducerReferenceTimeBoxes in the same track with the same flag values (notably the value 8, which promises consistency), a receiver can estimate the drift between the producer's media clock and real time; the accuracy and variability of this estimation can depend on the technique used to establish the times, as reported in the flag values.

For live-captured media, flags may be set to 24 (i.e. the two bits corresponding to value 8 and 16 are set). When the flags have this value, the UTC time shall be at, or close to, the wall-clock-time of the experience captured in the media. For example, if the media is a video that shows an accurate public clock timed to UTC that displays 09:15, then the UTC time in this box also reads close to 09:15. The receiver can then estimate the real-time latency of presentation, from the time the captured experience occurred, to the time it is presented to the user.

Producer reference times should be associated with at most one track.

#### Syntax

aligned(8) class ProducerReferenceTimeBox  
 extends FullBox('prft', version, flags)   
{  
 unsigned int(32) reference\_track\_ID;  
 unsigned int(64) ntp\_timestamp;  
 if (version==0) {  
 unsigned int(32) media\_time;  
 } else {  
 unsigned int(64) media\_time;  
 }  
}

#### Semantics

reference\_track\_ID provides the track\_ID for the reference track.

ntp\_timestamp indicates a UTC time in NTP format associated to media\_time as follows:

* if flags is set to 0, the UTC time is the time at which the frame belonging to the reference track in the following movie fragment and whose presentation time is media\_time was input to the encoder.
* if flags is set to 1, the UTC time is the time at which the frame belonging to the reference track in the following movie fragment and whose presentation time is media\_time was output from the encoder.
* if flags is set to 2, the UTC time is the time at which the following MovieFragmentBox was finalized. media\_time is set to the presentation of the earliest frame of the reference track in presentation order of the movie fragment.
* if flags is set to 4, the UTC time is the time at which the following MovieFragmentBox was written to file. media\_time is set to the presentation of the earliest frame of the reference track in presentation order of the movie fragment.
* if flags is set to 8, the association between the media\_time and UTC time is arbitrary but consistent between multiple occurrences of this box in the same track
* if flags is set to 24 (i.e. the two bits corresponding to value 8 and 16 are set), the UTC time has a consistent, small (ideally zero), offset from the real-time of the experience depicted in the media at media\_time

media\_time is expressed in the time units used for the reference track.

NOTE In most cases this time will not be equal to the time of the first sample of the adjacent segment of the reference track.

## Void

## Entity grouping

### General

An entity group is a grouping of items, which may also group tracks. The entities in an entity group share a particular characteristic or have a particular relationship, as indicated by the grouping type.

Entity groups are indicated in GroupsListBox. Entity groups specified in GroupsListBox of a file-level MetaBox refer to tracks or file-level items. Entity groups specified in GroupsListBox of a movie-level MetaBox refer to movie-level items. Entity groups specified in GroupsListBox of a track-level MetaBox refer to track-level items of that track.

GroupsListBox contains EntityToGroupBoxes, each specifying one entity group.

### Groups list box

#### Definition

Box Type: 'grpl'  
Container: MetaBox   
Mandatory: No  
Quantity: Zero or One

The GroupsListBox includes the entity groups specified for the file. This box contains a set of full boxes, each called an EntityToGroupBox, with four-character codes denoting a defined grouping type.

When GroupsListBox is present in a file-level MetaBox, there shall be no item\_ID value in ItemInfoBox in any file-level MetaBox that is equal to the track\_ID value in any TrackHeaderBox.

#### Syntax

aligned(8) class GroupsListBox extends Box('grpl')   
{  
}

### Entity to group box

#### Definition

Box Type: As specified below with the grouping\_type value for the EntityToGroupBox  
Container: GroupsListBox  
Mandatory: No  
Quantity: One or more

The EntityToGroupBox specifies an entity group.

The box type (grouping\_type) indicates the grouping type of the entity group. Each grouping\_type code is associated with semantics that describe the grouping. The following grouping\_type values are specified in this document:

'altr': The items and tracks mapped to this grouping are alternatives to each other, and only one of them should be played (when the mapped items and tracks are part of the presentation; e.g. are displayable items or tracks) or processed by other means (when the mapped items or tracks are not part of the presentation; e.g. are metadata). A player should select the first entity from the list of entity\_id values that it can process (e.g. decode and play for mapped items and tracks that are part of the presentation) and that suits the application needs. Any entity\_id value shall be mapped to only one grouping of type 'altr'. An alternate group of entities consists of those items and tracks that are mapped to the same entity group of type 'altr'.

'prsl': The tracks mapped to this grouping are belonging to a preselection as specified in 8.18.4.1.

NOTE EntityToGroupBox can have grouping\_type specific extensions.

#### Syntax

aligned(8) class EntityToGroupBox(grouping\_type, version, flags)  
 extends FullBox(grouping\_type, version, flags)   
{  
 unsigned int(32) group\_id;  
 unsigned int(32) num\_entities\_in\_group;  
 for (i=0; i<num\_entities\_in\_group; i++) {  
 unsigned int(32) entity\_id;  
 }  
 // the remaining data may be specified for a particular grouping\_type  
}

#### Semantics

version shall be 0 unless defined otherwise for the grouping\_type. Any values of flags such that (flags & 0x000FFF) is not equal to 0 are reserved. The values of flags shall be such that (flags & 0xFFF000) is equal to 0 unless defined otherwise for the grouping\_type.

group\_id is a non-negative integer assigned to the particular grouping that shall not be equal to any group\_id value of any other EntityToGroupBox, any item\_ID value of the hierarchy level (file, movie. or track) that contains the GroupsListBox, or any track\_ID value (when the GroupsListBox is contained in the file level).

num\_entities\_in\_group specifies the number of entity\_id values mapped to this entity group.

entity\_id is resolved to one of the following:

* an item, when an item with item\_ID equal to entity\_id is present in the hierarchy level (file, movie or track) that contains the GroupsListBox, or
* a track, when a track with track\_ID equal to entity\_id is present and the GroupsListBox is contained in the file level, or
* a track group, if the unified handling of identifiers is indicated with a brand as specified in Clause E.18, this EntityToGroupBox is present at file level, and a track group with track\_group\_id equal to entity\_id present, or
* a second entity group, if the unified handling of identifiers is indicated with a brand as specified in Clause E.18, this EntityToGroupBox is present at the same level that contains the EntityToGroupBox for the second entity group, and the EntityToGroupBox for the second entity group has group\_id equal to entity\_id.

### Entity group definitions

#### Preselection group box

##### Definition

Box Type: 'prsl'  
Container: GroupsListBox in a MetaBox on movie level  
Mandatory: No  
Quantity: Zero or more

[Ed.Note] The uniqueness of identifiers is specified within the file, movie, or track level but not across levels in subclause E.18. However, the uniqueness of identifiers on movie level is specified only on item\_ID and group\_id, but E.18 does not mention track\_ID and track\_group\_id for movie level uniqueness. Consequently, if the PreselectionGroupBox is contained in the movie-level MetaBox, it cannot refer to tracks. Two potential approaches to resolve this are: 1) Move the preselection entity group to file level; 2) Extend the scope of uniqueness at movie level. National bodies are encouraged to comment on this.

A preselection is represented by a PreselectionGroupBox. This box contains information on what experience is available when this preselection is selected. The characteristics of the preselection are given by the boxes contained in the PreselectionGroupBox. Preselections can be characterized, for example, by language, kind or media specific attributes like audio rendering indications, audio interactivity or channel layouts. Charcteristics signalled in a PreselectionGroupBox take precedence over characteristics signalled in contributing entities.

NOTE 1 The kind box might utilize the Role scheme defined in ISO/IEC 23009-1:2022, subclause 5.8.5.5 as it provides a commonly used scheme to describe characteristics of preselections.

NOTE 2 Optional boxes contained within this box can carry information about the initial experience of the preselection in the referenced tracks. The preselection experience can change during the playback of these tracks, e.g. audio language can change during playback. These changes are not subject to the information presented in this box.

The MetaBox containing the preselection entity group may have any handler\_type value, such as 'null' in its HandlerBox, when present, or exclude the HandlerBox, when allowed by the indicated brand(s).

A preselection may group multiple tracks. In some cases, for those tracks to be consumed by a single decoder, these tracks need to be processed to produce a single track. This processing can be dependent on a specific order. The order is given by the order of appearance in the entity\_id loop in the syntax.

The exact processing to produce the single track is signalled by the interleaving\_tag. If the interleaving\_tag starts with a 4CC of a sample entry, the document that specifies the 4CC shall define the exact processing to generate the resulting track.

EXAMPLE: If the interleaving\_tag is set to 'mhm2' the specific processing for this preselection is defined in ISO/IEC 23008-3:2019, subclause 14.

When the PreselectionGroupBox is used, the requirements from the 'unif' brand apply. Consequently, the entity\_id value may be equal to the group\_id of a different EntityToGroupBox. This allows nesting of entity groups. Circular references shall be avoided.

Each entity\_id value of a preselection shall either be equal to a track\_ID or to a group\_id of another EntityToGroupBox. This requirement shall also be fulfilled for every (directly or indirectly) referenced EntityToGroupBox. Consequently, a preselection always resolves to a (ordered) set of tracks.

##### Syntax

aligned(8) class PreselectionGroupBox  
 extends EntityToGroupBox('prsl', version=0, flags)  
{  
 if (flags & preselection\_tag\_present)  
 utf8string preselection\_tag;  
 if (flags & selection\_priority\_present)  
 unsigned int(8) selection\_priority;  
 utf8string interleaving\_tag;   
 Box boxes[]; // Boxes describing the preselection  
}

##### Semantics

flags is a 24-bit integer with flags; the following values are defined:

preselection\_tag\_present: Flag mask is 0x001000. The value 1 indicates the presence of the preselection\_tag element

selection\_priority\_present: Flag mask is 0x002000. The value 1 indicates the presence of the selection\_priority element

preselection\_tag is a codec specific value that a playback system can provide to a decoder to uniquely identify one out of several preselections in the media.

selection\_priority is an integer that declares the priority of the preselection in cases where no other differentiation such as through the media language is possible. A lower value of selection\_priority indicates a higher priority.

interleaving\_tag provides the interleaving processes to be used for interleaving samples or groups of samples of the entities belonging to this preselections. If the interleaving\_tag is empty, no process is specified for this preselection.

boxes is an array of boxes describing the preselection. Boxes suitable to describe a preselection include but are not limited to the following list of boxes defined in this document:

* + ExtendedLanguageBox (subclause 8.4.6)
  + UserDataBox (subclause 8.10.1)
  + KindBox (subclause 8.10.4)
  + LabelBox (subclause 8.10.5)
  + ChannelLayout (subclause 12.2.4)
  + AudioRenderingIndicationBox (subclause 12.2.8)
  + AudioElementBox (subclause 12.2.9)
  + AudioElementSelectionBox (subclause 12.2.13)

When contained in a PreselectionGroupBox, a UserDataBox shall not carry any of the above boxes. Further media type specific boxes may be used to describe properties of the preselection. Readers may ignore and skip boxes that are not recognized.

## Compressed boxes

### Overview and processing

A compressed box is a box that replaces another box, called original box, at the same top-level order in the file but whose payload is the BoxPayload of that original box, compressed with deflate(), as defined in IETF RFC 1951. A compressed box can only be defined for a top-level box; hence their container is always the file and is omitted in their box definitions. Only a subset of existing top-level boxes can be compressed.

The type of the box that a compressed box replaces is called the replacement type and is defined for each compressed box. The content that is compressed comprises all the remaining bytes after the BoxHeader of the original box.

Unless stated otherwise, the semantics of fields in the uncompressed payload is the same as the semantics of the box with the given replacement type. Especially, when boxes use file offsets within the containing file, unless stated otherwise these offsets are related to the file that results from expanding the compressed box(es).

All compressed boxes defined in this document share the same syntax as defined in subclause 8.19.3.

The MovieFragmentRandomAccessBox is not supported in files containing compressed boxes and shall not be present when a compressed box is present.

A reader that supports compressed boxes shall be capable of decompressing boxes and adjusting offsets in a way that is functionally equivalent to the processing model in subclause 8.19.2.2.

### Processing model

#### File parsing processing model

The processing model when reading compressed boxes is defined as follows:

* the BoxPayload of the compressed box (after the compressed box’s BoxHeader structure) is decompressed (Note that a FullBox also has a BoxPayload)
* the box type of the compressed box is replaced with the replacement type as specified for this particular compressed box
* the compressed box size is replaced with the sum of the uncompressed payload size and the BoxHeader size (8 bytes, in the case of a simple 32-bit size)
* the compressed box payload is replaced with the uncompressed payload
* the uncompressed box is read from the reconstructed BoxHeader and uncompressed payload
* the parsing is then resumed at the position of the end of the compressed box in the file.

#### File decompression processing model

The processing model when decompressing a file is defined as follows: the decompressed file is initialized as empty, and for each top-level box in the compressed file:

* if there is an OriginalFileTypeBox, then the FileTypeBox or SegmentTypeBox, and a following ExtendedTypeBox (if any), are replaced by the contents of the OriginalFileTypeBox;
* otherwise, if the box is uncompressed, it is copied to the decompressed file.
* otherwise, the decompressed box is computed as indicated in subclause 8.19.2.1; the decompressed box is written to the decompressed file as follows:
  + if the decompressed box is a MovieBox or MovieFragmentBox, the decompressed box is copied without modifications to the decompressed file.
  + if the decompressed box is a SegmentIndexBox
    - the first\_offset field is incremented by the number of extra bytes in the decompressed data between the beginning of the SegmentIndexBox and the indicated first\_offset in the compressed file, compared to the number of compressed bytes in that range; (this necessarily includes the expansion of the SegmentIndexBox itself); this step is needed when SegmentIndexBox(es) and SubSegmentIndexBox(es) are present between the end of an SegmentIndexBox and the first movie fragment following this SegmentIndexBox.
    - Each reference\_size field in the decompressed SegmentIndexBox is increased by the number of uncompressed bytes minus the number of compressed bytes of all top-level compressed boxes present in the corresponding range in the compressed file. (In general it is not possible to update a SegmentIndexBox immediately on reception, as the first\_offset and reference\_size are updated based on decompression of boxes later in the file.)
    - The modified uncompressed box is then copied to the decompressed file.
  + if the decompressed box is a SubsegmentIndexBox, each range\_size field in the uncompressed box is increased by the number of uncompressed bytes minus the number of compressed bytes of all top-level compressed boxes starting in the corresponding range in the compressed file. The modified uncompressed box is then copied to the decompressed file.

NOTE 1 There is no guarantee that the number of compressed bytes is less than the number of uncompressed bytes, although it is better that file writers avoid using a compressed box if it is larger than the uncompressed version. In the above processing model, this means that the number of bytes to add might be negative.

NOTE 2 In this processing mode, a file decompressor might need to load top-level boxes following the box currently being decompressed (e.g. SegmentIndexBox or SubsegmentIndexBox) to compute the byte difference between compressed and uncompressed versions of subsequent boxes referred to by the box currently being decompressed.

NOTE 3 Since, unless specified otherwise, byte offsets in compressed boxes describe the uncompressed domain file, a file reader processing a compressed file on-the-fly (without producing a complete uncompressed file) will need to maintain some correspondence table between byte offsets in the compressed domain and byte offsets in the uncompressed domain in order to correctly adjust file offsets when fetching data from the file. File offsets can only be interpreted once the reader is sure that all data preceding that file offset has been decompressed. This can be achieved by either (1) loading all that data and decompressing it or (2) knowing that the only boxes that precede the given offset, that are permitted to be compressed, have been decompressed. For example, in many cases a file is only permitted to contain only a single MovieBox, a MovieFragmentBox or a MetaBox and no other compressible box. Derived specification can further restrict the possible set and layout of compressed boxes to simplify this process.

NOTE 4 This is a processing model that describes the correspondence between a file containing compressed boxes and a hypothetical file containing uncompressed boxes; readers implement decompression as suits their processing needs. In particular, if SegmentIndexBoxes are used to guide what data to fetch and then not used further, it might not be necessary to recalculate the offsets and sizes that they contain.

### General syntax

aligned(8) class CompressedBox(box\_type, replacement\_type)  
 extends Box(box\_type)   
{  
 bit(8) compressed\_data[]; // to end of box  
}

### General semantics

compressed\_data is the compressed payload of a box defined by the replacement\_type type. This data contains the compressed box payload excluding the BoxHeader field of the uncompressed box.

replacement\_type indicates the corresponding uncompressed box type.

### Original file-type box

#### Definition

Box Type: 'otyp'  
Container: File or OriginalFileTypeBox  
Mandatory: Yes (see below)  
Quantity: Zero or more

A file conformant to this document may have further transformation of its box structure, for example it may use compressed top-level boxes. In this case, the resulting file may no longer be compliant with the brand promises of the original file, as it requires the support for new tools (such as compressed top-level boxes). For example, a file using a compressed MovieBox is no longer compliant to any brand defined prior to the introduction of compressed boxes.

The OriginalFileTypeBox is used to encapsulate brand information applying to the original file before transformation but not valid in the transformed domain. There shall be at most one OriginalFileTypeBox after each FileTypeBox or SegmentTypeBox. An OriginalFileTypeBox shall contain the FileTypeBox and, when present, the ExtendedTypeBox, of the file before transformation. In cases where a file uses multiple transformations, nested OriginalFileTypeBox shall be used, and there shall be at most one OriginalFileTypeBox in each OriginalFileTypeBox.

When present, an OriginalFileTypeBox shall follow a FileTypeBox or SegmentTypeBox, with at most an ExtendedTypeBox and/or FreeSpaceBox(es) in between.

The processing model for a file reader is equivalent to removing both FileTypeBox/SegmentTypeBox and OriginalFileTypeBox, and inserting in their place the child boxes of the OriginalFileTypeBox. In the case of compressed top-level boxes, the resulting replacement and decompression of the file shall be a compliant uncompressed ISOBMFF file.

#### Syntax

aligned(8) class OriginalFileTypeBox extends Box('otyp')   
{  
}

### Compressed movie box

#### Definition

Box Type: '!mov'  
Replacement Type: 'moov'  
Mandatory: No  
Quantity: Zero or One

A CompressedMovieBox contains a compressed version of a MovieBox BoxPayload. The replacement type of the CompressedMovieBox for the algorithm specified in subclause 8.19.1 is 'moov'.

There shall not be both a CompressedMovieBox and a MovieBox in a file.

#### Syntax

aligned(8) class CompressedMovieBox extends CompressedBox('!mov', 'moov')  
{  
}

### Compressed movie fragment box

#### Definition

Box Type: '!mof'  
Replacement Type: 'moof'  
Mandatory: No  
Quantity: Zero or One

A CompressedMovieFragmentBox contains a compressed version of a MovieFragmentBox BoxPayload. The replacement type of the CompressedMovieFragmentBox for the algorithm specified in subclause 8.19.1 is 'moof'.

#### Syntax

aligned(8) class CompressedMovieFragmentBox  
 extends CompressedBox('!mof', 'moof')   
{  
}

### Compressed segment index box

#### Definition

Box Type: '!six'  
Replacement Type: 'sidx'  
Mandatory: No  
Quantity: Zero or more

A CompressedSegmentIndexBox contains a compressed version of a SegmentIndexBox BoxPayload. The replacement type of the CompressedSegmentIndexBox for the algorithm specified in subclause 8.19.1 is 'sidx'.

The referenced\_size and first\_offset fields of the uncompressed SegmentIndexBox payload shall be expressed in the compressed domain: they document the size and position of the referenced item in the file, and the referenced items may contain compressed top-level boxes. This ensures that byte-ranges computed from the referenced\_size fields always resolve in one or more top-level boxes of the file, potentially using box compression.

If a physical version of the decompressed file is to be produced for later consumption, the referenced\_size and first\_offset fields in the uncompressed payload may need to be updated according to the new size of the referenced items after decompression.

If the SegmentIndexBox references an external file using box compression the referenced\_size and first\_offset fields shall also be expressed in the compressed domain for the same reason as stated above.

#### Syntax

aligned(8) class CompressedSegmentIndexBox  
 extends CompressedBox('!six', 'sidx')   
{  
}

### Compressed subsegment index box

#### Definition

Box Type: '!ssx'  
Replacement Type: 'ssix'  
Mandatory: No  
Quantity: Zero or more

A CompressedSubsegmentIndexBox contains a compressed version of a SubsegmentIndexBox BoxPayload. The replacement type of the CompressedSubsegmentIndexBox for the algorithm specified in subclause 8.19.1 is 'ssix'.

The range\_size fields of the uncompressed SubsegmentIndexBox payload shall be expressed in the compressed domain: it documents the size of the partial subsegment in the subsegment, potentially containing compressed top-level boxes. This ensures that byte-ranges computed from the range\_size fields always resolve in one or more top-level boxes of the file, potentially using box compression, or in a subset of a MediaDataBox payload.

#### Syntax

aligned(8) class CompressedSubsegmentIndexBox  
 extends CompressedBox('!ssx', 'ssix')   
{  
}

# Hint track formats

## RTP and SRTP hint track format

### Overview

This subclause defines a hint track format for RTP; when processed by a server, the hint track shall yield a stream of RTP packets that conform to IETF RFC 3550[17] and IETF RFC 3551[18].

In standard RTP, each media stream is sent as a separate RTP stream; multiplexing is achieved by using IP’s port-level multiplexing, not by interleaving the data from multiple streams into a single RTP session. However, if MPEG is used, it may be necessary to multiplex several media tracks into one RTP track (e.g. when using MPEG-2 transport in RTP, or FlexMux). Each hint track is therefore tied to a set of media tracks by track references. The hint tracks extract data from their media tracks by indexing through this table. Hint track references to media tracks have the reference type 'hint'.

This design decides the packet size at the time the server hint track is created; therefore, in the declarations for the hint track, we indicate the chosen packet size. This is in the sample-description. Note that it is valid for there to be several RTP hint tracks for each media track, with different packet size choices. Similarly the time-scale for the RTP clock is provided. The timescale of the server hint track is usually chosen to match the timescale of the media tracks, or a suitable value is picked for the server. In some cases, the RTP timescale is different (e.g. 90 kHz for some MPEG payloads), and this permits that variation. Session description (SAP/SDP) information is stored in UserDataBoxes in the track.

RTP hint tracks do not use the CompositionOffsetBox. Instead, the hinting process for server hint tracks establishes the correct transmission order and timestamps, perhaps using the transmission time offset to set transmission times.

Hinted content may require the use of SRTP for streaming by using the hint track format for SRTP, defined here. SRTP hint tracks shall form a stream of packets that shall conform to IETF RFC 3711, and are formatted identically to RTP hint tracks, except that:

1. the sample entry name is changed from 'rtp ' to 'srtp' to indicate to the server that SRTP is required;
2. an extra box is added to the sample entry which can be used to instruct the server in the nature of the on-the-fly encryption and integrity protection that must be applied.

### Sample entry format

#### Structure

RTP server hint tracks are hint tracks (media handler 'hint'), with an entry-format in the sample description of 'rtp ':

class RtpHintSampleEntry() extends HintSampleEntry ('rtp ')   
{  
 uint(16) hinttrackversion = 1;  
 uint(16) highestcompatibleversion = 1;  
 uint(32) maxpacketsize;  
}

The hinttrackversion is currently 1; the highest compatible version field specifies the oldest version with which this track is backward-compatible.

The maxpacketsize indicates the size of the largest packet that this track will generate.

The additional data is a set of boxes, from the following.

class timescaleentry() extends Box('tims')   
{  
 uint(32) timescale;  
}

class timeoffset() extends Box('tsro')   
{  
 int(32) offset;  
}

class sequenceoffset() extends Box('snro')   
{  
 int(32) offset;  
}

The timescale entry is required. The other two are optional. The offsets over-ride the default server behaviour, which is to choose a random offset. A value of 0, therefore, will cause the server to apply no offset to the timestamp or sequence number respectively.

An SRTP Hint Sample entry is used when it is required that SRTP processing is required.

class SrtpHintSampleEntry() extends HintSampleEntry ('srtp')   
{  
 uint(16) hinttrackversion = 1;  
 uint(16) highestcompatibleversion = 1;  
 uint(32) maxpacketsize;  
}

Fields and boxes are defined as for the RtpHintSampleEntry ('rtp ') of the ISO Base Media File Format. However, an SRTPProcessBox shall be included in an SrtpHintSampleEntry as one of the additionaldata boxes.

#### SRTP process box

Box Type: 'srpp'  
Container: SrtpHintSampleEntry  
Mandatory: Yes  
Quantity: Exactly one

The SRTPProcessBox may instruct the server as to which SRTP algorithms should be applied.

aligned(8) class SRTPProcessBox extends FullBox('srpp', version, 0)   
{  
 unsigned int(32) encryption\_algorithm\_rtp;  
 unsigned int(32) encryption\_algorithm\_rtcp;  
 unsigned int(32) integrity\_algorithm\_rtp;  
 unsigned int(32) integrity\_algorithm\_rtcp;  
 SchemeTypeBox scheme\_type\_box;  
 SchemeInformationBox info;  
}

The SchemeTypeBox and SchemeInformationBox have the syntax defined above for protected media tracks. They serve to provide the parameters required for applying SRTP. The SchemeTypeBox is used to indicate the necessary key-management and security policy for the stream in extension to the defined algorithmic pointers provided by the SRTPProcessBox. The key-management functionality is also used to establish all the necessary SRTP parameters as listed in IETF RFC 3711:2004, Section 8.2. The exact definition of protection schemes is out of the scope of the file format.

The algorithms for encryption and integrity protection are defined by SRTP. The following format identifiers are defined here. An entry of four spaces ($20$20$20$20) may be used to indicate that the choice of algorithm for either encryption or integrity protection is decided by a process outside the file format.

|  |  |
| --- | --- |
| Format | Algorithm |
| $20$20$20$20 | The choice of algorithm for either encryption or integrity protection is decided by a process outside the file format |
| ACM1 | Encryption using AES in Counter Mode with 128-bit key, as defined in IETF RFC 3711:2004, Section 4.1.1. |
| AF81 | Encryption using AES in F8-mode with 128-bit key, as defined in IETF RFC 3711:2004, Section 4.1.2. |
| ENUL | Encryption using the NULL-algorithm as defined in IETF RFC 3711:2004, Section 4.1.3. |
| SHM2 | Integrity protection using HMAC-SHA-1 with 160-bit key, as defined in IETF RFC 3711:2004, Section 4.2.1. |
| ANUL | Integrity protection not applied to RTP (but still applied to RTCP). NOTE   This is valid only for integrity\_algorithm\_rtp. |

### Sample format

#### Sample format definition

Each sample in a server hint track will generate one or more RTP packets, whose RTP timestamp is the same as the hint sample time. Therefore, all the packets made by one sample have the same timestamp. However, provision is made to ask the server to ‘warp’ the actual transmission times, for data-rate smoothing, for example.

Each sample contains two areas: the instructions to compose the packets, and any extra data needed when sending those packets (e.g. an encrypted version of the media data). The size of the sample is known from the sample size table.

aligned(8) class RTPsample   
{  
 unsigned int(16) packetcount;  
 unsigned int(16) reserved;  
 RTPpacket packets[packetcount];  
 byte extradata[];  
}

#### Packet entry format

Each packet in the packet entry table has the following structure:

aligned(8) class RTPpacket   
{  
 int(32) relative\_time;  
 // the next fields form initialization for the RTP  
 // header (16 bits), and the bit positions correspond  
 bit(2) RTP\_version;  
 bit(1) P\_bit;  
 bit(1) X\_bit;  
 bit(4) CSRC\_count;  
 bit(1) M\_bit;  
 bit(7) payload\_type;  
 unsigned int(16) RTPsequenceseed;  
 unsigned int(13) reserved = 0;  
 unsigned int(1) extra\_flag;  
 unsigned int(1) bframe\_flag;  
 unsigned int(1) repeat\_flag;  
 unsigned int(16) entrycount;  
 if (extra\_flag) {  
 uint(32) extra\_information\_length;  
 box extra\_data\_tlv[];  
 }  
 dataentry constructors[entrycount];  
}

The semantics of the fields for RTP server hint tracks is specified below. RTP reception hint tracks use the same packet structure. The semantics of the fields when the packet structure is used in an RTP reception hint track is specified in subclause 9.4.1.4.

In server hint tracks, the relative\_time field ‘warps’ the actual transmission time away from the sample time. This allows traffic smoothing.

The following 2 bytes exactly overlay the RTP header; they assist the server in making the RTP header (the server fills in the remaining fields). Within these 2 bytes, the fields RTP\_version and CSRC\_count are reserved in server (transmission) hint tracks and the server fills in these fields.

The sequence seed is the basis for the RTP sequence number. If a hint track causes multiple copies of the same RTP packet to be sent, then the seed value is the same for them all. The server normally adds a random offset to this value (but see above, under 'sequenceoffset').

extra\_flag equal to 1 indicates that there is extra information before the constructors, in the form of type-length-value sets.

extra\_information\_length indicates the length in bytes of all extra information before the constructors, which includes the four bytes of the extra information\_length field. The subsequent boxes before the constructors, referred to as the TLV boxes, are aligned on 32-bit boundaries. The box size of any TLV box indicates the actual bytes used, not the length required for padding to 32-bit boundaries. The value of extra\_information\_length includes the required padding for 32-bit boundaries.

The rtpoffsetTLV ('rtpo') gives a 32-bit signed integer offset to the actual RTP timestamp to place in the packet. This enables packets to be placed in the hint track in decoding order, but have their presentation timestamp in the transmitted packet be in a different order. This is necessary for some MPEG payloads.

The bframe\_flag indicates a disposable ‘b-frame’. The repeat\_flag indicates a ‘repeat packet’, one that is sent as a duplicate of a previous packet. Servers may wish to optimize handling of these packets.

#### Constructor format

There are various forms of the constructor. Each constructor is 16 bytes, to make iteration easier. The first byte is a union discriminator:

aligned(8) class RTPconstructor(type)   
{  
 unsigned int(8) constructor\_type = type;  
}

aligned(8) class RTPnoopconstructor extends RTPconstructor(0)  
{  
 uint(8) pad[15];  
}

aligned(8) class RTPimmediateconstructor extends RTPconstructor(1)  
{  
 unsigned int(8) count;  
 unsigned int(8) data[count];  
 unsigned int(8) pad[14 - count];  
}

aligned(8) class RTPsampleconstructor extends RTPconstructor(2)  
{  
 signed int(8) trackrefindex;  
 unsigned int(16) length;  
 unsigned int(32) samplenumber;  
 unsigned int(32) sampleoffset;  
 unsigned int(16) bytesperblock = 1;  
 unsigned int(16) samplesperblock = 1;  
}

aligned(8) class RTPsampledescriptionconstructor  
 extends RTPconstructor(3)  
{  
 signed int(8) trackrefindex;  
 unsigned int(16) length;  
 unsigned int(32) sampledescriptionindex;  
 unsigned int(32) sampledescriptionoffset;  
 unsigned int(32) reserved;  
}

The immediate mode permits the insertion of payload-specific headers (e.g. the RTP H.261 header). For hint tracks where the media is sent ‘in the clear’, the sample entry then specifies the bytes to copy from the media track, by giving the sample number, data offset, and length to copy. The track reference may index into the table of track references (a strictly positive value), name the hint track itself (-1), or the only associated media track (0). (The value zero is therefore equivalent to the value 1.)

The bytesperblock and samplesperblock concern compressed audio, using a scheme prior to MP4, in which the audio framing was not evident in the file. These fields have the fixed values of 1 for MP4 files.

The sampledescription mode allows sending of sample entries (which contain elementary stream descriptors), by reference, as part of an RTP packet. The index is the index of a SampleEntry in a SampleDescriptionBox, and the offset is relative to the beginning of that SampleEntry.

For complex cases (e.g. encryption or forward error correction), the transformed data is placed into the hint samples, in the extradata field, and then sample mode referencing the hint track itself is used.

Notice that there is no requirement that successive packets transmit successive bytes from the media stream. For example, to conform with RTP-standard packing of H.261, it is sometimes required that a byte be sent at the end of one packet and also at the beginning of the next (when a macroblock boundary falls within a byte).

### SDP information

#### Overview

Streaming servers using RTSP and SDP usually use SDP as the description format; and there are necessary relationships between the SDP information, and the RTP streams, such as the mapping of payload IDs to MIME names. Provision is therefore made for the hinter to leave fragments of SDP information in the file, to assist the server in forming a full SDP description. Note that there are required SDP entries, which the server should also generate. The information here is only partial.

SDP information is formatted as a set of boxes within UserDataBoxes, at both the movie and the track level. The text in the movie-level SDP box should be placed before any media-specific lines (before the first ‘m=’ in the SDP file).

#### Movie SDP information

At the movie level, within the UserDataBox, a hint information container box may occur:

aligned(8) class moviehintinformation extends Box('hnti')   
{  
}

aligned(8) class rtpmoviehintinformation extends Box('rtp ')   
{  
 uint(32) descriptionformat = 'sdp ';  
 char sdptext[];  
}

The moviehintinformation box may contain information for multiple protocols; only RTP is defined here. The RTP box may contain information for various description formats; only SDP is defined here. The sdptext is correctly formatted as a series of lines, each terminated by <crlf>, as required by SDP.

#### Track SDP information

At the track level, the structure is similar; however, we already know that this track is an RTP hint track, from the sample entry. Therefore the child box merely specifies the format.

aligned(8) class trackhintinformation extends Box('hnti')   
{  
}

aligned(8) class rtptracksdphintinformation extends Box('sdp ')   
{  
 char sdptext[];  
}

The sdptext is correctly formatted as a series of lines, each terminated by <crlf>, as required by SDP.

### Statistical information

In addition to the statistics in the hint media header, the hinter may place extra data in a hintstatisticsbox, in the track user-data box. This is a container box with a variety of sub-boxes that it may contain.

aligned(8) class hintstatisticsbox extends Box('hinf')   
{  
}

aligned(8) class hintBytesSent extends Box('trpy') {  
 uint(64) bytessent; } // total bytes sent, including 12-byte RTP headers  
aligned(8) class hintPacketsSent extends Box('nump') {  
 uint(64) packetssent; } // total packets sent  
aligned(8) class hintBytesSent extends Box('tpyl') {  
 uint(64) bytessent; } // total bytes sent, not including RTP headers

aligned(8) class hintBytesSent extends Box('totl') {  
 uint(32) bytessent; } // total bytes sent, including 12-byte RTP headers  
aligned(8) class hintPacketsSent extends Box('npck') {  
 uint(32) packetssent; } // total packets sent  
aligned(8) class hintBytesSent extends Box('tpay') {  
 uint(32) bytessent; } // total bytes sent, not including RTP headers

aligned(8) class hintmaxrate extends Box('maxr') { // maximum data rate  
 uint(32) period; // in milliseconds  
 uint(32) bytes; } // max bytes sent in any period 'period' long  
 // including RTP headers

aligned(8) class hintmediaBytesSent extends Box('dmed') {  
 uint(64) bytessent; } // total bytes sent from media tracks  
aligned(8) class hintimmediateBytesSent extends Box('dimm') {  
 uint(64) bytessent; } // total bytes sent immediate mode  
aligned(8) class hintrepeatedBytesSent extends Box('drep') {  
 uint(64) bytessent; } // total bytes in repeated packets

aligned(8) class hintminrelativetime extends Box('tmin') {  
 int(32) time; } // smallest relative transmission time, milliseconds  
aligned(8) class hintmaxrelativetime extends Box('tmax') {  
 int(32) time; } // largest relative transmission time, milliseconds

aligned(8) class hintlargestpacket extends Box('pmax') {  
 uint(32) bytes; } // largest packet sent, including RTP header  
aligned(8) class hintlongestpacket extends Box('dmax') {  
 uint(32) time; } // longest packet duration, milliseconds

aligned(8) class hintpayloadID extends Box('payt') {  
 uint(32) payloadID; // payload ID used in RTP packets  
 uint(8) count;  
 char rtpmap\_string[count]; }

NOTE It is possible that not all these sub-boxes are present, and that there can be multiple hintmaxrate boxes, covering different periods.

## ALC/LCT and FLUTE hint track format

### Overview

The file format supports multicast/broadcast delivery of files with FEC protection. Files to be delivered are stored as items in a container file (defined by the file format) and the MetaBox is amended with information on how the files are partitioned into source symbols. For each source block of a FEC encoding, additional parity symbols can be pre-computed and stored as FEC reservoir items. The partitioning depends on the FEC scheme, the target packet size, and the desired FEC overhead. Pre-composed source symbols can be stored as File reservoir items to minimize duplicate information in the container file especially with MBMS-FEC. The actual transmission is governed by hint tracks that contain server instructions that facilitate the encapsulation of source and FEC symbols into packets.

FD hint tracks have been designed for the ALC/LCT (asynchronous layered coding/layered coding transport) and FLUTE (file delivery over unidirectional transport) protocols. LCT provides transport level support for reliable content delivery and stream delivery protocols. ALC is a protocol instantiation of the LCT building block, and it serves as a base protocol for massively scalable reliable multicast distribution of arbitrary binary objects. FLUTE builds on top of ALC/LCT and defines a protocol for unidirectional delivery of files.

FLUTE defines a file delivery table (FDT), which carries metadata associated with the files delivered in the ALC/LCT session, and provides mechanisms for in-band delivery and updates of FDT. In contrast, ALC/LCT relies on other means for out-of-band delivery of file metadata, e.g. an electronic service guide that is normally delivered to clients well in advance of the ALC/LCT session combined with update fragments that can be sent during the ALC/LCT session.

File partitionings and FEC reservoirs can be used independently of FD hint tracks and vice versa. The former aid the design of hint tracks and allow alternative hint tracks, e.g. with different FEC overheads, to re-use the same FEC symbols. They also provide means to access source symbols and additional FEC symbols independently for post-delivery repair, which may be performed over ALC/LCT or FLUTE or out-of-band via another protocol. In order to reduce complexity when a server follows hint track instructions, hint tracks refer directly to data ranges of items or data copied into hint samples.

It is recommended that a server sends a different set of FEC symbols for each retransmission of a file.

The syntax for using the MetaBox as a container file for source files is defined in 8.10.4, partitions, file and FEC reservoirs are defined in 8.13, while the syntax for FD hint tracks is defined in 9.2.

### Design principles

The support for file delivery is designed to optimize the server transmission process by enabling ALC/LCT or FLUTE servers to follow simple instructions. It is enough to follow one pre-defined sequence of instructions per channel in order to transmit one session. The file format enables storage of pre-computed source blocks and symbol partitionings, i.e., files may be partitioned into symbols which fit an intended packet size, and pre-computing a certain amount of FEC-symbols that also can be used for post-session repair. The file format also allows storage of alternative ALC/LCT or FLUTE transmission session instructions that may lead to equivalent end results. Such alternatives may be intended for different channel conditions because of higher FEC protection or even by using different error correction schemes. Alternative sessions can refer to a common set of symbols. The hint tracks are flexible and can be used to compose FDT fragments and interleaving of such fragments within the actual object transmission. Several hint tracks can be combined into one or more sessions involving simultaneous transmission over multiple channels.

It is important to make a difference between the definition of sessions for transmission and the scheduling of such sessions. ALC/LCT and FLUTE server files only address optimization of the server transmission process. In order to ensure maximal usage and flexibility of such pre-defined sessions, all details regarding scheduling addresses, etc. are kept outside the definition of the file format. External scheduling applications decide such details, which are not important for optimizing transmission sessions per se. In particular, the following information is out-of-scope of the file format: time scheduling, target addresses and ports, source addresses and ports, and so-called transmission session identifiers (TSI).

The sample numbers associated with the samples of a file delivery hint track provide a numbered sequence. Hint track sample times provide send times of ALC/LCT or FLUTE packets for a default bitrate. Depending on the actual transmission bitrate, an ALC/LCT or FLUTE server may apply linear time scaling. Sample times may simplify the scheduling process, but it is up to the server to send ALC/LCT or FLUTE packets in a timely manner.

A schematic picture of a file containing three alternative hint tracks with different FEC overhead for a source file is provided in Figure 1. In this example, each source block consists of only one sub-block.



Figure 1 — Different FEC overheads of a source file provided by alternative hint tracks

The source file in Figure 1 is partitioned into 2 source blocks containing symbols of a fixed size. FEC redundancy symbols are calculated for both source blocks and stored as FEC reservoir items. As the hint tracks reference the same items in the file there is no duplication of information. The original source symbols and FEC reservoirs can also be used by repair servers that don’t use hint tracks.

### Sample entry format

* + - 1. Definition

FD hint tracks are tracks with handler\_type 'hint' and with the entry-format 'fdp ' in the SampleDescriptionBox. The FD hint sample entry is contained in the SampleDescriptionBox.

* + - 1. Syntax

class FDHintSampleEntry() extends HintSampleEntry ('fdp ')   
{  
 unsigned int(16) hinttrackversion = 1;  
 unsigned int(16) highestcompatibleversion = 1;  
 unsigned int(16) partition\_entry\_ID;  
 unsigned int(16) FEC\_overhead;  
}

* + - 1. Semantics

partition\_entry\_ID indicates the partition entry in the FDItemInformationBox. A zero value indicates that no partition entry is associated with this sample entry, e.g. for FDT. If the corresponding FD hint track contains only overhead data this value should indicate the partition entry whose overhead data is in question.

FEC\_overhead is a fixed 8.8 value indicating the percentage protection overhead used by the hint sample(s). The intention of providing this value is to provide characteristics to help a server select a session group (and corresponding FD hint tracks). If the corresponding FD hint track contains only overhead data this value should indicate the protection overhead achieved by using all FD hint tracks in a session group up to the FD hint track in question.

The hinttrackversion and highestcompatibleversion fields have the same interpretation as in the RTP hint sample entry described in 9.1.2. As additional data a timescaleentry box may be provided. If not provided, there is no indication given on timing of packets.

File entries needed for an FDT or an electronic service guide can be created by observing all sample entries of a hint track and the corresponding item information boxes of the items referenced by the above partition entry IDs. No sample entries shall be included in the hint track if they are not referenced by any sample.

### Sample format

#### Sample container

Each FD sample in the hint track will generate one or more FD packets.

Each sample contains two areas: the instructions to compose the packets, and any extra data needed when sending those packets (e.g. encoding symbols that are copied into the sample instead of residing in items for source files or FEC). The size of the sample is known from the sample size table.

aligned(8) class FDsample extends Box('fdsa')   
{  
 FDPacketBox packetbox[]  
 ExtraDataBox extradata; //optional  
}

Sample numbers of FD samples define the order they shall be processed by the server. Likewise, FDpacketBoxes in each FD sample should appear in the order they shall be processed. If the timescaleentry box is present in the FDHintSampleEntry, then sample times are defined and provide relative send times of packets for a default bitrate. Depending on the actual transmission bitrate, a server may apply linear time scaling. Sample times may simplify the scheduling process, but it is up to the server to send packets in a timely manner.

#### Packet entry format

Each packet in the FD sample has the following structure (see IETF RFC 3926[14], IETF RFC  3450[15], and IETF RFC  3451[16]):

aligned(8) class FDpacketBox extends Box('fdpa')   
{  
 LCTheaderTemplate LCT\_header\_info;  
 unsigned int(16) entrycount1;  
 LCTheaderExtension header\_extension\_constructors[ entrycount1 ];  
 unsigned int(16) entrycount2;  
 dataentry packet\_constructors[ entrycount2 ];  
}

The LCT header info contains LCT header templates for the current FD packet. Header extension constructors are structures which are used for constructing the LCT header extensions. Packet constructors are used for constructing the FEC payload ID and the source symbols in an FD packet.

#### LCT header template format

The LCT header template is defined as follows:

aligned(8) class LCTheaderTemplate   
{  
 unsigned int(1) sender\_current\_time\_present;  
 unsigned int(1) expected\_residual\_time\_present;  
 unsigned int(1) session\_close\_bit;  
 unsigned int(1) object\_close\_bit;  
 unsigned int(4) reserved;  
 unsigned int(16) transport\_object\_identifier;  
}

It can be used by a server to form an LCT header for a packet. Note that some parts of the header depend on the server policy and are not included in the template. Some field lengths also depend on the LCT header bits assigned by the server. The server may also need to change the value of the transport object identifier (TOI).

#### LCT header extension constructor format

The LCT header extension constructor format is defined as follows:

aligned(8) class LCTheaderextension   
{  
 unsigned int(8) header\_extension\_type;  
 if (header\_extension\_type > 127) {  
 unsigned int(8) content[3];  
 }  
 else {  
 unsigned int(8) length;  
 if (length > 0) {  
 unsigned int(8) content[(length\*4) - 2];  
 }  
}

A positive value of the length field specifies the length of the constructor content in multiples of 32 bit words. A zero value means that the header is generated by the server.

The usage and rules for LCT header extensions are defined in IETF RFC 3451[16] (LCT RFC). The header\_extension\_type contains the LCT header extension type (HET) value.

HET values between 0 and 127 are used for variable-length (multiple 32-bit word) extensions. HET values between 128 and 255 are used for fixed length (one 32-bit word) extensions. If the header\_extension\_type is smaller than 128, then the length field corresponds to the LCT header extension length (HEL) as defined in IETF RFC 3451[16]. The content field always corresponds to the header extension content (HEC).

NOTE A server can identify packets including FDT by observing whether EXT\_FDT (header\_extension\_type == 192) is present.

#### Packet constructor format

There are various forms of the constructor. Each constructor is 16 bytes in order to make iteration easier. The first byte is a union discriminator. The packet constructors are used to include FEC payload ID as well as source and parity symbols in an FD packet.

aligned(8) class FDconstructor(type)   
{  
 unsigned int(8) constructor\_type = type;  
}  
  
aligned(8) class FDnoopconstructor extends FDconstructor(0)  
{  
 unsigned int(8) pad[15];  
}  
  
aligned(8) class FDimmediateconstructor extends FDconstructor(1)  
{  
 unsigned int(8) count;  
 unsigned int(8) data[count];  
 unsigned int(8) pad[14 - count];  
}  
  
aligned(8) class FDsampleconstructor extends FDconstructor(2)  
{  
 signed int(8) trackrefindex;  
 unsigned int(16) length;  
 unsigned int(32) samplenumber;  
 unsigned int(32) sampleoffset;  
 unsigned int(16) bytesperblock = 1;  
 unsigned int(16) samplesperblock = 1;  
}  
  
aligned(8) class FDitemconstructor extends FDconstructor(3)  
{  
 unsigned int(16) item\_ID;  
 unsigned int(16) extent\_index;  
 unsigned int(64) data\_offset; //offset in byte within extent  
 unsigned int(24) data\_length; //non-zero length in bytes within extent or  
 //if (data\_length==0) rest of extent  
}

aligned(8) class FDitemconstructorLarge extends FDconstructor(5)  
{  
 unsigned int(32) item\_ID;  
 unsigned int(32) extent\_index;  
 unsigned int(64) data\_offset; //offset in byte within extent  
 unsigned int(24) data\_length; //non-zero length in bytes within extent or  
 //if (data\_length==0) rest of extent  
}

aligned(8) class FDxmlboxconstructor extends FDconstructor(4)  
{  
 unsigned int(64) data\_offset; //offset in byte within XMLBox or BinaryXMLBox  
 unsigned int(32) data\_length;  
 unsigned int(24) reserved;  
}

#### Extra data box

Each sample of an FD hint track may include extra data stored in an ExtraDataBox:

aligned(8) class ExtraDataBox extends Box('extr') {  
 FECInformationBox feci;  
 bit(8) extradata[];  
}

#### FEC information box

##### Definition

Box Type: 'feci'  
Container: ExtraDataBox  
Mandatory: No  
Quantity: Zero or One

The FECInformationBox stores FEC encoding ID, FEC instance ID and FEC payload ID which are needed when sending an FD packet.

##### Syntax

aligned(8) class FECInformationBox extends Box('feci')   
{  
 unsigned int(8) FEC\_encoding\_ID;  
 unsigned int(16) FEC\_instance\_ID;  
 unsigned int(16) source\_block\_number;  
 unsigned int(16) encoding\_symbol\_ID;  
}

##### Semantics

FEC\_encoding\_ID identifies the FEC encoding scheme and is subject to IANA registration (see IETF RFC 5052), in which (i) value zero corresponds to the "Compact No-Code FEC scheme" also known as "Null-FEC" (IETF RFC 3695[17]); (ii) value one corresponds to the “MBMS FEC” (3GPP TS 26.346[29]); (iii) for values in the range of 0 to 127, inclusive, the FEC scheme is Fully-Specified, whereas for values in the range of 128 to 255, inclusive, the FEC scheme is Under-Specified.

FEC\_instance\_ID provides a more specific identification of the FEC encoder being used for an Under-Specified FEC scheme. This value should be set to zero for Fully-Specified FEC schemes and shall be ignored when parsing a file with FEC\_encoding\_ID in the range of 0 to 127, inclusive. FEC\_instance\_ID is scoped by the FEC\_encoding\_ID. See IETF RFC 5052 for further details.

source\_block\_number identifies from which source block of the object the encoding symbol(s) in the FD packet are generated.

encoding\_symbol\_ID identifies which specific encoding symbol(s) generated from the source block are carried in the FD packet.

## MPEG-2 transport hint track format

### Overview

MPEG-2 TS (transport stream) is a stream multiplex which can carry one or more programs, consisting of audio, video and other media. The file format supports the storage of MPEG-2 TS in a hint track. An MPEG-2 TS hint track can be used for both storage of received TS packets (as a reception hint track), and as a server hint track used for the generation of an MPEG-2 TS.

The MPEG-2 TS hint track definition supports so-called “precomputed hints”. Precomputed hints make no use of including data by reference from other tracks, but rather MPEG-2 TS packets are stored as such. This allows reusing the MPEG-2 TS packets stored in a separate file. Furthermore, precomputed hints facilitate simple recording operation.

In addition to precomputed hint samples, it is possible to include media data by reference to media tracks into hint samples. Conversion of a received transport stream to media tracks allows existing players compliant with earlier versions of the ISO base media file format to process recorded files as long as the media formats are also supported. Storing the original transport headers retains valuable information for error concealment and the reconstruction of the original transport stream.

### Design principles

#### General principles

The design principles of the MPEG-2 TS hint track format are as follows.

A sequence of samples in an MPEG-2 TS hint track is a set of precomputed and constructed MPEG-2 TS packets. Precomputed packets are TS packets which are stored unchanged in the case of reception or will be sent as is. This is especially important where data cannot be de-multiplexed and elementary streams cannot be created – e.g. when the transport stream is encrypted and is not allowed to be stored decrypted. Therefore, it is necessary to be able to store the MPEG-2 TS as such in a hint track. Constructed packets use the same approach as RTP hint tracks, i.e., the sample contains instructions for a streaming server to construct the packet. The actual media data is contained in other tracks. A track reference of type 'hint' is used.

#### Reusing existing transport streams

It was desired to reuse existing TS instances and therefore an additional mechanism exists to cover a wide variety of existing TS recordings. These recordings may consist not only of TS packets but have preceding or trailing data with each TS packet. A specific case for preceding data is a 4-byte timestamp in front of each TS packet to remove the jitter of a transmission system. A specific case for trailing data is the addition of FEC when a TS packet is transmitted over an error-prone channel.

#### Timing

MPEG-2 TS defines a single clock for each program, running at 27MHz, which sampling value is transported as PCRs in the TS for clock recovery. The timescale of MPEG-2 TS Hint Tracks is recommended to be 90000, or an integer division or multiple thereof.

The decoding time of a sample in a MPEG-2 TS Hint Track is the reception/transmission time of the first bit of that packet or packet group which is recommended to be derived from the PCR timestamps of the TS, since if the PCR times are used, piece-wise linearity can be assumed and the 'stts' table compacts sensibly. The optional TSTimingBox in the sample entry can be used to signal whether reception timing with or without clock recovery was used when the hint track is a reception hint track. In the case of a server hint track PCR timing is assumed.

NOTE When there are multiple packets in a sample, they cannot be given independent transmission time offsets.

#### Packet grouping

The sample format for MPEG-2 Transport Stream Hint Tracks allows multiple TS packets in one sample. Specific applications, such as some IPTV applications, convey TS packets in an RTP stream. Only one reception timestamp can be derived for all TS packets carried in one RTP packet. Another application for storing multiple TS packets in a sample is SPTSs, where a sample contains all the TS packets for a GoP. In this case every sample is a random access point.

NOTE random-access to every TS packet is not possible by the means of the file format if multiple TS packets per sample are used.

In the case of an MPTS only one packet per sample should be used. This facilitates the use of the sample group mechanism on a per-packet basis.

#### Random-access points

A sync sample is a point at which processing of a track may begin without error. Both MPTS and SPTS are supported by MPEG-2 TS Hint Tracks, however a random access point that is marked as a sync sample is normally only defined for SPTS, where it specifies the beginning of a packet that contains the first byte of an independently decodable media access unit (e.g. MPEG-2 video I-frames or MPEG-4 AVC IDR pictures) of a stream that uses differential coding. For MPTS, the SyncSampleBox is normally present but empty, indicating that there is no point in the track at which processing of the entire track may begin without error. It is recommended that the PSI/SI be in the sample entry so that true random-access with just the media data is possible.

NOTE 1 in the case of an MPTS, the SyncSampleBox is present but empty (which means essentially that no sample is a sync sample).

Note also that in case of an SPTS, samples including multiple TS packets should have a sync point (e.g. GoP boundary) at the start of a sample. The SyncSampleBox then marks the samples the sync points (e.g. the start of GoPs); if the SyncSampleBox is absent, all the samples are sync points. If the SyncSampleBox is present but empty, the sync sample positions are unknown and may be not at the start of samples.

NOTE 2 An application searching for a key frame can start reading at that location, but in general it also has to read further MPEG-2 TS packets (regarding the file format these are subsequent samples) so that the decoder can decode a complete frame.

#### Application as a reception hint track

Reception hint tracks may be used when one or more packet streams of data are recorded. They indicate the order, reception timing, and contents of the received packets among other things.

NOTE 1 Players can reproduce the packet stream that was received based on the reception hint tracks and process the reproduced packet stream as if it was newly received.

Reception hint tracks have the same structure as hint tracks for servers.

The format of the reception hint samples is indicated by the sample entry for the reception hint track. Each protocol has its own reception hint sample format and name.

Servers using reception hint tracks as hints for sending of the received streams should handle the potential degradations of the received streams, such as transmission delay jitter and packet losses, gracefully and ensure that the constraints of the protocols and contained data formats are obeyed regardless of the potential degradations of the received streams.

NOTE 2 As with server hint tracks, the sample formats of reception hint tracks can enable construction of packets by pulling data out of other tracks by reference. These other tracks can be hint tracks or media tracks. The exact form of these pointers is defined by the sample format for the protocol, but in general they consist of four pieces of information: a track reference index, a sample number, an offset, and a length. Some of these can be implicit for a particular protocol. These 'pointers' always point to the actual source of the data, i.e., indirect data referencing is disallowed. If a hint track is built 'on top' of another hint track, then the second hint track will need to have direct references to the media track(s) used by the first where data from those media tracks is placed in the stream.

If received data is extracted to media tracks, the de-hinting process must ensure that the media streams are valid, i.e. the streams must be error-free (which requires e.g. error concealment).

A sample with a size of zero is permitted in reception hint tracks, and such samples may be ignored.

### Sample entry format

#### Definition

The sample entry for an MPEG2-TS reception hint track contains all static metadata that describe the stream or a portion thereof, especially the PSI/SI tables. MPEG-2 TS reception hint tracks use an entry-format in the sample entry of 'rm2t' (which indicates *MPEG-2 transport stream*). The entry-format for MPEG2‑TS server hint tracks is 'sm2t'.

The static metadata documents e.g. PSI/SI tables. The presence of static metadata is optional. When present, the static metadata shall be valid for the MPEG2-TS packets it describes. Consequently, if a piece of static metadata changes in the stream, a new sample entry is needed for the first sample at or after the change. If static metadata is not present in the sample entry, structures, such as PSI/SI tables, stored in the MPEG2-TS packets are valid and the stream must be scanned in order to find out which values of static metadata are valid for a particular sample.

#### Syntax

class MPEG2TSReceptionSampleEntry() extends MPEG2TSSampleEntry(`rm2t´)   
{  
}

class MPEG2TSServerSampleEntry() extends MPEG2TSSampleEntry(`sm2t´)   
{  
}

class MPEG2TSSampleEntry(name) extends HintSampleEntry(name)   
{  
 uint(16) hinttrackversion = 1;  
 uint(16) highestcompatibleversion = 1;  
 uint(8) precedingbyteslen;  
 uint(8) trailingbyteslen;  
 uint(1) precomputed\_only\_flag;  
 uint(7) reserved;  
}

#### Semantics

hinttrackversion is currently 1; the highestcompatibleversion field specifies the oldest version with which this track is backward-compatible.

precedingbyteslen indicates the number of bytes that are preceding each MPEG2-TS packet (which may e.g. be a time-code from an external recording device).

trailingbyteslen indicates the number of bytes that are at the end of each MPEG2-TS packet (which may e.g. contain checksums or other data that was added by a recording device).

precomputed\_only\_flag indicates whether the associated samples are purely precomputed if set to 1;

additionaldata is a set of boxes. This set can contain boxes that describe one common version of the PSI/SI tables by means of the PATBox or the PMTBox or other data, e.g. boxes that are only valid for a sample (which contains multiple packets) and describe the initial conditions of the STC or boxes that define the content of the preceding or trailing data. There shall be at most one of each of PATBox, TSTimingBox, InitialSampleTimeBox present within additionaldata

The following optional boxes for additionaldata are defined:

aligned(8) class PATBox extends Box('tPAT')   
{  
 uint(3) reserved;  
 uint(13) PID;  
 uint(8) sectiondata[];  
}

aligned(8) class PMTBox extends Box('tPMT')   
{  
 uint(3) reserved;  
 uint(13) PID;  
 uint(8) sectiondata[];  
}

aligned(8) class ODBox extends Box ('tOD ')   
{  
 uint(3) reserved;  
 uint(13) PID;  
 uint(8) sectiondata[];  
}

aligned(8) class TSTimingBox extends Box('tsti')   
{  
 uint(1) timing\_derivation\_method;  
 uint(2) reserved;  
 uint(13) PID;  
}

aligned(8) class InitialSampleTimeBox extends Box('istm')   
{  
 uint(32) initialsampletime;  
 uint(32) reserved;  
}

The PATBox contains the section data of the PAT and each PMTBox contains the section data of one of the PMTs.

In the case of an SPTS, it is strongly recommended that the PMTBox is present in the additionaldata. If the PMT is not present in the sample data, then it shall be present in the additionaldata. If the PMTBox is present, it shall be the PMT for the program contained in the sample data (although the recorded stream may contain other programs and be an MPTS).

PID is the PID of the MPEG2-TS packets from which the data was extracted. In the case of the PATBox this value is always 0.

sectiondata extends to the end of the box and is the complete MPEG2-TS table, containing the concatenated sections, of an identical version number.

initialsampletime specifies the initial value of the sample times in case the sample times do not start from 0. Unlike media tracks, MPEG-2 TS hint track usually have sample times not starting from 0, e.g. PCR times and reception times. Since 'stts' only stores the delta between sample times, this field is required for reconstructing the original sample times:

OriginalSampleTime(n) = initialsampletime + STTS(n).

In case PCR times are used for sample times, the reconstructed sample time can be used to initialize the STC when the sample is randomly accessed. Note that this field may need to be updated after editing.

timing\_derivation\_method is a flag which specifies the method which was used to set the sample time for a given PID. The values for timing\_derivation\_method are as follows:

0x0 reception time: the sample timing is derived from the reception time. It is not guaranteed that the STC was recovered for derivation of the reception time.

0x1 piecewise linearity between PCRs: the sample time is derived from a reconstructed STC for this program. Piecewise linearity between adjacent PCRs is assumed and all TS packets in the samples have a constant duration in this range.

### Sample format

#### Definition

Each sample of an MPEG-2 TS Hint track consists of a set of

 pre-computed packets: one or more MPEG-2 TS packets with the associated headers and trailers

 constructed packets: instructions to compose one or more MPEG2-TS packets with the associated headers and trailers by pointing to data of another track.

Each MPEG-2 TS packet in the sample may be preceded with a preheader (precedingbytes), or followed by a posttrailer (trailingbytes), as detailed in the sample entry Format. The size of the preheader and the posttrailer are specified by precedingbyteslen and trailingbyteslen, respectively, in the sample entry to allow compact sample tables with fewer chunks.

It is possible for a mixture of precomputed and constructed samples to occur in the same track. If padding of the transport stream packet is required, this can be accomplished with the adaptation\_field or explicitly by using the MPEG2TSImmediateConstructor as appropriate.

NOTE 1 The number of MPEG-2 TS packets in the sample can be derived from the sample size table directly if the sample consists of pre-computed packets only, which is a conclusion if the precomputed\_only\_flag in the sample entry is set. The number of MPEG-2 TS packets in the sample can be variable or restricted, e.g. extensions of this document can define a sample to contain exactly one packet.

NOTE 2 It is possible to compact common sequences of bytes in transport packets by including those bytes in one or more packets directly for example in their precedingbytes or trailingbytes section, and then using the MPEG2TSSampleConstructor in other places to refer to them; this is especially relevant for runs of 0xFF bytes.

#### Syntax

// Constructor format  
aligned(8) abstract class MPEG2TSConstructor (uint(8) type)   
{  
 uint(8) constructor\_type = type;  
}

aligned(8) class MPEG2TSImmediateConstructor  
 extends MPEG2TSConstructor(1)   
{  
 uint(8) immediatedatalen;  
 uint(8) data[immediatedatalen];  
}

aligned(8) class MPEG2TSSampleConstructor  
 extends MPEG2TSConstructor(2)   
{  
 uint(8) sampledatalen;  
 uint(16) trackrefindex;  
 uint(32) samplenumber;  
 uint(32) sampleoffset;  
}

// Packet format  
aligned(8) class MPEG2TSPacketRepresentation   
{  
 uint(8) precedingbytes[precedingbyteslen];  
 uint(8) sync\_byte;  
 if (sync\_byte == 0x47) {  
 uint(8) packet[187];  
 } else if (sync\_byte == 0x00 || sync\_byte == 0x01) {  
 uint(8) headerdatalen;  
 uint(4) reserved;  
 uint(4) num\_constructors;  
 bit(1) transport\_error\_indicator;  
 bit(1) payload\_unit\_start\_indicator;  
 bit(1) transport\_priority;  
 bit(13) PID;  
 bit(2) transport\_scrambling\_control;  
 bit(2) adaptation\_field\_control;  
 bit(4) continuity\_counter;  
 if (sync\_byte == 0x00 && (adaptation\_field\_control == ´10´ ||  
 adaptation\_field\_control == ´11´)) {  
 uint(8) adaptation\_field[headerdatalen-3];  
 }  
 MPEG2TSConstructor constructors[num\_constructors];  
 } else if (sync\_byte == 0xFF) {  
 // implicit null packet that has been removed  
 }  
 uint(8) trailingbytes[trailingbyteslen];  
}

// Sample format  
aligned(8) class MPEG2TSSample   
{  
 MPEG2TSPacketRepresentation sample[];  
}

#### Semantics

precedingbytes contains any extra data preceding the packet, typically provided by the recording device. For example, this may include a timestamp.

sync\_byte: if this value is 0x47, then the packet representation contains a transport stream packet (a precomputed reception hint track sample), with the remaining bytes following in the field packet. The values 0x00 and 0x01 are used for constructed packet representation(s). If MPEG2TSSampleConstructor is used to construct packet representation(s), it points to a track indexed by trackrefindex in the TrackReferenceBox with reference type 'hint'. If this value is 0xFF, it implies that a null packet has been removed at this position. All other values are currently reserved.

trackrefindex indexes in the TrackReferenceBox with reference type 'hint' to indicate with which media track the current sample is associated. The samplenumber and sampleoffset fields in the MPEG2TSSampleConstructor point into this media track. The trackrefindex starts from value 1. The value 0 is reserved for future use.

packet: The MPEG-2 TS packet, apart from the sync byte (0x47).

The MPEG2TSConstructor array is a collection of one or more constructor entries, to allow for multiple access units in one transport stream packet. An MPEG2TSImmediateConstructor can contain, amongst others, the PES header. An MPEG2TSSampleConstructor references data in the associated media track. The sum of headerdatalen and the datalen fields of all constructors of an MPEG2TSPacket shall be equal to the length of the transport stream packet being constructed, minus 1 byte, which is 187.

trailingbytes contains any extra data following the packet. For example, this may include a checksum.

samplenumber indicates the sample within the referred track contained in the packet and sampleoffset indicates the starting byte position of the referred media sample contained in the packet of which sampledatalen bytes are included. sampleoffset starts from value 0.

immediatedatalen indicates the number of bytes within the field data that are included in the sample rather than data being included into the sample by reference to a media track.

headerdatalen indicates the length of the TS packet header (without the sync byte) in bytes. This field has the value 3 if the adaptation\_field is not present or the value (adaptation\_field\_length+3), where adaptation\_field\_length is the first octet of the structure adaptation\_field as defined in ISO/IEC 13818-1[1].

Neither the format of precedingbytes nor trailingbytes are defined by this document.

The remaining fields (transport\_error\_indicator, payload\_unit\_start\_indicator, transport\_priority, PID, transport\_scrambling\_control, adaptation\_field\_control, continuity\_counter, adaptation\_field) of the sample structure contain a copy of the packet header of the TS packet, as defined in in ISO/IEC 13818-1[1].

### Protected MPEG 2 transport stream hint track

#### Overview

This subclause defines a mechanism for marking media streams as protected. This works by changing the four character code of the SampleEntry, and appending boxes containing both details of the protection mechanism and the original four character code. However, in this case the track is not protected; it is an ‘in the clear’ hint track which contains protected data. This subclause describes how hint tracks should be marked as carrying protected data, using a similar mechanism, and utilizing the same boxes.

#### Syntax

class ProtectedMPEG2TransportStreamSampleEntry  
 extends MPEG2TSSampleEntry('pm2t')   
{  
 ProtectionSchemeInfoBox SchemeInformation;  
}

#### Semantics

The ProtectionSchemeInfoBox (defined in 13.4.2) shall contain details of the protection scheme applied. This shall include the OriginalFormatBox which shall contain the original sample entry type of the MPEG2TSSampleEntry.

## RTP, RTCP, SRTP and SRTCP reception hint tracks

### RTP reception hint track

#### Overview

This subclause specifies the reception hint track format for the real-time transport protocol (RTP), as defined in IETF RFC 3550[17].

RTP is used for real-time media transport over the Internet Protocol. Each RTP stream carries one media type, and one RTP reception hint track carries one RTP stream. Hence, recording of an audio-visual program results into at least two RTP reception hint tracks.

The design of the RTP reception hint track format follows as much as possible the design of the RTP server hint track format. This design should ensure that RTP packet transmission operates very similarly regardless whether it is based on RTP reception hint tracks or RTP server hint tracks. Furthermore, the number of new data structures in the file format was consequently kept as small as possible.

The format of the RTP reception hint tracks allow storing of the packet payloads in the hint samples, or converting the RTP packet payloads to media samples and including them by reference to the hint samples, or combining both approaches. As noted earlier, conversion of received streams to media tracks allows existing players compliant with earlier versions of the ISO base media file format to process recorded files as long as the media formats are also supported. Storing the original RTP headers retains valuable information for error concealment and the reconstruction of the original RTP stream. It is noted that the conversion of packet payloads to media samples may happen "off-line" after recording of the streams in precomputed RTP reception hint tracks has been completed.

#### Sample entry format

The entry-format in the sample entry for the RTP reception hint tracks is 'rrtp'. The syntax of the sample entry is the same as for RTP server hint tracks having the entry-format 'rtp '.

class ReceivedRtpHintSampleEntry() extends HintSampleEntry ('rrtp')   
{  
 uint(16) hinttrackversion = 1;  
 uint(16) highestcompatibleversion = 1;  
 uint(32) maxpacketsize;  
}

The entry-format identifier in the sample entry of the RTP reception hint track is different from the entry-format in the sample entry of the RTP server hint track, in order to avoid using an RTP reception hint track that contains errors as a valid server hint track.

The additionaldata set of boxes may include the timescaleentry and timeoffset boxes. Moreover, the additionaldata may contain a timestamp synchrony box.

The timescaleentry box shall be present and the value of timescale shall be set to match the clock frequency of the RTP timestamps of the stream captured in the reception hint track.

The timeoffset may be present. If the timeoffset box is not present, the value of the field offset is inferred to be equal to 0. The value of the field offset is used for the derivation of the RTP timestamp, as specified in 9.4.1.4.

RTP timestamps typically do not start from zero, especially if an RTP receiver 'tunes' into a stream. The timeoffset box should therefore be present in RTP reception hint tracks and the value of offset in the timeoffset box should be set equal to the first RTP timestamp of the RTP stream in reception order.

Zero or one timestampsynchrony boxes may be present in the additionaldata of the sample entry for a RTP reception hint track. If a timestampsynchrony box is not present, the value of timestamp\_sync is inferred to be equal to 0.

class timestampsynchrony() extends Box('tssy')   
{  
 unsigned int(6) reserved;  
 unsigned int(2) timestamp\_sync;  
}

timestamp\_sync equal to 0 indicates that the RTP timestamps of the present RTP reception hint track derived from Formula 1 (in 9.4.1.4) may or may not be synchronized with RTP timestamps of other RTP reception hint tracks.

timestamp\_sync equal to 1 indicates that the RTP timestamps of the present RTP reception hint track derived from Formula 1 (in 9.4.1.4) reflect the received RTP timestamps exactly (without corrected synchronization to any other RTP reception hint track).

timestamp\_sync equal to 2 indicates that RTP timestamps of the present RTP reception hint track derived from Formula 1 (in 9.4.1.4) are synchronized with RTP timestamps of other RTP reception hint tracks.

When timestamp\_sync is equal to 0 or 1, a player should correct the inter-stream synchronization using stored RTCP sender reports. When timestamp\_sync is equal to 2, the media contained in the RTP reception hint tracks can be played out synchronously according to the reconstructed RTP timestamps without synchronization correction using RTCP Sender Reports. If it is expected that the RTP reception hint track will be used for re-sending the recorded RTP stream, it is recommended that timestamp\_sync be set equal to 0 or 1, because the stored RTCP sender reports can be reused.

timestamp\_sync equal to 3 is reserved.

The value of timestamp\_sync shall be identical for all RTP reception hint tracks present in a file.

When RTCP is also stored, using an RTCP hint track, the timestamp relationship between the RTP and RTCP hint tracks can only be maintained if the RTP timestamps are anchored by using a set time offset ('tsro') in the RTP track, and hence the time offset is mandatory if RTCP is stored in an RTCP hint track.

Zero or one ReceivedSsrcBox identified with the four-character code 'rssr' shall be present in the additionaldata of a sample descriptor entry of a RTP reception hint track:

class ReceivedSsrcBox extends Box('rssr')   
{  
 unsigned int(32) SSRC  
}

The SSRC value shall equal the SSRC value in the header of all recorded SRTP packets described by the sample entry.

#### Sample format

The sample format of RTP reception hint tracks is identical to the syntax of the sample format of the RTP server hint tracks. Each sample in the reception hint track represents one or more received RTP packets. If media frames are not both fragmented and interleaved in an RTP stream, it is recommended that each sample represents all received RTP packets that have the same RTP timestamp, i.e., consecutive packets in RTP sequence number order with a common RTP timestamp.

Each RTP reception hint sample contains two areas: the instructions to compose the packet, and any extra data needed for composing the packet, such as a copy of the packet payload. The size of the sample is known from the sample size table.

Since the reception time for the packets may vary, this variation can be signalled for each packet as specified subsequently.

A sample with a size of zero is permitted in reception hint tracks, and such samples may be ignored.

#### Packet entry format

Each packet in the packet entry table has same structure as for server (transmission) hint tracks, in 9.1.3.2.

Where i is the sample number of a sample, the sum of the sample time DT(i) as specified in 8.6.1.2 and relative\_time indicates the reception time of the packet. The clock source for the reception time is undefined and may be, for instance, the wall clock of the receiver. If the range of reception times of a reception hint track overlaps entirely or partly with the range of reception times of another reception hint track, the clock sources for these hint tracks shall be the same.

It is recommended that receivers may use a constant value for sample\_delta in the decoding TimeToSampleBox as much as reasonable and smooth out packet scheduling and end-to-end delay variation by setting relative\_time adaptively in stored reception hint samples. This arrangement of setting the values of sample\_delta and relative\_time can facilitate a compact decoding TimeToSampleBox. In this case timestamp\_sync is set to 1, the sample durations are mostly constant, and the timeoffset is stored in the sample entry.

The values of RTP\_version, P\_bit, X\_bit, CSRC\_count, M\_bit, payload\_type, and RTPsequenceseed shall be set equal to the V, P, X, CC, M, PT and sequence number fields of the RTP packet captured in the sample.

The fields bframe\_flag and repeat\_flag are reserved in reception hint tracks and shall be zero.

The semantics of extra\_flag and extra\_information\_length are identical to those of specified for the RTP server hint tracks.

The following TLV boxes are specified: rtphdrextTLV, rtpoffsetTLV, receivedCSRC.

If the X\_bit is set a single rtphdrextTLV box shall be present for storing the received RTP header extension.

aligned(8) class rtphdrextTLV extends Box('rtpx') {  
 unsigned int(8) data[];  
}

data is the raw RTP header extension which is application-specific.

The syntax of the rtpoffsetTLV box is specified in 9.1.3.2.

offset indicates a 32-bit signed integer offset to the RTP timestamp of the received RTP packet. Let i be the sample number of a sample, DT(i) be equal to DT as specified in 8.6.1.2 for sample number i, tsro.offset be the value of offset in the timeoffset box of the referred reception hint sample entry, and % be the modulo operation. The value of offset shall be such that Formula (1) is true:

 (1)

NOTE 1 When each reception hint sample represents all received RTP packets that have the same RTP timestamp, the value of sample\_delta in the decoding TimeToSampleBox can be set to match the RTP timestamp. In other words, DT(i), as specified above, can be set equal to (the RTP timestamp – tsro.offset – offset) (assuming that the resulting value is greater than or equal to 0). This is recommended.

NOTE 2 RTP timestamps do not necessarily increase as a function of RTP sequence number in all RTP streams, i.e., transmission order and playback order of packets might not be identical. For example, many video coding schemes allow bi-prediction from previous and succeeding pictures in playback order. As samples appear in tracks in their decoding order, i.e., in reception order in case of RTP reception hint tracks, offset in the rtpoffsetTLV box can be used to warp the RTP timestamp away from the sample time DT(i).

For the purpose of edits in EditListBoxes, the composition time of a received RTP packet is inferred to be the sum of the sample time DT(i) and offset as specified above.

If the value of CSRC\_count is not equal to zero, a receivedCSRC box may be present for storing the received CSRC header fields for each RTP packet. The receivedCSRC box is identified with the four-character code 'rcsr'.

aligned(8) class receivedCSRC extends Box('rcsr')   
{  
 unsigned int(32) CSRC[]; //to end of the box  
}

The number of entries in CSRC[] equals the CC value of received SRTP packets. The nth entry of CSRC[] shall equal the nth CSRC value of the RTP packet header.

#### SDP information

Both movie and track SDP information may be present, as specified in 9.1.4.

### RTCP reception hint track

#### Overview

This subclause specifies the reception hint track format for the real-time control protocol (RTCP), defined in IETF RFC 3550[17].

RTCP is used for real-time transport of control information for an RTP session over the Internet Protocol. During streaming, each RTP stream typically has an accompanying RTCP stream that carries control information for the RTP stream. One RTCP reception hint track carries one RTCP stream and is associated to the corresponding RTP reception hint track through a track reference.

The format of the RTCP reception hint tracks allows the storage of RTCP Sender Reports in the hint samples.

The RTCP sender reports are of particular interest for stream recording, because they reflect the current status of the server, e.g. the relationship of the media timing (RTP timestamp of audio/video packets) to the server time (absolute time in NTP format). Knowledge of this relationship is also necessary for playback of recorded RTP reception hint tracks to be able to detect and correct clock drift and jitter.

The timestampsynchrony box as specified in 9.4.1.2 makes it possible to correct clock drift and jitter before playing a file, and therefore recording of RTCP streams is optional when timestamp\_sync is equal to 2.

There is no server hint track equivalent for the RTCP reception hint track, since RTCP messages are generated on-the-fly during transmission.

#### General

There shall be zero or one RTCP reception hint track for each RTP reception hint track. An RTCP reception hint track shall contain a TrackReferenceBox including a reference of type 'cdsc' to the associated RTP reception hint track.

When i is the sample number of a sample, the sample time DT(i) as specified in 8.6.1.2 indicates the reception time of the packet. The clock source for the reception time shall be the same as for the associated RTP reception hint track. The value of timescale in the MediaHeaderBox of an RTCP reception hint track shall be equal to the value of timescale in the MediaHeaderBox of the associated RTP reception hint track.

#### Sample entry format

The entry-format in the sample entry for the RTCP reception hint tracks is 'rtcp'. It is otherwise identical in structure to the sample entry format for RTP. There are no defined boxes for the additionaldata field.

#### Sample format

##### Overview

Each sample in the reception hint track represents one or more received RTCP packets. Each sample contains two areas: the raw RTCP packets and any extra data needed. The size of the sample is known from the sample size table, and that the size of an RTCP packet is indicated within the packet itself (as documented in IETF RFC 3550[17]), as a count one less than the number of 32-bit words in that packet.

##### Syntax

aligned(8) class receivedRTCPpacket   
{  
 unsigned int(8) data[];  
}

aligned(8) class receivedRTCPsample   
{  
 unsigned int(16) packetcount;  
 unsigned int(16) reserved;  
 receivedRTCPpacket packets[packetcount];  
}

##### Semantics

data contains a raw RTCP packet including the RTCP report header, the 20-byte sender information block and any number of report blocks. The size of each RTCP packet is known by parsing the 16-bit length field of the RTCP header.

packetcount indicates the number of received RTCP packets contained in the sample.

packets contains the received RTCP packets.

### SRTP reception hint track

#### Overview

When reception hint tracks are used to store secure real-time transport protocol (SRTP) streams, as defined in IETF RFC 3711, the formats in this subclause shall be used.

SRTP is a secure extension of the real-time media transport (RTP) over the internet protocol. Each SRTP stream carries one media type, and one SRTP reception hint track carries one SRTP stream. Hence, recording of an audio-visual program results into at least two SRTP reception hint tracks.

The design of the SRTP reception hint track format follows the design of RTP reception hint tracks and reuses most of the framework provided by RTP reception hint tracks. The major difference between RTP and SRTP reception hint tracks is that the actual media payload is stored in an encrypted form for SRTP reception hint tracks, whereas it is unencrypted for RTP reception hint tracks. SRTP reception hint tracks provide additional boxes to store information necessary to decrypt encrypted content on playback. Additionally, all header fields of the SRTP packet header shall be stored with the payload, as this information is necessary to check the integrity of the received data. SRTP reception hint tracks are commonly used together with SRTCP reception hint tracks.

SRTP reception hint tracks may, for example, be used to store protected mobile TV content.

#### Sample entry format

##### Sample entry

The sample entry format for SRTP reception hint tracks is identical to that for RTP reception hint tracks with the exception that the sample entry name is changed from 'rrtp' to 'rsrp' and that it may contain additional boxes:

class ReceivedSrtpHintSampleEntry() extends HintSampleEntry ('rsrp')   
{  
 uint(16) hinttrackversion = 1;  
 uint(16) highestcompatibleversion = 1;  
 uint(32) maxpacketsize;  
}

Fields and boxes are identical to those of the ReceivedRtpHintSampleEntry ('rrtp'). The addtionaldata[] of each sample entry of a SRTP reception hint track shall contain exactly one ReceivedSsrcBox.

Additionally, the additionaldata[] may contain the ReceivedCryptoContextIdBox and the RolloverCounterBox defined below. Furthermore, an SRTPProcessBox shall also be included as one of the additionaldata boxes. As the content is stored encrypted, the integrity and the encryption algorithm fields in the SRTP Process box specify the algorithm that was applied to the received stream. An entry of four spaces ($20$20$20$20) may be used to indicate that the algorithm is defined by means outside the scope of this document.

##### Received cryptographic context ID box

Zero or one ReceivedCryptoContextIdBox, identified with the four-character code 'ccid', may be present in the additionaldata of a sample descriptor entry of an SRTP reception hint track. Information to recover the cryptographic context for the received SRTP stream may be stored here.

aligned(8) class ReceivedCryptoContextIdBox extends Box ('ccid')   
{  
 unsigned int(16) destPort;  
 unsigned int(8) ip\_version;  
 switch (ip\_version) {  
 case 4: // IPv4  
 unsigned int(32) destIP;  
 break;  
 case 6: // IPv6  
 unsigned int(64) destIP;  
 break;  
 }  
}

The destPort and destIP parameters contain the port number and the IP address (as present in the received IPv4 or IPv6 packages), respectively, of the SRTP session via which the recorded SRTP packets were received. ip\_version contains either 4 or 6 representing IPv4 or IPv6, respectively.

##### Rollover counter box

Zero or one RolloverCounterBox, identified with the four-character code 'sroc', may be present in the additionaldata of a sample descriptor entry of an SRTP reception hint track. Typically, the rollover counter value changes every 65536 SRTP package.

aligned(8) class RolloverCounterBox extends Box ('sroc') {  
 unsigned int(32) rollover\_counter;  
 }

The rollover\_counter is a non-zero integer that gives the value of the ROC field for all associated received SRTP packets.

NOTE The rollover counter (ROC) is an element of the cryptographic context of a SRTP stream and depends on the absolute position of a packet in an RTP stream. Knowledge of the ROC value is necessary in order to decrypt a received SRTP packet. It is optional to use the RolloverCounterBox as IETF RFC 4771[22] defines as an optional mechanism to signal the ROC value explicitly in the authentication tag of a SRTP package.

#### Sample and packet entry format

Both, sample format and packet entry format for SRTP reception hint tracks are identical to those of RTP reception hint tracks, defined in 9.4.1.3 and 9.4.1.4. The packet payload is stored as received in the SRTP packets, i.e., all information received in the SRTP packet excluding the header or, in other words, the encrypted payload together with the key identifier (MKI) and the authentication tag.

If the value of CSRC\_count is not equal to zero for a received SRTP packet, the extra\_data\_tlv corresponding to this receivedSRTPpacket shall contain exactly one receivedCSRC box.

### SRTCP reception hint tracks

#### Overview

When reception hint tracks are used to store secure real-time control protocol (SRTCP) streams, as defined in IETF RFC 3711, the formats in this subclause shall be used.

SRTCP is used for real-time transport of control information for a SRTP session over the Internet Protocol. SRTCP takes for SRTP the role that RTCP takes for RTP, in comparison to 9.4.2. During streaming, each SRTP stream typically has an accompanying SRTCP stream that carries control information for the SRTP stream. One SRTCP reception hint track carries one SRTCP stream and is associated to the corresponding SRTP reception hint track through a track reference.

The format of the SRTCP reception hint tracks allows the storage of SRTCP Packets in the hint samples, e.g. of SRTCP Sender Reports.

The SRTCP Sender Reports are of particular interest for stream recording, because they reflect the current status of the server, e.g. the relationship of the media timing (SRTP timestamp of audio/video packets) to the server time (absolute time in NTP format). Knowledge of this relationship is also necessary for playback of recorded SRTP reception hint tracks in order to be able to detect and correct clock drift and jitter.

The timestampsynchrony box as specified in 9.4.1.2 makes it possible to correct clock drift and jitter before playing a file, and therefore recording of SRTCP streams is optional.

There is no server hint track equivalent for the SRCTP reception hint track, since SRTCP messages are generated on-the-fly during transmission.

#### General

There shall be zero or one SRTCP reception hint track for each SRTP reception hint track. An SRTCP reception hint track shall contain a TrackReferenceBox including a reference of type 'cdsc' to the associated SRTP reception hint track.

When i is the sample number a sample, the sample time DT(i) as specified in 8.6.1.2 indicates the reception time of the packet. The clock source for the reception time shall be the same as for the associated SRTP reception hint track. The value of timescale in the MediaHeaderBox of an SRTCP reception hint track shall be equal to the value of timescale in the MediaHeaderBox of the associated SRTP reception hint track.

#### Sample entry format

The entry-format in the sample entry for the SRTCP reception hint tracks is 'stcp'. It is otherwise identical in structure to the sample entry format for RTCP. The encryption and authentication method of the SRTCP hint tracks are defined by the respective entries in SRTPProcessBox of the corresponding SRTP hint track.

NOTE An equivalent to the ROC boxes defined for SRTP is not necessary for SRTCP, as the SRTCP packet contains an explicitly signalled initialization vector.

#### Sample format

Sample format is the sample format for RTCP reception hint tracks as defined in 9.4.2.4.

### Protected RTP reception hint track

#### Overview

This document defines a mechanism for marking media streams as protected. This works by changing the four character code of the SampleEntry, and appending boxes containing both details of the protection mechanism and the original four character code. However, in this case the track is not protected; it is an ‘in the clear’ hint track which contains protected data. This subclause describes the how reception hint tracks should be marked as carrying protected data, using a similar mechanism, and utilizing the same boxes.

#### Syntax

Class ProtectedRtpReceptionHintSampleEntry  
 extends RtpReceptionHintSampleEntry ('prtp')   
{  
 ProtectionSchemeInfoBox SchemeInformation;  
}

#### Semantics

The ProtectionSchemeInfoBox shall contain details of the protection scheme applied. This shall include the OriginalFormatBox which shall contain the four character code 'rrtp' (the four character code of the original ReceivedRtpHintSampleEntry).

### Recording procedure

See Annex H.

### Parsing procedure

See Annex H.

# Sample groups

## Random access recovery points

* + 1. Definition

In some coding systems it is possible to random access into a stream and achieve correct decoding after having decoded a number of samples. This is known as gradual decoding refresh. For example, in video, the encoder might encode intra-coded macroblocks in the stream, such that it knows that within a certain period the entire picture consists of pixels that are only dependent on intra-coded macroblocks supplied during that period.

Samples for which such gradual refresh is possible are marked by being a member of one of these groups. The definition of the groups allows the marking to occur at either the beginning of the period or the end. However, when used with a particular media type, the usage of these groups may be restricted to marking only one end (i.e. restricted to only positive or negative roll values). A roll-group is defined as that group of samples having the same roll distance.

The roll groups have the following semantics.

A VisualRollRecoveryEntry documents samples that enable entry points into streams that are alternatives to sync samples.

An AudioRollRecoveryEntry documents the pre-roll distance required in audio streams in which every sample can be independently decoded, but the decoder output is only assured to be correct after pre-rolling by the indicated number of samples.

An AudioPreRollEntry documents samples that enable entry points into streams that are independently decodable and are thus alternatives to sync samples. It should be used with audio streams in which not every sample can be independently decoded; decoding can only start at an independently decodable sample and decoder output is only assured to be correct after pre-rolling by the indicated number of samples.

The roll\_distance shall be a positive value. Decoding starts at a member sample, but decoder output is only assured to be correct after decoding the indicated number of samples.

* + 1. Syntax

class VisualRollRecoveryEntry() extends VisualSampleGroupEntry ('roll')  
{  
 signed int(16) roll\_distance;  
}

class AudioRollRecoveryEntry() extends AudioSampleGroupEntry ('roll')  
{  
 signed int(16) roll\_distance;  
}

class AudioPreRollEntry() extends AudioSampleGroupEntry ('prol')  
{  
 signed int(16) roll\_distance;  
}


* + 1. Semantics

roll\_distance is a signed integer that gives the number of samples that need to be decoded in order for a sample to be decoded correctly. A positive value indicates the number of samples after the sample that is a group member that need to be decoded such that at the last of these recovery is complete, i.e. the last sample is correct. A negative value indicates the number of samples before the sample that is a group member that need to be decoded in order for recovery to be complete at the marked sample. The value zero shall not be used; the samples with zero roll\_distance can be signalled by other signaling mechanisms such as the sync sample information, the 'rap ' sample grouping and the 'sap ' sample grouping.

## Rate share groups

### Overview

Rate share instructions are used by players and streaming servers to help allocating bitrates dynamically when several streams share a common bandwidth resource. The instructions are stored in the file as sample group description entries and apply when scalable or alternative media streams at different bitrates are combined with other scalable or alternative tracks. The instructions are time-dependent as samples in a track may be associated with different sample group description entries. In the simplest case, only one target rate share value is specified per media and time range as illustrated in Figure 2.



**Key**

t Time

R Audio/Video Rate Share (%)


V Video

A Audio

*i* interval where higher audio rate is required

Figure 2 — Audio/Video rate share as function of time

In order to accommodate for rate share values that vary with the available bitrate, it is possible to specify more than one operation range. One may for instance indicate that audio requires a higher percentage (than video) at low available bitrates. Technically this is done by specifying two operation points as shown in Figure 3.



**Key**

BR Available bitrate

R Audio Rate Share (%)

A region where higher audio rate is required

B region where lower audio rate is required

OP1 operation point 1

OP2 operation point 2

Figure 3 — Audio rate share as function of available bitrate

Operation points are defined in terms of total available bandwidth. For more complex situations it is possible to specify more operation points.

In addition to target rate share values, it is also possible to specify maximum and minimum bitrates for a certain media, as well as discard priority.

### Rate share sample group description entry

* + - 1. Definition

Each sample of a track may be associated to (zero or) one of a number of sample group descriptions, each of which defines a record of rate-share information. Typically the same rate-share information applies to many consecutive samples and it may therefore be enough to define two or three sample group descriptions that can be used at different time intervals.

The grouping\_type 'rash' (short for rate share) is defined as the grouping criterion for rate share information. Zero or one SampleToGroupBoxes for the grouping\_type 'rash' can be contained in the SampleTableBox of a track. It shall reside in a hint track, if a hint track is used, otherwise in a media track.

Target rate share may be specified for several operation points that are defined in terms of the total available bitrate, i.e., the bitrate that should be shared. If only one operation point is defined, the target rate share applies to all available bitrates. If several operation points are defined, then each operation point specifies a target rate share. Target rate share values specified for the first and the last operation points also specify the target rate share values at lower and higher available bitrates, respectively. The target rate share between two operation points is specified to be in the range between the target rate shares of those operation points. One possibility is to estimate with linear interpolation.

* + - 1. Syntax

class RateShareEntry() extends SampleGroupDescriptionEntry('rash')   
{  
 unsigned int(16) operation\_point\_count;  
 if (operation\_point\_count == 1) {  
 unsigned int(16) target\_rate\_share;  
 }  
 else {  
 for (i=0; i < operation\_point\_count; i++) {  
 unsigned int(32) available\_bitrate;  
 unsigned int(16) target\_rate\_share;  
 }  
 }  
 unsigned int(32) maximum\_bitrate;  
 unsigned int(32) minimum\_bitrate;  
 unsigned int(8) discard\_priority;  
}

* + - 1. Semantics

operation\_point\_count is a non-zero integer that gives the number of operation points.

available\_bitrate is a positive integer that defines an operation point (in kilobits per second). It is the total available bitrate that can be allocated in shares to tracks. Each entry shall be greater than the previous entry.

target\_rate\_share is an integer. A non-zero value indicates the percentage of available bandwidth that should be allocated to the media for each operation point. The value of the first (last) operation point applies to lower (higher) available bitrates than the operation point itself. The target rate share between operation points is bounded by the target rate shares of the corresponding operation points. A zero value indicates that no information on the preferred rate share percentage is provided.

maximum\_bitrate is an integer. A nonzero value indicates (in kilobits per second) an upper threshold for which bandwidth should be allocated to the media. A higher bitrate than maximum bitrate should only be allocated if all other media in the session has fulfilled their quotas for target rate-share and maximum bitrate, respectively. A zero value indicates that no information on maximum bitrate is provided.

minimum\_bitrate is an integer. A nonzero value indicates (in kilobits per second) a lower threshold for which bandwidth should be allocated to the media. If the allocated bandwidth corresponds to a smaller value, then no bitrate should be allocated. Instead preference should be given to other media in the session or alternate encodings of the same media. Zero minimum bitrate indicates that no information on minimum bitrate is provided.

discard\_priority is an integer indicating the priority of the track when tracks are discarded to meet the constraints set by target rate share, maximum bitrate and minimum bitrate. Tracks are discarded in discard priority order and the track that has the highest discard priority value is discarded first.

### Relationship between tracks

The purpose of defining rate share information is to aid a server or player extracting data from a track in combination with other tracks. Note that a server/player streams/plays tracks simultaneously if they belong to different alternate groups and can switch between tracks that belong to the same switch group within an alternate group. By default, all tracks are served/played simultaneously if no alternate groups are defined.

Rate share information should be provided for each track. A track that does not include rate share information has one operation point and can be treated as a constant-bitrate track with discard priority 128. Target rate share, minimum and maximum bitrates do not apply in this case.

Tracks that are alternates to each other shall (at each instance of time) define the same number of operation points at the same set of total available bitrates and have the same discard priorities. Note that the number and definition of operation points may depend on time. Alternate tracks may have different target rate shares, minimum and maximum bitrates.

### Bitrate allocation

Rate share information on maximum bitrate, minimum bitrate, and target rate share can be combined for a track. If this is the case, the target rate share shall be applied to find an allocated bitrate before the impact of the maximum and minimum bitrates is considered.

When allocating bandwidth to several tracks, the following considerations apply:

1. In the case all tracks have explicit target rate share values and they don’t sum up to 100 per cent, treat them as weights, i.e., normalize them.
2. The total allocation shall not exceed total available bitrate.
3. In a choice between alternate tracks, the chosen track should be the track that causes the alternate group to have an allocation most closely in accord with its target rate share, or the track that desires the highest bitrate that can be allocated without discarding other tracks (see below).
4. Tracks must have an allocation between their minimum and maximum bitrates, or be discarded.
5. Tracks should have an allocation in accord with their target rate shares, but this may be distorted to allow some tracks to achieve their minima, or in case some have reached their maxima.
6. If an allocation cannot be done including a track from every alternate group, then tracks should be discarded in discard priority order.
7. The allocation must be re-calculated whenever the operating set for an active track (one that has been selected from an alternate group) changes or the available bitrate changes.

## Alternative startup sequences

* + 1. Definition

An alternative startup sequence contains a subset of samples of a track within a certain period starting from a sync sample or a sample marked by 'rap ' sample grouping, which are collectively referred to as the initial sample below. By decoding this subset of samples, the rendering of the samples can be started earlier than in the case when all samples are decoded.

An 'alst' sample group description entry indicates the number of samples in any of the respective alternative startup sequences, after which all samples should be processed.

Either version 0 or version 1 of the SampleToGroupBox may be used with the alternative startup sequence sample grouping. If version 1 of the SampleToGroupBox is used, the same algorithm to derive alternative startup sequences should be used consistently for a particular value of grouping\_type\_parameter.

A player utilizing alternative startup sequences can operate as follows. First, an initial sync sample from which to start decoding is identified by using the SyncSampleBox, the sample\_is\_non\_sync\_sample flag for samples enclosed in track fragments, or the 'rap ' sample grouping. Then, if the initial sync sample is associated to a sample group description entry of type 'alst' where roll\_count is greater than 0, the player can use the alternative startup sequence. The player then decodes only those samples that are mapped to the alternative startup sequence until the number of samples that have been decoded is equal to roll\_count. After that, all samples are decoded.

* + 1. Syntax

class AlternativeStartupEntry() extends VisualSampleGroupEntry ('alst')  
{  
 unsigned int(16) roll\_count;  
 unsigned int(16) first\_output\_sample;  
 for (i=1; i <= roll\_count; i++)  
 unsigned int(32) sample\_offset[[i]];  
 j=1;  
 do { // optional, until the end of the structure  
 unsigned int(16) num\_output\_samples[[j]];  
 unsigned int(16) num\_total\_samples[[j]];  
 j++;  
 }  
}

* + 1. Semantics

roll\_count indicates the number of samples in the alternative startup sequence. If roll\_count is equal to 0, the associated sample does not belong to any alternative startup sequence and the semantics of first\_output\_sample are unspecified. The number of samples mapped to this sample group description entry per one alternative startup sequence shall be equal to roll\_count.

first\_output\_sample indicates the index of the first sample intended for output among the samples in the alternative startup sequence. The index of the sync initial sample starting the alternative startup sequence is 1, and the index is incremented by 1, in decoding order, per each sample in the alternative startup sequence.


sample\_offset[i] indicates the decoding time delta of the i-th sample in the alternative startup sequence relative to the regular decoding time of the sample derived from the TimeToSampleBox or the TrackFragmentHeaderBox. The sync initial sample starting the alternative startup sequence is its first sample.

num\_output\_samples[j] and num\_total\_samples[j] indicate the sample output rate within the alternative startup sequence. The alternative startup sequence is divided into k consecutive pieces, where each piece has a constant sample output rate which is unequal to that of the adjacent pieces. The first piece starts from the sample indicated by first\_output\_sample. num\_output\_samples[j] indicates the number of the output samples of the j-th piece of the alternative startup sequence. num\_total\_samples[j] indicates the total number of samples, including those that are not in the alternative startup sequence, from the first sample in the j-th piece that is output to the earlier one (in composition order) of the sample that ends the alternative startup sequence and the sample that immediately precedes the first output sample of the (j+1)th piece.

* + 1. Examples

Hierarchical temporal scalability (e.g. in AVC and SVC) improves compression efficiency but increases the decoding delay due to reordering of the decoded pictures from the (de)coding order to composition order. When the temporal hierarchy is deep and the operation speed of the decoder is limited (to no faster than real-time processing), the initial delay from the start of the decoding to the start of rendering is substantial and may affect the end-user experience negatively.

Figure 4 illustrates a typical hierarchically scalable bitstream with five temporal levels. Figure 4a shows the example sequence in composition order. Values enclosed in boxes indicate the frame\_num value of the picture. Values in italics indicate a non-reference picture while the other pictures are reference pictures. Figure 4b shows the example sequence in decoding order. Figure 4c shows the example sequence in composition order when assuming that the composition timeline coincides with that of the decoding timeline and the decoding of one picture lasts one picture interval. It can be seen that playback of the stream starts five picture intervals later than the decoding of the stream started. If the pictures were sampled at 25 Hz, the picture interval is 40 msec, and the playback is delayed by 0.2 sec.



**Key**

1. Example sequence in output order
2. Example sequence in decoding order
3. Example sequence at decoder output (delay outout order)


Horizontal grid denotes picture intervals, vertical grid denotes temporal level

Boxes denote frames with their respective frame numbers, where bold numbers are reference pictures and italic numbers are non-reference pictures

Figure 4 — Decoded picture buffering delay of an example sequence with five temporal levels

Thanks to the temporal hierarchy, it is possible to decode only a subset of the pictures at the beginning of the sequence. Consequently, rendering can be started faster but the displayed picture rate is lower at the beginning. In other words, a player can make a trade-off between the duration of the initial startup delay and the initial displayed picture rate. Figure 5 and Figure 6 show two examples of alternative startup sequences where a subset of the bitstream of Figure 4 is decoded.

The samples selected for decoding and the decoder output are presented in Figure 5a and Figure 5b, respectively. The reference picture having frame\_num equal to 4 and the non-reference pictures having frame\_num equal to 5 are not decoded. In this example, the rendering of pictures starts four picture intervals earlier than in Figure 4. When the picture rate is 25 Hz, the saving in startup delay is 160 msec. The saving in the startup delay comes with the disadvantage of a lower displayed picture rate at the beginning of the bitstream.




**Key**

1. Processing of the example sequence
2. Example sequence at decoder output

Figure 5 — An example of an alternative startup sequence

In the example of Figure 6, another way of selecting the pictures for decoding is presented. The decoding of the pictures that depend on the picture with frame\_num equal to 3 is omitted and the decoding of non-reference pictures within the second half of the first group of pictures is omitted too. The decoded picture resulting from the sample with frame\_num equal to 2 is the first one that is output. As a result, the output picture rate of the first group of pictures is half of normal picture rate, but the display process starts two frame intervals (80 msec in 25 Hz picture rate) earlier than in the conventional solution illustrated in Figure 4.



**Key**

1. Processing of the example sequence
2. Example sequence at decoder output

Figure 6 — Another example of an alternative startup sequence

## Random access point (RAP) sample group

* + 1. Definition

Open random-access points can be marked by being a member of this group. Samples marked by this group shall be random access points, and may also be sync points (i.e. it is not required that samples marked by the sync sample information be excluded).

* + 1. Syntax

class VisualRandomAccessEntry() extends VisualSampleGroupEntry ('rap ')  
{  
 unsigned int(1) num\_leading\_samples\_known;  
 unsigned int(7) num\_leading\_samples;  
}

* + 1. Semantics

num\_leading\_samples\_known equal to 1 indicates that the number of leading samples is known for each sample in this group, and the number is specified by num\_leading\_samples.

num\_leading\_samples specifies the number of leading samples for each sample in this group. When num\_leading\_samples\_known is equal to 0, this field should be ignored.

## Temporal level sample group

* + 1. Definition

Many video codecs support temporal scalability where it is possible to extract one or more subsets of frames that can be independently decoded. A simple case is the extraction of I frames for a bitstream with a regular I-frame interval, e.g,, IPPPIPPP…, where every 4th picture is an I frame. Also subsets of these I frames can be extracted for even lower frame rates. More elaborate situations with several temporal levels can be constructed using hierarchical B or P frames.

The temporal level sample grouping ('tele') provides a codec-independent sample grouping that can be used to group samples in a track (and potential track fragments) according to temporal level, where samples of one temporal level have no coding dependencies on samples of higher temporal levels. The temporal level equals the sample group description index (taking values 1, 2, 3, etc). The bitstream containing only the samples from the first temporal level to a higher temporal level remains conforming to the coding standard.

A grouping according to temporal level facilitates easy extraction of temporal subsequences, for instance using the SubsegmentIndexBox in 8.16.4.

* + 1. Syntax

class TemporalLevelEntry() extends VisualSampleGroupEntry('tele')  
{  
 bit(1) level\_independently\_decodable;  
 bit(7) reserved=0;  
}

* + 1. Semantics

The temporal level of samples in a sample group equals to the sample group description index.

level\_independently\_decodable is a flag. 1 indicates that all samples of this level have no coding dependencies on samples of other levels. 0 indicates that no information is provided.

## Stream access point sample group

* + 1. Definition

A stream access point, as defined in Annex I, enables random access into a container of media stream(s). The SAP sample grouping identifies samples (the first byte of which is the position ISAU for a SAP as specified in Annex I) as being of the indicated SAP type.

The syntax and semantics of grouping\_type\_parameter are specified as follows.

{  
 unsigned int(28) target\_layers;  
 unsigned int(4) layer\_id\_method\_idc;  
}

target\_layers specifies the target layers for the indicated SAPs according to Annex I. The semantics of target\_layers depends on the value of layer\_id\_method\_idc. When layer\_id\_method\_idc is equal to 0, target\_layers is reserved.

layer\_id\_method\_idc specifies the semantics of target\_layers. layer\_id\_method\_idc equal to 0 specifies that the target layers consist of all the layers represented by the track. layer\_id\_method\_idc not equal to 0 is specified by derived media format specifications.

* + 1. Syntax

class SAPEntry() extends SampleGroupDescriptionEntry('sap ')  
{  
 unsigned int(1) dependent\_flag;  
 unsigned int(3) reserved;  
 unsigned int(4) SAP\_type;  
}

* + 1. Semantics

reserved shall be equal to 0. Parsers shall allow and ignore all values of reserved.

dependent\_flag shall be 0 for non-layered media. dependent\_flag equal to 1 specifies that the reference layers, if any, for predicting the target layers may have to be decoded for accessing a sample of this sample group. dependent\_flag equal to 0 specifies that the reference layers, if any, for predicting the target layers need not be decoded for accessing any SAP of this sample group.

sap\_type values equal to 0 and 7 are reserved; sap\_type values in the range of 1 to 6, inclusive, specify the SAP type, as specified in Annex I, of the associated samples (for which the first byte of a sample in this group is the position ISAU).

## Sample-to-item sample group

* + 1. Definition

Samples of a track can be linked to one or more metadata items using the sample-to-item sample grouping. The MetaBox containing the referred items is resolved as specified in the semantics below.

The sample-to-item sample grouping is allowed for any types of tracks, and its syntax and semantics are unchanged regardless of the track handler type.

In the absence of this sample group, the entire track-level MetaBox, if any, is applicable to every sample.

* + 1. Syntax

class SampleToMetadataItemEntry()   
 extends SampleGroupDescriptionEntry('stmi')   
{  
 unsigned int(32) meta\_box\_handler\_type;  
 unsigned int(32) num\_items;  
 for (i = 0; i < num\_items; i++) {  
 unsigned int(32) item\_id[[i]];  
 }  
}

* + 1. Semantics

meta\_box\_handler\_type informs about the type of metadata schema used by the MetaBox which is referenced by the items in this sample group. When there are multiple MetaBoxes with the same handler types, the MetaBox referred to in this sample group description entry is the first MetaBox fulfilling one of the following ordered constraints:

* A MetaBox included in the current track, with handler\_type equal to meta\_box\_handler\_type.
* A MetaBox included in MovieBox, with handler\_type equal to meta\_box\_handler\_type.
* A MetaBox included in the root level of the file, with handler\_type equal to meta\_box\_handler\_type.

num\_items counts the number of items referenced by this sample group.

item\_id[i] specifies the item\_ID value of an item that applies to or is valid for the sample mapped to this sample group description entry.

## Dependent random access point (DRAP) sample group

* + 1. Definition

The DRAP sample group documents some or all of the DRAP samples in a track. A dependent random access point (DRAP) sample is a sample after which all samples in decoding order and in output order can be correctly decoded if the closest SAP sample of type 1, 2, or 3 preceding the DRAP sample is available for reference..

NOTE 1 The closest SAP sample can be a sync sample or marked by the SAP sample group.

NOTE 2 DRAP samples can only be used in combination with SAP samples of type 1, 2 and 3. This is in order to enable the functionality of creating a decodable sequence of samples by concatenating the preceding SAP sample with the DRAP sample and the samples following the DRAP sample decoding order and in output order

The following applies for any DRAP sample sampleA that is mapped to a DRAP sample group:

* Let sampleSeq be a sequence of samples consisting of the following samples in the order listed below:
  + the closest preceding SAP sample of type 1, 2, or 3,
  + sampleA, and
  + all samples following sampleA in both decoding and output order in the track.
* For each sample sampleB in sampleSeq, all data needed for processing sampleB shall be accessible in the referenced sample entry, in sampleB itself, or in any sample that precedes sampleB in decoding order and is present in sampleSeq.

NOTE 3 For some video codecs, all data needed for processing a sample sampleB includes parameter sets needed for decoding sampleB.

* + 1. Syntax

class VisualDRAPEntry() extends VisualSampleGroupEntry('drap')   
{  
 unsigned int(3) DRAP\_type;  
 unsigned int(29) reserved = 0;  
}

* + 1. Semantics

DRAP\_type is a non-negative integer. When DRAP\_type is in the range of 1 to 3, it indicates the SAP\_type (as specified in Annex I) of a sample that is othewise like the DRAP sample but does depend on the closest preceding SAP. Other type values are reserved.

reserved shall be equal to 0. The semantics of this subclause only apply to sample group description entries with reserved equal to 0. Parsers shall allow and ignore sample group description entries with reserved greater than 0 when parsing this sample group.

## Pixel Aspect Ratio Sample Grouping

* + 1. Definition

The Pixel Aspect Ratio sample group ('pasr') may be used to signal the pixel aspect ratio of samples in a video track, when the pixel aspect ratio of the samples within a track change dynamically and a single value in a PixelAspectRatioBox in a sample entry, specified in 12.1.4 cannot therefore be used.

When the Pixel Aspect Ratio sample group is used in a track, the PixelAspectRatioBox shall not be present in any sample entry of that track.

* + 1. Syntax

class PixelAspectRatioEntry() extends VisualSampleGroupEntry ('pasr')  
{  
 unsigned int(32) hSpacing;  
 unsigned int(32) vSpacing;  
}

* + 1. Semantics

hSpacing, vSpacing: define the relative width and height of a pixel as defined for the PixelAspectRatioBox in 12.1.4

## Clean Aperture Sample Grouping

* + 1. Definition

The Clean Aperture sample group ('casg') may be used to signal the clean aperture of samples in a video track, when the clean aperture of the samples within a track change dynamically and a single value in a CleanApertureBox in a sample entry, specified in 12.1.4 cannot therefore be used.

When the Clean Aperture sample group is used in a track, the CleanApertureBox shall not be present in any sample entry of that track.

* + 1. Syntax

class CleanApertureEntry() extends VisualSampleGroupEntry ('casg')  
{  
 signed int(32) cleanApertureWidthN;  
 signed int(32) cleanApertureWidthD;  
  
 signed int(32) cleanApertureHeightN;  
 signed int(32) cleanApertureHeightD;  
  
 signed int(32) horizOffN;  
 signed int(32) horizOffD;  
  
 signed int(32) vertOffN;  
 signed int(32) vertOffD;  
}

* + 1. Semantics

cleanApertureWidthN, cleanApertureWidthD, cleanApertureHeightN, cleanApertureHeightD, horizOffN, horizOffD, vertOffN and vertOffD define the clean aperture width, height and horizontal and vertical offsets of the clean aperture center as defined for the CleanApertureBox in 12.1.4

## 10.11 EDRAP sample group

### 10.11.1 Definition

The EDRAP sample group documents some or all of the EDRAP samples in a track. This sample group is similar to the DRAP sample group as specified in subclause 10.8; however, it enables signalling additional samples that can also be used for random access that have more flexible dependencies.

NOTE 1 A DRAP sample is always an EDRAP sample.

The following applies for any EDRAP sample sampleA that is mapped to an EDRAP sample group:

* Let sampleSeq be a sequence of samples consisting of the following samples in the order of the bullets below:
  + the SAP or EDRAP samples identified by ref\_sap\_or\_edrap\_idx\_delta[i] for i in the range of 0 to num\_ref\_sap\_or\_edrap\_samples\_minus1, inclusive, in decoding order,
  + sampleA, and
  + all samples following sampleA in both decoding and output order in the track.
* For each sample sampleB in sampleSeq, all data needed for processing sampleB shall be accessible in the referenced sample entry, in sampleB itself, or in any sample that precedes sampleB in decoding order and is present in sampleSeq.

NOTE 2 For some video codecs, all data needed for processing a sample sampleB includes parameter sets needed for decoding sampleB.

### 10.11.2 Syntax

class VisualEdrapEntry() extends VisualSampleGroupEntry('edrp')   
{  
 unsigned int(3) edrap\_type;  
 unsigned int(3) num\_ref\_sap\_or\_edrap\_samples\_minus1;  
 unsigned int(2) reserved = 0;  
 for (i=0; i<=num\_ref\_sap\_or\_edrap\_samples\_minus1; i++) {  
 unsigned int(16) ref\_sap\_or\_edrap\_idx\_delta[[i]];  
 }  
}

### 10.11.3 Semantics

edrap\_type is a non-negative integer. When edrap\_type is in the range of 1 to 3 it indicates the SAP\_type (as specified in Annex I) of a sample that is othewise like the EDRAP sample but does depend on the closest preceding SAP or other EDRAP samples. Other values of edrap\_type are reserved.

NOTE 1 An EDRAP sample and all the subsequent samples in the same track may depend on the closest preceding SAP and/or some preceding EDRAP samples and does not depend on any other samples preceding the EDRAP sample. Therefore, if the encoder chooses to encode an EDRAP sample such that it does not depend on the closest preceding SAP or any preceding EDRAP sample, then the EDRAP sample becomes a SAP.

num\_ref\_sap\_or\_edrap\_samples\_minus1 plus 1 indicates the number of samples in the required preceding SAP or EDRAP samples as defined in subclause 3.1.7, which are earlier in decoding order than the EDRAP sample and are needed for reference to be able to correctly decode the EDRAP sample and all samples following the EDRAP sample in both decoding and output order when starting decoding from the EDRAP sample.

NOTE 2 For an EDRAP sample that is also a DRAP sample, the value of num\_ref\_sap\_or)edrap\_samples\_minus1 is equal to 0.

reserved shall be equal to 0. The semantics of this subclause only apply to sample group description entries with reserved equal to 0. Parsers shall ignore sample group description entries when reserved is greater than 0.

ref\_sap\_or\_edrap\_idx\_delta[i] indicates the i-th required preceding SAP or EDRAP sample of the current EDRAP sample. Let the list of SAP or EDRAP samples associated with a SAP sample of type 1, 2 or 3 be the SAP sample and all the EDRAP samples following the SAP sample and preceding the next SAP sample, when present. The SAP\_or\_EDRAP sample index is defined as the index to this list of SAP or EDRAP samples. The value of ref\_sap\_or\_edrap\_idx\_delta[i] is equal to the difference between the SAP\_or\_EDRAP sample index of the current EDRAP sample and the SAP\_or\_EDRAP sample index of the i-th required preceding SAP or EDRAP sample. The value 1 indicates that the i-th required SAP or EDRAP sample is the last SAP or EDRAP sample preceding this EDRAP sample in decoding order, the value 2 indicates that the i-th required SAP or EDRAP sample is the second last EDRAP sample preceding this EDRAP sample in decoding order, and so on.

## 10.12 Essential descriptions hierarchy sample grouping

### 10.12.1 Definition

When an essential sample group (i.e., a sample group for which the version of the SampleGroupDescriptionBox is equal to 3), which describes essential information for the associated samples, is used, parsers can only attempt to process tracks for which there are no unrecognized sample group descriptions marked as essential.

The essential descriptions hierarchy sample group ('esgh') indicates the processing order of the essential sample group descriptions or reserved transformation values applying to a given sample. This sample group description is an essential sample group description and shall use version 3 of the SampleGroupDescriptionBox. It shall be present if at least one essential sample group description with grouping\_type other than 'esgh' is present.

Each essential sample group description, except the essential descriptions hierarchy sample group itself, shall be listed in the EssentialDescriptionsHierarchyEntry.

The grouping\_type\_paramater for an essential descriptions hierarchy sample group description is not defined, and its value shall be set to 0.

The syntax of EssentialDescriptionsHierarchyEntry is the same for all media types.

Samples associated with essential sample groups shall use a restricted sample entry indicating the original media type (e.g. 'resv', 'resa') with a scheme\_type equal to 'essg'. The original sample entry type prior to any transformation is stored within an OriginalFormatBox contained in the RestrictedSchemeInfoBox.

For a restricted sample entry with a scheme\_type equal to 'essg', the following applies:

* The restricted sample entry shall contain a single RestrictedSchemeInfoBox (with a scheme\_type equal to 'essg').
* The payload of the SchemeInformationBox consists of zero or more RestrictedSchemeInfoBox containing no OriginalFormatBox, with at most one occurrence of a given scheme\_type.
* The payload of the SchemeInformationBox of the 'essg' transformation shall not contain a RestrictedSchemeInfoBox with scheme\_type equal to 'essg'.

The transformations given in sample\_group\_description\_type are listed in the order in which a file reader shall apply each transformation: any sample processing described by a sample group of type sample\_group\_description\_type[i] shall be applied before any sample processing described by a sample group of type sample\_group\_description\_type[i+1].

When a sample mapped to an essential descriptions hierarchy sample group description entry, with sample\_group\_description\_type [*SG1* … *SGN*], is not mapped to a sample group description with grouping\_type *SGi* or doesn’t contain a ProtectionSchemeInfoBox or a RestrictedSchemeInfoBox with a scheme\_type equal to *SGi*, the processing described by *SGi* is ignored for this sample.

In the sample\_group\_description\_type list, the following transformation values are allowed:

* 'stsd' : indicates the position of the decoding process in the transformation chain.
* 'cenc' : indicates the position of the content protection removal in the transformation chain. The content protection removal information is provided by the ProtectionSchemeInfoBox that shall be present in the protected sample entry associated with the sample mapped to this sample group.
* Any scheme\_type value contained in the SchemeTypeBox of a RestrictedSchemeInfoBox contained in the SchemeInformationBox of a RestrictedSchemeInfoBox with the scheme\_type 'essg' of the restricted sample entry associated with sample(s) mapped to this sample group; this indicates the position of the corresponding restricted media transformation in the transformation chain.
* Any grouping\_type of an essential sample group description describing a sample processing applying to a sample mapped to this sample group description entry; this indicates the position of the corresponding transformation in the transformation chain.

If 'stsd' is absent from the list of sample\_group\_description\_type, all listed transformations shall apply to decoded samples. If 'cenc' is present in the list, 'stsd' shall be present.

### 10.12.2 Syntax

class EssentialDescriptionsHierarchyEntry ()  
 extends SampleGroupDescriptionEntry ('esgh')  
{  
 unsigned int(32) num\_groupings;  
 unsigned int(32) sample\_group\_description\_type[num\_groupings];  
}

### 10.12.3 Semantics

num\_groupings indicates the number of essential sample group description types listed.

sample\_group\_description\_type[] provides a list of the four-character code values of grouping\_type of the essential sample group descriptions (i.e. with the version field equal to 3) or reserved transformation values applying to the associated samples. Four-character code values of grouping\_type of non-essential sample group descriptions shall not be present in this list.

# Derived file formats

This document may be used as the basis of a specific file format for a restricted purpose: for example, the MP4 file format for MPEG-4 and the Motion JPEG 2000 file format are both derived from it. When a derived specification is written, the following must be specified:

* The name of the new format, and its brand and compatibility types for the FileTypeBox. Generally a new file extension will be used, a new MIME type, and Macintosh file type also, though the definition and registration of these are outside the scope of this document.
* Any template fields used must be explicitly declared; their use must be conformant with this document.
* The exact codingname and protocol identifiers as used in a SampleEntry must be defined. The format of the samples that these code points identify must also be defined. However, it may be preferable to fit the new coding systems into an existing framework (e.g. the MPEG-4 systems framework), than to define new coding points at this level. For example, a new audio format can use a new codingname, or can use 'mp4a' and register new identifiers within the MPEG-4 audio framework.

New boxes may be defined, though this is discouraged.

If the derived specification needs a new track type other than those defined here or registered, then a new handler-type must be registered. The media header required for this track must be identified. If it is a new box, it must be defined and its box type registered. In general, it is expected that most systems can use existing track types.

Any new track reference types should be registered and defined.

The sample entry may be extended with optional or required boxes. The usual syntax for doing this is to define a new box with a specific name, extending (for example) VisualSampleEntry, and containing new boxes.

# Media-specific definitions

## Video media

### Media handler

Video media uses the 'vide' handler type in the HandlerBox of the MediaBox, as defined in 8.4.3.

Auxiliary video media uses the 'auxv' handler type in the HandlerBox of the MediaBox, as defined in 8.4.3.

An auxiliary video track is coded the same as a video track, but uses this different handler type, and is not intended to be visually displayed (e.g. it contains depth information, or other monochrome or color two-dimensional information). Auxiliary video tracks are usually linked to a video track by an appropriate track reference.

### Video media header

#### Definition

Box Types: 'vmhd'  
Container: MediaInformationBox  
Mandatory: Yes  
Quantity: Exactly one

Video tracks use the VideoMediaHeaderBox in the MediaInformationBox as defined in 8.4.5. The VideoMediaHeaderBox contains general presentation information, independent of the coding, for video media. Note that the flags field has the value 1.

#### Syntax

aligned(8) class VideoMediaHeaderBox  
 extends FullBox('vmhd', version = 0, 1)   
{  
 template unsigned int(16) graphicsmode = 0; // copy, see below  
 template unsigned int(16) opcolor[3] = {0, 0, 0};  
}

#### Semantics

version is an integer that specifies the version of this box

graphicsmode specifies a composition mode for this video track, from the following enumerated set, which may be extended by derived specifications:

copy = 0 copy over the existing image

opcolor is a set of 3 colour values (red, green, blue) available for use by graphics modes

### Sample entry

#### Definition

Video tracks use VisualSampleEntry.

In video tracks, the frame\_count field shall be 1 unless the specification for the media format explicitly documents this template field and permits larger values. That specification must document both how the individual frames of video are found (their size information) and their timing established. That timing might be as simple as dividing the sample duration by the frame count to establish the frame duration.

The width and height in the video sample entry document the pixel counts that the codec will deliver; this enables the allocation of buffers. Since these are counts they do not take into account pixel aspect ratio.

#### Syntax

class VisualSampleEntry(codingname) extends SampleEntry (codingname)  
{  
 unsigned int(16) pre\_defined = 0;  
 const unsigned int(16) reserved = 0;  
 unsigned int(32) pre\_defined[3] = 0;  
 unsigned int(16) width;  
 unsigned int(16) height;  
 template unsigned int(32) horizresolution = 0x00480000; // 72 dpi  
 template unsigned int(32) vertresolution = 0x00480000; // 72 dpi  
 const unsigned int(32) reserved = 0;  
 template unsigned int(16) frame\_count = 1;  
 uint(8) compressorname[32];  
 template unsigned int(16) depth = 0x0018;  
 int(16) pre\_defined = -1;  
 // other boxes from derived specifications  
 CleanApertureBox clap; // optional  
 PixelAspectRatioBox pasp; // optional  
}

#### Semantics

resolution fields give the resolution of the image in pixels-per-inch, as a fixed 16.16 number

frame\_count indicates how many frames of compressed video are stored in each sample. The default is 1, for one frame per sample; it may be more than 1 for multiple frames per sample

compressorname is a name, for informative purposes. It is formatted in a fixed 32-byte field, with the first byte set to the number of bytes to be displayed, followed by that number of bytes of displayable data encoded using UTF-8, and then padding to complete 32 bytes total (including the size byte). The field may be set to 0.

depth takes one of the following values

0x0018 – images are in colour with no alpha

width and height are the maximum visual width and height of the stream described by this sample entry, in pixels

### Pixel aspect ratio and clean aperture

#### Definition

The pixel aspect ratio and clean aperture of the video may be specified using the PixelAspectRatioBox and CleanApertureBox sample entry boxes, respectively. These are both optional; if present, they over-ride the declarations (if any) in structures specific to the video codec, which structures should be examined if these boxes are absent. For maximum compatibility, these boxes should follow, not precede, any boxes defined in or required by derived specifications.

The PixelAspectRatioBox is informative; if the decoded output of the codec is re-formatted to the dimensions in the track header, this will accomplish any needed adjustment to a uniformly-scaled grid.

In the PixelAspectRatioBox, hSpacing and vSpacing have the same units, but those units are unspecified: only the ratio matters. hSpacing and vSpacing may or may not be in reduced terms, and they may reduce to 1/1. Both of them shall be strictly positive.

NOTE 1 The pixel aspect ratio should not be confused with the picture aspect ratio, also known as the display aspect ratio, which is the ratio of the width to the height of the final displayed image (e.g. 16:9).

They are defined as the aspect ratio of a pixel, in arbitrary units. If a pixel appears H wide and V tall, then hSpacing/vSpacing is equal to H/V. This means that a square on the display that is n pixels tall needs to be n\*vSpacing/hSpacing pixels wide to appear square.

There are notionally four values in the CleanApertureBox. These parameters are represented as a fraction N/D. The fraction may or may not be in reduced terms. We refer to the pair of parameters fooN and fooD as foo. For horizOff and vertOff, D shall be strictly positive and N may be positive or negative. For cleanApertureWidth and cleanApertureHeight, N shall be positive and D shall be strictly positive.

NOTE 2 These are fractional numbers for several reasons. First, in some systems the exact width after pixel aspect ratio correction is integral, not the pixel count before that correction. Second, if video is resized in the full aperture, the exact expression for the clean aperture might not be integral. Finally, because this is represented using centre and offset, a division by two is needed, and so half-values can occur.

The relation of width and height of the VisualSampleEntry, the horizontal and vertical coordinates of the picture centre of the image denoted as pcX and pcY respectively, and horizOff and vertOff is defined as follows:

pcX = horizOff + (width - 1)/2  
pcY = vertOff + (height - 1)/2;

Typically, horizOff and vertOff are zero, so the image is centred about the picture centre.

The leftmost/rightmost pixel and the topmost/bottommost line of the clean aperture fall at:

pcX ± (cleanApertureWidth - 1)/2  
pcY ± (cleanApertureHeight - 1)/2;

The cropping implied by the CleanApertureBox is applied before any transformation defined by track or movie matrices.

#### Syntax

class PixelAspectRatioBox extends Box('pasp')  
{  
 unsigned int(32) hSpacing;  
 unsigned int(32) vSpacing;  
}

class CleanApertureBox extends Box('clap')  
{  
 signed int(32) cleanApertureWidthN;  
 signed int(32) cleanApertureWidthD;  
  
 signed int(32) cleanApertureHeightN;  
 signed int(32) cleanApertureHeightD;  
  
 signed int(32) horizOffN;  
 signed int(32) horizOffD;  
  
 signed int(32) vertOffN;  
 signed int(32) vertOffD;  
}

#### Semantics

hSpacing, vSpacing: define the relative width and height of a pixel;

cleanApertureWidthN, cleanApertureWidthD: a fractional number which defines the width of the clean aperture image

cleanApertureHeightN, cleanApertureHeightD: a fractional number which defines the height of the clean aperture image

horizOffN, horizOffD: a fractional number which defines the horizontal offset between the clean aperture image centre and the full aperture image centre. Typically 0.

vertOffN, vertOffD: a fractional number which defines the vertical offset between clean aperture image centre and the full aperture image centre. Typically 0.

### Colour information

#### Definition

Colour information may be supplied in one or more ColourInformationBoxes placed in a VisualSampleEntry. These should be placed in order in the sample entry starting with the most accurate (and potentially the most difficult to process), in progression to the least. These are advisory and concern rendering and colour conversion, and there is no normative behaviour associated with them; a reader may choose to use the most suitable. A ColourInformationBox with an unknown colour type may be ignored.

If used, an ICC profile may be a restricted one, under the code 'rICC', which permits simpler processing. That proﬁle shall be of either the monochrome or three-component matrix-based class of input proﬁles, as deﬁned by ISO 15076‑1. If the profile is of another class, then the 'prof' indicator shall be used.

If colour information is supplied in both this box, and also in the video bitstream, this box takes precedence, and over-rides the information in the bitstream.

NOTE When an ICC profile is specified, SMPTE RP 177[27] is possibly of assistance if there is a need to form the Y'CbCr to R'G'B' conversion matrix for the colour primaries described by the ICC profile.

#### Syntax

class ColourInformationBox extends Box('colr')  
{  
 unsigned int(32) colour\_type;  
 if (colour\_type == 'nclx') /\* on-screen colours \*/  
 {  
 unsigned int(16) colour\_primaries;  
 unsigned int(16) transfer\_characteristics;  
 unsigned int(16) matrix\_coefficients;  
 unsigned int(1) full\_range\_flag;  
 unsigned int(7) reserved = 0;  
 }  
 else if (colour\_type == 'rICC')  
 {  
 ICC\_profile; // restricted ICC profile  
 }  
 else if (colour\_type == 'prof')  
 {  
 ICC\_profile; // unrestricted ICC profile  
 }  
}

#### Semantics

colour\_type: an indication of the type of colour information supplied.

colour\_primaries carries a **ColourPrimaries** value as defined in ISO/IEC 23091-2

transfer\_characteristics carries a **TransferCharacteristics** value as defined in ISO/IEC 23091-2

matrix\_coefficients carries a **MatrixCoefficients** value as defined in ISO/IEC 23091-2

full\_range\_flag carries a **VideoFullRangeFlag** as defined in ISO/IEC 23091-2

ICC\_profile: an ICC profile as defined in ISO 15076‑1 or ICC.1[23] is supplied.

### Content light level

#### Definition

This box may be used to provide information about the light level in the content and may be present in a VisualSampleEntry. It is functionally equivalent to, and shall be as described in, the content light level information SEI message in ITU-T H.265 | ISO/IEC 23008-2, with the addition that the provisions of CTA-861-G[35], in which zero in some cases codes an unknown value, may be used.

NOTE This is a Box, not a FullBox (similar to PixelAspectRatioBox).

#### Syntax

class ContentLightLevelBox extends Box('clli')  
{  
 unsigned int(16) max\_content\_light\_level;  
 unsigned int(16) max\_pic\_average\_light\_level;  
}

### Mastering display colour volume

#### Definition

This box may be used to provide information about the colour primaries, white point, and mastering luminance in the content and may be present in a VisualSampleEntry. It is functionally equivalent to, and shall be as described in, the mastering display colour volume SEI message in ITU-T H.265 | ISO/IEC 23008-2, with the addition that the provisions of CTA-861-G[35] in which zero in some cases codes an unknown value may be used.

NOTE This is a Box, not a FullBox (similar to PixelAspectRatioBox).

#### Syntax

class MasteringDisplayColourVolumeBox extends Box('mdcv')  
{  
 for (c = 0; c<3; c++) {  
 unsigned int(16) display\_primaries\_x;  
 unsigned int(16) display\_primaries\_y;  
 }  
 unsigned int(16) white\_point\_x;  
 unsigned int(16) white\_point\_y;  
 unsigned int(32) max\_display\_mastering\_luminance;  
 unsigned int(32) min\_display\_mastering\_luminance;  
}

### Content colour volume

#### Definition

This box describes the colour volume characteristics of the associated pictures. These colour volume characteristics are expressed in terms of a nominal range, although deviations from this range may occur. It is functionally equivalent to, and shall be as described in, the content colour volume SEI message in Rec. ITU-T H.265 | ISO/IEC 23008-2 except that the box, in a sample entry, applies to the associated content and hence the initial two bits (corresponding to the ccv\_cancel\_flag and ccv\_persistence\_flag) take the value 0.

NOTE This is a Box, not a FullBox (similar to PixelAspectRatioBox).

#### Syntax

class ContentColourVolumeBox extends Box('cclv')  
{  
 unsigned int(1) reserved = 0; // ccv\_cancel\_flag  
 unsigned int(1) reserved = 0; // ccv\_persistence\_flag  
 unsigned int(1) ccv\_primaries\_present\_flag;  
 unsigned int(1) ccv\_min\_luminance\_value\_present\_flag;  
 unsigned int(1) ccv\_max\_luminance\_value\_present\_flag;  
 unsigned int(1) ccv\_avg\_luminance\_value\_present\_flag;  
 unsigned int(2) reserved = 0;  
 if( ccv\_primaries\_present\_flag ) {  
 for ( c = 0; c < 3; c++ ) {  
 signed int(32) ccv\_primaries\_x[[c]];  
 signed int(32) ccv\_primaries\_y[[c]];  
 }  
 }  
 if( ccv\_min\_luminance\_value\_present\_flag )  
 unsigned int(32) ccv\_min\_luminance\_value;  
 if( ccv\_max\_luminance\_value\_present\_flag )  
 unsigned int(32) ccv\_max\_luminance\_value;  
 if( ccv\_avg\_luminance\_value\_present\_flag )  
 unsigned int(32) ccv\_avg\_luminance\_value;  
}

### Ambient viewing environment

#### Definition

This box may be used to provide information about the characteristics of the nominal ambient viewing environment for the display of the associated video content and may be present in a VisualSampleEntry. The syntax elements of the ambient viewing environment box may assist the receiving system in adapting the received video content for local display in viewing environments that may be similar or may substantially differ from those assumed or intended when mastering the video content. It is functionally equivalent to, and shall be as described in, the ambient viewing environment SEI message in ITU-T H.265 |I ISO/IEC 23008-2.

NOTE This is a Box, not a FullBox (similar to PixelAspectRatioBox).

#### Syntax

class AmbientViewingEnvironmentBox extends Box('amve')  
{  
 unsigned int(32) ambient\_illuminance;   
 unsigned int(16) ambient\_light\_x;  
 unsigned int(16) ambient\_light\_y;  
}

## Audio media

### Media handler

Audio media uses the 'soun' handler type in the HandlerBox of the MediaBox, as defined in 8.4.3.

### Sound media header

#### Definition

Box Types: 'smhd'  
Container: MediaInformationBox Box  
Mandatory: Yes  
Quantity: Exactly one specific media header shall be present

Audio tracks use the SoundMediaHeaderBox in the MediaInformationBox as defined in 8.4.5. The sound media header contains general presentation information, independent of the coding, for audio media. This header is used for all tracks containing audio.

#### Syntax

aligned(8) class SoundMediaHeaderBox  
 extends FullBox('smhd', version = 0, 0)   
{  
 template int(16) balance = 0;  
 const unsigned int(16) reserved = 0;  
}

#### Semantics

version is an integer that specifies the version of this box

balance is a fixed-point 8.8 number that places mono audio tracks in a stereo space; 0 is centre (the normal value); full left is -1.0 and full right is 1.0.

### Sample entry

#### Definition

Audio tracks use AudioSampleEntry or AudioSampleEntryV1.

The samplerate, samplesize and channelcount fields document the default audio output playback format for this media. The timescale for an audio track should be chosen to match the sampling rate, or be an integer multiple of it, to enable sample-accurate timing. When channelcount is a value greater than zero, it indicates the total number of channels in the audio stream.

The audio output format (samplerate, samplesize and channelcount fields) in the sample entry should be considered definitive only for codecs that do not record their own output configuration. If the audio codec has definitive information about the output format, it shall be taken as definitive; in this case the samplerate, samplesize and channelcount fields in the sample entry may be ignored, though sensible values should be chosen (for example, the highest possible sampling rate).

When it is desired to indicate an audio sampling rate greater than the value than can be represented in the samplerate field, then one of the following may be used:

1. If the system needs to rely on this signalling alone, e.g. because the codec does not itself provide the sample rate:
   * an AudioSampleEntryV1 is used
   * a SamplingRateBox is present in the AudioSampleEntryV1, and it overrides the samplerate field and documents the actual sampling rate;
2. Otherwise:
   * a SamplingRateBox is present in the AudioSampleEntryV1 or AudioSampleEntry, and it documents the actual sampling rate.

When a SamplingRateBox is present:

* the media timescale should be the same as the sampling rate, or an integer division or multiple of it;
* the samplerate field in the sample entry should contain a value that matches the media timescale left-shifted 16 bits (as for AudioSampleEntry), or be an integer division or multiple of it.

An AudioSampleEntryV1 should only be used when needed; otherwise, for maximum compatibility, an AudioSampleEntry should be used. For maximum compatibility, the SamplingRateBox, ChannelLayoutBox and any DownMix and DRC boxes should follow, not precede, any boxes defined in or required by derived specifications.

Encoders should encode the DRC-related boxes in the AudioSampleEntry in the order given in subclause 12.2.3.2. Decoders may ignore and discard the DRC-related boxes if they are not in that order. DRC-related boxes include ChannelLayout, DownMixInstructions, DRCCoefficientsBasic, DRCInstructionsBasic, DRCCoefficientsUniDrc, DRCInstructionsUniDrc, and UniDrcConfigExtension. The DownMixInstructions and DRCInstructionsUniDrc box cannot occur more than once if the box has version==1, but it can occur multiple times if version==0.

#### Syntax

class AudioSampleEntry(codingname) extends SampleEntry (codingname)  
{  
 const unsigned int(32) reserved[2] = 0;  
 unsigned int(16) channelcount;  
 template unsigned int(16) samplesize = 16;  
 unsigned int(16) pre\_defined = 0;  
 const unsigned int(16) reserved = 0 ;  
 template unsigned int(32) samplerate = { default samplerate of media}<<16;  
 ChannelLayout(); // optional  
 DownMixInstructions() []; // optional  
 DRCCoefficientsBasic() []; // optional  
 DRCInstructionsBasic() []; // optional  
 DRCCoefficientsUniDRC() []; // optional  
 DRCInstructionsUniDRC() []; // optional  
 UniDrcConfigExtension(); // optional  
 SamplingRateBox(); // optional  
 Box() []; // optional  
}

aligned(8) class SamplingRateBox extends FullBox('srat')   
{  
 unsigned int(32) sampling\_rate;  
}

class AudioSampleEntryV1(codingname) extends SampleEntry (codingname)  
{  
 unsigned int(16) entry\_version; // shall be 1,   
 // and shall be in an stsd with version ==1  
 const unsigned int(16) reserved[3] = 0;  
 template unsigned int(16) channelcount; // shall be correct  
 template unsigned int(16) samplesize = 16;  
 unsigned int(16) pre\_defined = 0;  
 const unsigned int(16) reserved = 0 ;  
 template unsigned int(32) samplerate = 1<<16;  
 SamplingRateBox(); ChannelLayout();  
 DownMixInstructions() []; // optional  
 DRCCoefficientsBasic() []; // optional  
 DRCInstructionsBasic() []; // optional  
 DRCCoefficientsUniDRC() []; // optional  
 DRCInstructionsUniDRC() []; // optional  
 UniDrcConfigExtension(); // optional  
 Box (); // optional  
}

#### Semantics

channelcount is the number of channels

0 — inapplicable/unknown

1 — mono

2 — stereo (left/right)

all other values — the codec configuration should identify the channel assignment.

SampleSize is in bits, and takes the default value of 16

SampleRate when a SamplingRateBox is absent is the sampling rate; when a SamplingRateBox is present, is a suitable integer multiple or division of the actual sampling rate. This 32-bit field is expressed as a 16.16 fixed-point number (hi.lo)

sampling\_rate is the actual sampling rate of the audio media in samples/second, expressed as a 32-bit integer

### Channel layout

#### Definition

Box Types: 'chnl'  
Container: Audio sample entry, AudioElementBox, or PreselectionGroupBox  
Mandatory: No  
Quantity: Zero or one

This box may appear in an audio sample entry to document the assignment of channels in the audio stream. It is recommended to use this box to convey the base channel count for the DownMixInstructions box and other DRC-related boxes specified in ISO/IEC 23003‑4.

The channel layout can be all or part of a standard layout (from an enumerated list), or a custom layout (which also allows a track to contribute part of an overall layout).

A stream may contain channels, objects, neither, or both. A stream that is neither channel nor object structured can implicitly be rendered in a variety of ways.

#### Syntax

aligned(8) class ChannelLayoutZero()  
{  
 for (i = 1 ; i <= layout\_channel\_count ; i++) {  
 unsigned int(8) speaker\_position;  
 if (speaker\_position == 126) { // explicit position  
 signed int (16) azimuth;  
 signed int (8) elevation;  
 }  
 }  
}

aligned(8) class ChannelLayout extends FullBox('chnl', version, flags=0)  
{  
 if (version==0) {  
 unsigned int(8) stream\_structure;  
 if (stream\_structure & channelStructured) {  
 unsigned int(8) definedLayout;  
 if (definedLayout==0) {  
 ChannelLayoutZero(layout\_channel\_count)  
 // layout\_channel\_count comes from the sample entry  
 } else {  
 unsigned int(64) omittedChannelsMap;   
 // a ‘1’ bit indicates ‘not in this track’  
 }  
 }  
 if (stream\_structure & objectStructured) {  
 unsigned int(8) object\_count;  
 }  
 } else {  
 unsigned int(4) stream\_structure;  
 unsigned int(4) format\_ordering;  
 unsigned int(8) baseChannelCount;  
 if (stream\_structure & channelStructured) {  
 unsigned int(8) definedLayout;  
 if (definedLayout==0) {  
 unsigned int(8) layout\_channel\_count;  
 ChannelLayoutZero(layout\_channel\_count)  
 } else {  
 int(4) reserved = 0;  
 unsigned int(3) channel\_order\_definition;  
 unsigned int(1) omitted\_channels\_present;  
 if (omitted\_channels\_present == 1) {  
 unsigned int(64) omittedChannelsMap;   
 // a ‘1’ bit indicates ‘not in this track’  
 }  
 }  
 }  
 if (stream\_structure & objectStructured) {  
 // object\_count is derived from baseChannelCount  
 }  
 }  
}

#### Semantics

version is an integer that specifies the version of this box (0 or 1). When authoring, version 1 should be preferred over version 0. Version 1 conveys the channel ordering, which is not always the case for version 0. Version 1 should be used to convey the base channel count for DRC.

stream\_structure is a field of flags that define whether the stream has channel or object structure (or both, or neither); the following flags are defined, all other values are reserved:

channelStructured: Flag mask is 0x01 / 0x1. If the flag is set, it indicates that the stream carries channels. If the flag is not set, it indicates that the stream does not carry any channel based audio.

objectStructured: Flag mask is 0x02 / 0x2. If the flag is set, it indicates that the stream carries objects. If the flag is not set, it indicates that the stream does not carry any audio objects.

format\_ordering indicates the order of formats in the stream starting from the lowest channel index (see Table). Each format shall only use contiguous channel indices.

|  |  |
| --- | --- |
| **format\_ordering** | **Order** |
| 0 | unknown |
| 1 | Channels, possibly followed by Objects |
| 2 | Objects, possibly followed by Channels |
| Remaining values are reserved | - |

definedLayout is a **ChannelConfiguration** from ISO/IEC 23091-3.

speaker\_position is an **OutputChannelPosition** from ISO/IEC 23091-3. If an explicit position is used, then the azimuth and elevation are as defined as for speakers in ISO/IEC 23091-3. The channel order corresponds to the order of speaker positions.

azimuth is a signed value in degrees, as defined for **LoudspeakerAzimuth** in ISO/IEC 23091-3.

elevation is a signed value, in degrees, as defined for **LoudspeakerElevation** in ISO/IEC 23091-3.

channel\_order\_definition indicates where the ordering of the audio channels for the definedLayout are specified (see Table).

|  |  |
| --- | --- |
| **channel\_order\_definition** | **Channel order specification** |
| 0 | as listed for the **ChannelConfigurations** in ISO/IEC 23091-3 |
| 1 | Default order of audio codec specification |
| 2 | Channel ordering #2 of audio codec specification |
| 3 | Channel ordering #3 of audio codec specification |
| 4 | Channel ordering #4 of audio codec specification |
| Remaining values are reserved | - |

omitted\_channels\_present is a flag that indicates if it is set to 1 that the omittedChannelsMap is present.

omittedChannelsMap is a bit-map of omitted channels; the bits in the channel map are numbered from least-significant to most-significant, and correspond in that ordering with the order of the channels for the configuration as documented in ISO/IEC 23091-3 ChannelConfiguration. 1-bits in the channel map mean that a channel is absent. A zero value of the map therefore always means that the given standard layout is fully present. The default value is 0.

layout\_channel\_count is the count of channels for the channel layout. The default value is 0 if stream\_structure indicates that no channel structure is present. Otherwise, the value is the number of channels of the defined layout, if present, otherwise it is the value from the sample entry.

object\_count is the count of channels that contain audio objects. The default value is 0. For version 1 and if the objectStructured flag is set, the value is computed as baseChannelCount minus the channel count of the channel structure.

baseChannelCount represents the combined channel count of the channel layout and the object count. The value must match the base channel count for DRC (see ISO/IEC 23003‑4).

### Downmix instructions

#### Definition

Box Types: 'dmix'  
Container: Audio sample entry  
Mandatory: No  
Quantity: Zero or more

The downmix can be controlled by the production facility if necessary. For instance, some content may require more attenuation of the surround channels before downmixing to maintain intelligibility.

The downmix support is designed so that any downmix (e.g. from 7.1 to quad as well as to stereo) can be described.

It is possible to declare the loudness characteristics of the signal after downmix, and after DRC and downmix.

If targetChannelCount\*baseChannelCount is odd, the box is padded with 4 bits set to 0xF. The targetChannelCount shall be consistent with the targetLayout (if given), and shall be less than or equal to the channelcount.

Each downmix is uniquely identified by an ID.

In the following definition, ceil() is the ceiling function.

#### Syntax

aligned(8) class DownMixInstructions   
 extends FullBox('dmix', version, flags=0)   
{  
 if (version >= 1) {  
 bit(1) reserved = 0;  
 bit(7) downmix\_instructions\_count;  
 } else {  
 int downmix\_instructions\_count = 1;  
 }  
 for (a=1; a<=downmix\_instructions\_count; a++) {   
 unsigned int(8) targetLayout;  
 unsigned int(1) reserved = 0;  
 unsigned int(7) targetChannelCount;  
 bit(1) in\_stream;   
 unsigned int(7) downmix\_ID;  
 if (in\_stream==0)   
 { // downmix coefficients are out of stream and supplied here  
 int i, j;  
 if (version >= 1) {  
 bit(4) bs\_downmix\_offset;  
 int size = 4;  
 for (i=1; i <= targetChannelCount; i++){  
 for (j=1; j <= baseChannelCount; j++) {  
 bit(5) bs\_downmix\_coefficient\_v1;  
 size += 5;  
 }  
 }  
 bit(8 ceil(size / 8) – size) reserved = 0; // byte align  
 } else {  
 for (i=1; i <= targetChannelCount; i++){  
 for (j=1; j <= baseChannelCount; j++) {  
 bit(4) bs\_downmix\_coefficient;  
 }  
 }  
 }  
 }  
 }  
}

#### Semantics

targetLayout is a **ChannelConfiguration** from ISO/IEC 23091-3 and defines the resulting layout after downmix

targetChannelCount is the count of channels in the resulting stream, and shall correspond with the target layout

downmix\_ID is an arbitrary value that identifies this downmix, and shall be unique among the DownMixInstructions in a given sample entry; there are two reserved values, 0 and 0x7F, which shall not be used

version is an integer that specifies the version of this box (0 or 1)

bs\_downmix\_offset is an offset in dB for all downmix coefficients that are defined in the bs\_downmix\_coefficient\_v1 field. It is encoded as defined in Table 8 using the following expression for:

Table 8 — Downmix offset encoding

|  |  |
| --- | --- |
| **Value [dB]** | **Hex encoding (3 bits)** |
| 0.0 | 0x0 |
|  | 0x1 |
|  | 0x2 |
| reserved | other |

baseChannelCount is the channel count of the audio signal in the base layout as also defined in ISO/IEC 23003‑4. It should be derived from the ChannelLayout box, if present.

in\_stream has a value of 1 when the downmix coefficients are in the stream. Otherwise, it is zero.

bs\_downmix\_coefficient is encoded as defined in Table 9 and Table 10:

**Table 9 — Downmix coefficient encoding for non-LFE channel and version==0 (bs\_downmix\_coefficient)**

|  |  |
| --- | --- |
| Value | Hex encoding (4 bits) |
| 0.00 dB | 0x0 |
| -0.50 dB | 0x1 |
| -1.00 dB | 0x2 |
| -1.50 dB | 0x3 |
| -2.00 dB | 0x4 |
| -2.50 dB | 0x5 |
| -3.00 dB | 0x6 |
| -3.50 dB | 0x7 |
| -4.00 dB | 0x8 |
| -4.50 dB | 0x9 |
| -5.00 dB | 0xA |
| -5.50 dB | 0xB |
| -6.00 dB | 0xC |
| -7.50 dB | 0xD |
| -9.00 dB | 0xE |
| -∞ dB | 0xF |

Table 10 — Downmix coefficient encoding for LFE channel and version==0 (bs\_downmix\_coefficient)

|  |  |
| --- | --- |
| **Value** | **Hex encoding (4 bits)** |
| 10.00 dB | 0x0 |
| 6.00 dB | 0x1 |
| 4.5 dB | 0x2 |
| 3.00 dB | 0x3 |
| 1.50 dB | 0x4 |
| 0.00 dB | 0x5 |
| -1.50 dB | 0x6 |
| -3.00 dB | 0x7 |
| -4.50 dB | 0x8 |
| -6.00 dB | 0x9 |
| -10.00 dB | 0xA |
| -15.00 dB | 0xB |
| -20.00 dB | 0xC |
| -30.00 dB | 0xD |
| -40.00 dB | 0xE |
| -∞ dB | 0xF |

bs\_downmix\_coefficient\_v1 is encoded as defined in Table 11:

Table 11 — Downmix coefficient encoding for version>=1 (bs\_downmix\_coefficient\_v1)

|  |  |
| --- | --- |
| **Value** | **Hex encoding (5 bits)** |
| 10.00 dB | 0x00 |
| 6.00 dB | 0x01 |
| 4.50 dB | 0x02 |
| 3.00 dB | 0x03 |
| 1.50 dB | 0x04 |
| 0.00 dB | 0x05 |
| -0.50 dB | 0x06 |
| -1.00 dB | 0x07 |
| -1.50 dB | 0x08 |
| -2.00 dB | 0x09 |
| -2.50 dB | 0x0A |
| -3.00 dB | 0x0B |
| -3.50 dB | 0x0C |
| -4.00 dB | 0x0D |
| -4.50 dB | 0x0E |
| -5.00 dB | 0x0F |
| -5.50 dB | 0x10 |
| -6.00 dB | 0x11 |
| -6.50 dB | 0x12 |
| -7.00 dB | 0x13 |
| -7.50 dB | 0x14 |
| -8.00 dB | 0x15 |
| -9.00 dB | 0x16 |
| -10.00 dB | 0x17 |
| -11.00 dB | 0x18 |
| -12.00 dB | 0x19 |
| -15.00 dB | 0x1A |
| -20.00 dB | 0x1B |
| -25.00 dB | 0x1C |
| -30.00 dB | 0x1D |
| -40.00 dB | 0x1E |
| -∞ dB | 0x1F |

### DRC information

A DRC is used in the encoder to generate gain values using one of the pre-defined DRC characteristics as defined in ISO/IEC 23091-3 or a characteristic defined in ISO/IEC 23003‑4. The coefficients are placed either in-stream or in an associated meta-data track. Alternatively, coefficients are generated at the decoder based on transmitted parametric DRC configurations.

For some content, such as some multi-channel content, it may be advantageous to use different DRC characteristics in different channels. For instance, if speech is exclusively present in the center channel, this feature can be very useful. It is supported by the assignment of DRC characteristics to audio channels.

It is possible to declare the loudness characteristics of the signal after DRC.

DRC support includes supporting in-stream DRC coefficients, and a separate track carrying them; the latter is particularly useful for legacy coding systems (including uncompressed audio) that have no provision for in-stream coefficients.

In the ISO base media file format, the audio content may be carried in multiple tracks where a base track contains the DRC metadata for all tracks. The additional tracks are referenced by the base track using a track reference of type 'adda' (additional audio). The channels processed by the DRC are all the channels in the base track, plus all the channels in track(s) referenced, in the order of the references. The DRC channel groups apply to all those channels (even if they are channels in a track that is disabled or not currently being played).

The boxes DRCCoefficientsBasic, DRCCoefficientsUniDRC, DRCInstructionsBasic, DRCInstructionsUniDRC, and UniDrcConfigExtension may occur in an AudioSampleEntry and are defined in ISO/IEC 23003‑4.

### Audio stream loudness

#### Definition

Box Types: 'ludt'  
Container: UserDataBox of the corresponding TrackBox  
Mandatory: No  
Quantity: Zero or more

Loudness declarations are placed in UserDataBoxes, to enable their presence and update in movie fragments. In particular, in live scenarios, user-data in the initial MovieBox may be a ‘promise not to exceed’ or ‘best guess’, and then user-data updates give better (but still generally valid) values. Thus, for example, a loudness range in this user data that is associated with a particular set of DRC instructions constitutes a ‘promise’ rather than a measurement, under these circumstances.

Several metadata values are available that describe aspects of the dynamic range. The size of the dynamic range can be useful in adjusting the DRC characteristic, e.g. the DRC is less aggressive if the dynamic range is small or the DRC can even be turned off.

True Peak and maximum loudness values can be useful for estimating the headroom, for instance when loudness normalization results in a positive gain [dB] or when headroom is needed to avoid clipping of the downmix. The DRC characteristic can then be adjusted to approach a headroom target. The peak level of the associated content is represented here in a coding-independent way.

The audio sound pressure level that the content was mixed to can also be documented. (If audio is listened to at a level other than the mixing level, this can affect the perceived tonal balance.)

The following measures may also be used:

* Maximum of the loudness range derived from EBU-Tech 3342[33]
* Maximum momentary loudness derived from ITU-R BS.1771-1[11] or EBU-Tech 3341[32]
* Maximum short-term loudness derived from ITU-R BS.1771-1[11] or EBU-Tech 3341[32]
* Short-term loudness defined in ITU-R BS.1771-1[11] or EBU-Tech 3341[32]

Under some circumstances it can be desirable to indicate the loudness characteristics of an album, in each song that the album contains. A separate box can be specified for that purpose. The TrackLoudnessInfo and AlbumLoudnessInfo provide loudness information for the song, and for the entire album which contains the song, respectively.

The program loudness shall be measured using ITU-R BS.1770-4 over the associated content; the ‘anchor loudness’ is the loudness of the anchor content, where what that content is, is determined by the content author; one suitable value (especially for content for which the main content is speech) is ‘dialog normal level’ or DialNorm as defined in ATSC Doc. A/52:2012[34]. ISO/IEC 23003‑4 specifies the measurement systems, measurement methods and the coding of all loudness and peak-related values.

#### Syntax

aligned(8) class LoudnessBaseBox   
 extends FullBox(loudnessType, version, flags=0)   
{  
 if (version >= 2) {  
 unsigned int(2) loudness\_info\_type;  
 unsigned int(6) loudness\_base\_count;  
 if (loudness\_info\_type == 1 || loudness\_info\_type == 2) {  
 unsigned int(1) reserved = 0;  
 unsigned int(7) mae\_group\_ID;  
 }  
 else if (loudness\_info\_type == 3) {  
 unsigned int(3) reserved = 0;  
 unsigned int(5) mae\_group\_preset\_ID;  
 }  
 }  
 else if (version == 1) {  
 unsigned int(2) reserved = 0;  
 unsigned int(6) loudness\_base\_count;  
 } else {  
 int loudness\_base\_count = 1;  
 }  
 for (a=1; a<=loudness\_base\_count; a++) {  
 if (version >= 1) {  
 unsigned int(2) reserved = 0;  
 unsigned int(6) EQ\_set\_ID; // to match an EQ box  
 }  
 unsigned int(3) reserved = 0;  
 unsigned int(7) downmix\_ID; // matching downmix  
 unsigned int(6) DRC\_set\_ID; // to match a DRC box  
 signed int(12) bs\_sample\_peak\_level;  
 signed int(12) bs\_true\_peak\_level;  
 unsigned int(4) measurement\_system\_for\_TP;  
 unsigned int(4) reliability\_for\_TP;  
 unsigned int(8) measurement\_count;  
 int i;  
 for (i = 1 ; i <= measurement\_count; i++){  
 unsigned int(8) method\_definition;  
 unsigned int(8) method\_value;  
 unsigned int(4) measurement\_system;  
 unsigned int(4) reliability;  
 }  
 }  
}

aligned(8) class TrackLoudnessInfo extends LoudnessBaseBox('tlou')   
{  
}

aligned(8) class AlbumLoudnessInfo extends LoudnessBaseBox ('alou')  
{  
}

aligned(8) class LoudnessBox extends Box('ludt')   
{  
 // not more than one TrackLoudnessInfo box with version>=1 is allowed  
 loudness TrackLoudnessInfo[];  
 // not more than one AlbumLoudnessInfo box with version>=1 is allowed albumLoudness AlbumLoudnessInfo[];  
}

#### Semantics

version is an integer that specifies the version of this box (0, 1 or 2)

loudness\_info\_type is the type of audio scene described by the loudness information. It shall take a value of zero unless other types are supported by the loudness processing. For defined values refer to the corresponding loudnessInfoType specification in ISO/IEC 23008-3[8].

mae\_group\_ID is a unique identifier for a group of metadata elements as specified in ISO/IEC 23008-3[8].

mae\_group\_preset\_ID is a unique identifier for a group preset as specified in ISO/IEC 23008-3[8].

downmix\_ID when zero, declares the loudness characteristics of the layout without downmix. If non-zero, this box declares the loudness after applying the downmix with the matching downmix\_ID and shall match a value in exactly one box in the sample entry of this track

DRC\_set\_ID when zero, declares the characteristics without applying a DRC. If non-zero, this box declares the loudness after applying the DRC with the matching DRC\_set\_ID and shall match a value in exactly one box in the sample entry of this track

EQ\_set\_ID when zero, declares the characteristics without applying EQ. If non-zero, this box declares the loudness after applying the EQ with the matching EQ\_set\_ID and shall match a value in exactly one box in the UniDrcConfigExtension of this track

bs\_sample\_peak\_level takes a value for the sample peak level as defined in ISO/IEC 23003‑4; all other values are reserved

bs\_true\_peak\_level takes a value for the true peak level as defined in ISO/IEC 23003‑4; all other values are reserved

measurement\_system\_for\_TP takes an index for the measurement system as defined in ISO/IEC 23003‑4; all other values are reserved

method\_definition takes an index for the measurement method as defined in ISO/IEC 23003‑4; all others are reserved

measurement\_system takes an index for the measurement system as defined in ISO/IEC 23003‑4; all others are reserved

reliability and reliability\_for\_TP each take one of the following values (all other values are reserved):

0: Reliability is unknown

1: Value is reported/imported but unverified

2: Value is a ‘not to exceed’ ceiling

3: Value is measured and accurate

### Audio rendering indication box

#### Definition

Box Type: 'ardi'  
Container: PreselectionGroupBox   
Mandatory: No  
Quantity: Zero or one

The audio rendering indication box contains a hint for a preferred reproduction channel layout.

#### Syntax

aligned(8) class AudioRenderingIndicationBox   
 extends FullBox('ardi', version=0, 0 )  
{  
 unsigned int(8) audio\_rendering\_indication = 0;  
}

#### Semantics

audio\_rendering\_indication contains a hint for a preferred reproduction channel layout, coded according to Table 12.

Table 12 — Coding of audio rendering indication

|  |  |
| --- | --- |
| **audio\_rendering\_indication** | **Description** |
| 0 | no preference given for the reproduction channel layout |
| 1 | preferred reproduction channel layout is stereo |
| 2 | preferred reproduction channel layout is two-dimensional (e.g. 5.1 multi-channel) |
| 3 | preferred reproduction channel layout is three-dimensional |
| 4 | content is pre-rendered for consumption with headphones |
| 5 to 255 | reserved for future use |

### Audio element box

#### Definition

Box Type: 'aelm'  
Container: AudioElementSelectionBox,   
 PreselectionGroupBox  
Mandatory: Yes (required within AudioElementSelectionBox)   
 No (optional within PreselectionGroupBox)  
Quantity: Zero or more

This box aggregates all semantic information about the audio element.

#### Syntax

aligned(8) class AudioElementBox extends Box('aelm')  
{  
}

### Audio element description box

#### Definition

Box Type: 'aedb'  
Container: AudioElementBox  
Mandatory: Yes  
Quantity: Exactly One

This box contains information about the interactivity options of the audio element.

#### Syntax

aligned(8) class AudioElementDescriptionBox   
 extends FullBox('aedb', version=0, flags)  
{  
 utf8string audioElementTag;  
 unsigned int(1) isToggleable;  
 unsigned int(1) isDefaultEnabled;  
 unsigned int(6) reserved;  
 AudioElementPosInteractivityPolar aePosIntAct; // optional  
 AudioElementProminenceInteractivity aePromIntAct; // optional  
}

#### Semantics

audioElementTag is a string that uniquely identifies the audio element that is described by this box within the preselection.

isToggleable specifies whether the described audio element can be switched on / off independently.

isDefaultEnabled specifies whether the described audio element is enabled or disabled by default.

aePosIntAct specifies whether and, if present, within which parameters the described audio element can be interactively placed within the audio scene.

aePromIntAct specifies whether and, if present, to which extend prominence interactivity is allowed for the described audio element

### Audio element positioning interactivity polar box

#### Definition

Box Type: 'aepp'  
Container: AudioElementDescriptionBox, AudioElementSelectionBox  
Mandatory: No  
Quantity: Zero or one

This box contains information about the positioning interactivity options of the audio element when the format is based on a polar coordinate system.

If this box is not present, no position interactivity on polar coordinates is allowed for the described audio element.

If this box is contained within an AudioElementSelectionBox, all AudioElementDescriptionBoxes grouped within this selection shall not contain an AudioElementPosInteractivityPolar box. The semantics of having this box on the AudioElementSelectionBox level is similar to having a copy of this box within each contained audio element description box.

Syntax

aligned(8) class AudioElementPosInteractivityPolar   
 extends FullBox('aepp', version=0, flags)  
{  
 if (flags & 1) {  
 signed int(16) minAzimuth;  
 signed int(16) maxAzimuth;  
 signed int(16) defaultAzimuth;  
 }  
 if (flags & 2) {  
 signed int(8) minElevation;   
 signed int(8) maxElevation;  
 signed int(8) defaultElevation;  
 }  
 if (flags & 4) {  
 unsigned int(32) minDistance;  
 unsigned int(32) maxDistance;  
 unsigned int(32) defaultDistance;  
 }  
}

#### Semantics

minAzimuth is a value in degrees, as defined for LoudspeakerAzimuth in ISO/IEC 23001-8. It specifies the minimum allowed Azimuth angle for the described audio element.

maxAzimuth is a value in degrees, as defined for LoudspeakerAzimuth in ISO/IEC 23001-8. It specifies the maximum allowed Azimuth angle for the described audio element.

defaultAzimuth is a value in degrees, as defined for LoudspeakerAzimuth in ISO/IEC 23001-8. It specifies the default Azimuth angle setting for the described audio element.

minElevation is a value, in degrees, as defined for LoudspeakerElevation in ISO/IEC 23001-8. It specifies the minimum allowed elevation for the described audio element.

maxElevation is a value, in degrees, as defined for LoudspeakerElevation in ISO/IEC 23001-8. It specifies the maximum allowed elevation for the described audio element.

defaultElevation is a value, in degrees, as defined for LoudspeakerElevation in ISO/IEC 23001-8. It specifies the default elevation setting for the described audio element.

minDistance specifies the minimum allowed distance of the described audio element from the listener in millimetres.

maxDistance specifies the maximum allowed distance of the described audio element from the listener in millimetres.

defaultDistance specifies the default distance of the described audio element from the listener in millimetres.

### Audio element prominence interactivity box

#### Definition

Box Type: 'aepr'  
Container: AudioElementDescriptionBox, AudioElementSelectionBox  
   
Mandatory: No  
Quantity: Zero or one

This box contains information about the prominence interactivity options of the audio element.

If this box is not present, no prominence interactivity is allowed for the described audio element.

If this box is contained within an AudioElementSelectionBox, all AudioElementDescriptionBoxes grouped within this selection shall not contain an AudioElementProminenceInteractivity box. The semantics of having this box on the AudioElementSelectionBox level is similar to having a copy of this box within each contained audio element description box.

#### Syntax

aligned(8) class AudioElementProminenceInteractivity  
 extends FullBox('aepr', version=0, flags)  
{  
 double(32) minProminence;   
 double(32) maxProminence;  
 double(32) defaultProminence;   
}

#### Semantics

minProminence specifies the minimum allowed prominence of the described audio element in dB.

maxProminence specifies the maximum allowed prominence of the described audio element in dB.

defaultProminence specifies the default prominence setting of the described audio element in dB.

### Audio element selection box

#### Definition

Box Type: 'aesb'  
Container: PreselectionGroupBox  
Mandatory: No  
Quantity: Zero or more

The audio element selection box signals a collection of audio elements where just one of the objects can be switched on at a given time.

#### Syntax

aligned(8) class AudioElementSelectionBox extends Box('aesb')  
{  
}

### Audio element selection description box

#### Definition

Box Type: 'aesd'  
Container: AudioElementSelectionBox  
Mandatory: Yes  
Quantity: Exactly One

This box contains semantic information about the audio element selection.

#### Syntax

aligned(8) class AudioElementSelectionDescriptionBox  
 extends FullBox('aesd', version=0, flags)  
{  
 utf8string selectionTag;  
}

#### Semantics

selectionTag is a string that contains an identifier for the audio element selection. This identifier shall uniquely identify the signalled audio element selection.

## Metadata media

### Media handler

Timed metadata media uses the 'meta' handler type in the HandlerBox of the MediaBox, as defined in 8.4.3.

NOTE 1 MPEG-7 streams, which are a specific kind of metadata stream, have their own handler declared, documented in the MP4 file format (ISO/IEC 14496-14[3]).

Metadata tracks should be linked to the track they describe using a track-reference of type 'cdsc'.

### Media header

Metadata tracks use a NullMediaHeaderBox, as defined in subclause 8.4.5.2.

### Sample entry

#### Definition

Timed metadata tracks use MetaDataSampleEntry.

In case of XML metadata a BitRateBox in the SampleEntry can be used to choose the appropriate memory representation format (DOM, STX).

The URIMetaSampleEntry entry contains, in a box, the URI defining the form of the metadata, and optional initialization data. The format of both the samples and of the initialization data is defined by all or part of the URI form.

It may be the case that the URI identifies a format of metadata that allows there to be more than one ‘stated fact’ within each sample. However, all metadata samples in this format are effectively ‘I frames’, defining the entire set of metadata for the time interval they cover. This means that the complete set of metadata at any instant, for a given track, is contained in (a) the time-aligned samples of the track(s) (if any) describing that track, plus (b) the track metadata (if any), the movie metadata (if any) and the file metadata (if any).

If incrementally-changed metadata is needed, the MPEG-7 framework provides that capability.

Information on URI forms for some metadata systems can be found in Annex G.

#### Syntax

class MetaDataSampleEntry(codingname) extends SampleEntry (codingname)   
{  
}

class XMLMetaDataSampleEntry() extends MetaDataSampleEntry ('metx')   
{  
 utf8string content\_encoding; // optional  
 utf8list namespace;  
 utf8list schema\_location; // optional  
}

class TextConfigBox extends Fullbox ('txtC', 0, 0)   
{  
 utf8string text\_config;  
}

class TextMetaDataSampleEntry() extends MetaDataSampleEntry ('mett')   
{  
 utf8string content\_encoding; // optional  
 utf8string mime\_format;  
 TextConfigBox (); // optional  
}

class MIMEBox extends Fullbox ('mime', 0, 0)   
{   
 utf8string content\_type;   
}

aligned(8) class URIBox extends FullBox('uri ', version = 0, 0)   
{  
 utf8string theURI;  
}

aligned(8) class URIInitBox extends FullBox('uriI', version = 0, 0)   
{  
 unsigned int(8) uri\_initialization\_data[];  
}

class URIMetaSampleEntry() extends MetaDataSampleEntry ('urim')   
{  
 URIbox the\_label;  
 URIInitBox init; // optional  
}

#### Semantics

content\_encoding provides a MIME type which identifies the content encoding of the timed metadata. It is defined in the same way as for an ItemInfoEntry in this document. If not present (an empty string is supplied) the timed metadata is not encoded. An example for this field is ‘application/zip’. Note that no MIME types for BiM [ISO/IEC 23001-1] and TeM [ISO/IEC 15938-1] currently exist. Thus, the experimental MIME types ‘application/x-BiM’ and ‘text/x-TeM’ shall be used to identify these encoding mechanisms.

namespace provides one or more XML namespaces to which the sample documents conform. When used for metadata, this is needed for identifying its type, e.g. gBSD or AQoS [MPEG-21-7] and for decoding using XML aware encoding mechanisms such as BiM.

schema\_location provides zero or more URLs for XML schema(s) to which the sample document conforms. If there is one namespace and one schema, then this field shall be the URL of the one schema. If there is more than one namespace, then the syntax of this field shall adhere to that for xsi:schemaLocation attribute as defined by XML. When used for metadata, this is needed for decoding of the timed metadata by XML aware encoding mechanisms such as BiM.

mime\_format provides a MIME type which identifies the content format of the samples. Examples for this field include ‘text/html’ and ‘text/plain’.

text\_config provides the initial text of each document which is prepended before the contents of each sync sample.

content\_type is a string corresponding to the MIME type each XML document carried in the stream has when delivered on its own, possibly including sub-parameters.

NOTE This implies that if two XML documents carried in the same track have different MIME types (or sub-parameters), each document is associated with a different sample entry.

theURI is a URI formatted according to the rules in 6.3.3;

uri\_initialization\_data is opaque data whose form is defined in the documentation of the URI form.

## Hint media

### Overview

Hint tracks are used to describe media stream data in the file. Each protocol or each family of related protocols has its own hint track format. A server hint track format and a reception hint track format for the same protocol are distinguishable from the associated four character code of the sample entry. In other words, a different four character code is used for a server hint track and a reception hint track of the same protocol. The syntax of the server hint track format and the reception hint track format for the same protocol should be the same or compatible so that a reception hint track can be used for re-sending of the stream provided that the potential degradations of the received streams are handled appropriately. Most protocols will need only one sample entry format for each track.

Servers find their hint tracks by first finding all hint tracks, and then looking within that set for server hint tracks using their protocol (identified by the sample entry ). If there are choices at this point, then the server chooses on the basis of preferred protocol or by comparing features in the hint track header or other protocol-specific information in the sample entries. Particularly in the absence of server hint tracks, servers may also use reception hint tracks of their protocol. However, servers should handle potential degradations of the received stream described by the used reception hint track appropriately.

Tracks having the track\_in\_movie flag set are candidates for playback, regardless of whether they are media tracks or reception hint tracks.

Hint tracks construct streams by pulling data out of other tracks by reference. These other tracks may be hint tracks or media stream tracks. The exact form of these pointers is defined by the sample format for the protocol, but in general they consist of four pieces of information: a track reference index, a sample number, an offset, and a length. Some of these may be implicit for a particular protocol. These ‘pointers’ always point to the actual source of the data. If a hint track is built ‘on top’ of another hint track, then the second hint track shall have direct references to the media track(s) used by the first where data from those media tracks is placed in the stream.

All hint tracks use a common set of declarations and structures.

* Hint tracks are linked to the media stream tracks they carry, by track references of type 'hint'
* They use a handler-type of 'hint' in the HandlerBox
* They use a HintMediaHeaderBox
* They use a HintSampleEntry in the SampleDescriptionBox, with a name and format unique to the protocol they represent.

Server hint tracks are usually marked as disabled for local playback, with their track header track\_in\_movie and track\_in\_preview flags set to 0.

Hint tracks may be created by an authoring tool, or may be added to an existing presentation by a hinting tool. Such a tool serves as a ‘bridge’ between the media and the protocol, since it intimately understands both. This permits authoring tools to understand the media format, but not protocols, and for servers to understand protocols (and their hint tracks) but not the details of media data.

Hint tracks shall not use composition time offsets. The process of hinting computes transmission times correctly as the presentation time derived from the decoding time.

Servers using reception hint tracks as hints for sending of the received streams should handle the potential degradations of the received streams, such as transmission delay jitter and packet losses, gracefully and ensure that the constraints of the protocols and contained data formats are obeyed regardless of the potential degradations of the received streams.

Conversion of received streams to media tracks allows existing players compliant with earlier versions of the ISO base media file format to process recorded files as long as the media formats are supported. However, most media coding standards only specify the decoding of error-free streams, and consequently it should be ensured that the content in media tracks can be correctly decoded. Players may utilize reception hint tracks for handling of degradations caused by the transmission, i.e., content that may not be correctly decoded is located only within reception hint tracks. The need for having a duplicate of the correct media samples in both a media track and a reception hint track can be avoided by including data from the media track by reference into the reception hint track.

### Media handler

Hint media uses the 'hint' handler type in the HandlerBox of the MediaBox, as defined in 8.4.3.

### Hint media header

#### Hint media header box

Box Types: 'hmhd'  
Container: MediaInformationBox  
Mandatory: Yes  
Quantity: Exactly one specific media header shall be present

Hint tracks use the HintMediaHeaderBox in the MediaInformationBox, as defined in 8.4.5. The hint media header contains general information, independent of the protocol, for hint tracks. (A PDU is a protocol data unit.)

#### Syntax

aligned(8) class HintMediaHeaderBox  
 extends FullBox('hmhd', version = 0, 0)   
{  
 unsigned int(16) maxPDUsize;  
 unsigned int(16) avgPDUsize;  
 unsigned int(32) maxbitrate;  
 unsigned int(32) avgbitrate;  
 unsigned int(32) reserved = 0;  
}

#### Semantics

version is an integer that specifies the version of this box

maxPDUsize gives the size in bytes of the largest PDU in this (hint) stream

avgPDUsize gives the average size of a PDU over the entire presentation

maxbitrate gives the maximum rate in bits/second over any window of one second

avgbitrate gives the average rate in bits/second over the entire presentation

### Sample entry

#### Definition

Hint tracks use an entry format specific to their protocol, with an appropriate name.

For hint tracks, the sample entry contains appropriate declarative data for the streaming protocol being used, and the format of the hint track. The definition of the sample entry is specific to the protocol.

The protocol (codingname) field is a registered identifier that uniquely identifies the streaming protocol or compression format decoder to be used. A given protocol may have optional or required extensions to the sample entry (e.g. codec initialization parameters). All such extensions shall be within boxes; these boxes occur after the required fields. Unrecognized boxes shall be ignored.

#### Syntax

class HintSampleEntry() extends SampleEntry (protocol)   
{  
}

## Text media

### Media handler

The timed text media type indicates that the associated decoder will process only text data. Timed text media uses the 'text' handler type in the HandlerBox of the MediaBox, as defined in 8.4.3.

### Media header

Timed text tracks use a NullMediaHeaderBox, as defined in subclause 8.4.5.2.

### Sample entry

#### Definition

Timed text tracks use PlainTextSampleEntry.

#### Syntax

class PlainTextSampleEntry(codingname) extends SampleEntry (codingname)   
{  
}

class SimpleTextSampleEntry() extends PlainTextSampleEntry ('stxt')   
{  
 utf8string content\_encoding; // optional  
 utf8string mime\_format;   
 TextConfigBox (); // optional  
}

#### Semantics

content\_encoding provides a MIME type which identifies the content encoding of the timed text. It is defined in the same way as for an ItemInfoEntry in this document. If not present (an empty string is supplied) the timed text is not encoded. An example for this field is ‘application/zip’.

mime\_format provides a MIME type which identifies the content format of the samples. Examples for this field include ‘text/html’ and ‘text/plain’.

## Subtitle media

### Media handler

The subtitle media type indicates that the associated decoder will process text data and possibly images. Subtitle media uses the 'subt' handler type in the HandlerBox of the MediaBox, as defined in 8.4.3.

### Subtitle media header

#### Definition

Subtitle tracks use the SubtitleMediaHeaderBox in the MediaInformationBox, as defined in 8.4.5. The subtitle media header contains general presentation information, independent of the coding, for subtitle media. This header is used for all tracks containing subtitles.

#### Syntax

aligned(8) class SubtitleMediaHeaderBox  
 extends FullBox ('sthd', version = 0, flags = 0)  
{  
}

#### Semantics

version - is an integer that specifies the version of this box.

flags - is a 24-bit integer with flags (currently all zero).

### Sample entry

#### Definition

Subtitle tracks use SubtitleSampleEntry.

#### Syntax

class SubtitleSampleEntry(codingname) extends SampleEntry (codingname)   
{  
}

class XMLSubtitleSampleEntry() extends SubtitleSampleEntry ('stpp')   
{  
 utf8list namespace;  
 utf8list schema\_location; // optional  
 utf8list auxiliary\_mime\_types;  
 // optional, required if auxiliary resources are present  
}

class TextSubtitleSampleEntry() extends SubtitleSampleEntry ('sbtt')   
{  
 utf8string content\_encoding; // optional  
 utf8string mime\_format;  
 TextConfigBox (); // optional  
}

#### Semantics

content\_encoding provides a MIME type which identifies the content encoding of the subtitles. It is defined in the same way as for an ItemInfoEntry in this document. If not present (an empty string is supplied) the subtitle samples are not encoded. An example for this field is ‘application/zip’.

namespace is one or more XML namespaces to which the sample documents conform. When used for metadata, this is needed for identifying its type, e.g. gBSD or AQoS [MPEG-21-7] and for decoding using XML aware encoding mechanisms such as BiM.

schema\_location is zero or more URLs for XML schema(s) to which the sample document conforms. If there is one namespace and one schema, then this field shall be the URL of the one schema. If there is more than one namespace, then the syntax of this field shall adhere to that for xsi:schemaLocation attribute as defined by XML. When used for metadata, this is needed for decoding of the timed metadata by XML aware encoding mechanisms such as BiM.

mime\_format provides a MIME type which identifies the content format of the samples. Examples for this field include ‘text/html’ and ‘text/plain’.

auxiliary\_mime\_types indicates the media type of all auxiliary resources, such as images and fonts, if present, stored as subtitle sub-samples.

optional\_box may be a BitRateBox or a MIMEBox or other box. When both BitRateBox and MIMEBox are present, they may be in any order. Parsers shall allow other boxes to be present.

## Font media

### Media handler

Font media uses the 'fdsm' handler type in the HandlerBox of the MediaBox, as defined in 8.4.3.

### Media header

Font tracks use a NullMediaHeaderBox.

### Sample entry

#### Definition

Font streams use a FontSampleEntry.

#### Syntax

class FontSampleEntry(codingname) extends SampleEntry (codingname)  
{  
 //other boxes from derived specifications  
}

## Void

## Multiplexed timed metadata tracks

### General

Multiplexed timed metadata tracks

1. allow the carriage of any user-data item (untimed metadata) as timed metadata; this allows the 'radio station' case where song title, performer, etc. need to change as songs change;
2. allow the multiplexing together of formats; so, for example, a camera might record both location and facing direction in the same sample.

### Overall design

Timed metadata multiplex is a specific format of a metadata track (subclause 12.3); it has a sample entry code, sample entry definitions, and a sample format. The sample entry code is 'mebx', standing for 'metadata boxed'.

The track reference 'cdsc' should be used as described in subclause 12.3.1.

The sample entry sets up an association between a compact, fixed-size, identifier used in the streams (repeatedly) and the permanent, possibly long-format, identifier, of the metadata and any parameters.

### Sample format

A media sample is structured as a concatenation of one or more value Boxes (as defined in subclause 4.2). The four-character-codes of these boxes are local keys and shall be declared in the sample entry; the setup for these keys allows various associations (e.g. as equivalent to a user-data item, as equivalent to an un-multiplexed timed metadata sample, etc.). The content of the box is defined by the association.

If no value for a particular key is present in the sample at the given time, the interpretation should be that there is no metadata of that type at the time. Metadata values for that key for other times (e.g. from a previous sample) should not be interpreted as applying to the target time.

If no values for any key are present for a time range, the best practice is to include a sample with only a “NULL” data entry for the time range as defined in subclause 12.9.5.

### Sample entry format

#### General

The sample entry for boxed timed metadata is the BoxedMetadataSampleEntry:

aligned(8) class BoxedMetadataSampleEntry  
 extends MetaDataSampleEntry ('mebx')   
{  
 MetadataKeyTableBox(); // mandatory  
 BitRateBox (); // optional  
}

The only required box within BoxedMetadataSampleEntry is MetadataKeyTableBox which defines what metadata values may be found in the AUs of the track.

MetadataKeyTableBox (defined in 12.9.4.2) is a table indicating the set of keys and information about each key that may occur in associated samples.

BitRateBox is an optional box to signal the bitrate of the metadata stream.

#### Metadata key table box

Box Type: 'keys'  
Container: BoxedMetadataSampleEntry  
Mandatory: Yes  
Quantity: Exactly one

The MetadataKeyTableBox contains a table of keys and mappings to payload data in the corresponding samples. It is defined as:

aligned(8) class MetadataKeyTableBox extends Box('keys')   
{  
 MetadataKeyBox[];  
}

This is a box containing one or more instances of MetadataKeyBox, one for each “configuration” of key that may occur in the samples of the track. For example, if there are two keys, there will be two MetadataKeyBox boxes in the MetadataKeyTableBox – one for each key.

If the MetadataKeyTableBox does not contain a key for which a client is searching no samples associated with this sample entry contain values with that key.

If the MetadataKeyTableBox does contain a particular key, this does not however guarantee that any samples containing a value for the key were written. Clients finding a key in the MetadataKeyTableBox may still need to look through the track’s samples for values to determine if the track has the particular metadata.

NOTE This rule allows a sample entry to be populated (say during a capture process) with keys that might be discovered and then samples to be written with a binding only for the keys found. There is no requirement that the sample entry be rewritten to exclude the key that was not needed. This makes writing using movie fragments easier as the sample entries in the initial movie never need to be rewritten.

Whenever possible, it is preferred to remove unused sample entries efficiently and rewrite the sample entry.

#### Metadata key box

##### Definition

Box Type: locally defined  
Container: MetadataKeyTableBox  
Mandatory: Yes  
Quantity: One or more

The box type for each MetadataKeyBox is here referred to as 'local\_key\_id' and serves (1) as a unique identifier among all MetadataKeyBoxes and (2) as the identifier for the metadata value boxes within samples that have that key.

The box type for the contained MetadataKeyBox is 'local' to the containing track and corresponds to the box types (32-bit integers or four-character-codes) for boxes within metadata samples that hold that particular metadata value. For example, if the MetadataKeyBox has the box type of 'stuf', any boxes of type 'stuf' in samples sharing this sample entry hold the value for this key. Values fitting in a 32-bit big endian integer can be used (e.g. 'stuf', the integer 72). It is recommended that it be mnemonic if possible. Values 0 and 0xFFFFFFFF are reserved and shall not be used to defiend new boxes.

There are two reserved box types for boxes of type MetadataKeyBox: 0 and 0xFFFFFFFF. A local\_key\_id of 0 in the MetadataKeyBox indicates that the MetadataKeyBox is unused and should not be interpreted. This allows the key to be marked as unused in the sample entry without requiring the sample entry and parent atoms to be rewritten/resized. (A box-type of 0 in a sample indicates 'null' metadata, see below). A local\_key\_id of 0xFFFFFFFF should never occur in MetadataKeyBox as this special value can be used to signal inline key/value boxes within samples.

All other box types are available to define box types used in samples.

NOTE Because the children boxes within MetadataKeyTableBox can take on any box type, there is be no special interpretation of the box type for contained boxes other than the special value 0. Therefore, including a FreeSpaceBox does not have the conventional meaning in the MetadataKeyBox. Even so, it is suggested that the use of overly confusing use of existing four-character-codes be avoided.

Each MetadataKeyBox contains a variable number of boxes that define the key structure, the datatype for values, optionally the locale for the values, and optional setup information needed to interpret the value. In future versions of this document, new children boxes may be introduced.

##### Syntax

aligned(8) class MetadataKeyBox extends Box(local\_key\_id)   
{   
 MetadataKeyDeclarationBox();  
 MetadataLocaleBox(); // optional   
 MetadataSetupBox(); // optional  
 // other boxes may be present  
}

#### Metadata key declaration box

##### Definition

Box Type: 'keyd'  
Container: MetadataKeyBox  
Mandatory: Yes  
Quantity: Exactly one

The MetadataKeyDeclarationBox holds the key namespace and key value of that namespace for the given values.

##### Syntax

aligned(8) class MetadataKeyDeclarationBox extends Box('keyd')   
{   
 unsigned int(32) key\_namespace;  
 unsigned int(8) key\_value[];  
}

##### Semantics

key\_namespace is a 32-bit identifier describing the domain and the structure of the key\_value. For example, this can indicate that key\_value is a reverse-address style null-terminated string using UTF-8 (e.g. "com.foo.mymetadata"), a binary four-character codes (e.g. 'cprt' user data key), a Uniform Resource Identifier (URI), or other structures (e.g. native formats from metadata standards such as MXF). New key\_namespaces are registered, but as a URI can often be used, using the URI key namespace may be sufficient for most uses. Unrecognized key namespaces shall cause the associated key, and the sample data for that key, data to be ignored.

key\_value is an array of bytes holding the key and whose interpretation is defined by the associated key\_namespace field.

#### Metadata locale box

##### Definition

Box Type: 'loca'  
Container: MetadataKeyBox  
Mandatory: No  
Quantity: Zero or one

A metadata value may optionally be tagged with its locale so that it may be chosen based upon the user's language, country, etc. This makes it possible to include several keys of the same key type (e.g. copyright or scene description) but with differing locales for users of different languages or locations. This allows one track to hold different localizations for a particular key.

This is accomplished by including a MetadataLocaleBox within the MetadataKeyBox.

If the MetadataLocaleBox is absent, corresponding metadata values should be considered appropriate for all locales. Example locale strings include 'en-US', 'fr-FR', or 'zh-CN'.

##### Syntax

aligned (8) class MetadataLocaleBox extends Box('loca')   
{   
 utf8string locale\_string;  
}

##### Semantics

locale\_string holds a language tag complying with IETF  BCP 47.

#### Metadata setup box

##### Definition

Box Type: 'setu'  
Container: MetadataKeyBox  
Mandatory: No  
Quantity: Zero or one

For some key\_namespaces, setup data is needed. The contents of the MetadataSetupBox are defined by the key\_namespace. (For example, it contains the boxes present in the sample entry, for the case of multiplexed timed metadata).

##### Syntax

aligned(8) class MetadataSetupBox extends Box('setu')   
{   
 // leaf data or array of Boxes  
}

### Defined formats

#### Null

A NULL value (and hence sample) can be signalled using a single box with the reserved value of 0 for local\_key\_id. The contents of any such boxes should be ignored and may be present. No setup is needed for NULL values; they may be present in any multiplex without declaration.

Null values may also be used to pad samples e.g. to a constant size, or to mark a value as no longer relevant without having to edit the file or samples, simply by changing the box type to 0.

#### User-data

The key\_namespace 'uiso' (ISO user-data) indicates that the key is mapped to the user-data four-character-code indicated by the key\_value, which shall be 4 bytes in big-endian order, and shall be a code valid as user-data. When key\_namespace equal to 'uiso' is used, the MetadataSetupBox shall not be used.

For ease of reading and inspection, it is suggested that the local\_key\_id and the original user-data four-character-code be equal. However readers shall not rely on any particular values of local\_key\_id.

#### Storing timed metadata in multiplexed timed metadata tracks

The key\_namespace 'me4c' (metadata sample entry four-character-code) indicates that the values are valid timed metadata samples in their own right.

This key\_namespace indicates that the key is mapped to the sample-entry four-character-code, that is valid for metadata tracks, indicated by the key\_value, which shall be 4 bytes in big-endian order, and shall be a code valid for a metadata track sample entry. All the extra data present as mandatory extensions to the MetaDataSampleEntry for that sample entry four-character-code shall be present in the MetadataSetupBox.

For ease of reading and inspection, it is suggested that the local\_key\_id and the original sample-entry four-character-code be equal. However readers shall not rely on any particular values of local\_key\_id.

NOTE These are already defined by this document, and there are others defined elsewhere (e.g. 3GPP): XMLMetaDataSampleEntry, TextMetaDataSampleEntry and URIMetaSampleEntry.

#### Other forms

Other key\_namespaces may be registered and used. If an unrecognized key\_namespace is found, the associated sample entry and sample data shall be ignored.

Other possible key\_namespaces include URI and URNs, though formats for timed metadata (and hence that can be multiplexed) for URIs already exist.

## Volumetric visual media

### Media handler

Volumetric visual media uses the 'volv' handler type in the HandlerBox of the MediaBox, as defined in 8.4.3. Multiple volumetric visual tracks may be present in the file.

### Media header

#### Definition

Box Type: 'vvhd'  
Container: MediaInformationBox  
Mandatory: Yes  
Quantity: Exactly one

Volumetric visual tracks use the VolumetricVisualMediaHeaderBox in the MediaInformationBox as defined in 8.4.5. The volumetric visual media header contains general presentation information, independent of the coding, for volumetric visual media. This header shall be used in any track containing volumetric visual media.

#### Syntax

aligned(8) class VolumetricVisualMediaHeaderBox  
 extends FullBox('vvhd', 0, 0)   
{  
}

### Sample entry

#### Definition

Volumetric visual media tracks shall use a VolumetricVisualSampleEntry.

#### Syntax

class VolumetricVisualSampleEntry(codingname)   
 extends SampleEntry (codingname)  
{  
 unsigned int(8) compressorname[32];  
 // other boxes from derived specifications  
}

#### Semantics

compressorname is a name, for informative purposes. It is formatted in a fixed 32-byte field, with the first byte set to the number of bytes to be displayed, followed by that number of bytes of displayable data encoded using UTF-8, and then padding to complete 32 bytes total (including the size byte). The field may be set to 0.

### Sample format

The format of a volumetric visual sample is defined by the coding system.

## Haptic media

### Media handler

Haptic media uses the 'hapt' handler type in the HandlerBox of the MediaBox, as defined in 8.4.3.

### Media header

Haptics tracks use the NullMediaHeaderBox in the MediaInformationBox as defined in 8.4.5.

### Sample entry

#### Definition

Haptic tracks use HapticSampleEntry.

The HapticSampleEntry extends the SampleEntry class and holds haptic configuration information. This configuration information may be further extended using boxes for codec-specific information.

#### Syntax

aligned(8) class HapticSampleEntry(codingname)  
 extends SampleEntry(codingname)   
{  
 Box otherboxes[];  
}

### Sample format

The haptics coding format defines the format of a haptics sample. It also defines whether the coding format is all sync-sample, and if not, defines what a sync sample is.

# Transformed media tracks

## General

Protected media is described in 13.4.

Restricted media is described in 13.5.

Incomplete media is described in 13.6.

## Multiple transformations for a single transformed media track

A transformed media track may have undergone several transformations of different types and shall not have undergone more than one transformation of any particular type.

NOTE For example, a transformed media track can be both protected and restricted.

The following process applies to conclude the untransformed sample entry type of a transformed media track:

1. Let schemeInfoContainerBox be ProtectionSchemeInfoBox, RestrictedSchemeInfoBox, or CompleteTrackInfoBox when the track sample entry type indicates an encrypted, restricted, or incomplete media track, respectively.
2. Let dataFormat be equal to the data\_format value of OriginalFormatBox of schemeInfoContainerBox.
3. If dataFormat indicates a transformed media track, schemeInfoContainerBox is updated to be ProtectionSchemeInfoBox, RestrictedSchemeInfoBox, or CompleteTrackInfoBox when dataFormat indicates an encrypted, restricted, or incomplete media track, respectively. The process continues from step 2.
4. Otherwise (dataFormat does not indicate a transformed media track), the untransformed sample entry type is concluded to be equal to dataFormat.

## Determining the untransformed sample entry type

#### General

A transformed media track may have undergone several transformations of different types but cannot have undergone more than one transformation of any particular type.

The following process applies to conclude the untransformed sample entry type (as defined in the following subclause) of a transformed media track:

1. Let schemeInfoContainerBox be any ProtectionSchemeInfoBox, the RestrictedSchemeInfoBox, or the CompleteTrackInfoBox when the sample entry type of the track (i.e., the format value of a SampleEntry directly contained in the SampleDescriptionBox) indicates an encrypted, restricted, or incomplete media track, respectively.
2. Let dataFormat be equal to the data\_format value of OriginalFormatBox of schemeInfoContainerBox.
3. If dataFormat indicates a transformed media track, schemeInfoContainerBox is updated to be ProtectionSchemeInfoBox, RestrictedSchemeInfoBox, or CompleteTrackInfoBox when dataFormat indicates an encrypted, restricted, or incomplete media track, respectively. The process continues from step 2.
4. Otherwise (dataFormat does not indicate a transformed media track), the untransformed sample entry type is concluded to be equal to dataFormat.

### Example for protected and restricted media (informative)

For example, a transformed media track can be both protected and restricted, in which case the relevant boxes in the sample entry can be set as follows:

SampleEntry('encv')   
{  
 ProtectionSchemeInfoBox {  
 OriginalFormatBox; // data\_format is 'resv'  
 SchemeTypeBox;  
 SchemeInformationBox;  
 }  
 RestrictedSchemeInfoBox {  
 OriginalFormatBox; // data\_format indicates a codec, e.g. 'avc1'  
 SchemeTypeBox;  
 SchemeInformationBox;  
 }  
 // Boxes specific to the untransformed sample entry type  
 // For 'avc1', these include AVCConfigurationBox  
}

### The 'codecs' MIME parameter for a transformed media track

The 'codecs' parameter value for transformed media tracks is described in Annex K.

## Support for protected streams

### Overview

This subclause documents the file-format transformations which are used for protected content. These transformations can be used under several circumstances:

* They shall be used when the content has been transformed (e.g. by encryption) in such a way that it can no longer be decoded by the normal decoder;
* They may be used when the content should only be decoded when the protection system is understood and implemented.

The transformation functions by *encapsulating* the original media declarations. The encapsulation changes the four character-code of the sample entries, so that protection-unaware readers see the media stream as a new stream format.

Because the format of a sample entry varies with media-type, a different encapsulating four character-code is used for each media type (audio, video, text etc.). They are shown in Table 13.

Table 13 — Protected sample-entry codes

|  |  |  |
| --- | --- | --- |
| **Stream (Track) Type** | **Sample-Entry Code** | **SampleEntry Class** |
| Video | encv | VisualSampleEntry |
| Audio | enca | AudioSampleEntry or AudioSampleEntryV1 |
| Metadata | encm | MetaDataSampleEntry |
| Text | enct | SimpleTextSampleEntry |
| Subtitle | encu | XMLSubtitleSampleEntry |
| Systema | encs |  |
| Font | encf | FontSampleEntry |
| Haptics | encp | HapticSampleEntry |
| Volumetric visual | enc3 | VolumetricVisualSampleEntry |
| a   System streams are defined in ISO/IEC 14496-14[3]. | | |

The transformed sample entry type shall only be used with the indicated sample entry classes, or classes derived from them that add only boxes (but not fields).

A protected sample entry is defined as using one of the preceding sample entry codes, and the following transformation procedure:

1. The four character code of the sample entry is replaced with a four character code indicating protection encapsulation: these codes vary only by media-type. For example, 'mp4v' is replaced with 'encv' and 'mp4a' is replaced with 'enca'.
2. A ProtectionSchemeInfoBox (*defined below*) is added to the sample entry, leaving all other boxes unmodified.
3. The original sample entry type (four character code) is stored within the ProtectionSchemeInfoBox, in a new box called the OriginalFormatBox (defined below);

There are then three methods for signalling the nature of the protection, which may be used individually or in combination.

1. When MPEG-4 systems is used, then IPMPshall be used to signal that the streams are protected.
2. IPMP descriptors may also be used outside the MPEG-4 systems context using boxes containing IPMP descriptors.
3. The protection applied may also be described using the scheme type and information boxes.

When IPMP is used outside of MPEG-4 systems, then a ‘global’ IPMPControlBox may also occur within the MovieBox.

NOTE When MPEG-4 systems is used, an MPEG-4 systems terminal can effectively treat, for example, 'encv' with an original format of 'mp4v' exactly the same as 'mp4v', by using the IPMP descriptors.

### Protection scheme information box

* + - 1. Definition

Box Types: 'sinf'  
Container: Protected Sample Entry, or ItemProtectionBox  
Mandatory: Yes  
Quantity: One or More

The ProtectionSchemeInfoBox contains all the information required both to understand the encryption transform applied and its parameters, and also to find other information such as the kind and location of the key management system. It also documents the original (unencrypted) format of the media. The ProtectionSchemeInfoBox is a container Box. It is mandatory in a sample entry that uses a code indicating a protected stream.

When used in a protected sample entry, this box shall contain the OriginalFormatBox to document the original format. At least one of the following signalling methods shall be used to identify the protection applied:

1. MPEG-4 systems with IPMP: no other boxes, when IPMP descriptors in MPEG-4 systems streams are used;
2. Scheme signalling: a SchemeTypeBox and SchemeInformationBox, when these are used (either both shall occur, or neither).

At least one ProtectionSchemeInfoBox shall occur in a protected sample entry. When more than one occurs, they are equivalent, alternative, descriptions of the same protection. Readers should choose one to process.

* + - 1. Syntax

aligned(8) class ProtectionSchemeInfoBox(fmt) extends Box('sinf')   
{  
 OriginalFormatBox(fmt) original\_format;  
 // mandatory for sample protection,   
 // shall not be present for item protection  
  
 SchemeTypeBox scheme\_type\_box; // optional  
 SchemeInformationBox info; // optional  
}

### Original format box

* + - 1. Definition

Box Types: 'frma'  
Container: ProtectionSchemeInfoBox, RestrictedSchemeInfoBox, or  
 CompleteTrackInfoBox  
Mandatory: Yes when used in a protected sample entry, in a restricted sample entry, or  
 in a sample entry for an incomplete track.  
Quantity: Exactly one.

The OriginalFormatBox contains the four character code of the original un-transformed sample entry.

* + - 1. Syntax

aligned(8) class OriginalFormatBox(codingname) extends Box ('frma')   
{  
 unsigned int(32) data\_format = codingname;  
 // format of decrypted, encoded data (in case of protection)  
 // or un-transformed sample entry (in case of restriction  
 // and complete track information)  
}

* + - 1. Semantics

data\_format is the four character code of the original un-transformed sample entry (e.g. 'mp4v' if the stream contains protected or restricted MPEG-4 visual material).

### IPMPInfoBox

This box has been deprecated and is no longer defined in this document.

### IPMP control box

This box has been deprecated and is no longer defined in this document.

### Scheme type box

* + - 1. Definition

Box Types: 'schm'  
Container: ProtectionSchemeInfoBox, RestrictedSchemeInfoBox,  
 or SRTPProcessBox  
Mandatory: No  
Quantity: Zero or one in 'sinf', depending on the protection structure; Exactly one in 'rinf' and 'srpp'

The SchemeTypeBox identifies the protection or restriction scheme.

* + - 1. Syntax

aligned(8) class SchemeTypeBox extends FullBox('schm', 0, flags)   
{  
 unsigned int(32) scheme\_type; // 4CC identifying the scheme  
 unsigned int(32) scheme\_version; // scheme version  
 if (flags & 0x000001) {  
 utf8string scheme\_uri; // browser uri  
 }  
}

* + - 1. Semantics

scheme\_type is the code defining the protection or restriction scheme, normally expressed as a four character code;

scheme\_version is the version of the scheme (used to create the content)

scheme\_URI is an absolute URI allowing for the option of directing the user to a web-page if they do not have the scheme installed on their system.

### Scheme information box

* + - 1. Definition

Box Types: 'schi'  
Container: ProtectionSchemeInfoBox, RestrictedSchemeInfoBox,  
 or SRTPProcessBox  
Mandatory: No  
Quantity: Zero or one

The SchemeInformationBox is a container Box that is only interpreted by the scheme being used. Any information the encryption or restriction system needs is stored here. The content of this box is a series of boxes whose type and format are defined by the scheme declared in the SchemeTypeBox.

* + - 1. Syntax

aligned(8) class SchemeInformationBox extends Box('schi')   
{  
 Box scheme\_specific\_data[];  
}

### Scramble Scheme Information Box

* + - 1. Definition

Box Types: 'scrb'  
Container: Sample entry or ItemPropertyContainerBox  
Mandatory: Yes, if the media sample(s) associated with the sample entry or the associated item(s)   
 use a scrambling scheme  
Quantity: One or More

In the context of this document, a scrambling operation on media stream is the process of modifying binary patterns in a compressed media stream without modifying the media bitstream syntax (i.e. decoding without reverting the scramble is syntactically correct). The ScrambleSchemeInfoBox contains all the information required both to understand the scrambling operation applied and its parameters, and also to find other information such as the kind and location of the key management system. The ScrambleSchemeInfoBox is a container box.

It is mandatory in a sample entry for which media samples use a scrambling scheme resulting in media content compliant with the requirements of the media format identified by the sample entry type of the track, if the track is not a transformed media track, or by the untransformed sample entry type, otherwise.

For an item consisting of media using a scrambling scheme resulting in media content compliant with the requirements of the media format identified by the item type, this property shall be present in the ItemPropertyContainerBox and the protected item shall have this property listed as a non-essential property.

This box shall not be used for any scrambling scheme resulting in a cyphered media stream not compatible with the requirements of the media format identified by the sample entry type or item type.

NOTE The ScrambleSchemeInfoBox is identical to the ProtectionSchemeInfoBox except that (a) it uses the four-character code 'scrb' and (b) does not contain an OriginalFormatBox.

* + - 1. Syntax

aligned(8) class ScrambleSchemeInfoBox extends Box('scrb')   
{  
 SchemeTypeBox scheme\_type\_box;  
 SchemeInformationBox info; // optional  
}

## Restricted media tracks

### General

In order to handle situations where the file author requires certain actions on the player or renderer, this subclause specifies a mechanism that enables players to simply inspect a file to find out such requirements for rendering a bitstream and stops legacy players from decoding and rendering files that require further processing. The mechanism applies to any type of video codec. In particular it applies to AVC and for this case specific signalling is defined in the AVC file format (ISO/IEC 14496-15[3]) that allows a file author to list occurring SEI message IDs and distinguish between required and non-required actions for the rendering process.

The mechanism is similar to the content protection transformation where sample entries are hidden behind generic sample entries, 'encv', 'enca', etc., indicating encrypted or encapsulated media. The analogous mechanism for restricted video uses a transformation with the generic sample entry 'resv'. The method may be applied when the content should only be decoded by players that present it correctly.

### Restricted sample entry transformation

A restricted sample entry is defined as a sample entry on which the following transformation procedure has been applied:

* 1. The four character code of the sample entry is replaced by a sample entry code as defined in Table 14 below.
  2. A RestrictedSchemeInfoBox is added to the sample entry, leaving all other boxes unmodified.
  3. The original sample entry type is stored within an OriginalFormatBox contained in the RestrictedSchemeInfoBox.

Table 14 — Restricted sample-entry codes

|  |  |  |
| --- | --- | --- |
| **Stream (Track) Type** | **Sample-Entry Code** | **SampleEntry Class** |
| Video | resv | VisualSampleEntry |
| Audio | resa | AudioSampleEntry or AudioSampleEntryV1 |
| Metadata | resm | MetaDataSampleEntry |
| Text | rest | SimpleTextSampleEntry |
| Subtitle | resu | XMLSubtitleSampleEntry |
| Systema | ress |  |
| Font | resf | FontSampleEntry |
| Haptics | resp | HapticSampleEntry |
| Volumetric visual | res3 | VolumetricVisualSampleEntry |
| a System streams are defined in ISO/IEC 14496-14**[8]**. | | |

A RestrictedSchemeInfoBox is formatted exactly the same as a ProtectionSchemeInfoBox, except that is uses the identifier 'rinf' instead of 'sinf' (see below).

The original sample entry type is contained in the OriginalFormatBox located in the RestrictedSchemeInfoBox (in an identical way to the ProtectionSchemeInfoBox for encrypted media).

The exact nature of the restriction is defined in the SchemeTypeBox, and the data needed for that scheme is stored in the SchemeInformationBox, again, analogously to protection information.

Restriction and protection can be applied at the same time. The order of the transformations follows from the four-character code of the sample entry. For instance, if the sample entry type is 'resv', undoing the above transformation may result in a sample entry type 'encv', indicating that the media is protected.

If the file author only wants to provide advisory information without stopping legacy players from playing the file, the RestrictedSchemeInfoBox may be placed inside the sample entry without transforming the four character code. In this case it is not necessary to include an OriginalFormatBox.

### Restricted scheme information box

#### Definition

Box Types: 'rinf'  
Container: Restricted Sample Entry or Sample Entry  
Mandatory: Yes in Restricted Sample Entry, no otherwise  
Quantity: Zero or one

The RestrictedSchemeInfoBox contains all the information required both to understand the restriction scheme applied and its parameters. It also documents the original (un-transformed) sample entry type of the media. The RestrictedSchemeInfoBox is a container Box. It is mandatory in a sample entry that uses a code indicating a restricted stream, i.e., 'resv'.

When used in a restricted sample entry, this box shall contain the OriginalFormatBox to document the original sample entry type and a SchemeTypeBox. A SchemeInformationBox may be required depending on the restriction scheme.

#### Syntax

aligned(8) class RestrictedSchemeInfoBox(fmt) extends Box('rinf')   
{  
 OriginalFormatBox original\_format(fmt);  
 SchemeTypeBox scheme\_type\_box;  
 SchemeInformationBox info; // optional  
}

### Scheme for stereoscopic video arrangements

#### General

When stereo-coded video frames are decoded, the decoded frames either contain a representation of two spatially packed constituent frames that form a stereo pair (frame packing) or only one view of a stereo pair (left and right views in different tracks). Restrictions due to stereo-coded video are contained in the StereoVideoBox.

scheme\_type equal to 'stvi' (stereoscopic video) is used.

#### Stereo video box

##### Definition

Box Type: 'stvi'  
Container: SchemeInformationBox  
Mandatory: Yes (when scheme\_type is 'stvi')  
Quantity: One

The StereoVideoBox is used to indicate that decoded frames either contain a representation of two spatially packed constituent frames that form a stereo pair or contain one of two views of a stereo pair. The StereoVideoBox shall be present when scheme\_type is 'stvi'.

When the value of stereo\_indication\_type indicates the temporal interleaving frame packing arrangement and the display system in use presents two views simultaneously, readers should implicitly set the composition timestamp for constituent picture 0 to coincide with the composition timestamp for constituent picture 1.

##### Syntax

aligned(8) class StereoVideoBox extends FullBox('stvi', version = 0, 0)  
{  
 template unsigned int(30) reserved = 0;  
 unsigned int(2) single\_view\_allowed;  
 unsigned int(32) stereo\_scheme;  
 unsigned int(32) length;  
 unsigned int(8) stereo\_indication\_type[length];  
 Box any\_box[]; // optional  
}

##### Semantics

single\_view\_allowed is an integer. A zero value indicates that the content may only be displayed on stereoscopic displays. When (single\_view\_allowed & 1) is equal to 1, it is allowed to display the right view on a monoscopic single-view display. When (single\_view\_allowed & 2) is equal to 2, it is allowed to display the left view on a monoscopic single-view display.

stereo\_scheme is an integer that indicates the stereo arrangement scheme used and the stereo indication type according to the used scheme. The following values for stereo\_scheme are specified:

1: the frame packing scheme as specified by the Frame packing arrangement Supplemental Enhancement Information message of ISO/IEC 14496-10:2014,

2: the arrangement type scheme as specified in ISO/IEC 10646, Annex D

3: the stereo scheme as specified in ISO/IEC 23000-11[6] for both frame/service compatible and 2D/3D mixed services.

4,5: values of VideoFramePackingType, QuincunxSamplingFlag. PackedContentInterpretationTypeas defined in ISO/IEC 23091-2.

Other values of stereo\_scheme are reserved.

length indicates the number of bytes for the stereo\_indication\_type field.

stereo\_indication\_type indicates the stereo arrangement type according to the used stereo indication scheme. The syntax and semantics of stereo\_indication\_type depend on the value of stereo\_scheme. The syntax and semantics for stereo\_indication\_type for the following values of stereo\_scheme are specified as follows:

stereo\_scheme equal to 1: The value of length shall be 4 and stereo\_indication\_type shall be unsigned int(32) which contains the frame\_packing\_arrangement\_type value from ISO/IEC 14496-10:2014,, Table D-8. (‘Definition of frame\_packing\_arrangement\_type’).

stereo\_scheme equal to 2: The value of length shall be 4 and stereo\_indication\_type shall be unsigned int(32) which contains the type value from ISO/IEC 10646, Table D.1 (‘Definition of arrangement\_type’).

stereo\_scheme equal to 3: The value of length shall be 2 and stereo\_indication\_type shall contain two syntax elements of unsigned int(8). The first syntax element shall contain the stereoscopic composition type from ISO/IEC 23000-11:2009[6], Table 4. The least significant bit of the second syntax element shall contain the value of is\_left\_first as specified in ISO/IEC 23000-11:2009[6], subclause 8.4.3, while the other bits are reserved and shall be set to 0.

stereo\_scheme equal to 4: The value of length shall be 2 and stereo\_indication\_type shall contain two syntax elements of unsigned int(8). The first syntax element shall contain a **VideoFramePackingType** from ISO/IEC 23091-2. The least significant bit of the second syntax element shall contain the value of **QuincunxSamplingFlag** as specified in ISO/IEC 23091-2, while the other bits are reserved and shall be set to 0. **PackedContentInterpretationType** specified in ISO/IEC 23091-2 is inferred to be equal to 1.

stereo\_scheme equal to 5: The value of length shall be 3 and stereo\_indication\_type shall contain three syntax elements of type unsigned int(8). The first syntax element shall contain a **VideoFramePackingType** from ISO/IEC 23091-2. The least significant bit of the second syntax element shall contain the value of **QuincunxSamplingFlag** as specified in ISO/IEC 23091-2, while the other bits are reserved and shall be set to 0. The third syntax element shall contain the **PackedContentInterpretationType** from ISO/IEC 23091-2.

The following applies when the StereoVideoBox is used:

* In the TrackHeaderBox
  + width and height in the TrackHeaderBox specify the visual presentation size of a single view after unpacking.
* The following specifications apply for syntax elements and boxes in a SampleEntry in the SampleDescriptionBox
  + frame\_count shall be 1, because the decoder physically outputs a single frame. In other words, the constituent frames included within a frame-packed picture are not documented by frame\_count.
  + width and height document the pixel counts of a frame-packed picture (and not the pixel counts of a single view within a frame-packed picture).
  + the PixelAspectRatioBox documents the pixel aspect ratio of each view when the view is displayed on a monoscopic single-view display. For example, in many spatial frame packing arrangements, the pixel aspect ratio box therefore indicates 2:1 or 1:2 pixel aspect ratio, as the spatial resolution of one view of frame-packed video is typically halved along one coordinate axis compared to that of the single-view video of the same format.

### Compatible scheme type box

#### Definition

Box Type: 'csch'  
Container: RestrictedSchemeInfoBox  
Mandatory: No  
Quantity: Zero or more

CompatibleSchemeTypeBox identifies a scheme type that the track conforms to. The SchemeTypeBox and the instances of CompatibleSchemeTypeBox provide the possibility to indicate several scheme\_type values for the same track. The track conforms to all the constraints imposed by all indicated scheme\_type values among the SchemeTypeBox and the instances of CompatibleSchemeTypeBox within the same RestrictedSchemeInfoBox.

Parsers that are capable of processing any indicated scheme\_type value among the SchemeTypeBox or any instance of CompatibleSchemeTypeBox are allowed to process the track provided that they process all the boxes contained in the SchemeInformationBox.

#### Syntax

aligned(8) class CompatibleSchemeTypeBox   
 extends FullBox('csch', 0, flags)   
{  
 // identical syntax to SchemeTypeBox  
 unsigned int(32) scheme\_type; // 4CC identifying the scheme  
 unsigned int(32) scheme\_version; // scheme version   
 if (flags & 0x000001) {  
 utf8string scheme\_uri; // browser uri  
 }  
}

#### Semantics

The semantics of the syntax elements are identical to the semantics of the syntax elements with the same name in SchemeTypeBox.

### Sample-packed tracks

#### Introduction

When a restricted scheme with scheme\_type equal to 'spkt' is in use for a track, a sample associated with the sample entry may be a packed sample, i.e., it may contain more than one sample of an original track. Such a current track is referred to as a sample-packed track.

#### Sample packing information box

##### Definition

Box Type: 'spki'  
Container: SchemeInformationBox  
Mandatory: Yes (when scheme\_type is 'spkt')  
Quantity: One

##### Syntax

aligned(8) class SamplePackingInformationBox   
 extends FullBox('spki', version = 0, flags = 0)  
{  
 unsigned int(8) mode;  
}

##### Semantics

mode equal to 0 specifies that all the samples of the original streams have been preserved. The value 1 specifies that only some samples have been preserved. All other values are reserved for future use.

## Support for incomplete tracks

### General

This subclause documents the sample entry formats for tracks that are incomplete. Incomplete tracks may contain samples that are marked empty or not received using the sample format.

Incomplete tracks may result, for example, when subsegments are received partially according to level assignments and padding\_flag in the LevelAssignmentBox indicates that the data in a MediaDataBox that is not received can be replaced by zeros. Consequently, sample data assigned to non-accessed levels is not present, and care should be taken not to attempt to process such samples. However, in partially received subsegments some tracks might remain complete in content while other tracks might be incomplete and only contain data that is included by reference into the complete tracks.

This subclause specifies support for sample entry formats for incomplete tracks. With this support, readers can detect incomplete tracks from their sample entries and avoid processing such tracks or take the possibility of empty or not received samples into account when processing such tracks.

The support for incomplete tracks is similar to the content protection transformation where sample entries are hidden behind generic sample entries, such as 'encv' and 'enca'. Because the format of a sample entry varies with media-type, a different encapsulating four character code is used for incomplete tracks of each media type (audio, video, text etc.). They are:

|  |  |
| --- | --- |
| **Stream (Track) Type** | **Sample-Entry Code** |
| Video | icpv |
| Audio | icpa |
| Text | icpt |
| System | icps |
| Hint | icph |
| Haptics | icpp |
| Volumetric visual | icp3 |
| Timed Metadata | icpm |

Sample data of incomplete tracks may be included into samples of other tracks by reference, and hence an incomplete track should not be removed as long as any track reference points to it.

NOTE 1 The choice of level by the original recording client can vary over time, and at times represent the complete track. The level is not indicated here, and it is not required that the sample entry change from ‘incomplete’ to ‘complete’ when all levels were, in fact, received, for a period.

NOTE 2 The ‘original format’ might have indicated encryption, if partial reception and decryption works for that encryption format.

### Transformation

The sample entry for a track that becomes incomplete e.g. through partial reception, should be modified as follows:

1. The four character code of the sample entry, e.g. 'avc1', is replaced by a new sample entry code 'icpv' meaning an incomplete track.
2. A CompleteTrackInfoBox is added to the sample entry, leaving all other boxes unmodified.
3. The original sample entry type, e.g. 'avc1', is stored within an OriginalFormatBox contained in the CompleteTrackInfoBox.

After transformation, an example AVC sample entry might look like:

class IncompleteAVCSampleEntry() extends VisualSampleEntry ('icpv')  
{  
 CompleteTrackInfoBox();  
 AVCConfigurationBox config;  
}

NOTE The sample entry type 'avc1' and the AVCConfigurationBox are specified in ISO/IEC 14496-15[3].

### Complete track information box

#### Definition

Box Types: 'cinf'  
Container: Sample Entry for an Incomplete Track  
Mandatory: Yes  
Quantity: Exactly one

The CompleteTrackInfoBox contains, within the OriginalFormatBox, the sample entry format of the complete track that was transformed to the present incomplete track. It may contain optional boxes for example including information required to process samples of the present incomplete track. The CompleteTrackInfoBox is a container box. It is mandatory in a sample entry that uses a code indicating an incomplete track.

#### Syntax

aligned(8) class CompleteTrackInfoBox(fmt) extends Box('cinf')   
{  
 OriginalFormatBox(fmt) original\_format;  
}

1. (informative)  
     
   Overview and tutorial
   1. Annex overview

This annex provides an overview to the file format, that potentially assists readers in understanding the overall concepts underlying the file format.

* 1. Design considerations
     1. Usage
        1. Multi-purpose

The file format is intended to serve as a basis for a number of operations. In these various roles, it can be used in different ways, and different aspects of the overall design exercised.

* + - 1. Interchange

When used as an interchange format, the files would normally be self-contained (not referencing media in other files), contain only the media data actually used in the presentation, and not contain any information related to streaming. This will result in a small, protocol-independent, self-contained file, which contains the core media data and the information needed to operate on it.

Figure A.1 gives an example of a simple interchange file, containing two streams.




Figure A.1 — Simple interchange file

* + - 1. Content creation

During content creation, a number of areas of the format can be exercised to useful effect, particularly:

* the ability to store each media stream separately (not interleaved), possibly in separate files.
* the ability to work in a single presentation that contains media data and other streams (e.g. editing the audio track in the uncompressed format, to align with an already-prepared video track).

These characteristics mean that presentations can be prepared, edits applied, and content developed and integrated without either iteratively re-writing the presentation on disc – which would be necessary if interleave was required and unused data had to be deleted; and also without iteratively decoding and re-encoding the data – which would be necessary if the data must be stored in an encoded state.

In Figure A.2, a set of files being used in the process of content creation is shown.




Figure A.2 — **Content** creation file

* 1. Design principles

The file structure is object-oriented; a file can be decomposed into constituent objects very simply, and the structure of the objects inferred directly from their type.

Media-data is not ‘framed’ by the file format; the file format declarations that give the size, type and position of media data units are not physically contiguous with the media data. This makes it possible to subset the media-data, and to use it in its natural state, without requiring it to be copied to make space for framing. The structure-data is used to describe the media data by reference, not by inclusion.

The file format does not require that a single presentation be in a single file. This enables both sub-setting and re-use of content. When combined with the non-framing approach, it also makes it possible to include media data in files not formatted to this document (e.g. ‘raw’ files containing only media data and no declarative information, or file formats already in use in the media or computer industries).

The file format is based on a common set of designs and a rich set of possible structures and usages. The same format serves all usages; translation is not required. However, when used in a particular way (e.g. for local presentation), the file possibly needs structuring in certain ways for optimal behaviour (e.g. time-ordering of the data). No normative structuring rules are defined by this document, unless a restricted profile is used.

* 1. Core concepts

In the file format, the overall presentation is called a **movie**. It is logically divided into **track**s; each track represents a timed sequence of media (frames of video, for example). Within each track, each timed unit is called a **sample**; this might be a frame of video or audio. Samples are implicitly numbered in sequence. Note that a frame of audio typically decompresses into a sequence of audio samples (in the sense this word is used in audio); in general, this document uses the word sample to mean a timed frame or unit of data. Each track has one or more **sample entries**; each sample in the track is tied to an entry by reference. The description defines how the sample can be decoded (e.g. it identifies the compression algorithm used).

Unlike many other multi-media file formats, this format, with its ancestors, separates several concepts that are often linked. Understanding this separation is key to understanding the file format. In particular:

The physical structure of the file is not tied to the physical structures of the media itself. For example, many file formats ‘frame’ the media data, putting headers or other data immediately before or after each frame of video; this document does not do this.

Neither the physical structure of the file, nor the layout of the media, is tied to the time ordering of the media. Frames of video need not be laid down in the file in time order (though they can be).

This means that there are file structures that describe the placement and timing of the media; these file structures permit, but do not require, time-ordered files.

All the data within a conforming file is encapsulated in **box**es (called **atoms** in predecessors of this document). There is no data outside the box structure. All the structure-data, including that defining the placement and timing of the media, is contained in structured boxes. This document defines the boxes. The media data (frames of video, for example) is referred to by this structure-data. The media data can be in the same file (contained in one or more boxes), or can be in other files; the structure-data permits referring to other files by means of URLs. The placement of the media data within these secondary files is entirely described by the structure-data in the primary file. They need not be formatted to this document, though they can be; it is possible that there are no boxes, for example, in these secondary media files.

Tracks can be of various kinds. Three are important here. **Video track**s contain samples that are visual; **audio track**s contain audio media. **Hint track**s are rather different; they contain instructions for a streaming server in how to form packets for a streaming protocol, from the media tracks in a file. Hint tracks can be ignored when a file is read for local playback; they are only relevant to streaming.

* 1. Physical structure of the media

The boxes that define the layout of the media data are found in the sample table. These include the data reference, the sample size table, the sample to chunk table, and the chunk offset table. Between them, these tables allow each sample in a track to be both located, and its size to be known.

The **data reference**s permit locating media within secondary media files. This allows a composition to be built from a ‘library’ of media in separate files, without actually copying the media into a single file. This greatly facilitates editing, for example.

The tables are compacted to save space. In addition, it is expected that the interleave will not be sample by sample, but that several samples for a single track will occur together, then a set of samples for another track, and so on. These sets of contiguous samples for one track are called **chunk**s. Each chunk has an offset relative to the containing resource that is identified through a reference to a data reference entry. For example, a chunk offset can be provided relative to the beginning of the file. Within the chunk, the samples are contiguously stored. Therefore, if a chunk contains two samples, the position of the second can be found by adding the size of the first to the offset for the chunk. The chunk offset table provides the offsets; the sample to chunk table provides the mapping from sample number to chunk number.

Note that in between the chunks (but not within them) there can be ‘dead space’, un-referenced by the media data. Thus, during editing, if some media data is not needed, it can simply be left unreferenced; the data need not be copied to remove it. Likewise, if the media data is in a secondary file formatted to a ‘foreign’ file format, headers or other structures imposed by that foreign format can simply be skipped.

* 1. Temporal structure of the media

Timing in the file can be understood by means of a number of structures. The movie, and each track, has a **timescale**. This defines a time axis which has a number of ticks per second. By suitable choice of this number, exact timing can be achieved. Typically, this is the sampling rate of the audio, for an audio track. For video, a suitable scale is to be chosen. For example, a media TimeScale of 30000 and media sample durations of 1001 exactly define NTSC video (often, but incorrectly, referred to as 29.97) and provide 19.9 hours of time in 32 bits.

The time structure of a track can be affected by an **edit list**. These provide two key capabilities: the movement (and possible re-use) of portions of the timeline of a track, in the overall movie, and also the insertion of ‘blank’ time, known as empty edits. Note in particular that if a track does not start at the beginning of a presentation, an initial empty edit is needed.

The overall duration of each track is defined in headers; this provides a useful summary of the track. Each sample has a defined **duration**. The exact decoding timestamp of a sample is defined by summing the durations of the preceding samples.

* 1. Interleave

The temporal and physical structures of the file can be aligned. This means that the media data has its physical order within its container in time order, as used. In addition, if the media data for multiple tracks is contained in the same file, this media data can be interleaved. Typically, in order to simplify the reading of the media data for one track, and to keep the tables compact, this interleave is done at a suitable time interval (e.g. 1 second), rather than sample by sample. This keeps the number of chunks down, and thus the chunk offset table small.

* 1. Composition

If multiple audio tracks are contained in the same file, they are implicitly mixed for playback. This mixing is affected by the overall track **volume**, and the left/right **balance**.

Likewise, video tracks are composed, by following their layer number (from back to front), and their composition mode. In addition, each track can be transformed by means of a matrix, and also the overall movie transformed by **matrix**. This permits both simple operations (e.g. pixel doubling, correction of 90º rotation) as well as more complex operations (shearing, arbitrary rotation, for example).

Derived specifications can over-ride this default composition of audio and video with more powerful systems (e.g. MPEG-4 BIFS).

* 1. Random access

This clause describes how to seek. Seeking is accomplished primarily by using the child boxes contained in the SampleTableBox. If an edit list is present, it must also be consulted.

To seek a given track to a time T, where T is in the time scale of the MovieHeaderBox, the following operations can be performed:

1. If the track contains an edit list, determine which edit contains the time T by iterating over the edits. The start time of the edit in the movie time scale must then be subtracted from the time T to generate T', the duration into the edit in the movie time scale. T' is next converted to the time scale of the track's media to generate T''. Finally, the time in the media scale to use is calculated by adding the media start time of the edit to T''.
2. The TimeToSampleBox for a track indicates what times are associated with which sample for that track. Use this box to find the first sample prior to the given time.
3. Possibly, the sample that was located in step 1 is not a sync sample. The SyncSampleBox documents sync samples, which are random access points (Note that there can be random access points that are not documented by the SyncSampleBox). Using this table, the first sync sample prior to the specified time can be located. The absence of the SyncSampleBox indicates that all samples are synchronization points, and makes this problem easy. Having consulted the SyncSampleBox, the next step is likely to be seeking to whichever resultant sample is closest to, but prior to, the sample found in step 1.
4. At this point the sample that will be used for random access is known. Use the SampleToChunkBox to determine in which chunk this sample is located.
5. Knowing which chunk contained the sample in question, use the ChunkOffsetBox to figure out where that chunk begins.
6. Starting from this offset, use the information contained in the SampleToChunkBox and the SampleSizeBox to figure out where within this chunk the sample in question is located. This is the desired information.
   1. Fragmented movie files

This clause introduces a technique that can be used in movie files, where the construction of a single MovieBox in a movie is burdensome. This can arise in at least the following cases:

* Recording. If un-fragmented movie files are used, if a recording application crashes, runs out of disk, or some other incident happens, after it has written a lot of media to disk but before it writes the MovieBox, the recorded data is unusable. This occurs because the file format insists that all structure-data (the MovieBox) be written in one contiguous area of the file.
* Recording. On embedded devices, particularly still cameras, there is not the RAM to buffer a MovieBox for the size of the storage available, and re-computing it when the movie is closed is too slow. The same risk of crashing applies, as well.
* HTTP fast-start. If the movie is of reasonable size (in terms of the MovieBox, if not time), the MovieBox can take an uncomfortable period to download before fast-start happens.
* Segmented streaming. Segment-based streaming systems divide presentations into a sequence of segments which are transmitted and played. An initial segment (often called an initialization segment) contains a MovieBox in which the track(s) contain no samples, and subsequent segments contain one or more MovieFragmentBox(es).

The basic 'shape' of the movie is set in initial MovieBox: the number of tracks, the available sample entries, width, height, composition, and so on. However the MovieBox does not contain the information for the full duration of the movie; in particular, it can have few or no samples in its tracks.

To this minimal or empty movie, extra samples are added, in structure called movie fragments.

The basic design philosophy is the same as in the MovieBox; data is not 'framed'. However, the design is such that it can be treated as a 'framing' design if that is needed. The structures map readily to the MovieBox, so a fragmented presentation can be rewritten as a single MovieBox.

The approach is that defaults are set for each sample, both globally (once per track) and within each fragment. Only those fragments that have non-default values need include those values. This makes the common case — regular, repeating, structures — compact, without disabling the incremental building of movies that have variations.

The regular MovieBox sets up the structure of the movie. It can occur anywhere in the file, though it is best for readers if it precedes the fragments. (This is not a rule, as trivial changes to the MovieBox that force it to reside at the end of the file would then be impossible). This MovieBox:

* must represent a valid movie in its own right (though the tracks can have no samples at all);
* has a box in it to indicate that fragments are to be found and used;
* is used to contain the complete edit list (if any).

Note that software that doesn't understand fragments will play just this initial movie. Software that does understand fragments and gets a non-fragmented movie won't scan for fragments as the fragment indication MovieExtendsBox won't be found.

* 1. Construction of fragmented movies

When constructing a fragmented file for playback, there are some recommendations for structuring the content to optimize playback and random access. The recommendations are as follows:

 The file consists of boxes in the following order:

- FileTypeBox

- MovieBox

- pair of MovieFragmentBox and MediaDataBox (arbitrary number)

- MovieFragmentRandomAccessBox

 A MovieFragmentBox consists of at most one TrackFragmentBox for each media. When the file contains a single video track and a single audio track, the MovieFragmentBox will contain two TrackFragmentBoxes, one for the video and one for the audio.

 For video, random accessible samples are stored as the first sample of each TrackFragmentBox. In the case of gradual decoder refresh, a random accessible sample and the corresponding recovery point are stored in the same movie fragment. For audio, samples having the closest presentation time for every video random accessible sample are stored as the first sample of each TrackFragmentBox. Hence, the first samples of each media in the MovieFragmentBox have the approximately equal presentation times.

 First (random accessible) samples are recorded in the MovieFragmentRandomAccessBox for both video and audio.

 All samples in MediaDataBox are interleaved with an appropriate interleave depth.

The offset and the initial presentation time of every MovieFragmentBox are given in the MovieFragmentRandomAccessBox for both audio and video.

The player will load the MovieBox and MovieFragmentRandomAccessBox initially, and hold them in memory during playback. When random access is needed, the player will search MovieFragmentRandomAccessBox in order to find the random access point having the closest presentation time for the indicated time.

Since the first sample in the MovieFragmentBox is random accessible, the player can directory jump in on the random access point. The player can read the MovieFragmentBox of the random access point from the beginning. The subsequent MediaDataBox starts from the random accessible sample. As such, a two-step seeking is not necessary for random access.

Note that an MovieFragmentRandomAccessBox box is optional, and might never occur in a given file.

* 1. Transformed streaming over streaming protocols
     1. Design considerations for streaming protocols
        + 1. Preparation for transformed streaming

When prepared for transformed streaming, the file needs to contain information to direct the streaming server in the process of sending the information. In addition, it is helpful if these instructions and the media data are interleaved so that excessive seeking can be avoided when serving the presentation. It is also important that the original media data be retained unscathed, so that the files may be verified, or re-edited or otherwise re-used. Finally, it is helpful if a single file can be prepared for more than one protocol, so differing servers can use it over disparate protocols.

* + - * 1. Local presentation

‘Locally’ viewing a presentation (i.e. directly from the file, not over a streamed interconnect) is an important application; it is used when a presentation is distributed (e.g. on CD or DVD ROM), during the process of development, and when verifying the content on streaming servers. Such local viewing is supported, with full random access. If the presentation is on CD or DVD ROM, interleave is important as seeking can be slow.

* + - * 1. Streamed presentation

When a server operates from the file to make a stream, the resulting stream has to be conformant with the specifications for the protocol(s) used, and should contain no trace of the file-format information in the file itself. The server needs to be able to random access the presentation. It can be useful to re-use server content (e.g. to make excerpts) by referencing the same media data from multiple presentations; it can also assist streaming if the media data can be on read-only media (e.g. CD) and not copied, merely augmented, when prepared for streaming.

Figure 3 shows a presentation prepared for streaming over a multiplexing protocol, only one hint track is required.




Figure A.3 — Hinted presentation for streaming

* + 1. Design considerations for streaming protocols
       1. General

Transmission or server hint tracks contain instructions to assist a streaming server in the formation of packets for transmission. These instructions can contain immediate data for the server to send (e.g. header information) or reference parts of the media data. These instructions are encoded in the file in the same way that editing or presentation information is encoded in a file for local playback. Instead of editing or presentation information, information is provided which allows a server to packetize the media data in a manner suitable for streaming using a specific network transport.

The protocol information for a particular streaming protocol does not frame the media data; the protocol headers are not physically contiguous with the media data. Instead, the media data can be included by reference. This makes it possible to represent media data in its natural state, not favouring any protocol. It also makes it possible for the same set of media data to serve for local presentation, and for multiple protocols.

The same media data is used in a file that contains hints, whether it is for local playback, or streaming over a number of different protocols. Separate ‘hint’ tracks for different protocols can be included within the same file and the media will play over all such protocols without making any additional copies of the media itself. In addition, existing media can be easily made streamable by the addition of appropriate hint tracks for specific protocols. The media data itself need not be recast or reformatted in any way.

This approach to streaming and recording is more space efficient than an approach that requires that the media information be partitioned into the actual data units that will be transmitted for a given transport and media format. Under such an approach, local playback requires either re-assembling the media from the packets, or having two copies of the media — one for local playback and one for streaming. Similarly, streaming such media over multiple protocols using this approach requires multiple copies of the media data for each transport. This is inefficient with space, unless the media data has been heavily transformed for streaming (e.g. by the application of error-correcting coding techniques, or by encryption).

Reception hint tracks can be used when one or more packet streams of data are recorded. Reception hint tracks indicate the order, reception timing, and contents of the received packets among other things.

NOTE Players can reproduce the packet stream that was received based on the reception hint tracks and process the reproduced packet stream as if it was newly received.

* + - 1. Protocol ‘hint’ tracks

Support for streaming is based upon the following three design parameters:

* The media data is represented as a set of network-independent standard tracks, which can be played, edited, and so on, as normal;
* There is a common declaration and base structure for hint tracks; this common format is protocol independent, but contains the declarations of which protocol(s) are described in the hint track(s);
* There is a specific design of the hint tracks for each protocol that can be transmitted; all these designs use the same basic structure. For example, there can be designs for RTP (for the Internet) and MPEG-2 transport (for broadcast), or for new standard or vendor-specific protocols.

The resulting streams, sent by the servers under the direction of the server hint tracks or reconstructed from the reception hint tracks, need contain no trace of file-specific information. This design does not require that the file structures or declaration style, be used either in the data on the wire or in the decoding station. For example, a file using ITU-T H.261 video and DVI audio, streamed under RTP, results in a packet stream that is fully compliant with the IETF specifications for packing those codings into RTP.

If a movie file contains hint tracks, the media tracks that reference the media data from which the hints were built remain in the file, even if the data within them is not directly referenced by the hint tracks; after deleting all hint tracks, the entire un-hinted presentation remain. The media tracks can, however, refer to external files for their media data.

The protocol information is built in such a way that the streaming servers need to know only about the protocol and the way it is to be sent; the protocol information abstracts knowledge of the media so that the servers are, to a large extent, media-type agnostic. Similarly, the media-data, stored as it is in a protocol-unaware fashion, enables the media tools to be protocol-agnostic.

1. (informative)  
     
   Guidance on deriving from this document
   1. General

This annex provides guidance explaining how to derive a specific file format from the ISO base media file format.

This document defines the basic structure of the file format. Media-specific and user-defined extensions can be provided in other specifications that are derived from the ISO base media file format.

* 1. General principles
     1. General

A number of existing file formats use the ISO base media file format, not least the MPEG-4 MP4 file format (ISO/IEC 14496-14[8]), and the Motion JPEG 2000 MJ2 file format (ISO/IEC 15444-3[5]). When considering a new specification derived from the ISO base media file format, all the existing specifications ought to be used both as examples and a source of definitions and technology. Check with the maintenance agency (see Annex D) to find what might already exist, and what specifications exist.

In particular, if an existing specification already covers how a particular media type is stored in the file format (e.g. MPEG-4 video in MP4), that definition ought to be used and a new one ought not to be invented. In this way specifications which share technology will also share the definition of how that technology is represented.

Be as permissive as possible with respect to the presence of other information in the file; indicate that unrecognized boxes and media "may be ignored" (not “should be ignored”). This permits the creation of hybrid files, drawing from more than one specification, and the creation of multi-format players, capable of handling more than one specification.

When layering on this document, it's worth observing that there are some characteristics that are intentionally ‘parameters’ to the lower specification (this document), that need to be specified. Equally, there are some characteristics of this document that are internal and ought rarely be discussed by other specifications. Of course, there are some characteristics in between.

Derived specifications are ideally written solely in terms of the parameters of the file format in this document; what a sample is, what its decoding and composition times mean, and so on. Mentioning specific existing boxes in a derived specification can often turn out to be an error, except in limited cases (e.g. adding a UserDataBox, or an extension box).

* + 1. Base layer operations

It ought to be possible to perform some operations on a file based on this document without knowing anything about any potential derived specifications. These operations might include the obvious reading tracks, finding the data and timing for samples, and their sample entry and track type, and so on. This might be done, for example, by a file-format inspector or general library like the reference software.

Less obvious are a class of manipulations of the files:

a) re-interleaving the data; making the media data in time order, with the samples for various tracks grouped into chunks of a sensible size, with the chunks interleaved;

b) making files that use data references self-contained, by copying the data from external files into the new file;

c) removing free space boxes and compacting the box structure;

d) removing data from MediaDataBoxes that appears to be un-referenced by tracks, items, or structure-data boxes;

e) removing sample entries that have no associated samples;

f) removing sample groups that have no associated samples;

g) extracting some tracks and making a new file with just those (e.g. an audio track from an audio/video presentation);

h) inserting, or removing, movie fragments, or re-fragmenting a movie.

This list is not exhaustive, of course.

* 1. Boxes

Boxes can be added to the file format, but be careful about how they interact with other boxes. In particular, if they ‘cross-link’ into existing boxes, it might not be possible to mark such files as compliant with this document.

All new boxes must be registered, except those using the 'uuid' type. Likewise, codec (sample entry) names, brands, track reference types, handlers (media types), group types, and protection scheme types ought to be registered. It really is a bad idea to use one of these without registration, as collisions can occur – or someone else has registered the same identifier with a different meaning.

A box outght not to be written using the ‘UUID escape’ (the reserved ISO UUID pattern 0xXXXXXXXX-0011-0010-8000-00AA00389B71, where the four-character code replaces the Xs) if a simple four character code can be used, and ideally it outght not to be designed to use a UUID box; it’s better to place data in known ‘expansion points’ of the file format if at all possible, or register a new box type if really needed.

Don’t forget that *all* data in ISO base media files must be, or be contained in, boxes. A signature can be introduced, but it must ‘look like’ a box.

Do not require that any existing or new boxes you define be in a particular position, if at all possible. For example, the existing JPEG 2000 specifications require a signature box and that it be first in the file. If another specification also defines a signature box and also requires that it be first, then a file conformant to both specifications cannot be constructed.

It must be possible to ‘walk’ the top-level of a file by finding box lengths. Don’t forget that ‘implied length’ is permitted at file level.

Unless absolutely unavoidable, boxes ought not to contain either data (e.g. in fields), or other boxes, but not both. All boxes containing data ought to be a full box to allow later changes to syntax and semantics. Boxes containing other boxes are known as container boxes, and are normally a plain (non-full) box, since their semantics will never change if they are documented to contain only boxes.

* 1. Brand identifiers
     1. Overview

This subclause covers the use of brand identifiers in the file-type box, including:

- Introduction of a new brand.

- Player’s behaviour depending on the brand.

- Setting of the brand on the creation of the ISO base media file.

Brands identify a specification and make a simple set of statements:

a) the file conforms to all requirements of the identified specification;

b) the file contains nothing contrary to the identified specification;

c) a reader implementing potentially that single specification may read, interpret, and possibly present the file, ignoring data it does not recognize.

Therefore specifications ought to specify (if they need a brand) “the brand that identifies files conformant to this specification is XXXX”, and register the brand.

* + 1. Usage of the brand

In order to identify the specifications to which the file complies, brands are used as identifiers in the file format. These brands are set in the FileTypeBox.

For example, a brand might indicate:

1. the codecs that may be present in the file,
2. how the data of each codec is stored,
3. constraints and extensions that are applied to the file.

New brands can be registered if it is necessary to make a new specification that is not fully conformant to the existing standards. For example, 3GPP allows using AMR and H.263 in the file format. Since these codecs were not supported in any standards at that time, 3GPP specified the usage of the SampleEntry and template fields in the ISO base media format as well as defining new boxes to which these codecs refer. Considering that the file format is used more widely in the future, it is expected that more brands will be needed.

Brands are not additive; they stand alone. It is not possible to say: “this brand indicates that support for Y is also required” because the ‘also’ has no referent.

Systems that re-write files ought to remove brands that they do not recognize, as they do not know whether the file still conforms to that brand’s requirements (e.g. re-interleaving a file possibly takes it out of conformance with a specification that requires a certain style of interleaving).

Note that the major brand usually implies the file extension, which in turn implies the MIME type. But these are not rules. In addition, when serving under a MIME type do not forget that MIME types can take parameters, and the list of compatible brands can often be useful to the receiving system.

* + 1. Introduction of a new brand

A new brand can be defined if conformance to a new specification must be indicated. This generally means that for the definition of a new brand at least one of the following conditions ought to be satisfied:

* + - 1. Use of a codec that is not supported in any existing brands.
      2. Use more than one codec in a combination that is not supported in any existing brands. In addition, the playback of the file is allowed only when decoding of all the media in the file is supported by the player.
      3. Use constraints and/or extensions (boxes, template fields, etc.) that are user-specific.

However, the file format contains both a major\_brand field and a compatible\_brands array. These fields are owned by the file author and this document. Do not write a specification that talks about these fields, merely about brands and what they mean. In particular, do *not* claim the major\_brand field (“files conformant to this specification must set the major\_brand to XXXX”) as a file can never be conformant to two such specifications written that way, and it also blocks someone also from deriving a specification from yours. However, brands that are only permitted as compatible brands can be defined.

Brands can be used as a tracer, however. It’s permissible to have a brand which has no requirements, and is placed in a file as an ‘I was there’ point (or strictly “this brand requires that the file was last written by ZZZZ”).

* + 1. Player guideline

If more than one brand is present in the list of the compatible\_brands, and one or more brands are supported by the player, the player necessarily plays those aspects of the file that comply with those specifications. In this case, the player is possibly not able to decode unsupported media.

* + 1. Authoring guideline

If the author wants to create a file that complies with more than one specification, the following considerations apply:

1. There must be nothing contrary to the specification identified by a brand within the file. For example, if a specification requires that files be self-contained, then the brand indication of that specification must not be used on non-self-contained files.

2. If the author is satisfied that a player compliant with only one of the specifications play only that media compliant with that specification, then that brand can be indicated.

3. If the author requires that the media from more than one specification be played, then a new brand is needed as this represents a new conformance requirement for the player.

* + 1. Example

This subclause covers an example case when a new brand can be defined.

First of all, consider two currently existing brands. If the brand '3gp5' is in the list of the compatible\_brands, it indicates that the file contains the media defined in 3GPP TS 26.234[1] (Release 5) in the way specified by the standard. For example, the file of '3gp5' brand can contain H.263. Likewise, if the brand 'mp42' is in the list of the compatible\_brands, it indicates that the file contains the media defined in ISO/IEC 14496-14[8] in the specified way. For example, the file of 'mp42' brand can contain MP3. However, MP3 is not supported in '3gp5' brand.

Given that the file contains H.263 and MP3, and has '3gp5' and 'mp42' as the compatible\_brands. If the player complies only with '3gp5' and does not support MP3, the recommended behaviour of the player is to play only H.263. If the content’s author does not expect such behaviour, a new brand is defined to indicate that both H.263 and MP3 are supported in the file. By specifying the newly defined brand in the list of the compatible\_brands, it can prevent the above behaviour and the file is played only when the player supports both H.263 and MP3.

* 1. Storage of new media types

This document defines an abstraction layer on which derived specifications are ideally built, leaving to this document how these abstractions are built. These abstractions fall into two main groups: timed and un-timed media.

The support for timed media views such media as a succession of timed samples, associated with setup information in a "sample entry". Derived specifications are recommended to:

* + identify the general track type (as defined in Clause 12) used by the media;
  + define the **four-character code** of the "sample entry" for the coding system;
  + identify the values of the fields in the base sample entry for the identified media type;
  + define a **sample** for the coding system (e.g. "a sample is an encoded visual access unit as defined in XXXX");
  + define the **decoder initialization** is required (e.g. "the decoder configuration information is a metadata-setup structure, contained in a FullBox of type 'medc', in the sample entry);
  + define a '**sync sample**' for the coding system; example "a sync sample is a metadata-frame with the IndependentProperty flag set as defined in XXXX"). The definition must conform to the general definition (i.e. a place where decoding and playback can start);
  + the type of **Stream Access Points** that are supported by the coding system (see Annex I) and what is a leading sample, to enable the use of the stream access point and random access point sample groups.
  + define the values for the common shared fields, e.g. in the track header, media header, or base sample entry type for the media type.

Notice that these definitions do not need to discuss where the sample data is (in the same file, or another) or whether movie fragments are in use or not.

Other tools for timed media include:

* **Sample groups**. Here, there is some property of a given type that is shared by a set of samples in a track – a group definition. Multiple groups of the same type can be defined, and each sample in a track mapped to either a definition, or nothing. For example, if each sample were a frame of audio, some of which contain speech content, and some contain musical content, is is possible to define a sample group, with an enumeration of content type (e.g. 1 predominantly speech, 2 predominantly music). The classifiable samples are associated with the matching group definition.
* **Random Access Point (RAP) types**. There is a general definition of RAP points in Annex I; it can be useful to define or identify which RAP types apply to this format; they can then be used in the appropriate sample group.
* **Sample auxiliary information**. If the information for each sample is unique, sample groups do not work, as they rely on sharing a definition. Sample auxiliary information provides a unique piece of data for each sample. The usual example is initialization vectors for decoding.
* **Related tracks**. Tracks can be linked by typed, directional, track references, or they can be grouped into TrackGroups.
* **Sub-sample information**. If a given coding format naturally and usefully has a way to split a sample into sub-samples (e.g. base data, olfactory data, and gustatory data) then sub-sample structure can be documented to ease the finding of only the desired sub-samples.
* **Independent and disposable sample** tagging.
* **Padding bits**; most coding systems define their coded content as occupying at least whole bytes, but for those that have frames ending in the middle of a byte, and which are not self-framing (i.e. the end of the data cannot be determined) this table can document the padding bits present.
* **Degradation Priority**; this table is sometimes used to indicate sample priority (especially when packet-based streaming protocols are used or expected).
* **Shadow Sync**; this table has been used to provide extra, optional, sync samples.

If MPEG-4 systems constructs are desired or acceptable, then:

a) a new ObjectTypeIndication ought to be requested and used;

b) the decoderspecificinformation for this codec ought to be defined as an MPEG-4 descriptor;

c) the sample format ought to be defined for this media.

The media then uses the MPEG-4 code points in the file format; for example, a new video codec uses a sampleentry of type 'mp4v'.

If the coding format supports a variety of options, not all of which every player will support (e.g. video codec profiles), then defining sub-parameters for the codec type to use in the codecs MIME parameter is desirable, to give advance notice of the format of the content.

Similarly, for untimed data, the MetaBox provides a number of tools. Again, the definition of such items ought to include what constitutes an item body, what initialization data is needed and what item property it is in. Items can be linked, by reference, to other items, just like track; and indeed, it is possible to unify the item\_ID and track\_ID number spaces so that references can be made between tracks and items, either way.

If the 'codecs' MIME parameter is important for this coding type, sub-parameters can be defined (e.g. to identify profiles or levels).

* 1. Tracks
     1. Data location

A track is a timed sequence of samples; each sample is defined by its data (the bytes it contains), their length and location. The length and data of a sample are external parameters to the file format; the location of the bytes is not.

The exact way that the data is stored is *internal* to this document. When defining what a sample in a new format is, simply define the length and the data of a sample.

Do not mention the following boxes, however, as the way that they are structured is open to change, and the information that they store can be stored in other ways (e.g. it is possible that sample size information is present in an SampleSizeBox, a CompactSampleSizeBox, or a movie fragment):

SampleSizeBox, CompactSampleSizeBox

Samples are, in fact, stored in contiguous runs of samples for one track; these runs are called chunks, and it is chunks from different tracks that are interleaved. But files can be re-interleaved or re-chunked; the following boxes are about how chunking is done:

chunk offsets (ChunkOffsetBox or ChunkLargeOffsetBox), SampleToChunkBox

Most critically, locating data must be done through these boxes (or their equivalent in movie fragments). The MediaDataBox is merely one possible location, and looked at by itself, it can only be considered an un-ordered bag of un-identifiable bits. There is no assurance that the desirable material in a MediaDataBox is the only data in the box or in any particular order, and, especially if data references are used, there is no assurance that any particular sample is even in a MediaDataBox at all. Mentioning the MediaDataBox in a derived specification is almost certainly a mistake, and attempting to define (or assume) its structure is usurping this document, and is an error.

It is perfectly permissible to require a certain style, duration, or size of interleaving in an integration specification (“this specification requires that the file be self-contained, and that the media-data be in decoding timestamp order, interleaved on a granularity of no greater than one second”).

* + 1. Time

Similarly, samples are parameterized in time in the file format by their decoding timestamp, and optionally by their composition timestamp. Define what these mean for your media. However, the way that these are stored is again *internal* to this document.

Do not mention the following boxes, however, as the way that they are structured is open to change, and the information that they store can be stored in other ways:

TimeToSampleBox, CompositionOffsetBox

Likewise, the time-structure effect of edits ought to be preserved by the file format, but there a file simplifier can, for example, merge two adjacent edits that in fact belong together (e.g. two empty edits, or an edit that selects time A-B followed by one that selects B-C).

* + 1. Media types

There are a number of media types in this document: video, audio, metadata, and so on. These are represented by track handler types and by media-specific media headers. It is possible to register new media handlers, but this is rarely required. It might be needed, for example, if a track type were needed for say, laboratory instrument traces, or for a ‘timed aroma’ track. Registrations are recommended to be checked; the needed handler might be already defined in another derived specification.

* + 1. Coding types

The name of a sample entry identifies the coding format used. This is one of the principal ways that this document is parameterized; AVC (ISO/IEC 14496-10:2014,) uses 'avc1' for example, as a sample entry type. Defining this name for a codec, and registering it, and then defining what extra boxes are in a sample entry for this codec, are primary ways that format of this document is used. These ought to be defined for a coding system. Note that technically the coding type is ‘scoped’ by the media type (though the intention is not to define the same four character code as two different codecs in two media types, such as video and audio, in order to avoid confusion).

* + 1. Sub-sample information

The specifications of this document can carry information about ‘sub-sample’ boundaries for each sample. However, the definition of what a sub-sample *is*, is specific to a coding system. There might be a value in defining it when defining how a coding system is stored.

* + 1. Sample dependency

The format defined in this document allows the identification of some of the decoding dependency information for a coding system. In particular, what constitutes a valid ‘sync’ or random access point (points from which decoding can be started) ought to be identified. They can be marked in the file format (in the SyncSampleBox, or by flags in movie fragments). How sync sample are marked is likely not a concern.

Similarly, it is possible to indicate which samples:

a) depend on others, or can be decoded independently;

b) are depended on by others, or can be discarded without affecting decoding;

c) contain multiple encodings of the same information, possibly with different dependencies (are redundantly coded).

For most coding systems the meanings of these are self-evident and do not need spelling out; however, they possibly need explicit statement for some coding systems.

* + 1. Sample groups

Sample groups provide another way to describe samples and their characteristics. To use sample groups, define a group type, and then how a group is defined (the group description). The file format can then map a given sample to a single definition of a group of any given type. Defining new grouping\_types and the way that they are parameterized is an important way to parameterize the file format.

* + 1. Track-level

Tracks can be associated with each other in the file format, in two important ways. Track references are a typed link indicating a reference or dependency of one track to or on another (e.g. a metadata track that describes a media track has a dependency on that media track, as it makes no sense without it). New track reference types can be registered and used in derived specifications.

Similarly tracks can be grouped into sets of alternatives, where the reader is expected to be able to pick one that suits it (e.g. on the basis of supported codecs, bit-rates, screen sizes, and so on). 3GPP 26.234[1] has taken this concept and included user-data (a permitted extension) to give a hint as to why a track is a member of a group (‘I contain a different codec’).

Lastly, tracks can be enabled or disabled in the file format. Disabled tracks might be used, for example, for optional features (e.g. closed captions).

* + 1. Protection

Similarly to the parameterization of coding schemes by using the same entry type, and extra boxes in the sample entry, the format defined in this documentallows protection to be applied to tracks, parameterized by the scheme type and the contents of the scheme information box. The SchemeInformationBox is ‘owned’ by the scheme type – to the extent that contained boxes there do not need to be registered, as they are already scoped by the scheme type.

Protection can be subtle; many encryption systems, for example, ‘chain’ together. It’s tempting to encrypt ‘the contents of the mdat box’, but that is very badly non-resilient to minor changes to the file. It’s also tempting to protect chunks – they do seem to represent contiguous runs of media data for one track. But again, re-chunking the file can break the ability to de-protect.

Instead, consider modifying the sample, or introducing time-parallel metadata, or use sample groups, to introduce enough context to enable both file-based manipulation and decryption. Time-parallel metadata are in a track, and a track reference ought to be used to indicate that the protected data depends on the parallel encryption-context track.

* 1. Metadata

Much of what is said above about tracks and their data applies to metadata items, except that, of course, metadata items have no time structure. In particular, the division of items into extents – allowing them to be interleaved – is again, a property of the file format. It is a mistake to design some new support based on extent structure.

* 1. Sample groups, timed metadata tracks, and sample auxiliary information

The ISO base media file format contains three mechanisms for timed metadata that can be associated with particular samples: sample groups, timed metadata tracks, and sample auxiliary information. Derived specifications can provide similar functionality with one or more of these three mechanisms. This clause provides guidelines for derived specifications to choose between the three mechanisms.

Sample groups and timed metadata are less tightly coupled to the media data and are typically ‘descriptive’, whereas sample auxiliary information might be required for decoding.

Sample auxiliary information is only intended for use where the information is directly related to the sample on a one-to-one basis, and is required for the media sample processing and presentation. For general content, the existing solution of additional tracks ought to be used. Sample auxiliary information and sample media data are both addressed using byte pointers and size information, and so when the same bytes form the data for more than one sample it is possible to share that data by re-using the same byte pointer.

Sample groups can be useful in the following occasions.

* When several samples share the same metadata values, it is space-efficient to specify the metadata in a SampleGroupDescriptionBox and the association of samples to metadata in SampleToGroupBox(es).
* As the sample group information is stored in MovieBox and MovieFragmentBox(es), they provide an index to the data in the MediaDataBoxes. No data from the MediaDataBoxes need be fetched, which can therefore reduce disk accesses when compared to timed metadata tracks and sample auxiliary information.

Timed metadata tracks can be useful in the following occasions.

* The same timed metadata track can be associated to more than one track. In other words, a timed metadata track can be more independent of the content of the associated tracks than sample groups and sample auxiliary information.
* It can be easier to append a file with a timed metadata track than with sample auxiliary information or sample groups, because sample auxiliary information and SampleToGroupBoxes have to reside in the same TrackFragmentBox as the associated samples, whereas timed metadata can reside in its own MovieFragmentBox(es). For example, it can be easier to provide an additional subtitle track as timed metadata than use sample auxiliary information.
* The duration of timed metadata samples need not match the duration of associated media or hint samples. In cases where the duration of timed metadata samples spans over multiple associated media or hint samples, timed metadata tracks can be more space-efficient than sample auxiliary information.

Sample auxiliary information can be useful in the following occasions.

* The data associated with samples is changing sufficiently frequently such that specifying sample groups cannot be justified from storage space point of view.
* The amount of data associated with samples is such large that its carriage within the MovieBox or MovieFragmentBox (as required by sample grouping) cause disadvantages. For example, in progressive downloading, it can be beneficial to make the size of MovieBox small in order to keep the initial buffering time small.
* When each sample is associated with metadata, sample auxiliary information provides a more straightforward association of the auxiliary information to samples when compared to the same functionality with timed metadata tracks, which typically requires resolving sample decoding timestamps to establish the association between timed metadata samples and media/hint samples.

1. (normative)  
     
   Fragment identifiers for ISO base media resources
   1. Overview

This annex defines fragment identifiers usable for any media resource conformant to the ISO base media file format. They can address items or tracks. Such fragment identifiers are compliant to the generic syntax for URIs defined by IETF RFC 3986[24] and therefore can be used after the ‘#’ character in a URI. Where appropriate, such fragment identifiers can also be used in IRIs as specified by IETF RFC 3987[21].

Additional fragment identifiers may be defined by derived specifications.

The MPEG-21 fragment identifiers scheme, defined in ISO/IEC 21000-17:2006[6] may also be used.

In this annex, where the notation uses a syntax name in angle brackets, e.g. "track\_ID=<track\_ID>", it is to be replaced by the decimal string representation of the value of the indicated syntax element, e.g. "track\_ID=23".

* 1. Syntax and semantics

Fragment identifiers for ISOBMFF resources shall start consist of either:

1. track\_ID=<track\_ID>, identifying the track with the given track\_ID;
2. item\_ID=<item\_ID>, identifying the item of the MetaBox at the file level that has the given id;
3. item\_name=<item\_name>, identifying the item of the MetaBox at the file level that has the given name (as provided in the ItemInfoBox);
4. /item\_ID=<item\_ID>, identifying the item of the MetaBox at the movie level that has the given id;
5. /item\_name=<item\_name>, identifying the item of the MetaBox at the movie level that has the given name (as provided in the ItemInfoBox);
6. track\_ID=<track\_ID>/item\_ID=<item\_ID>, identifying the item that has the given id in the MetaBox located in the track with the given track\_ID;
7. track\_ID=<track\_ID>/item\_name=<item\_name>, identifying the item that has the given name (as provided in the ItemInfoBox) in the MetaBox located in the track with the given track\_ID.

NOTE For fragment identifiers identifying items in MetaBoxes at the track or movie level, the id or name may identify items stored in movie fragments.

If a fragment within a contained item must be addressed, then the initial “#” character of that fragment shall be replaced by “\*”. For example, if the URL for the desired resource when it is not in an item is /example.html#secure, then when that same resource is in an item the URL might be /container#item\_name=example.html\*secure.

1. (informative)  
     
   Management of extension code-points
   1. Code points

The code-points within the file format are all 32-bit fields, normally four printable characters (commonly known as four-character compact types, four-character-codes, or 4CCs). An objecttype identifier is an 8-bit integer.

Extension code-points can be entered into the database by the maintenance agency. More types of code-points can be added later, but they include at least:

1. File format box identifiers. Note that in some specifications boxes were known as atoms. Note that the introduction of new box types is discouraged; in general, other extensibility features of the file format ought to be used if possible.
2. File format track type identifiers. A pair of identifiers is usually used here, to identify the track type (audio, video, etc.) and, if required, a media-specific header box (video media header, etc.). It is expected that the need for new track types is rare, however; most media likely fall into existing types (e.g. video codecs ought to use video tracks, hint protocols ought to use hint tracks, and so on).
3. File format sample entry and sample format identifiers (also known as codec names). This includes audio and video codecs, and also protocol identifiers for hint tracks. It is permitted that any request of a new sample format code requests issuing an object-type identifier also (see below), thus making the identification of the carriage of this format within the MPEG-4 systems object descriptor framework possible.
4. File format track reference identifiers. Dependencies between tracks are typed in the file format (for example, hint tracks depend on the media tracks they hint, using a track dependency of type 'hint').
5. This document includes a FileTypeBox which includes a list of ‘brands’ which identify which specifications the file is conformant to. Bodies defining standards based on the structural definition of this document are normally expected to use a new brand to identify files conformant to their specification. Any documentation of a new brand ought to specify the precise specification which the brand identifies.
6. Within the MPEG-4 object descriptor framework, the objecttype value is used to identify the format of the streams. An objecttype identifier can be requested independently of the file format identifiers above.
7. Sample groups associate typed information with groups of samples, for which a grouping\_type can be documented.
8. Both media and metadata can be protected and the protection scheme used identified with a registered protection scheme type.

These code- points are referred to in the rest of this annex as registered identifiers, abbreviated as RIDs.

* 1. Procedure for the request of an extension code-point

The name and contact information of the maintenance agency for this document (ISO/IEC 14496-12) can be found at https://www.iso.org/mara.

1. (normative)  
     
   File format brands
   1. General

The presence of a brand in the compatible\_brands list of the FileTypeBox is a claim and a permission. It is a claim that the file conforms to all the requirements of that brand, and a permission to a reader implementing potentially only that brand to read the file.

In general, readers are required to implement all features documented for a brand unless one of the following applies:

1. the media they are using does not use or require a feature: for example, I-frame video does not need a SyncSampleBox, and if composition re-ordering is not used, then no composition time offset table is needed; similarly, if content protection is not needed, then support for the structures of content protection is not required.
2. another specification with which the file is conformant forbids the use of a feature (for example, some derived specifications explicitly forbid use of movie fragments);
3. the context in which the product operates means that some structures are not relevant; for example, hint track structures are only relevant to products preparing content for, or performing, file delivery (such as streaming) for the protocol in the hint track.

The following clauses list the brands defined in this document; no inheritance is implied by the clause order – when inheritance occurs, it is specifically stated. Other brands may be defined in other specifications. Note that if one brand is a subset of another (e.g. 'isom' requirements are a subset of the 'iso2' requirements) then:

1. files labelled as compatible with the subset can always be labelled as also compatible with the superset; a file compatible with 'isom' can always be labelled as compatible with 'iso2';
2. products supporting the superset automatically can support the subset; a product that supports 'iso2' also necessarily supports 'isom'.

No brands defined here require support for any particular media type (e.g. video, audio, metadata) or media encoding (e.g. a particular codec), or structures supporting a specific media type (e.g. visual sample entries or the boxes contained in a specific kind of sample entry).

More specific identifiers can be used to identify precise versions of specifications providing more detail. These brands should not be used as the major brand; this base file format should be derived into another specification to be used. There is therefore no defined normal file extension, or MIME type assigned to these brands, nor definition of the minor version when one of these brands is the major brand.

* 1. The 'isom' brand

The type 'isom' (ISO base media file) is defined in this clause, as identifying files that conform to the first version of ISO base media file format.

Support for the structural boxes according to Table E. 1 is required.

Table E. 1: Boxes required under the 'isom' brand

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| moov |  |  |  |  |  | *container for all the meta-data* |
|  | mvhd |  |  |  |  | *movie header, overall declarations* |
|  | trak |  |  |  |  | *container for an individual track or stream* |
|  |  | tkhd |  |  |  | *track header, overall information about the track* |
|  |  | tref |  |  |  | *track reference container* |
|  |  | edts |  |  |  | *edit list container* |
|  |  |  | elst |  |  | *an edit list* |
|  |  | mdia |  |  |  | *container for the media information in a track* |
|  |  |  | mdhd |  |  | *media header, overall information about the media* |
|  |  |  | hdlr |  |  | *handler, at this level, the media (handler) type* |
|  |  |  | minf |  |  | *media information container* |
|  |  |  |  | vmhd |  | *video media header, overall information (video track only)* |
|  |  |  |  | smhd |  | *sound media header, overall information (sound track only)* |
|  |  |  |  | hmhd |  | *hint media header, overall information (hint track only)* |
|  |  |  |  | <mpeg> |  | *mpeg stream headers* |
|  |  |  |  | dinf |  | *data information box, container* |
|  |  |  |  |  | dref | *data reference box, declares source(s) of media in track* |
|  |  |  |  | stbl |  | *sample table box, container for the time/space map* |
|  |  |  |  |  | stts | *(decoding) time-to-sample* |
|  |  |  |  |  | ctts | *composition time-to-sample table* |
|  |  |  |  |  | stss | *sync (key, I-frame) sample map* |
|  |  |  |  |  | stsd | *sample description box (codec types, initialization etc.)* |
|  |  |  |  |  | stsz | *sample sizes (framing)* |
|  |  |  |  |  | stsc | *sample-to-chunk, partial data-offset information* |
|  |  |  |  |  | stco | *chunk offset, partial data-offset information* |
|  |  |  |  |  | co64 | *64-bit chunk offset* |
|  |  |  |  |  | stsh | *shadow sync* |
|  |  |  |  |  | stdp | *degradation priority* |
| mdat |  |  |  |  |  | *Media data container* |
| free |  |  |  |  |  | *free space* |
| skip |  |  |  |  |  | *free space* |
| udta |  |  |  |  |  | *user-data, copyright etc.* |
| ftyp |  |  |  |  |  | *file type and compatibility* |
|  |  |  |  |  | stz2 | *compact sample sizes (framing)* |
|  |  |  |  |  | padb | *sample padding bits* |
|  | mvex |  |  |  |  | *movie extends box* |
|  |  | mehd |  |  |  | *movie extends header box* |
|  |  | trex |  |  |  | *track extends defaults* |
| moof |  |  |  |  |  | *movie fragment* |
|  | mfhd |  |  |  |  | *movie fragment header* |
|  | traf |  |  |  |  | *track fragment* |
|  |  | tfhd |  |  |  | *track fragment header* |
|  |  | trun |  |  |  | *track fragment run* |
| mfra |  |  |  |  |  | *movie fragment random access* |
|  | tfra |  |  |  |  | *track fragment random access* |
|  | mfro |  |  |  |  | *movie fragment random access offset* |

Hint tracks shall be recognized, and in hint tracks, RTP protocol hint tracks.

Support for only version 0 of the CompositionOffsetBox is required; version 1 support is not required.

Support for only version 0 of the TrackRunBox is required; version 1 support is not required.

NOTE 1 The default-base-is-moof flag (8.8.7.1) cannot be set where a file is marked with this brand.

NOTE 2 Some requirements of the TrackHeaderBox do not apply to this brand; see subclause 8.3.2.1.

Under this brand and its derivatives the media\_rate in the EditListBox is restricted such that the fraction shall have the value 0 and the integer shall have the value 0 or 1.

* 1. The 'avc1' brand

The brand 'avc1' shall be used to indicate that the file is conformant with the ‘AVC extensions’ in subclauses 8.6.4 and 8.9. If used without other brands, this implies that support for those extensions is required. The use of 'avc1' as a major-brand may be permitted by specifications; in that case, that specification defines the file extension and required behaviour.

The 'avc1' brand requires support for the 'isom' brand. In addition, support of the boxes according to Table E. 2 is required.

Table E. 2: Boxes required under the 'avc1' brand

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  | sdtp | *independent and disposable samples* |
|  |  |  |  |  | sbgp | *sample-to-group* |
|  |  |  |  |  | sgpd | *sample group description* |

Within the sample groups, support for roll groups (grouping\_type 'roll') is required.

NOTE 1 The default-base-is-moof flag (8.8.7.1) cannot be set where a file is marked with this brand.

NOTE 2 Some requirements of the TrackHeaderBox do not apply to this brand; see subclause 8.3.2.1.

Support for only version 0 of the CompositionOffsetBox is required; version 1 support is not required.

Support for only version 0 of the TrackRunBox is required; version 1 support is not required.

Support of SampleGroupDescriptionBoxes in movie fragments is not required.

* 1. The 'iso2' brand

The brand 'iso2' shall be used to indicate compatibility with the second version of the ISO base media file format; it may be used in addition to or instead of the 'isom' brand and the same usage rules apply. If used without the brand 'isom' identifying the first version of this document, it indicates that support for some or all of the technology in subclauses 8.6.4, 8.8.15, 8.11.1 through 8.11.7, 8.11.10, 13.1, or the SRTP support in subclause 9.1, is required.

The 'iso2' brand requires support for all features of the 'avc1' brand.

In addition, support for the boxes according to Table E. 3 is required.

Table E. 3: Boxes required under the 'iso2' brand

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| pdin |  |  |  |  |  | *progressive download information* |
|  |  |  |  |  | subs | *sub-sample information* |
| meta |  |  |  |  |  | *metadata* |
|  | iloc |  |  |  |  | *item location* |
|  | ipro |  |  |  |  | *item protection* |
|  |  | sinf |  |  |  | *protection scheme information box* |
|  |  |  | frma |  |  | *original format box* |
|  |  |  | schm |  |  | *scheme type box* |
|  |  |  | schi |  |  | *scheme information box* |
|  | iinf |  |  |  |  | *item information (version field set to 0)* |
|  | xml |  |  |  |  | *XML container* |
|  | bxml |  |  |  |  | *binary XML container* |
|  | pitm |  |  |  |  | *primary item reference* |

[Ed.Note] It is suggested to add hdlr under meta in the table above and the following sentence: When a file is indicated to conform to the 'iso2' brand and the file includes a MetaBox, a HandlerBox shall be present in the MetaBox.

In the context of RTP hint tracks, SRTP hint tracks shall now be recognized. Content protection and generalized metadata boxes support is required.

Only support for version 0 of the item information box, and version 0 of the item location box, is required.

Support for only version 0 of the CompositionOffsetBox is required; version 1 support is not required.

Support for only version 0 of the TrackRunBox is required; version 1 support is not required.

Support for SampleGroupDescriptionBoxes in movie fragments is not required.

NOTE 1 The default-base-is-moof flag (8.8.7.1) cannot be set where a file is marked with this brand.

NOTE 2 Some requirements of the TrackHeaderBox do not apply to this brand; see subclause 8.3.2.1.

Support for only 16-bit item\_ID and item\_count values in MetaBox is required; 32-bit item\_ID and item\_count values in MetaBox is not required

Support for MetaBox in movie fragments is not required

Support for only one SubSampleInformationBox per track is required

* 1. The 'mp71' brand

If a MetaBox with an MPEG-7 handler type is used at the file level, then the brand 'mp71' should be a member of the compatible-brands list in the FileTypeBox.

* 1. The 'iso3' brand

The brand 'iso3' requires support for all features of the 'iso2' brand.

In addition, support for the boxes according to Table E. 4 is required.

Table E. 4: Boxes required under the 'iso3' brand

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | fiin |  |  |  |  | *file delivery item information* |
|  |  | paen |  |  |  | *partition entry* |
|  |  |  | fpar |  |  | *file partition* |
|  |  |  | fecr |  |  | *FEC reservoir* |
|  |  | segr |  |  |  | *file delivery session group* |
|  |  | gitn |  |  |  | *group id to name* |

Support for version 0 and version 1 of the ItemInfoBox is required. Within the sample groups, support for rate share information (grouping\_type 'rash') is required. File delivery hint tracks (sample entry 'fdp ') shall be recognized.

Support for only version 0 of the CompositionOffsetBox is required; version 1 support is not required.

Support for only version 0 of the TrackRunBox is required; version 1 support is not required.

Support for SampleGroupDescriptionBoxes in movie fragments is not required.

Only support for version 0 of the ItemLocationBox is required.

NOTE The default-base-is-moof flag (8.8.7.1) cannot be set where a file is marked with this brand.

Support for only 16-bit item\_ID and item\_count values in MetaBox is required; 32-bit item\_ID and item\_count values in MetaBox is not required

Support for MetaBox in movie fragments is not required

Support for only one SubSampleInformationBox per track is required

* 1. The 'iso4' brand

The brand 'iso4' requires support for all features of the 'iso3' brand.

Support for version 1 of the CompositionOffsetBox boxis required under this brand.

Support for version 1 of the ItemLocationBox, version 2 of the ItemInfoBox, and the ItemDataBox and ItemReferenceBox is required.

In addition, support for the boxes according to Table E. 5 is required.

Table E. 5: Boxes required under the 'iso4' brand

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | trgr |  |  |  |  | *track grouping indication* |
|  |  |  |  |  | cslg |  | *composition to decoding timeline mapping* |
|  | idat |  |  |  |  |  | *item data* |
|  | iref |  |  |  |  |  | *item reference* |

Support for only version 0 of the TrackRunBox is required; version 1 support is not required.

Support for SampleGroupDescriptionBoxes in movie fragments is not required.

NOTE The default-base-is-moof flag (8.8.7.1) cannot be set where a file is marked with this brand.

Support for only 16-bit item\_ID and item\_count values in MetaBox is required; 32-bit item\_ID and item\_count values in MetaBox is not required

Support for MetaBox in movie fragments is not required

Support for only one SubSampleInformationBox per track is required

Support for only 32-bit values in CompositionToDecodeBox is required; 64-bit values in CompositionToDecodeBox is not required.

Within the sample groups, support for alternative startup sequence information (grouping type 'alst') is required.

* 1. The 'iso5' brand

The brand 'iso5' requires support for all features of the 'iso4' brand.

Support for the default-base-is-moof flag is required under this brand.

Processing of restricted sample entries (i.e. 'resv') is required under this brand.

Support for only version 0 of the TrackRunBox is required; version 1 support is not required.

Support for SampleGroupDescriptionBoxes in movie fragments is not required.

Support for only 16-bit item\_ID and item\_count values in MetaBox is required; 32-bit item\_ID and item\_count values in MetaBox is not required

Support for MetaBox in movie fragments is not required

Support for only one SubSampleInformationBox per track is required

Support for only 32-bit values in CompositionToDecodeBox is required; 64-bit values in CompositionToDecodeBox is not required.

* 1. The 'iso6' brand

The brand 'iso6' requires support for all features of the 'iso5' brand.

Support for the boxes according to Table E. 6 is required under this brand.

Table E. 6: Boxes required under the 'iso6' brand

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | saiz |  |  |  |  | *sample auxiliary information sizes* |
|  |  | saio |  |  |  |  | *sample auxiliary information offsets* |
|  |  | tfdt |  |  |  |  | *track fragment decode time* |
| styp |  |  |  |  |  |  | *segment type* |
| sidx |  |  |  |  |  |  | *segment index* |
| ssix |  |  |  |  |  |  | *subsegment index* |
| prft |  |  |  |  |  |  | *producer reference time* |

Support for the following is required under this brand:

* SampleGroupDescriptionBoxes in movie fragments;
* Signed composition offsets in TrackRunBoxes (i.e. version 1 of TrackRunBoxes);
* Within the sample groups, support for random access point information  
  (grouping type 'rap ') and temporal level information (grouping type 'tele') is required.
* Support for only 16-bit item\_ID and item\_count values in MetaBox is required; 32-bit item\_ID and item\_count values in MetaBox is not required
* Support for MetaBox in movie fragments is not required
* Support for only one SubSampleInformationBox per track is required
* Support for only 32-bit values in CompositionToDecodeBox is required; 64-bit values in CompositionToDecodeBox is not required.
  1. The 'iso7' brand

The brand 'iso7' requires support for all features of the 'iso6' brand.

Support for the boxes according to Table E. 7 is required under this brand.

Table E. 7: Boxes required under the 'iso7' brand

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | trep |  |  |  |  |  | *track extension properties* |
|  |  |  | assp |  |  |  |  | *alternative startup sequence properties* |

Support for the following is required under this brand:

* Support for 32-bit item\_ID and item\_count values in MetaBox
* Recognizing incomplete tracks by detecting the following sample entries for incomplete tracks: 'icpv', 'icpa', 'icpt', 'icps', 'icph', 'icpp', 'icp3' and 'icpm'.

NOTE The process of detecting when a track becomes incomplete (before the transformation specified in subclause 13.6.2) and handling incomplete tracks in playback are outside the scope of this document

* Support for MetaBox in movie fragments is not required
* Support for only one SubSampleInformationBox per track is required
* Support for only 32-bit values in CompositionToDecodeBox is required; 64-bit values in CompositionToDecodeBox is not required.
  1. The 'iso8' brand

The brand 'iso8' requires support for all features of the 'iso7' brand.

Support for the boxes according to Table E. 8 is required under this brand.

Table E. 8: Boxes required under the 'iso8' brand

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  | sthd |  |  |  | *subtitle media header, overall information (subtitle track only)* |

Support for the following is required under this brand:

* Support for MetaBox in movie fragments
* Support for one or more SubSampleInformationBox per track
* Support for only 32-bit values in CompositionToDecodeBox is required; 64-bit values in CompositionToDecodeBox is not required.
  1. The 'iso9' brand

The brand 'iso9' requires support for all features of the 'iso8' brand.

Support for the boxes according to Table E. 9 is required under this brand.

Table E. 9: Boxes required under the 'iso9' brand

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | elng |  |  |  |  | *extended language tag* |

Support for the following is required under this brand:

* Support for 64-bit values in CompositionToDecodeBox.
  1. The 'isoa' brand

The brand 'isoa' requires support for all features of the 'iso9' brand.

Support for the boxes according to Table E. 10 is required under this brand.

Table E. 10: Boxes required under the 'isoa' brand

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | iprp |  |  |  |  |  |  | *item property* |
|  | grpl |  |  |  |  |  |  | *entity groups list* |

Support for the following is required under this brand:

* Within the sample groups, support for Sample-to-item ('stmi') and dependent random access point ('drap') grouping types is required.
* Within the entity groups, support for EntityToGroupBox with grouping\_type equal to 'altr' is required.

Within the sample groups, support for audio pre-roll information (grouping type 'prol') and stream access point information (grouping type 'sap ') is required.

NOTE Although the above sample groups were defined in former versions of this document, no support was required in any brands.

* 1. The 'isob' brand

The brand 'isob' requires support for all features of the 'isoa' brand.

Support for the boxes according to Table E. 11 is required under this brand.

Table E. 11: Boxes required under the 'isob' brand

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | ttyp |  |  |  |  |  | *track type of the track* |
|  |  |  | brnd |  |  |  |  | *brand property* |

Under the 'isob' brand the restriction, given for 'isom' and its derivatives, in the media\_rate in the EditListBox is lifted and any value is permitted for the integer and fraction parts.

Under the 'isob' brand support for (flags & 1) of the TrackGroupTypeBox is mandatory.

* 1. The 'relo' brand
     1. Requirements for files

Files having the 'relo' brand among compatible\_brands of a TypeCombinationBox associated with the FileTypeBox shall be constrained as follows:

* When construction\_method equal to 0 (file\_offset) is in use for an item in ItemLocationBox, data\_reference\_index for the item shall point to a DataEntryImdaBox.
* Each data\_reference\_index value in the sample entries of all tracks shall point to DataEntryImdaBox or DataEntrySeqNumImdaBox.

NOTE 1 By including 'relo' in the compatible\_brands of TypeCombinationBox associated with a TrackTypeBox or included in ExtendedTypeBox used as an item property, it is possible to limit the scope of the constraints above to individual tracks or items.

A file having the 'relo' brand in the compatible\_brands of a TypeCombinationBox associated with the FileTypeBox shall be accompanied by a BoxFileIndexBox that indexes the file and is provided separately from the file, for example using the fileindex MIME parameter with the file. The BoxFileIndexBox shall contain FrontPartBox including imda\_identifier for each IdentifiedMediaDataBox. BoxFileIndexBox, FrontPartBox, and the fileindex MIME parameters shall be as specified in ISO/IEC 23001-14[10].

NOTE 2 Rather than traversing the top-level boxes of the file, parsers can use the BoxFileIndexBox to conclude the byte locations of each IdentifiedMediaDataBox referred to by the DataReferenceBox(es).

* + 1. Requirements for readers

Support for the boxes according to Table E. 12 is required under this brand.

Table E. 12: Boxes required under the 'relo' brand

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| imda |  |  |  |  |  |  |  | *identified media data* |
|  |  |  | imdt |  |  |  |  | *data entry of imda* |
|  |  |  | snim |  |  |  |  | *data entry sequence number for imda* |

When a data reference refers to an IdentifiedMediaDataBox of the containing file but no IdentifiedMediaDataBox with imda\_identifier equal to the imda\_ref\_identifier given in the data reference is present in the file, readers shall omit the processing of the associated track or item. Furthermore, readers shall omit the processing of any tracks or items depending on such an associated track or item, for example through a track reference or an item reference.

* + 1. Use cases (informative)
       1. File editing

When the 'relo' brand is in use, removal and addition of tracks and items can be done as described below.

When a track or item is added into a file complying with the 'relo' brand, its media data can be included in a new IdentifiedMediaDataBox. The MovieBox is appended with a new TrackBox or item information. The location offset information of the tracks or items that were already present in the file does not have to be updated, because the offsets are relative to the IdentifiedMediaDataBox that carries the respective media data. The location offset information of the added track or item is relative to the newly added IdentifiedMediaDataBox and is hence also straightforward to compute. It is easy to locate the amended MovieBox into the beginning of the file, because no location offsets depend on the size of the boxes preceding the IdentifiedMediaDataBoxes in the file order.

When a track or item is removed from a file complying with the 'relo' brand, it can be checked if no other media data than that of the removed track or item is present in the IdentifiedMediaDataBox. If so, the IdentifiedMediaDataBox can be removed without affecting the location offsets of the remaining tracks or items. Likewise, the TrackBox or the item information can be removed from the file without a need to re-compute the location offsets of the remaining tracks and items.

A file editor can maintain a file index that is a data structure containing the box types and either the sizes or byte ranges of all the file-level boxes and the imda\_identifier values of all instances of IdentifiedMediaDataBox. The file editor should be able to output the file index data structure formatted as a BoxFileIndexBox.

* + - 1. Partial image file reception

In the file writing, the following two steps are carried out:

* A file with 'relo' brand and with image items as specified in ISO/IEC 23008-12 (HEIF) is created, and each image item is located in its own IdentifiedMediaDataBox.
* A BoxFileIndexBox for the HEIF file is created as a sequence of BoxIndexBoxes and has the following structure:

BoxIndexBox {  
 indexed\_box\_type = 'ftyp';  
 indexed\_box\_size = X1;  
}  
BoxIndexBox {  
 indexed\_box\_type = 'etyp';  
 indexed\_box\_size = X2;  
}  
BoxIndexBox {  
 indexed\_box\_type = 'meta';  
 indexed\_box\_size = X3;  
}  
BoxIndexBox {  
 indexed\_box\_type = 'imda';  
 indexed\_box\_size = X4;  
 FrontPartBox { box\_content[4]; // containing imda\_identifier  
 }  
}  
... // one BoxIndexBox per IdentifiedMediaDataBox  
BoxIndexBox {  
 indexed\_box\_type = 'imda';  
 indexed\_box\_size = X5;  
 FrontPartBox {  
 box\_content[4]; // containing imda\_identifier  
 }  
}

* The file is made available for downloading e.g. in a web page, by referring to its HTTP URL and providing its MIME media type, including the fileindex parameter.

Reception of a subset of the image items is enabled by:

* parsing the file index from the fileindex parameter,
* concluding from the file index the byte ranges for the FileTypeBox, the ExtendedTypeBox, and the root-level MetaBox,
* fetching the FileTypeBox, the ExtendedTypeBox, and the root-level MetaBox with a byte range request,
* determining which image items are of interest based on the item information in the MetaBox,
* resolving from the file index the byte ranges of the IdentifiedMediaDataBoxes containing the image items of interest,
* fetching the concluded byte ranges,
* creating a local file by concatenating all the fetched byte ranges, and
* when the reader expects a file index as input, pruning the parsed file index by keeping only the top-level BoxIndexBoxes of the received top-level boxes.

The local file is a compliant HEIF file with the 'relo' brand.

* 1. The 'isoc' brand

The brand 'isoc' requires support for all features of the 'isob' brand. Support for the boxes according to Table E. 13 is required under this brand.

Table E. 13: Boxes required under the 'isoc' brand

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | !mov |  |  |  |  |  | *compressed movie* |
|  |  | !six |  |  |  |  |  | *compressed segment index* |
|  |  | !ssx |  |  |  |  |  | *compressed subsegment index* |
|  |  | !mof |  |  |  |  |  | *compressed movie fragment* |
|  |  | otyp |  |  |  |  |  | *original file type box* |

* 1. The 'comp' brand

The 'comp' brand indicates that the file conforms to the compressed box requirements of 8.19 and that a reader is required to conform to the reader requirements of that subclause.

Under this brand, , a reader shall process an OriginalFileTypeBox (if present).

NOTE There are a number of ways to mark a file as using compression and requiring decompression, including:

• The use of the 'isoc' brand, in combination with brands that permit (or do not forbid) compression.

• This brand ('comp') probably with little else, in the main type box (e.g. FileTypeBox or SegmentTypeBox), followed by an OriginalFileTypeBox; the full file is delivered and described by doing the decompression, and then using the OriginalFileTypeBox

• This brand ('comp') with brands that permit (or do not forbid) compression, in the main type box (e.g. FileTypeBox or SegmentTypeBox), without an OriginalFileTypeBox;

• This brand ('comp') used in the TypeCombinationBox, without an OriginalFileTypeBox.

* 1. The 'unif' brand
     1. General

The brand 'unif' may be used to indicate unified handling of identifiers, for example across tracks, track groups, entity groups, and file-level MetaBoxes. The consequences are

* that a given identifier identifies at most one of those (or nothing at all); for example, there is no identifier which is used to label both a track and an entity group;
* that where an identifier is restricted, without this brand, to refer to a particular type (e.g. to a track by track\_ID) that reference is no longer so restricted, and can refer to any type (e.g. to a track group), if the semantics of the reference permit it.

It is recommended that this brand be used in the ExtendedTypeBox, in combination with the brands of other specifications which readers must support.

There are three levels:

1. file-level: comprising tracks, track groups, and items and entity groups in a MetaBox not contained in any other box;
2. movie-level: a MetaBox contained in a MovieBox
3. track-level: a MetaBox contained in a TrackBox
   * 1. Requirements for files

The set of types so unified are, at file-level:

* track\_ID in the TrackHeaderBox in all tracks;
* track\_group\_id in the TrackGroupTypeBox of a TrackGroupBox in all tracks;
* item\_ID value in ItemInfoBox in a file-level MetaBox
* group\_id in an EntityToGroupBox in the GroupsListBox in the file-level MetaBox

The set of types so unified are, at movie-level or track-level:

* item\_ID value in ItemInfoBox in the MetaBox at that level
* group\_id in an EntityToGroupBox in the GroupsListBox in the MetaBox at that level

In files compliant with this brand, there shall not be two IDs with the same value in the same level.

In the MovieHeaderBox, the value of next\_track\_ID shall be larger than the largest identifier value in use at file level. If this value is equal to all 1s (32-bit maxint), and an identifier is needed, then a search must be made in the file for an unused identifier value.

NOTE The uniqueness of entity group IDs and item IDs in a MetaBox is required, at any level, irrespective of this brand.

References used in boxes using reference by ID, such as TrackReferenceBox or ItemReferenceBox, only resolve within a given level. References do not cross levels. A reference to an identifier that is not present at the same level does not resolve.

* + 1. Requirements for readers

A reader supporting this brand shall locate the target of the reference using an ID by checking the IDs of the unified types at the same level (file, movie, track) as permitted by the semantics of the reference in question.

* 1. The 'isod' brand

The brand 'isod' requires support for all features of the 'isoc' brand. Support for the boxes according to Table E. 14is required under this brand.

Table E. 14: Boxes required under the 'isod' brand

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  | hdlp |  |  |  |  |  | *handler property* |
|  |  |  |  | spki |  |  |  | *sample packing information* |
|  |  |  | prsl |  |  |  |  | *preselection group* |

Support for the following is required under this brand:

* The associated external stream 'aest' track reference shall be supported.
* Sample-packed tracks shall be recognized.
* The SampleGroupDescriptionBox with version equal to 3, which describes an essential sample group, shall be supported.
* Within the sample groups, support for EDRAP sample group (grouping type 'edrp') and essential descriptions hierarchy sample group (grouping type 'esgh') is required.
* Support for track\_in\_movie flag is required.

A file that is indicated to conform to the 'isod' brand shall be constrained with the same constraints that apply files conforming to the 'isoc' brand except the following:

* The presence of a HandlerBox in the MetaBox is optional unless specified otherwise in subclause 8.11.1.1.

1. (normative)  
     
   MIME type registration of segments
   1. Overview

This annex provides the formal MIME registration of media segments formatted according to 8.16.

* 1. Registration

MIME media type name: video

MIME subtype name: iso.segment

Required parameters: none

Optional parameters: as specified by RFC 6381 and its successors

Encoding considerations: as for video/mp4

Security considerations: See section 4 of RFC 4337.

Interoperability considerations: A number of interoperating implementations exist within the ISO/IEC 14496 community, and that community has reference software for reading and writing the file format.

Published specification: ISO/IEC 14496-12

Applications: Multimedia

Additional information:

Magic number(s): none

File extension(s): m4s

Macintosh File Type Code(s): None

Intended usage: Common

1. (informative)  
     
   URI-labelled metadata forms
   1. UUID-labelled metadata

The format of the URI for UUID-labelled metadata is defined in IETF RFC 4122.

There are no general statements about the form of the primary metadata, the initialization data for temporal metadata, or the temporal metadata itself. The form of all of these depends on the precise UUID and its definition.

Note that UUIDs cannot easily be traced to their point of origin, and so they may be unsuitable if it is desired that recipients of metadata be able to find, if needed, the associated documentation.

If traceability is needed, then a standardized metadata framework, such as MPEG-7, or a registered framework, such as SMPTE, or a de-referencable URL should be used.

* 1. ISO OID-labelled metadata

When OID-labelled metadata is carried the URI form defined in IETF RFC 3061 shall be used.

There are no general statements about the form of the primary metadata, the initialization data for temporal metadata, or the temporal metadata itself. The form of all of these depends on the precise object identifier and its definition.

A number of more specific labelling systems can also be expressed as object identifiers. The more specific UUID form should be used.

Object identifiers starting {joint-iso-itu(2) uuid(25)} (i.e. starting urn:oid:2.25) should not be used; UUID URIs should be used directly.

Object identifiers starting {iso(1) identified-organizations(3) SMPTE(52) metadata-dictionary(1)} (i.e. urn:oid:1.3.52.1) should not be used, nor should any other OID being used as a label according to SMPTE 298M or 336M; the more specific SMPTE URI form should be used.

Object Identifiers are registered to specific organizations, and so it may be possible to identify the organization owning a particular identifier. However, some sections of the object identifier tree are delegated to unregistered uses (such as UUIDs, as noted above), and traceability is then lost.

If traceability is needed, then a standardized metadata framework, such as MPEG-7, or a registered framework, such as SMPTE, or a de-referencable URL should be used.

* 1. SMPTE-labelled metadata

The format of the URI for SMPTE-labelled metadata is in IETF RFC 5119[24].

The primary metadata is exactly the value (V) part of a KLV (key, length, value) triplet as defined in SMPTE 336[31], with the key being the label given in the URN, and the length (L) being derived from the item length.

Similarly, each temporal metadata sample is the value (V) part of a KLV, where the key is the URN label given in the matching sample entry, and the length (L) is derived from the sample size (as given in the sample size or compact sample size tables).

The initialization data may be present. It contains the key (K) and value (V) of a KLV that provides an initialization context for the KLVs formed from the samples, with the length (L) being derived from the DataBox size. The first 16 bytes are a SMPTE label of the initialization data, stored as defined in SMPTE 336[31], followed by the data.

The typical value of these bytes, as defined in SMPTE 377M, is ‘primer pack’ (in hexadecimal): 06 0E 2B 34 02 05 01 01 0D 01 02 01 01 05 01 00. If the label of the initialization data does not, in fact, identify a structure giving context information (such as a primer pack), the behaviour is undefined. This enables each sample to be a local set. The rules for the construction of local sets, as defined in SMPTE 377M, shall be followed.

SMPTE 377M uses locators to locate other resources outside the metadata itself. For static metadata, these should use the ItemLocationBox in the MetaBox. For temporal metadata, external pointers may be used directly.

The initialization data may be absent, and the label then identifies a specific metadata item (e.g. a geographic locator) not needing a context.

1. (informative)  
     
   Processing of RTP streams and reception hint tracks
   1. General
      1. Overview

This Annex provides recommendations for recording of RTP streams and the use of recorded RTP streams for playback and re-sending.

* + 1. Structure

This annex is organized as follows:

* H.2 introduces the potential sources why the playback of RTP streams might become unsynchronized and provides an overview how proper synchronization is facilitated in recording and playback. It precedes the other clauses, because both the recording unit and the player have to take actions to achieve proper synchronization.
* H.3 provides recommendations for storing RTP streams.
* H.4 provides recommendations how to play files containing recorded RTP streams.
* H.5 provides recommendations for re-sending received RTP streams stored in files as described in H.3.
  + 1. Specific definitions

Within the context of this annex:

* a player is an entity that parses a file, decodes at least a subset of the tracks in the file, and renders the decoded tracks;
* a recording unit is an entity that receives one or more packet streams of encapsulated and compressed media and stores the received media into a file;
* a re-sending unit is an entity that parses a file containing media that originates from one or more received packet streams of encapsulated and compressed media and transmits at least a subset of the media stored in the file.
  1. Synchronization of RTP streams

There are several potential sources of unsynchronized playback for received RTP streams. When RTP streams are recorded as RTP reception hint tracks, the necessary information for guaranteeing synchronized playback is also recorded. When RTP streams are recorded as media tracks, the synchronization of the playback of the media tracks has to be guaranteed by creating the composition times of the media samples appropriately. The following list describes the sources of unsynchronized playback for received RTP streams, summarizes the recommended synchronization means, and points to the relevant clauses for further information.

1. The RTP timestamp of the first packet of the stream has a random offset. Hence, the RTP timestamps of two streams are shifted by the difference of their initial random offsets even if the potentially different clock rate of the RTP timestamps of the different streams were compensated. The random offset ought to be reflected in the value of the offset field of the timeoffset box of the referred reception hint sample entry as described in H.3.5.
2. The first received and recorded packet of the different streams do not necessarily have an identical playback time as discussed in H.3.2. The unequal start time of the different recorded streams is compensated by parsing one or more RTCP sender reports to derive the playback time as the wallclock time of the sender and creating an initial offset of the playback using the EditListBox as described in H.3.2. The EditListBox is interpreted by the player as described in H.4.4.
3. There is no guarantee that the clock for producing the RTP timestamps of a certain RTP stream runs at the same pace as the wallclock time of the sender, which is used to create the RTCP Sender Reports. For example, the RTP timestamps can be generated on the basis of a constant sampling frequency, e.g. 44.1 kHz for audio, and hence governed by the clock rate of the audio capturing hardware. However, the RTCP Sender Reports can be generated according to the system clock running at a different pace than the clock of the audio capturing hardware. Moreover, the clock used to generate RTP timestamps for audio might run at a different pace than the clock used to generate RTP timestamps for video (when both a normalized to the same clock tick frequency).

A similar problem in the player arises if the clock pacing the output of a decoded stream runs at a different pace than the wallclock of the player or the clocks pacing the rendering of different decoded streams are not synchronized.

The recommended approach for all these potential problems of clocks running at a different pace is to use RTCP sender reports to align the RTP timestamps of different streams onto the same wallclock timeline, which is used for inter-stream synchronization. This alignment can be done while recording the streams by modifying the representation of the recorded RTP timestamps or while playing the recorded streams by using the recorded RTCP sender reports as described in H.3.6. Moreover, it is recommended to pace the playback according to the audio playout rate as described in H.4.4.

1. The wallclock of the sender possibly run at a different pace than the wallclock of the player.

It is recommended to play a recorded program at the pace of the wallclock of the player and to use the audio playout clock as the wallclock of the player. Consequently, the audio timescale does not typically have to be modified. Even if the wallclock of the player ran at a different pace than the wallclock of the sender, it is typically unnoticeable.

Pacing of the output of decoded media samples is described in H.4.4.

* 1. Recording of RTP streams
     1. Overview

Recording of RTP streams can result into three basic file structures.

1. A file containing only RTP reception hint tracks. No media tracks are included. This file structure enables efficient processing of packet losses, but only players capable of parsing RTP reception hint tracks can play the file.
2. A file containing only media tracks. No RTP reception hint tracks are included. This file structure allows existing players compliant with the earlier versions of the ISO base media file format process recorded files as long as the media formats are also supported. However, sophisticated processing of transmission errors is not possible due to reasons explained in subsequent clauses.
3. A file containing both RTP reception hint tracks and media tracks. This file structure has both the benefits mentioned above and is recommended to be used for as good interoperability as possible with other file formats derived from the ISO base media file format.

If an RTP stream being recorded is protected, a protected RTP reception hint track is used instead of an RTP reception hint track, while the operation of the recording unit remains unchanged otherwise. At the time of playback, the data included in the protected RTP reception hint track is unprotected first and then processed similarly to a conventional unprotected RTP stream. Alternatively, the RTP stream can be unprotected before storing it as a RTP reception hint track, but then care has to be taken that the rights to use the content in the protected RTP stream are obeyed.

Some of the recording operations are common for all the three file structures, while others differ. Table H.1 indicates which recording operations are required for the basic file structures.

Table H.1: RTP Recording Operations

|  |  |  |  |
| --- | --- | --- | --- |
|  | **File containing only RTP reception hint tracks** | **File containing only media tracks** | **File containing both RTP reception hint tracks and media tracks** |
| Compensation for unequal starting position of received RTP streams (H.3.2) | no, when RTCP reception hint tracks are stored; yes, otherwise | yes | no, when RTCP reception hint tracks are stored; yes, otherwise |
| Recording of SDP (H.3.3) | yes | no | yes, for RTP reception hint tracks only |
| Creation of a sample within an RTP reception hint track (H.3.4) | yes | no | yes, for RTP reception hint tracks only |
| Representation of RTP timestamps (H.3.5) | yes | no | yes, for RTP reception hint tracks only |
| Recording operations to facilitate inter-stream synchronization in playback (H.3.6) | yes | yes, the composition times of media tracks ought to be compensated as described in H.3.6.3 | yes |
| Representation of reception times (H.3.7) | yes | no | yes, for RTP reception hint tracks only |
| Creation of media samples (H.3.8) | no | yes | yes, for media tracks only |
| Creation of hint samples referring to media samples (H.3.9) | no | no | yes |

Some implementations can record first to RTP reception hint tracks only and create a file with a combination of media tracks and RTP reception hint tracks off-line.

* + 1. Compensation for unequal starting for position of received RTP streams

When the recording of RTP streams is started, it can happen that the presentation time of the first media sample in one RTP stream is not equal to the presentation time of the first media sample in another RTP stream at least due to the following reasons:

* The sampling frequency of audio and video typically differ.
* Audio and video streams are not perfectly interleaved in terms of presentation times in transmission order.

If RTCP reception hint tracks are stored, the compensation for unequal starting position of received RTP streams ought to be done at playback time and no EditListBox concerning RTP reception hint tracks ought to be created. If RTCP reception hint tracks are not stored or if media tracks are stored it is essential that the recording unit indicates the relative initial delay of the streams in order to synchronize audio and video correctly at the beginning of the playback of the streams as described subsequently in this clause. The recording unit ought to perform the following operations.

1. An RTCP sender report indicates which RTP timestamp corresponds to the wallclock time of the time instant the report was sent. At least the first RTCP sender report for each RTP stream ought to be parsed in order to establish an equivalence of an RTP timestamp of each RTP stream and a wallclock time of the sender. The wallclock timestamp of the earliest received RTP packet, in presentation order, is derived for each RTP stream by simple linear extrapolation.
2. The smallest wallclock timestamp derived above among all the received RTP streams is mapped to presentation timestamp zero in the movie timeline, i.e., is presented immediately at the beginning of the playback of the recorded file. The movie timeline is the master timeline for the playback of the file.
3. The media timeline for each track starts from 0. In order to shift the media timeline to a correct starting position in the movie timeline, an EditBox and an EditListBox are created for each of the other RTP tracks (which do not contain a packet having the earliest wallclock timestamp) as follows:
4. The EditListBox contains two entries:
5. The first entry is an empty edit (indicated by media\_time equal to -1), and its duration (edit\_duration) is equal to the difference of the presentation times of the earliest media sample among all the RTP streams and the earliest media sample of the track. Figure H.1 presents an example of how the edit\_duration of the first entry in an EditListBox is derived.
6. The value of media\_time of the second entry is equal to the composition time of the earliest sample in presentation order, and the value of edit\_duration of the second entry spans over the entire track. As the actual duration of the track might not be known at the time of creating the EditListBox, it is recommended to set the edit\_duration equal to the maximum possible value (either the maximum 32-bit unsigned integer or the maximum 64-bit unsigned integer, depending on which version of the box is used).

The value of media\_rate\_integer is equal to 1 in both the entries of the EditListBox.



Figure H.1 — Example of an EditListBox to compensate the unequal starting of the received RTP streams, edit\_duration is copied to the first entry of the EditListBox

Some recording units are able to detect packets from which decoding can be started, which are here referred to as random access points. An IDR picture of an H.264/AVC stream is an example of a random access point. If a stream contains a packet having the earliest wallclock timestamp among all the received streams and the same stream contains packets preceding, in decoding order, the first random access point of the stream, it is recommended not to store the packets preceding the first random access point of the stream and not to consider them when determining the earliest wallclock timestamp among all the received streams.

* + 1. Recording of SDP

The SDP is recommended to be stored as follows. Session-level SDP, i.e., all lines before the first media-specific line (“m=” line), are recommended be stored as movie SDP information within the UserDataBox, as specified in 9.1.4.2. Each media-level section within the SDP description starts with an 'm=' line and continues to the next media-level section or the end of the whole session description. Each media-level section is recommended be stored as Track SDP information within the UserDataBox of the corresponding RTP reception hint track.

* + 1. Creation of a sample within an RTP reception hint track

It is recommended that each sample represents all received RTP packets that have the same RTP timestamp, i.e., consecutive packets in RTP sequence number order with a common RTP timestamp. The RTPsample structure is set to contain one RTPpacket structure per each received RTP packet having the same RTP timestamp. Each RTPpacket is recommended to contain one packet constructor of type 2 (RTPsampleconstructor). An RTPsampleconstructor copies a particular byte range, indicated by the sampleoffset and length fields of the constructor, of a particular sample, indicated by the samplenumber field of the constructor, by reference into the packet payload being constructed. The payload of each received RTP packet having the same RTP timestamp is copied to the extradata section of the sample. The track reference of each constructor is set to point to the hint track itself, i.e., is set equal to -1, and sampleoffset and length are set to match to the location and size of the packet payload within the sample.

Figure H.2 presents a pseudo-code example of an RTP reception hint sample, which contains two RTP packets.



Figure H.2 — Example of a RTP reception hint sample containing two packets  
(their header and payload)

The use of an error occurrence indexing event to indicate an RTP packet loss is not recommended, because the RTPsequenceseed field can be used for detecting packet losses without any increase in the storage space. Furthermore, the minimum unit the error occurrence event can refer to is a sample (in an RTP reception hint track). Since a sample can contain many packets, it is ambiguous which ones of these packets the error occurrence indexing event concerns.

* + 1. Representation of RTP timestamps

RTP timestamps are represented in a RTP reception hint track by a sum of three values, one of which is the decoding time DT in the media timeline of the track. The decoding time is run-length coded into the TimeToSampleBox and additionally to one or more TrackRunBoxes, if a sample resides in a movie fragment. The TimeToSampleBox includes a number of sample\_count and sample\_delta pairs, where sample\_delta is the decoding time increment (i.e., the sample duration in terms of decoding time) for each sample in a set of consecutive samples, the number of which equals to sample\_count. The TrackRunBox indicates one pair of sample\_count and sample\_duration, where sample\_duration is the decoding time increment (i.e., the sample duration) for each sample in a set of consecutive samples, the number of which equals to sample\_count. Each TrackFragmentBox can contain a number of TrackRunBoxes. The decoding time DT(i) for sample number i is derived by summing up the sample durations of all the samples preceding sample i from the TimeToSampleBox and, if needed, the TrackRunBoxes referring to any sample preceding sample i.

The RTP timestamp for sample i, RTPTS(i), is represented by a sum of three values specified as follows:

RTPTS(i) = (DT(i) + tsro.offset + offset) mod 232 (H.1)

where tsro.offset is the value of offset in the timeoffset box of the referred reception hint sample entry and offset is the value included in the rtpoffsetTLV box in the RTPpacket structure, and mod is the modulo operation.

A timeoffset box ought to be present in RTP reception hint sample entries. The value of offset in any timeoffset box of a track ought to be equal to the RTP timestamp of the first packet of the respective stream in RTP sequence number order.

Provided that no wrap-around of the RTP timestamp values over the maximum 32-bit unsigned integer happened between sample i-1 and i, the difference between consecutive unequal RTP timestamps, in RTP sequence number order, is

RTPTS\_DIFF(i) = RTPTS(i) – RTPTS(i – 1) for any i > 1 (H.2)

RTPTS\_DIFF(i) remains unchanged, when the frame rate is constant, the number of frames in any packet is constant, and the transmission order is the same as the presentation order. These constraints are typically met by audio streams and temporally non-scalable video streams. If RTPTS\_DIFF(i) is a constant denoted as RTPTS\_DIFF, the following is recommended. The value of sample\_delta in the TimeToSampleBox and, if movie fragments are used, the value of sample\_duration in the TrackRunBox(es) are set to RTPTS\_DIFF, which results into compact TimeToSampleBox and TrackRunBoxes. The rtpoffsetTLV box ought not to be used within the RTP reception hint samples, if RTCP reception hint tracks are used (see H.3.6). Otherwise (if RTCP reception hint tracks are not used), offset in the rtpoffsetTLV box ought to be set to 0.

When temporal scalability is used in a video stream, the transmission order and the playback order of packets are not identical, RTP timestamps do not increase as a function of RTP sequence number, and RTPTS\_DIFF(i) is not constant. However, RTP timestamps typically have a constant behaviour in periods determined by the GOP\_size, which is one plus the number of pictures between two consecutive pictures in the lowest temporal level in RTP sequence number order. For example, if two non-reference pictures are coded for each pair of reference pictures as illustrated in Figure H.3, GOP\_size is equal to 3. Figure H.4 presents an example of a hierarchically temporally scalable bitstream with GOP\_size equal to 4.

In these diagrams RTP sequence numbers (SN) are normalized to start from 0, and one packet per frame is assumed. RTP timestamps (TS) are normalized to start from 0 and indicated as clock ticks lasting one frame interval. Inter prediction arrows are indicated for the first GOP only, while pictures in other GOPs are predicted similarly.



Figure H.3 — Example of a temporally scalable bitstream with GOP\_size equal to 3



Figure H.4 — Example of a hierarchically temporally scalable bitstream with GOP\_size equal to 4

The RTP timestamp increment caused by one GOP is derived as follows, when no wrap-around of the RTP timestamp values over the maximum 32-bit unsigned integer happened between sample i and i + GOP\_size, inclusive:

RTPTS\_GOP\_DIFF(i) = RTPTS(i + GOP\_size) – RTPTS(i) (H.3)

If RTPTS\_GOP\_DIFF(i) is a constant equal to RTPTS\_GOP\_DIFF, when no sample i, i + 1, …, i + GOP\_size is a picture starting a so-called closed group of pictures, such as an IDR picture of H.264/AVC streams, the following is recommended. The value of sample\_delta in the TimeToSampleBox and, if movie fragments are used, the value of sample\_duration in the TrackRunBox(es) are set to RTPTS\_GOP\_DIFF / GOP\_size. The rtpoffsetTLV box ought not to be used for pictures in the lowest temporal level, if RTCP reception hint tracks are used (see H.3.6). Otherwise (if RTCP reception hint tracks are not used), offset in the rtpoffsetTLV box ought to be set to 0. The value of offset in the rtpoffsetTLV box is recommended to be set for pictures in other temporal levels to such that Formula (H.1) is fulfilled. Figure H.5 indicates how the decoding time and offset are set for a hierarchically temporally scalable video bitstream presented in Figure H.4. In this example, the decoding time increment between samples is set equal to RTPTS\_GOP\_DIFF / GOP\_size to have a compact encoding decoding times. The value of offset in the rtpoffsetTLV box is adjusted for each sample to store a representation of the RTP timestamp. For this illustration, RTP timestamps and decoding times are normalized to start from 0 and indicated as clock ticks lasting one frame interval.



Figure H.5 — Example of setting the decoding time (DT) and the value of offset in the rtpoffsetTLV box of a hierarchically temporally scalable bitstream with GOP\_size equal to 4

If no linear and periodical behaviour of RTP timestamps is detected from the received packets, and no two received packets of different samples have the same reception time, it is recommended to set the value of sample\_delta in the TimeToSampleBox and, if movie fragments are used, the value of sample\_duration in the TrackRunBox(es) to represent the reception time of the first packet of the sample. That is, the derived decoding time DT(i) ought to be equal to the reception time of the first packet of the sample subtracted by the reception time of the first packet of the first received sample of the stream.

It is noted that composition timestamps are not explicitly indicated in the file for samples in any hint tracks. Consequently, for RTP reception hint tracks, the composition timestamps are inferred from the information related the RTP timestamps indicated in the stored packet stream. For an RTP reception hint track that is not associated with an RTCP reception hint track, the composition time of a received RTP packet is inferred to be the sum of the sample time DT(i) and the value of the offset field in the rtpoffsetTLV box including the sample. For an RTP reception hint track that is associated with an RTCP reception hint track, the composition time is inferred as follows. Let the received RTP packet having the earliest RTP timestamp within the same track have composition time equal to 0. Any remaining RTP packet has a composition time equal to the RTP timestamp difference of the present RTP packet and the earliest RTP packet in presentation order with clock drift correction similar to H.3.6.3. The composition time refers to the media timeline of the track.

* + 1. Recording operations to facilitate inter-stream synchronization in playback
       1. General

Lip synchronization, i.e., correct synchronization between recorded RTP streams, during playback can be facilitated at least with the following two means:

1. An RTCP reception hint track is generated for each RTP reception hint track. The potential clock drift between the RTP timestamp clocks of different streams is corrected at the time when the file is parsed and the media streams included in the file are decoded and played. The clock drift correction is done similarly to as would be done for RTP streams that are received and played simultaneously. This mode of operation is straightforward for the recording units. However, accessing a file from an exact playback position might be more cumbersome, because it requires compensation of the clock drift of all the recorded streams at the time of the access.
2. The potential clock drift between recorded RTP streams is corrected by modifying the RTP timestamps of one or more recorded streams. This mode of operation requires processing of RTCP sender reports at the time of recording and is hence more tedious for the recording units than creation of RTCP reception hint tracks. However, the operation of the player is straightforward.

Recording units ought to use the timestampsynchrony box [9.4.1.2] to indicate which lip synchronization approach has been used. The timestampsynchrony box includes the timestamp\_sync field. timestamp\_sync equal to 1 indicates that players ought to use RTCP reception hint tracks for lip synchronization. timestamp\_sync equal to 2 indicates that players ought to use composition timestamps for lip synchronization.

Some implementations create RTCP reception hint tracks first during the real-time recording operation and then compensate the clock drift by modifying RTP timestamps as an off-line post-processing step.

The following clauses provide more details about both approaches.

* + - 1. Facilitating lip synchronization based on RTCP sender reports

A recording unit stores all RTCP sender reports for a particular RTP stream as samples in the respective RTCP reception hint track.


* + - 1. Compensating clock drift in timestamps

It is not recommended to modify the RTP timestamps of the recorded audio streams. Such a modification would cause an audio timescale modification in the player, which is a non-trivial operation.

The recorded representation of the RTP timestamps of the video and other non-audio streams ought to be modified using the following procedure.

1. First, the wallclock timestamp *a* of a video frame is derived from the RTP timestamp corresponding to the video frame as a sum of the wallclock timestamp of the previous video frame and the difference of the RTP timestamps of the current and previous video frames in the units of the wallclock timeline.
2. Second, the playback time *b* for the video frame on the wallclock time is derived based on the RTCP Sender Reports. If no RTCP sender report that exactly indicates the wallclock time for the video frame is available, the wallclock time can be extrapolated assuming that the rate at which the RTP timestamp clock and the sender wallclock in RTCP sender reports deviates stays unchanged.
3. Third, based on the RTCP sender reports for audio, the audio RTP timestamp that is played simultaneously with the video frame at time *b* of the wallclock timeline is derived. There need not be an audio frame having exactly the derived audio RTP timestamp. The wallclock timestamp *c* of an audio sample is calculated from the derived audio RTP timestamp as a sum of the wallclock timestamp of the preceding audio frame and the difference of the RTP timestamps of the derived audio RTP timestamp and the RTP timestamp of the preceding audio frame.

The difference between *a* and *c*, if any, ought to be compensated in the fields that represent the video RTP timestamp in the file. In practice, the easiest way might be to add the difference to the offset field in the rtpoffsetTLV box, which is illustrated in Figure H.6. The other option, rewriting the TimeToSampleBox and the TrackRunBox(es) (if any), might be more cumbersome to implement, because of particular way of coding the sample times by a combination of sample counts and durations, and might require more storage space too.



**Key:**

*t* Sender's wallclock timeline

A Wallclock timestamp derived from a video RTP timestamp only

B Wallclock timestamp derived from RTCP Sender Report(s) of video

C Wallclock timestamp derived from an audio RTP timestamp only for an audio frame that is played at time *b* according to RTCP Sender Report(s) of audio

D Difference to be added to offset in the rtpoffsetTLV box of the video RTP reception hint track

Figure H.6 — Example of correcting the lip synchronization in the RTP timestamp representation

* + 1. Representation of reception times

As specified in 9.4.1.4, the reception time of a packet is indicated by the sum of the decoding time of the sample containing the packet and the value of relative\_time of the RTPpacket structure of the packet.

The reception time of the earliest received RTP packet ought to be zero, and the reception times of all subsequent packets ought to be relative to the reception time of the earliest received RTP packet.

The clock source for the reception time is undefined and can be, for instance, the wallclock of the receiver. If the range of reception times of a reception hint track overlaps entirely or partly with the range of reception times of another reception hint track, the clock sources for these hint tracks are expected to be the same.

The reception time of a packet ought to correspond to the time instant when the protocol stack layer underneath RTP, typically UDP, outputs the packet.

* + 1. Creation of media samples

Media samples are created from the received RTP packets as instructed by the relevant RTP payload specification and RTP itself. However, most media coding standards only specify the decoding of error-free streams and consequently it ought to be ensured that the content in media tracks can be correctly decoded by any standard-compliant media decoder. Handling of transmission errors therefore requires two steps: detection of transmission errors and inference of samples that can be decoded correctly. These steps are described in the subsequent paragraphs.

Lost RTP packets can be detected from a gap in RTP sequence number values. RTP packets containing bit errors are usually not forwarded to the application as their UDP checksum fails and packets are discarded in the protocol stack of the receiver. Consequently, bit-erroneous packets are usually treated as packet losses in the receiver.

The inference of media samples that can be correctly decoded depends on the media coding format and is therefore not described here in details. Generally, inter-sample prediction is weak or non-existing in audio coding formats, whereas most video coding formats utilize inter prediction heavily. Consequently, a lost sample in many audio formats can often be replaced by a silent or error-concealed audio sample. It ought to be analysed whether a loss of a video packet concerned a non-reference picture or a reference picture, or, more generally, in which level of the temporal scalability hierarchy the loss occurred. Then, it ought to be concluded which pictures are possibly not correctly decodable. For example, a loss of a non-reference picture does not affect the decoding of any other pictures, whereas a loss of a reference picture in the base temporal level typically affects all pictures until the next picture for random access, such as an IDR picture in H.264/AVC. Video tracks are not allowed to contain any samples dependent on any lost video sample.

* + 1. Creation of hint samples referring to media samples

Media samples are created from the received RTP packets as explained in H.3.8. RTP reception hint tracks are created as explained in H.3.4, but the contents of the RTPpacket structure depend on the existence of the corresponding media sample as follows.

If the packet payload of the received RTP packet is represented in a media track, the track reference of the relevant packet constructors are set to point to the media track and include the packet payload by reference. It is not recommended to have a copy of the packet payload in the extradata section of the received RTP sample in order to save storage space and make file editing operations easier to implement.

If the packet payload of the received RTP packet is not represented in a media track, the instance of the RTPpacket structure is created as explained in H.3.4.

* 1. Playing of recorded RTP streams
     1. Overview

This clause describes operations required for playback of a file containing recorded RTP streams. It is organized as follows:

* Before RTP streams can be played, the contents of the files ought to be analysed. Particularly, alternative tracks representing the same media stream ought to be identified and one of these tracks ought to be selected for decoding and playback. The coding format ought to be detected in order to conclude up front that it can be decoded by the player. These preparation operations are described in more details in H.4.2.
* If an RTP reception hint track is being processed, there are a few things to be taken into account as described in H.4.3. For example, packet losses ought to be detected and handled appropriately.
* The synchronization of the decoded media samples ought to be handled properly as described in H.4.4.
* If the RTP streams stored in a file are accessed from a position other than the beginning of the streams, proper inter-stream synchronization and decoder initialization are needed as described in H.4.5.
  + 1. Preparation for the playback

In the preparation phase for playback, the player selects which tracks are played. The basic track structure of the file is parsed first. The tracks are grouped according to which alternate group they belong to. Tracks that belong to the same alternate group are indicated by the same value of alternate\_group in the TrackHeaderBox. One track from each alternate group is selected for playback as follows.

If there is an RTP reception hint track in the alternate group, it is preferred for playback, because it contains an entire representation of the received RTP stream, unlike media tracks derived from the received RTP streams, which might use such subset of the received RTP packets that can be decoded by any standard-compliant decoder without capability for handling packet losses.

The compatibility of the player with the selected track ought to be ensured. For example, it ought to be examined whether the codec, the profile, and the level used in the track are such that the player is able to support.

The codec, profile, and level used for the coded bitstream in an RTP reception hint track can be concluded from the SDP description of the RTP stream. The SDP descriptions are stored in the movie-level index track. If SDP is unchanged throughout the file, it can be additionally stored as Movie SDP information and Track SDP information within UserDataBoxes. If Track SDP information is present, it can be parsed to find out the codec, profile, and level used for the bitstream contained in the RTP reception hint track. If Movie SDP information or Track SDP information is not present, the move-level index track is traversed to find and parse each SDP index and, consequently, the codec, profile, and level used for the bitstream contained in the RTP reception hint track.

If no RTP reception hint track exists in an alternate group, the sample entry or sample entries of the media tracks in the alternate group ought to be examined to find out which ones of them the player is able to support.

* + 1. Decoding of a sample within an RTP reception hint track

The original RTP packets can be reconstructed from an RTP reception hint sample by creating the RTP packet header from the RTPpacket structures and by resolving the constructors of the RTPpacket structures. Hence, one approach for file players to process RTP reception hint tracks is to re-create the packet stream that was received and process the re-created packet stream as if it was newly received.

The relative\_time field included in the RTPpacket structure can be used to schedule the insertion of the packet into the buffer for the RTP receiver. However, it is possibly more advisable to modify the decoding process of recorded RTP streams such a manner that the decoder output buffers are kept as full as possible in order to avoid interruptions or jerky playback caused by late packets or occasional problems in real-time decoding in systems running other processes in addition to the player.

Packet losses ought to be detected from gaps in the RTP sequence number. The reaction to packet losses depends on the particular media decoder implementation and can also depend on user preferences.

* + 1. Lip synchronization

The following steps are required for achieving correct synchronization between streams:

1. Inter-track synchronization at the start of the playback.

The starting position of the media timeline of a track can be shifted in the movie timeline of the file as described in the following two paragraphs.

For a media track and an RTP reception hint track that is not associated with an RTCP reception hint track, an EditListBox ought to be used to shift the starting position of the media timeline within the move timeline as described in H.3.2. The media timelines of the tracks selected for playback are mapped to the movie timeline by parsing the EditListBoxes of the tracks, if present. The playback of each media track and each RTP reception hint track that is not associated with an RTCP reception hint track starts at the movie timeline position indicated in the EditListBox of the track or from the beginning of the movie timeline, if no EditListBox exists for the track.

For RTP reception hint tracks that are associated with respective RTCP reception hint tracks, the shifting of the starting position of the media timeline within the movie timeline is inferred as follows. The media timeline of the RTP reception hint track containing the earliest RTP packet (in presentation time on the sender wallclock timeline) among all RTP reception hint tracks is not shifted within the movie timeline (i.e., starts at time 0 on the movie timeline). The starting time of the media timeline of the any other RTP reception hint track is equal to the timestamp difference of the earliest RTP packets of the present track and the track containing the earliest RTP packet among all RTP reception hint tracks.

1. Reconstruction of RTP timestamps and composition times on the media timeline (H.3.5).
2. Correction of RTP timestamps and composition times based on RTCP Sender Reports, if RTCP reception hint tracks are used.

The correction is done similarly to what is described in H.3.6.3. However, instead of adding the difference between times *a* and *c* into the representation of the RTP timestamps in the file, the difference is added during the playback to the presentation times of the video frames on the movie timeline.

1. Pacing the output of the decoded media samples.

It is recommended to play a recorded program at the pace of the wallclock of the player and to use the audio playout clock as the wallclock of the player. The audio playback is arranged to be continuous at the native sampling frequency of the audio signal. A presentation clock of the player runs at the pace of the audio playback, i.e., its value is always equal to the (the number of the most frequent uncompressed audio sample that was played out) × (sampling frequency of the audio signal). The playback of the video track (and potential other continuous media tracks) is synchronized to the presentation clock of the player. In other words, when the presentation clock of the player meets the composition time of a video sample on the movie timeline, the video sample is played out.

Only if a file being simultaneously recorded and played back and if the receiver wallclocks runs faster than the sender wallclock, pacing the playback according to the rate of the receiver wallclock might not be recommended and synchronizing the rate of the receiver wallclock to the rate of the sender wallclock can be done as follows.

The pace of the sender clock is recovered by creating a relationship between the reception times (according to the receiver clock) and the respective wallclock timestamps of the sender, which are reconstructed from RTCP Sender Reports. It is recommended to use the audio playout clock as the receiver clock. As the delay in the network and in the receiver can be varying, the relation between the reception times and the respective timestamps of the sender is recommended to be averaged over a large number of received packets. A timescale multiplication factor is concluded as a result of the averaging of the relation between the reception times and the respective timestamps of the sender.

A presentation time on a timeline of the receiver clock is derived for each sample. If RTCP reception hint tracks are in use, the presentation time is the composition time of the sample on the movie timeline, also including clock drift correction as described in step 3 above. If RTCP reception hint tracks are not in use, the presentation time is directly the composition time of the sample on the movie timeline. Then, for playback purposes only, the presentation times of the samples in all tracks being played ought to be multiplied by the timescale multiplication factor.

Time stretching of the signal ought to be done accordingly. Samples are played out at their presentation times.

In practice, the timescale multiplication factor and the mapping from the RTP timeline to the wallclock of the sender (step 3 above) can be implemented as a single operation.

* + 1. Random access

Random access refers to a non-linear access to the media streams represented in the file. In other words, in a random access operation the file is accessed from another sample than that which was previously played or the file is initially accessed from a position that is not the beginning of the movie timeline.

It is recommended to provide the random access functionality to the user relative to the movie timeline of the file rather than any other timelines, such as the sender wallclock timeline. By using the movie timeline as the basis, the number of steps for a random access operation is kept low.

First, it is derived which media frames are at a desired random access position (or closest to it, if there are none exactly at the desired random access position). In the case of media tracks, RTP reception hint tracks for audio, and any RTP reception hint tracks having the timestamp\_sync field equal to 2 (indicating pre-compensated lip synchronization), the media frame closest to the desired random access position can be directly derived based on the composition timestamps (on the media timeline) shifted by the initial starting position indicated in the EditListBox, if any. In the case of non-audio RTP reception hint tracks having the timestamp\_sync field equal to 1 (indicating the use of RTCP reception hint tracks), the presentation times of samples ought to be derived as described in H.4.4, until the closest presentation time to the desired random access position is found.

Second, decoding of many media bitstreams can be started only from frames of a particular type, such an IDR picture of H.264/AVC. Player implementations can therefore have different approaches, including the following:

1. Discover the closest frame at or preceding the desired random access position from which decoding can be started, start decoding from that frame, and start rendering only from the desired random access point. This approach possibly implies some processing delay before the rendering is started.
2. Start decoding and rendering at or after the desired random access point using the earliest frame from which decoding can be started. Typically, audio playback would start earlier than video playback, but the processing delay before the rendering is started is smaller than in the previous option.
   1. Re-sending recorded RTP streams
      1. Overview

It can be a desirable operation to re-send the RTP streams that have been recorded earlier to a file. For example, if RTP streams are received through a broadcast or streaming service and recorded into a file, it can be desirable to re-send them from one device to another device in a home environment using a WLAN connection. This clause provides recommendations for re-sending of recorded RTP streams.

A communication system based on RTP includes a source endpoint (also known as a sender) and a destination endpoint (also known as a receiver) and can contain one or more mixers and translators. The sender and the receiver are the endpoints of the RTP and RTCP sessions. The behaviour of RTP translators and mixers is specified in IETF RFC 3550[17] and clarified in IETF RFC 5117[23]. In general, the recording unit receiving RTP streams and storing them into a file acts as a destination endpoint, and a re-sending unit reading stored RTP streams from a file and sending them acts as a source. Typically, the payloads of the re-sent RTP stream are not modified, which makes a combination of a recording unit and a re-sending unit acting similarly to a transport translator as described in IETF RFC 5117[23]. However, the essential characteristic of a translator is that receivers cannot detect its presence. Consequently, a combination of a recording unit and a re-sending unit cannot act as a transport translator, unless re-sending happens simultaneously with the recording of the original streams. As this case is considered rare, the discussion in this clause regards a recording unit as a destination terminating the original RTP and RTCP sessions and a re-sending unit as a source of new RTP and RTCP sessions.

This clause is organized as follows:

* H.5.2 includes recommendations how to compose RTP packets from RTP reception hint tracks and how to schedule the transmission of the RTP packets.
* H.5.3 discusses how RTCP packets ought to be generated and how received RTCP packets ought to be processed.
  + 1. Re-sending RTP packets

The packets are recommended to be constructed and transmitted as follows.

The packet payloads are recommended to be constructed according to the constructors stored in the reception hint track, i.e., the packet payloads are recommended to be identical to those received, unless a different packet size is crucial for the network to which the packets are re-sent.

* The values of the header fields for the RTP packets created as suggested by an RTP reception hint track ought to be kept the same as in the respective RTPpacket structure except for the following cases:
* The initial RTP timestamp offset and the RTP sequence number offset ought to be selected randomly regardless of the values stored in the offset field of the timeoffset box of the referred reception hint sample entry or the values of the RTPsequenceseed field of the RTPpacket structure of any for any of the packets of the respective RTP reception hint track.
* The value of the RTP timestamp field is recommended to be a sum of the random initial offset, the value of offset in the RTPpacket structure, and the decoding time of the respective RTP sample. If the sum exceeds the maximum unsigned 32-bit integer, it is recommended to be wrapped over.
* The relative increments of the RTP sequence number are recommended to be the same as those recorded in the values of the RTPsequenceseed fields. Consequently, if there was a packet loss in the stream that was recorded, the stream that is re-sent also has a respective gap in the RTP sequence number, and the receiver is able to deduce a packet loss.
* The value of the CSRC count field is always recommended to be zero, because no contributing sources of the previous RTP session that was recorded are actively modifying the streams for the RTP session for the stream being re-sent. The source identifier space (for both SSRC and CSRC) is session specific. Consequently, the CSRC list of the RTP header ought to be empty regardless of the potentially stored CSRC values for the received streams, which are included in the receivedCSRC TLV box in the RTPpacket structure.
* The value of the payload type field can be dynamically selected depending on the signalling scheme in use.
* The value of the SSRC field ought to be randomly selected and potential collisions ought to be handled as specified in IETF RFC 3550[17]. The SSRC value of a received stream can be stored in the ReceivedSsrcBox of the referred reception hint sample entry but it ought to be ignored when the stream is re-sent.
* The recorded RTP header extensions, stored in rtphdrextTLV in the RTPpacket structure, if any, ought to be re-sent only if the re-sending unit can verify that they are valid for the re-sent stream. If the re-sending unit is not able to parse the semantics of the recorded RTP header extensions, they ought not to be re-sent.

The reception time of a packet, represented by the sum of the decoding time of the RTP reception hint sample containing the packet and the value of the relative\_time of the RTPpacket structure, equals to the transmission time of the packet with a skew caused by the transmission delay and the processing delay in the protocol stack of the receiver. The skew of adjacent packets might not be equal due to transmission delay jitter and varying processing delay. Moreover, the protocol stack used when receiving the stream might differ from the protocol stack used for re-sending the stream. Due to these reasons, the reception times are often not applicable as such to pace the transmission of the re-sent packets. In all cases, the re-sending unit ought to verify that the re-sent packet stream complies with the buffering model in use, if any. If the re-sending unit can conclude that the network environments and protocol stacks used when receiving the stream and when re-sending the recorded stream are similar, reception times can be used as a basis for scheduling the packet transmission. The re-sending unit ought to make an effort to remove or conceal the transmission delay jitter in the recorded stream. If the re-sending unit is unable to conclude that the network environments and protocol stacks used when receiving the stream and when re-sending the recorded stream are similar or is uncertain which kind of packet scheduling is appropriate, it can use the decoding time as the basis for scheduling.

* + 1. RTCP processing

RTCP sender reports and other RTCP messages are regenerated following the constraints specified in IETF RFC 3550[17] rather than directly using the RTCP messages recorded in RTCP reception hint tracks, if any.

An RTCP sender report contains the wallclock time when the report was sent and the RTP timestamp corresponding to the same time as the indicated wallclock time. The RTP timestamp for an RTCP Sender Report is generated as follows. A presentation time on a timeline of a reference clock is derived for the sample corresponding the indicated wallclock time in the RTCP sender report. The reference clock can be the wallclock of the re-sending unit initialized to 0 at the beginning of the session. The sample corresponding to the indicated wallclock time might not exist in the corresponding RTP reception hint track, because the sampling instants of the samples in the RTP reception hint tracks might not match with the transmission instants of the RTCP sender reports. However, as instructed by IETF RFC 3550[17], the RTP timestamp is derived as if there was a sample in the RTP stream corresponding to the indicated wallclock time. The RTP timestamp for an RTCP sender report ought to be linearly interpolated from the RTP timestamps of the samples immediately preceding and following the wallclock time indicated in the RTCP sender report. In order to conclude the samples immediately preceding and following the wallclock time indicated in the RTCP sender report, presentation times on the timeline of the reference clock ought to be derived until the closest samples are discovered. If RTCP reception hint tracks are present for the RTP reception hint track being re-sent, the presentation time is the composition time of the sample on the movie timeline, also including clock drift correction as described in step 3 of H.4.4. If RTCP reception hint tracks are not present, the presentation time is directly the composition time of the sample on the movie timeline.

When handling the received RTCP receiver reports, it ought to be noticed that the reported cumulative number of packets lost includes also the unsent packets that were never originally received and correspond to the gaps in the RTP sequence number in the RTP reception hint tracks. Any congestion management, retransmission, or other packet loss resilience method ought to take this into account.

1. (normative)  
     
   Stream access points
   1. General

This annex defines a stream access point (SAP) and specifies six types of SAPs.

The SAP definitions and SAP types are specified in a generic manner in I.1 through I.3 so that they can be applied to any container format, i.e. also other formats than the ISO base media file format. The terms container, media stream, and bitstream are used in I.1 through I.3 as defined in ISO/IEC 23009-1[10]. I.4 specifies the interpretation of the generic SAP definitions in the context of the ISO base media file format.

A stream access point (SAP) enables random access into a container of media stream(s). A container may contain more than one media stream, each being an encoded version of continuous media of certain media type. A SAP is a position in a container enabling playback of an identified media stream to be started using only (a) the information contained in the container starting from that position onwards, and (b) possible initialisation data from other part(s) of the container, or externally available. Derived specifications should specify if initialisation data is needed to access the container at a SAP, and how the initialisation data can be accessed.

A SAP for layered media may apply to all the layers, a particular set of layers, or only a single layer in a media stream. When a SAP applies to a set of layers that use inter prediction from a layer that is not a member of the set, there may be an indication if the SAP requires the correct decoding of the reference layer.

* When SAPs are used with layered media, derived specifications should specify or provides means to indicate which layers SAPs apply to and whether SAPs require correct decoding of the reference layer.
  1. SAP properties
     1. General

For each SAP the properties, ISAP, TSAP, ISAU, TDEC, TEPT, and TPTF are identified and defined as:

* TSAP is the earliest presentation time of any access unit of the media stream such that all access units of the media stream with presentation time greater than or equal to TSAP can be correctly decoded using data in the bitstream starting at ISAP and no data before ISAP.
* ISAP is the greatest position in the bitstream such that all access units of the media stream with presentation time greater than or equal to TSAP can be correctly decoded using Bitstream data starting at ISAP and no data before ISAP.
* ISAU is the starting position in the bitstream of the latest access unit in decoding order within the media stream such that all access units of the media stream with presentation time greater than or equal to TSAP can be correctly decoded using this latest access unit and access units following in decoding order and no access units earlier in decoding order.

NOTE 1 ISAU is always greater than or equal to ISAP.

* TDEC is the earliest presentation time of any access unit of the media stream that can be correctly decoded using data in the bitstream starting at ISAU and no data before ISAU.
* TEPT is the earliest presentation time of any access unit of the media stream starting at ISAU in the bitstream.
* TPTF is the presentation time of the first access unit of the media stream in decoding order in the bitstream starting at ISAU.

For the purposes of these definitions, the SAP is the access unit that is described as located at ISAU and/or ISAP.

NOTE 2 The distinction between ISAU and ISAP is only needed to distinguish between referring directly to the access unit, and referring to its containing structure.

* + 1. SAP properties for layers

The following properties apply to layered media streams for which SAPs are indicated for one or more layers, referred to as the target layers. In the following properties, an access-unit partition refers to a unit that contains the coded data of a single time instance for the target layers, and a media stream partition refers to a sequence of access-unit partition of the target layers in decoding order.

When the target layers cover all the layers of a media stream, the following properties are equivalent to those in I.2.1.

For each SAP the properties, ISAP, TSAP, ISAU, TDEC, TEPT, and TPTF are identified and defined as:

* TSAP is the earliest presentation time of any access-unit partitions of the target layers such that all access-unit partitions of target layers with presentation time greater than or equal to TSAP can be correctly decoded using data in the media stream partition starting at ISAP and no data before ISAP.
* ISAP is the greatest position in the container of the media stream partition such that all access-unit partition of the target layers with presentation time greater than or equal to TSAP can be correctly decoded using data of the media stream partition starting at ISAP and no data before ISAP.
* ISAU is the starting position, in the media stream partition, of the latest access-unit partition in decoding order such that all access-unit partition of the target layers with presentation time greater than or equal to TSAP can be correctly decoded using this latest access-unit partition and access-unit partitions following in decoding order and no access-unit partition earlier in decoding order.

NOTE ISAU is always greater than or equal to ISAP.

* TDEC is the earliest presentation time of any access-unit partition of the target layers that can be correctly decoded using data in the media stream partition starting at ISAU and no data before ISAU.
* TEPT is the earliest presentation time of any access-unit partition of the target layers starting at ISAU in the media stream partition.
* TPTF is the presentation time of the first access-unit partition of the target layers in decoding order in the media stream partition starting at ISAU.
  1. SAP types

Six types of SAPs are defined with properties as follows:

* Type 1: TEPT = TDEC = TSAP = TPTF
* Type 2: TEPT = TDEC = TSAP < TPTF
* Type 3: TEPT < TDEC = TSAP <= TPTF
* Type 4: TEPT <= TPTF < TDEC = TSAP
* Type 5: TEPT = TDEC < TSAP
* Type 6: TEPT < TDEC < TSAP

NOTE The type of SAP is dependent only on which access units are correctly decodable and their arrangement in composition order. The types informally correspond with some common terms:

* Type 1 corresponds to what is known in some coding schemes as a “Closed GoP random access point” (in which all access units, in decoding order, starting from ISAP can be correctly decoded, resulting in a continuous time sequence of correctly decoded access units with no gaps) and in addition the access unit in decoding order is also the first access unit in composition order.
* Type 2 corresponds to what is known in some coding schemes as a “Closed GoP random access point”, for which the first access unit in decoding order in the media stream starting from ISAU is not the first access unit in composition order.
* Type 3 corresponds to what is known in some coding schemes as an “Open GoP random access point”, in which there are some access units in decoding order following ISAU that cannot be correctly decoded and have presentation times less than TSAP.
* Type 4 corresponds to what is known in some coding schemes as an "gradual decoding refresh (GDR) starting point”, in which there are some access units in decoding order starting from and following ISAU that cannot be correctly decoded and have presentation times less than TSAP.
* Type 5 corresponds to the case for which there is at least one access unit in decoding order starting from ISAP that cannot be correctly decoded and has presentation time greater than TDEC and where TDEC is the earliest presentation time of any access unit starting from ISAU.
* Type 6 corresponds to the case for which there is at least one access unit in decoding order starting from ISAP that cannot be correctly decoded and has presentation time greater than TDEC and where TDEC is not the earliest presentation time of any access unit starting from ISAU.
  1. SAP definitions for the ISO base media file format

Clause 3 defines the terms container, media stream, and bitstream for the interpretation of SAP information for files and segments compatible with the ISO base media file format.

ISAU is the first byte of the SAP sample.

The mapping of specific values and terms is further specified in 8.16.3.1.

When the file structure-data (e.g. sample duration) of the SAP sample is included in a MovieFragmentBox, ISAP is the first byte of the MovieFragmentBox for the SAP sample or the MediaDataBox containing the SAP sample, whichever is earlier in the file order. When the file structure-data of the SAP sample is included in the MovieBox, ISAP is the first byte of the MovieBox or the MediaDataBox containing the SAP sample, whichever is earlier in the file order.

The MovieBox of a file shall be made available as initialisation data for utilizing the SAP information of the file.

1. (informative)  
     
   Segment index examples
   1. General

This annex gives some examples of the use of the SegmentIndexBox, and what values are inserted in it when it is used in various different ‘styles’ or configurations.

In the following examples, the size of *i*-th SegmentIndexBox is defined as *S*i,index, the size of *i*-th subsegment, e.g. *i*-th MovieFragmentBox and MediaDataBoxes, is defined as *Si*,media, the duration of *i*-th subsegment is defined as *Di*, the number of the last subsegment is defined as *N*, and the duration of the segment is defined as *D*segment.

* 1. Examples
     1. Simple one-level indexing

This example shows a simple segment index (Figure J. 1). All entries of the top level sidx point to media content (segments comprising one or more movie fragments), i.e. reference\_type is equal to 0. The value of referenced\_size and subsegment\_duration of each entry are calculated as in Table J. 1.




Figure J. 1 Simple segment index

Table J. 1 Simple segment index

|  |  |  |  |
| --- | --- | --- | --- |
| sidx | entries | referenced\_size | subsegment\_duration |
|  | e0 | *Si* | *Di* |
| e1 | *Si*+1 | *Di*+1 |

* + 1. Hierarchical

This example shows hierarchical segment index (Figure J. 2). All entries of the top level sidx point to another SegmentIndexBox, i.e. reference\_type is equal to 1, and all entries of the second level sidx point to media content, i.e. reference\_type is equal to 0. The value of referenced\_size and subsegment\_duration of each entry are calculated as in Table J. 2.




Figure J. 2 Hierarchical segment index

Table J. 2 Hierarchical segment index

|  |  |  |  |
| --- | --- | --- | --- |
| sidx# | entries | referenced\_size | subsegment\_duration |
| *i*-th | e0 | *Si*+1,index *+ Sj*,media *+ Sj*+1,media | *Dj + Dj*+1 |
| e1 | *Si*+2,index *+ Sj*+2,media *+ Sj*+3,media | *Dj*+2 *+ Dj*+3 |
| (*i*+1)th | e0 | *Sj*,media | *Dj* |
| e1 | *Sj*+1,media | *Dj*+1 |
| (*i*+2)th | e0 | *Sj*+2,media | *Dj*+2 |
| e1 | *Sj*+3,media | *Dj*+3 |

* + 1. Daisy-chain

This example shows daisy-chained segment index (Figure J. 3). Each SegmentIndexBox has two entries, the first entry points to media content, i.e. reference\_type is equal to 0, the second (the last) entry points to next SegmentIndexBox, i.e. reference\_type is equal to 1. The value of referenced\_size and subsegment\_duration of each entry are calculated as in Table J. 3.




Figure J. 3 Daisy-chained segment index

Table J. 3 Daisy-chained segment index

|  |  |  |  |
| --- | --- | --- | --- |
| sidx# | entries | referenced\_size | subsegment\_duration |
| *i*-th | e0 | *Si*,media | *Di* |
| e1 | *Si*+1,index |  |
| (*i*+1)th | e0 | *Si*+1,media | *Di*+1 |
| e1 | *Si*+2,index |  |

* + 1. Combination hierarchical and daisy-chain

This example shows hierarchical and daisy-chained segment index (Figure J. 4), which is combination of J.2.2 and J.2.3. The value of referenced\_size and subsegment\_duration of each entry are calculated as in Table J. 4.




Figure J. 4 Combined segment index

Table J. 4 Combined segment index

|  |  |  |  |
| --- | --- | --- | --- |
| sidx# | entries | referenced\_size | subsegment\_duration |
| *i*-th | e0 | *Si*+1,index + *Sj*,media + *Sj*+1,media | *Dj* + *Dj*+1 |
| e1 | *Si*+2,index + *Sj*+2,media + *Sj*+3,media | *Dj*+2 + *Dj*+3 |
| e2 | *Si*+3,index + *Sj*+4,media |  |
| (*i*+1)th | e0 | *Sj*,media | *Dj* |
| e1 | *Sj*+1,media | *Dj*+1 |
| (*i*+2)th | e0 | *Sj*+2,media | *Dj*+2 |
| e1 | *Sj*+3,media | *Dj*+3 |
| (*i*+3)th | e0 | *Sj*+4,media | *Dj*+4 |
| e1 | *Si*+4,index |  |

1. (normative)  
     
   Use of IETF RFC 6381 for ISOBMFF files
   1. General

IETF RFC 6381[25] specifies parameters that are used with various MIME types or type/subtype combinations to allow for unambiguous specification of the codecs employed by the media formats contained within, or the profile(s) of the overall container format. This annex defines generic rules on how to use these parameters for ISOBMFF and for derived specifications. These rules may be complemented by derived specifications.

* 1. Use of the 'codecs' parameter
     1. General rules

For files based on or derived from this document, each value in the comma separated list forming the "codecs" attribute and formed by dot-separated-elements corresponds to a given track. For each track, the first element of the dot-separated-elements is obtained as follows:

* It is set to the 'format' field of the first SampleEntry (respecting case), with the following exceptions:

NOTE 1 Some but not all uses of the ISOBMFF restrict the number of sample entries in a track to one. So, there are files potentially carrying multiple sample entries in which case the codecs parameter does not describe it all.

* + If the 'format' field contains a space, the character '.', or any character not supported by the encoding of the codecs string, the "encoded" version of the codecs parameter shall be used, as defined in IETF RFC 6381[25] (i.e. using 'codecs\*').

NOTE 2 Even though this is not recommended by this document, some sample entry four-character codes are using the character '.'. Care is needed when forming the codecs value for those tracks.

* + If the 'format' field refers to a transformed sample entry the procedures in K.3 apply.
    1. Syntax

id-simple :=/ id-iso  
 id-encoded :=/ id-iso  
 id-iso := iso-gen  
 iso-gen := cpid \*( element / encoded-elm )  
 ; <element> used with <codecs-simple>  
 ; <encoded-elm> used with <codecs-fancy>  
 ;  
 ; Note that the BNF permits "." within <element>  
 ; and <encoded-elm> but "." is reserved as the  
 ; hierarchy delimiter  
 cpid := 4(octet-simple / octet-fancy)  
 ; <octet-simple> used with <codecs-simple>  
 ; <octet-fancy> used with <codecs-fancy>

* 1. The 'codecs' parameter for transformed media tracks

For a transformed media track, the 'codecs' MIME parameter (as defined in this annex) may document the original format with no transformation or only a subset of the transformations, if the environment using that parameter separately documents the existence of the omitted transformations, such as protection.

For a transformed media track, the 'codecs' MIME parameter may document the transformed format, and in that case is a comma-separated list of one or more list items.

The following process applies to derive the value for a list item of the codecs MIME parameter of a transformed media track:

1. The value of the codecs MIME parameter is initialized to be an empty string.
2. Let schemeInfoContainerBox be any ProtectionSchemeInfoBox, the RestrictedSchemeInfoBox, or the CompleteTrackInfoBox when the sample entry type of the track (i.e., the format value of a SampleEntry directly contained in the SampleDescriptionBox) indicates an encrypted, restricted, or incomplete media track, respectively.
3. Let dataFormat be equal to the data\_format value of OriginalFormatBox of schemeInfoContainerBox.
4. The value of the codecs MIME parameter is appended by dataFormat followed by a dot ('.') character.
5. When dataFormat indicates a transformed media track:
   1. If the transformation type indicates an essential sample group (scheme\_type equal to 'essg'), the value of the codecs MIME parameter is appended by the four-character code 'essg' followed by a star ('\*'), further followed by the four-character codes listed in the Essential Descriptions Hierarchy sample description, from the first entry up to but excluding the first occurrence of 'stsd' or 'cenc'. A star ('\*') shall be used to separate the four-character codes listed in the Essential Descriptions Hierarchy sample description.

NOTE It can be known from the presence of the four-character code 'essg' or the star symbol ('\*') in the value of the codecs MIME parameter that an essential sample group is used.

* 1. Otherwise, the value of the codecs MIME parameter is appended by the scheme\_type four-character code contained in the SchemeTypeBox of schemeInfoContainerBox.

1. When schemeInfoContainerBox contains instances of CompatibleSchemeTypeBox, the following applies for each instance of the CompatibleSchemeTypeBox of schemeInfoContainerBox in any order: the value of the codecs MIME parameter is appended by a plus character ('+') followed by the scheme\_type four-character code contained in the CompatibleSchemeTypeBox.
2. The value of the codecs MIME parameter is appended by a dot ('.') character.
3. If dataFormat indicates a transformed media track, schemeInfoContainerBox is updated to be any ProtectionSchemeInfoBox, the RestrictedSchemeInfoBox, or the CompleteTrackInfoBox when dataFormat indicates an encrypted, restricted, or incomplete media track, respectively. The process continues from step 3.
4. Otherwise (dataFormat does not indicate a transformed media track), the value of the codecs MIME parameter is appended by the original format string.

The original format string starts with the untransformed sample entry type indicating a coding format and follows the specifications of the 'codecs' string for that coding format.

In the process above, steps 4 and 5 describe the derivation of a scheme type string.

For example, the value of the 'codecs' MIME parameter might be 'resv.stvi.avc1'.

* 1. Use of the 'profiles' parameter

For any file format based on this document, the 'profiles' parameter, if used, shall be a comma-separated list of brands constrained as follows:

* 1. The list shall include the major-brand, followed by the compatible-brands, as listed in the FileTypeBox ('ftyp') or SegmentTypeBox ('styp'). The major-brand shall be first, and may be removed from the compatible-brands list;
  2. The list should include the brands from each TypeCombinationBox in the top-level ExtendedTypeBox in the list, and the brands from a single TypeCombinationBox shall be separated by '+'.

NOTE This document recommends that the major brand be repeated in the compatible-brands, but this requirement is relaxed in the 'profiles' parameter for compactness.

An example might be profiles="qvXt,isoc,iso8+comp", indicating that 'qvXt' (whatever that might be) is the major-brand and preferred use, that the file is compatible with the version of the base file format identified by 'isoc', and that it is also compatible with the combination of 'iso8' and 'comp'.

* 1. Use of the 'itemtypes' parameter

For files derived on this document and containing a top-level MetaBox, the 'itemtypes' parameter shall be as defined in IANA media type registration: <http://www.iana.org/assignments/media-types/image/heic> [xx] and, when used, is composed of one or more comma-separated item descriptions.

An item description should be present for the primary item of the file and may be present for other items of the file. Each item description starts with an item type string and is followed by a plus-separated ('+') list of zero or more item property strings. The item type string starts with the four-character item\_type value of the item and may be followed by zero or more dot-separated ('.') qualifiers specified by derived specifications.

* 1. Use of the 'essential' parameter

For files containing essential sample group descriptions, the 'essential' parameter, when used, is composed of one or more comma-separated essential hierarchy descriptions.

Each essential hierarchy description is composed of one or more four-character code of essential sample group descriptions, separated with a dot.

* If the 'codecs' parameter includes description of the transformation used, the listed four-character codes shall be the ones listed in the Essential Descriptions Hierarchy sample group description, in the same order, from the first code following the last occurrence of 'stsd' until the last listed code.
* Otherwise, the listed four-character codes shall be the ones listed in the Essential Descriptions Hierarchy sample group description in the same order.

NOTE Derived specifications can have different practices whether codecs contains only the untransformed sample entry type or also four-character codes for transformations and essential sample groups. If no practices of derived specifications apply, it is suggested that codecs contains also four-character codes for transformations and essential sample groups and essential contains only the post-processing transformations and essential sample groups.

Example:

An HEVC sample is encrypted by means other than indicated through a protected sample entry type. The encryption is signaled through an essential sample group of type 'FOOv'. The resulted decoded sample needs to have a post-processing filter applied, signaled through an essential sample group of type 'BARv'. The EssentialDescriptionsHierarchyEntry lists the transformations as ['FOOv', 'stsd', 'BARv'].

The 'codecs' and 'essential' MIME type sub-parameters can be:

codecs=resv.essg\*FOOv.hvc1.1.6.L186.80

essential=BARv

or

codecs=hvc1.1.6.L186.80

essential=FOOv.stsd.BARv

Bibliography

1. ISO/IEC 8859-1, *Information technology — 8-bit single-byte coded graphic character sets — Part 1: Latin alphabet No. 1*
2. ISO/IEC 13818-1, *Information technology — Generic coding of moving pictures and associated audio information — Part 1: Systems*
3. ISO/IEC 14496-14*, Information technology — Coding of audio-visual objects — Part 14: MP4 file format*
4. ISO/IEC 14496-15, *Information technology — Coding of audio-visual objects — Part 15: Carriage of network abstraction layer (NAL) unit structured video in the ISO base media file format*
5. ISO/IEC 15444-3*, Information technology —* JPEG 2000 image coding system: Motion JPEG 2000 — Part 3: Motion JPEG 2000
6. ISO/IEC 21000-17:2006, *Information technology – Multimedia framework (MPEG-21) – Part 17: Fragment Identification of MPEG Resources*
7. ISO/IEC 23000-11, *Information technology — Multimedia application format (MPEG-A) — Part 11: Stereoscopic video application format*
8. ISO/IEC 23001-14, *Information technology — MPEG systems technologies — Part 14: Partial file format*
9. ISO/IEC 23008-3, *Information technology — High efficiency coding and media delivery in heterogeneous environments — Part 3: 3D audio*
10. ISO/IEC 23009-1:2022, *Information technology – Dynamic adaptive streaming over HTTP (DASH) – Part 1: Media presentation description and segment formats*
11. Rec. ITU-R BS.1771-1, *Requirements for loudness and true-peak indicating meters*
12. IETF RFC 1864, *The Content-MD5 Header Field*, October 1995
13. IETF RFC 2616, *Hypertext Transfer Protocol — HTTP/1.1*, June 1999
14. IETF RFC 3926, *FLUTE - File Delivery over Unidirectional Transport*, October 2004
15. IETF RFC 3450, *Asynchronous Layered Coding (ALC) Protocol Instantiation*, December 2002
16. IETF RFC 3451, *Layered Coding Transport (LCT) Building Block*, December 2002
17. IETF RFC 3550, *RTP: A Transport Protocol for Real-Time Applications*, July 2003
18. IETF RFC 3551, *RTP Profile for Audio and Video Conferences with Minimal Control*, July 2003
19. IETF RFC 3695, *Compact Forward Error Correction (FEC) Schemes*, February 2004
20. IETF RFC 3986, *Uniform Resource Identifier (URI): Generic Syntax,* January 2005
21. IETF RFC 3987, *Internationalized Resource Identifiers (IRIs)*, January 2005
22. IETF RFC 4771, *Integrity Transform Carrying Roll-Over Counter for the Secure Real-time Transport Protocol (SRTP)*, January 2007
23. IETF RFC 5117, *RTP Topologies*, January 2008.
24. IETF RFC 5119, *A Uniform Resource Name (URN) Namespace for the Society of Motion Picture and Television Engineers (SMPTE)*, February 2008
25. IETF RFC 6381, *The* 'Codecs' *and* 'Profiles' *Parameters for "Bucket" Media Types*, August 2011
26. ICC.1:2001-04, *File format for color profiles*, International Color Consortium
27. The Unicode Standard, https://www.unicode.org/versions/latest/
28. 3GPP TS 26.244, *3GPP file format (3GP)*
29. 3GPP TS 26.346, *Multimedia Broadcast/Multicast Service (MBMS); Protocols and codecs*
30. SMPTE RP 177, *Derivation of Basic Television Color Equations*; Society of Motion Picture and Television Engineers (SMPTE), 1993
31. SMPTE ST 336:2017 *Data Encoding Protocol Using Key-Length-Value*
32. EBU – Tech 3341, *Loudness Metering: EBU mode metering to supplement loudness normalization in accordance with EBU R128*
33. EBU – Tech 3342, *Loudness Range: A measure to supplement loudness normalisation in accordance with EBU R 128*
34. ATSC Doc. A/52:2012, *ATSC Standard: Digital Audio Compression (AC-3, E-AC-3)*
35. *Consumer Technology Association CTA-861-G*, A DTV Profile for Uncompressed High Speed Digital Interface